

**Research & Vehicle Technology**

**“Infotainment Systems Product Development”**

**Feature – Wi-Fi Hotspot**

**TCU Infotainment Subsystem Part Specific Specification (SPSS)**

Version 1.9

**UNCONTROLLED COPY IF PRINTED**

**Version Date: April 28, 2017**

**FORD CONFIDENTIALF**

**Revision History**

|  |  |  |  |
| --- | --- | --- | --- |
| **Date** | **Version** | **Notes** | |
| **September 4, 2015** | **1.0** | **Initial Release** |  |
|  |  |  |  |
| **November 30, 2015** | **1.1** | **Updated Release** |  |
|  | WFHS-STR-286735/B-Logical Signal Mapping | | jshelby5: Clarification: divided CarrierDataNotification\_St into two CAN signals. Clarification: Added the signal WifiHotspotMAC\_Rq Clarification: Added the signal TelematicsService\_St Clarification: Deleted NumberOfConnectedDevices\_St Clarification: added CarMode\_St and PowerMode\_St. Clarification: added VehicleGGCCData |
|  | WFHS-IIR-REQ-179285/B-WifiHotspotServer\_Tx | | MBORREL4: Added WifiHotpotMAC\_Rsp and TelematicsService\_St. Removed NumberOfConnectedDevices\_St |
|  | MD-REQ-179304/B-CarrierDataNotification\_St | | MBORREL4: Removed DataPlanExpired state, renumbered PercentDataUsed to 0x2 |
|  | MD-REQ-179305/B-TCUAvailability\_St | | MBORREL4: Updated literals to "Disabled" and "Enabled" |
|  | MD-REQ-179308/B-CarrierInfo\_Rsp | | MBORREL4: Removed MSISDN and updated signal to include two phone numbers (Ford & Lincoln) |
|  | MD-REQ-179309/B-DataUsage\_Rsp | | MBORREL4: Updated all parameters to now include CounterHour/Minute/Second, PlanType, ExpiryRenewal Date/Month/Day/Year/Hour/Minute/Second, DataUsed & TotalData (to 2 decimal places), OverageFlag, DataPlanStatus. Added Invalid values to DataUsedUnits, TotalDataUnits, and OverageFlag |
|  | MD-REQ-179310/B-DeviceList\_Rsp | | MBORREL4: Updated to remove BlackList encoding |
|  | MD-REQ-195174/A-WifiHotspotMAC\_Rsp | | MBORREL4: New Signal |
|  | WFHS-IIR-REQ-179315/B-WifiHotspotServer\_Rx | | MBORREL4: Added WifiHotpotMAC\_Rq, PowerMode\_St, BSBattSOC, and Delay\_Accy. Removed VehicleTorq\_St |
|  | MD-REQ-179296/B-DataUsage\_Rq | | MBORREL4: Updated description and renamed literal “RetrieveDataFromBackend” to “RefreshDataNoResponse” |
|  | MD-REQ-179298/B-DeviceList\_Rq | | MBORREL4: Updated to remove BlackList encoding |
|  | MD-REQ-195171/A-WifiHotspotMAC\_Rq | | MBORREL4: New Signal |
|  | MD-REQ-199634/A-BSBattSOC | | MBORREL4: New signal added |
|  | MD-REQ-201601/A-Delay\_Accy | | MBORREL4: New signal |
|  | STR-207866/B-Functional Definition | |  |
|  | STR-285877/B-Requirements | | MBORREL4: Moved REQ-194536 from FUN-REQ-192079 to FUN-REQ-195287 jshelby5: Change: deleted WFHS-REQ-192159. Combined WFHS-REQ-191784 with WFHS-REQ-191863. |
|  | WFHS-REQ-191639/B-WifiHotspotServer identifies the vehicle region | |  |
|  | WFHS-REQ-191705/B-Monitoring Wi-Fi Hotspot feature availability | | jshelby5: Change: Wi-Fi disabled state added to TCUAvailability\_St signal. WifiHotspotOnBoardClient shall still be required to monitor/transmit some signals if feature is disabled. Lost CAN communication parameter shall be configurable via EOL. |
|  | WFHS-REQ-191710/B-Disabling driver restricted screens | | jshelby5: Clarification: deleted the speed value and referred to a spec. |
|  | WFHS-REQ-191887/B-Configurable parameters | | jshelby5: Change: The WifiHotspotServer's Wi-Fi enablement parameter shall also be configurable via over the air. Change: Enhanced hotspot enablement mode shall NOT be configurable via FTCP Clarification: compiled all configurable parameters mentioned throughout the document into a single table Clarification: "Wi-Fi\_Enabled" parameter name was changed to "Wi-Fi\_Hotspot\_Feature\_Enabled". Clarification: Wi-Fi\_Min\_Initialization\_Time parameter deleted Clarification: deleted Number\_Blacklisted\_Devices parameter, Blocked clients parameter and Number\_Failed\_Attempts parameter Clarification: Added parameter WifiHotspotOnBoardClient\_Data\_Usage\_Refresh\_Timeout. Clarification: Deleted Data\_Usage\_Info\_Request\_Timeout parameter Clarification: Deleted CarrierDataNotification and added TrialEligible Clarification: deleted Wi-Fi\_Hotspot\_Enabled. Added 2\_4GHz\_Minimum\_Throuput and 5GHz\_Minimum\_Throughput. Wi-Fi APN shall also be configurable via EOL. Change: Updated entire table. Clarification: enhanced hotspot enablement timer is defaulted to on and the timer was changed to 30 min |
|  | WFHS-REQ-191890/B-Wi-Fi throughput | | jshelby5: Change: throughput value was added for the 5GHz band. Maximum throughput requirement was deleted. Change: Wi-Fi throughput shall be greater than cellular throughput |
|  | WFHS-REQ-191900/B-Maximum Wi-Fi initialization time | | jshelby5: Change: Wi-Fi\_Min\_Initialization requirement has been deleted. Clarification: maximum initialization time has been added. This shall not be configurable. |
|  | WFHS-REQ-191902/B-APN connections | | jshelby5: Change: APN shall also be updateable via EOL. Landing page redirection shall be done through the Wi-Fi APN |
|  | WFHS-REQ-191904/B-Shutting down and powering up the Wi-Fi chipset and WifiHotspotServer | | jshelby5: Clarification: clarified what powering down and powering up meant. Change: added Wi-Fi disabled requirements |
|  | WFHS-REQ-192111/B-Wi-Fi Chipset AP and STA mode | | jshelby5: Clarification: The Wi-Fi chipset shall not enable STA mode. |
|  | WFHS-REQ-192117/B-Operating on the 2.4 GHz band in AP mode | | jshelby5: Change: operational band shall also be configurable via EOL. |
|  | WFHS-REQ-194001/B-WifiHotspotServer EOL configuration for determining Wi-Fi Hotspot feature enablement | | jshelby5: Change: The Wi-Fi enablement parameter shall ALSO be configurable via over the air.  Clarification: The config block, byte, etc. shall not be added to this document at a later time. The part 2 spec shall be referenced. Change: The parameter "Wi-Fi\_Enabled" was changed to "Wi-Fi\_Hotspot\_Feature\_Enabled" in order to limit confusion between the hotspot enablement state and the Wi-Fi Hotspot feature enablement Change: added requirement for WifiHotspotServer to check the supplier configuration with the Ford EOL configuration to determine if the WifiHotspotServer is able to be configured as "Wi-Fi enabled". Change: added Wi-Fi disabled state to TCUAvailability\_St signal. WifiHotspotServer shall still be required to monitor certain signals if feature is disabled. Change: Wi-Fi\_Hotspot\_Feature\_Enabled parameter shall be checked at each ignition cycle. If it has changed, it shall be transmitted to the WifiHotspotOffBoardClient. |
|  | WFHS-REQ-191783/B-WifiHotspotServer over-the-air software updates | | jshelby5: Clarification: changed the reference requirement ID |
|  | WFHS-REQ-194010/B-Wi-Fi Hotspot parameters transmitted during provisioning | | jshelby5: Clarification: The "Wi-Fi\_Enabled" parameter name was changed to "Wi-Fi\_Hotspot\_Feature\_Enabled" jshelby5: Clarification: MSISDN is no longer needed |
|  | WFHS-REQ-194471/B-WifiHotspotServer becomes not authorized | | jshelby5: Clarification: changed CarrierDataNotification to TrialEligible parameter |
|  | WFHSv1-UC-REQ-191983/B-User wakes WifiHotspotOnBoardClient up before WifiHotspotServer wakes up | | jshelby5: Clarification: waiting symbol may be displayed |
|  | WFHSv1-FUN-REQ-191999/B-Displaying WifiHotspotServer icon | | jshelby5: Clarification: the icon shall be designed to inform the customer that the signal strength displayed is that of the vehicle. Clarification: the icon shall not display the number of connected devices |
|  | STR-285755/B-Requirements | | jshelby5: Change: removed WFHS-REQ-191711. |
|  | WFHS-REQ-191714/B-Displaying the dedicated WifiHotspotServer icon on the WifiHotspotOnBoardClient display | | jshelby5: Clarification: The config block, byte, etc. shall not be added to this document at a later time. The diagnostics spec shall be referenced. Change: number of connected devices shall no longer be displayed. |
|  | WFHS-REQ-191713/B-Reporting out technology used to connect to the cellular network | | jshelby5: Change: Added table. |
|  | WFHS-REQ-191706/B-Wi-Fi Hotspot enablement condition checks | | jshelby5: Clarification: The config block, byte, etc. shall not be added to this document at a later time. The part 2 spec shall be referenced. Clarification: Mentioned when the CAN signal HotspotEnablement\_St shall report the NULL state. Change: Added additional CAN signals to accommodate for different vehicle architectures. Clarification made under the Enhanced\_Hotspot\_Enablement\_Mode On section. Deleted PwPck CAN signal. IgnitionStatus\_St shall be used instead. If vehicle enters transport mode, the Wi-Fi chipset shall be powered down. If the hotspot is turned off due to battery issues, TCUAvailability\_St shall be set to NULL. Enhanced\_Hotspot\_Enablement\_Mode shall be defaulted to Off and shall be configurable via OTA or EOL. Hotspot\_Enablement\_Timer shall be defaulted to 0 min and shall be configurable via EOL. Enablement state shall be configurable via EOL. Change: Hotspot enablement timer shall be defaulted to 30 min, enhanced hotspot enablement mode shall be defaulted to on. The WifiHotspotServer shall not be required to monitor BSBattSOC when ignition is off. WifiHotspotServer shall check the BSBattSOC value when ignition transitions to off. |
|  | WFHS-REQ-191708/B-Displaying the Wi-Fi Hotspot's enablement state on the WifiHotspotOnBoardClient display | | jshelby5: Clarification: Changed the HMI description from power state to enablement state |
|  | WFHSv1-UC-REQ-191928/B-Wi-Fi Hotspot in On-disabled state when the Wi-Fi Hotspot enablement conditions become met | | jshelby5: Clarification: typo fixed |
|  | WFHSv1-UC-REQ-191916/B-User turns ignition to Run while the Wi-Fi Hotspot is on-disabled | | jshelby5: Clarification: enablement conditions are dependent on ignition status, not engine status. |
|  | WFHSv1-UC-REQ-191917/B-User turns ignition to Accessory and delayed accessory from Run | | jshelby5: Clarification: enablement conditions are dependent on ignition status. |
|  | WFHSv1-UC-REQ-191920/B-User turns vehicle completely off and exits the vehicle | | jshelby5: Clarification: enablement state is dependent on ignition status, not engine status. |
|  | WFHSv1-UC-REQ-191921/B-User enters vehicle and turns ignition to accessory | | jshelby5: Clarification: enablement state is dependent on ignition status. |
|  | WFHSv1-UC-REQ-191923/B-Vehicle enters transport mode | | jshelby5: Clarification: Wi-Fi shall be off, not on-disabled. |
|  | WFHSv1-UC-REQ-191924/B-Battery is used excessively | | jshelby5: Clarification: deleted mobile app update failed exception use case. User shall not be allowed into the Wi-Fi Hotspot menu. |
|  | WFHSv1-FUN-REQ-140746/B-Managing SSID | | jshelby5: fixed formatting |
|  | WFHS-REQ-191596/B-Generating the default SSID | | jshelby5: Change: SSID shall also be configurable via EOL. |
|  | STR-207816/B-Use Cases | | jshelby5: changed the name of WFHSv1-UC-REQ-191936 |
|  | WFHSv1-UC-REQ-191933/B-User changes SSID from WifiHotspotOnBoardClient | | jshelby5: deleted the speed value. |
|  | WFHSv1-UC-REQ-191936/B-E5 User attempts to view SSID/password through WifiHotspotOnBoardClient while under driver restriction | | jshelby5: Clarification: deleted speed value |
|  | WFHS-REQ-191610/B-Generating the initial password | | jshelby5: Change: password shall also be updateable via EOL. |
|  | WFHSv1-UC-REQ-191937/B-User enters into the Wi-Fi Hotspot Info screen | | jshelby5: Clarification: deleted speed value |
|  | WFHSv1-UC-REQ-191938/B-User views the password on the WifiHotspotOnBoardClient | | jshelby5: Clarification: deleted speed value |
|  | WFHSv1-UC-REQ-191939/B-User changes password from WifiHotspotOnBoardClient | | jshelby5: Clarification: deleted speed value |
|  | WFHS-REQ-191642/B-Security algorithm offerings per region | | jshelby5: Clarification: mentioned the scenario when the CAN signal HotspotSecurity\_St shall be set to NULL. Security algorithm shall be updateable via EOL. |
|  | WFHS-REQ-191647/B-Function of the visibility feature | | jshelby5: Change: visibility shall be configurable via EOL. |
|  | WFHS-REQ-191648/B-Reporting the visibility status | | jshelby5: Clarification: Added the scenario when WifiHotspotServer shall report out NULL in the CAN signal HotspotVisibility\_St. |
|  | WFHSv1-FUN-REQ-140752/B-Manage Devices | |  |
|  | STR-207812/B-Requirements | | jshelby5: Change: deleted WFHS-REQ-191700/B-Managing the monitored list and blacklist |
|  | WFHS-REQ-191652/B-Checklist for allowing a device to connect to the Wi-Fi Hotspot | | jshelby5: clarification item; the three lists are split into four lists: connected, blocked, blacklisted and monitored |
|  | WFHS-REQ-191653/B-Managing the connected devices list | | jshelby5: Clarification: The config block, byte, etc. shall not be added to this document at a later time. The part 2 spec shall be referenced. Change: the device name character length parameter shall be configurable via EOL. |
|  | WFHS-REQ-191701/B-Displaying the connected devices list on the WifiHotspotOnBoardClient display | | jshelby5: Change: if the screen takes awhile to load, a popup shall be displayed. |
|  | WFHS-REQ-191695/B-Setting the connected device update bit | | jshelby5: Clarification: specified the actual power mode the WifiHotspotServer will enter when it needs to clear the update bit. |
|  | WFHS-REQ-191702/B-Updating the connected devices screen while the user is in the screen | | jshelby5: Change: WifiHotspotOnBoardClient shall disable user input while updating the screen and a popup shall be displayed. |
|  | WFHS-REQ-191703/B-Displaying the blocked devices list on the WifiHotspotOnBoardClient display | | jshelby5: Change: if the blocked list takes a while to load, a popup shall be displayed. |
|  | WFHS-REQ-191704/B-User requests to unblock a device from the blocked list through WifiHotspotOnBoardClient display | |  |
|  | WFHS-REQ-191699/B-Request from the WifiHotspotOnBoardClient to remove a device from the blocked list | | jshelby5: Change: unblocked devices shall be required to enter password before connecting. |
|  | STR-207821/B-Use Cases | | jshelby5: Clarification: deleted use cases WFHSv1-UC-REQ-191976/A, WFHSv1-UC-REQ-191977/A, WFHSv1-REQ-191978/A |
|  | WFHSv1-UC-REQ-191982/B-Returning device configured to NOT automatically connect to hotspot | | jshelby5: Clarification: Deleted the pre-condition "SSID & password has not been changed since" since it is irrelevant |
|  | WFHSv1-ACT-REQ-167115/B-Connect A Device | | MBORREL4: Updated to remove Blacklist detail |
|  | WFHSv1-SD-REQ-167138/B-Connect A Device | | MBORREL4: Updated to remove Blacklist detail |
|  | WFHSv1-FUN-REQ-140754/B-Reporting Data Used | | jshelby5: Clarification: DataUsage\_Rsp CAN signal has been updated and UTC format has been deleted. Updated data usage fields. Expiration/renewal time added. |
|  | STR-207794/B-Requirements | | jshelby5: Addition: added WFHS-REQ-197429 Change: deleted WFHS-REQ-191870 Change: deleted WFHS-REQ-193978 Change: added WFHS-REQ-199543 & WFHS-REQ-199544 |
|  | WFHS-REQ-191871/B-WifiHotspotOnBoardClient initiates data usage request due to user entering into Wi-Fi Hotspot menu | | jshelby5: Clarification: the retrieve from backend request shall only be made if the user enters the Wi-Fi menu from outside the Wi-Fi screens. |
|  | WFHS-REQ-191864/B-Request to refresh data usage info without a response required | | jshelby5: Change: WifiHotspotServer shall transmit a "fail" response if timer expires or no connection is available Change: Data\_Usage\_Info\_Request\_Timeout timer was replaced with Data\_Usage\_Info\_Refresh\_Timeout Change: the WifiHotspotServer shall transmit a Refresh data usage FTCP request if it receives a refresh request with no response needed. Change: data usage refresh parameter shall be configurable via OTA or EOL. |
|  | WFHS-REQ-191872/B-Displaying data usage information | | jshelby5: Clarification: Added the CAN signal TelematicsService\_St for identifying if the WifiHotspotServer is authorized or not Change: WifiHotspotSOnBoardClient shall look at the data used percentage field instead of data left to determine what Data Usage screen to show. Clarification: updated table. Changed NULL to Invalid. HMI example updated. Change: VIN shall be displayed Change: Expiration/renewal time shall not be displayed. Clarification: Updated data usage table. Carrier info may not be displayed on the data usage screen. |
|  | WFHS-REQ-191873/B-Rounding data usage values | |  |
|  | WFHS-REQ-191866/B-Request from WifiHotspotOnBoardClient for the WifiHotspotServer's stored data usage information | | jshelby5: Change: WifiHotspotServer authorization is indicated through the CAN signal TelematicsService\_St. Clarification: deleted WifiHotspotServer authorization table. Clarification: added scenario if TCU does not have any data usage info stored. Changed Null to Invalid. |
|  | WFHS-REQ-191867/B-Request from WifiHotspotOnBoardClient for data usage while WifiHotspotServer is updating the data usage information | | jshelby5: Clarification: If WifiHotspotServer does not have any data usage info at the time of the request, it shall report Invalid. |
|  | WFHS-REQ-191874/B-User refreshes data usage screen | | jshelby5: Change: Added a timer that shall be configurable via EOL. |
|  | WFHS-REQ-191868/B-Request from WifiHotspotOnBoardClient to refresh the data usage values | | jshelby5: Clarification: a data usage Refresh will retrieve data usage information from the carrier. Clarification: Added the WifiHotspotServer authorization table. Clarification: Added a table to map the data plan status with the FTCP message Clarification: WifiHotspotServer shall mark data usage fields as invalid if no data usage info is stored Clarification: updated data usage table |
|  | WFHS-REQ-191869/B-Request from WifiHotspotOnBoardClient for a data usage refresh while WifiHotspotServer is updating the data usage information | | jshelby5: Clarification: changed the "updating" CAN signal status to "wait". Clarified the WifiHotspotServer's actions |
|  | WFHSv1-UC-REQ-191945/B-User accesses the data usage screen in a good network coverage area | | jshelby5: Clarification: added the possibility that the data usage information was last updated when the user entered into the Wi-Fi menu. Clarification: data usage is only stored during an ignition cycle |
|  | WFHSv1-UC-REQ-191946/B-User accesses the data usage screen in a no network coverage area | | jshelby5: Clarification: WifiHotspotServer clears data usage info at each ignition cycle. |
|  | WFHSv1-UC-REQ-191948/B-User refreshes the data usage values from the WifiHotspotOnBoardClient | | jshelby5: fixed typo |
|  | WFHSv1-UC-REQ-191949/B-User refreshes data usage values from WifiHotspotOnBoardClient when vehicle is in a no coverage area | | jshelby5: Clarification: old data usage info shall be displayed |
|  | WFHSv1-UC-REQ-191953/B-User refreshes the data usage values on the mobile app while in the Wi-Fi Hotspot screen on the WifiHotspotOnBoardClient display | | MBORREL4: Removed WFHSv1-UC-REQ-191954/B-User refreshes the data usage on the mobile app while NOT in the Wi-Fi Hotspot screen on the WifiHotspotOnBoardClient display |
|  | WFHSv1-UC-REQ-194537/B-User accesses the mobile app while WifiHotspotServer is not authorized | | jshelby5: Change: replaced MSISDN with VIN |
|  | WFHSv1-UC-REQ-194540/B-User accesses the data usage screen while WifiHotspotServer is un-authorized | | jshelby5: Clarification: refresh button may not be disabled. |
|  | WFHSv1-SD-REQ-167143/B-User Refreshes Data Usage Values From Centerstack | | MBORREL4: Updated diagram to reflect changes to DataUsage\_Rsp |
|  | WFHSv1-FUN-REQ-140748/B-Carrier Data Notification | | jshelby5: Clarification: took out FIFO statement Clarification: Only low balance notifications shall be sent to the WifiHotspotServer. No data usage information is stored in the WifiHotspotOffBoardClient |
|  | STR-207809/B-Requirements | | MBORREL4: Removed REQ-191886/B-Wi-Fi Hotspot notification icon |
|  | WFHS-REQ-191880/B-Receiving carrier data notifications and data usage updates | | jshelby5: Change: the FTCP message shall indicate whether it is a notification or not. The only notification that may be sent to the WifiHotspotServer shall be a XX% data used notification. Clarification: if a notification is received, the WifiHotspotServer shall also note when it was received. |
|  | WFHS-REQ-191882/B-Triggering free trial period reminders | | jshelby5: Clarification: The config block, byte, etc. shall not be added to this document at a later time. The part 2 spec shall be referenced. Change: CarrierDataNotification parameter deleted. TrialEligible parameter and requirements were added. The trial reminder parameter, trial reminder trigger parameter and trial repetition parameter shall be configurable via EOL and OTA. Trial eligible parameter shall be configurable via EOL. |
|  | WFHS-REQ-191881/B-Displaying critical data plan related popups | | jshelby5: Clarification: WifiHotspotServer shall never set the CAN signal CarrierDataNotification\_St to "data plan expired". Change: VIN shall be displayed instead of MSISDN. |
|  | STR-207818/B-Use Cases | | MBORREL4: Removed WFHSv1-UC-REQ-191965/B-Notification has not yet been viewed in the data usage screen through the WifiHotspotOnBoardClient or mobile app |
|  | WFHSv1-UC-REQ-191963/B-The vehicle's Wi-Fi Hotspot data plan changes to a low balance, expired or trial period waiting status | | jshelby5: Clarification: "Data plan expired" scenario deleted. |
|  | WFHSv1-ACT-REQ-167116/B-Carrier Data Notification Received | | MBORREL4: Removed DataPlanExpired from diagram. |
|  | WFHSv1-SD-REQ-167139/B-Carrier Data Notification Received | | MBORREL4: Updated parameters of CarrierInfo\_Rsp and added a note to clarify 1sec Null Reset Timer. |
|  | WFHSv1-FUN-REQ-192000/B-Managing Carrier Information | | jshelby5: Clarification: Deleted MSISDN, added two hotline numbers instead of one. Clarification: Data usage screen may not display carrier info. |
|  | STR-285756/B-Requirements | | jshelby5: Clarification: combined WFHS-REQ-191725 and WFHS-REQ-191726 Change: WFHS-REQ-191722 deleted |
|  | WFHS-REQ-191718/B-Initial carrier hotline number | | jshelby5: Change: There shall be two hotline numbers stored in the TCU instead of one. |
|  | WFHS-REQ-191719/B-Updating the carrier service hotline number | | jshelby5: Change: potentially two phone numbers may be updated. Updates may occur regardless of authorization state. Hotline numbers also configurable via EOL. |
|  | WFHS-REQ-191726/B-Updating the carrier landing page URL | | jshelby15: Clarification: Combined WFHS-REQ-191725 into this requirement Change: updates may occur regardless of authorization state. URLs also configurable via EOL. |
|  | WFHS-REQ-191875/B-Requesting for carrier information due to the user entering a specific screen | | jshelby5: carrier info may not be displayed on the data usage screen. VIN shall be displayed on the screen that displays carrier hotline number. |
|  | WFHS-REQ-191729/B-Reporting out the carrier information to the WifiHotspotOnBoardClient | | jshelby5: Clarification: updated the reference requirement from WFHS-REQ-191725 to WFHS-REQ-191726 Change: Two hotline number shall be transmitted to WifiHotspotOnBoardClient. Deleted MSISDN |
|  | WFHS-REQ-191876/B-Displaying carrier information | | jshelby5: WifiHotspotOnBoardClient shall determine whether it shall display the Ford or Lincoln hotline number. Replaces MSISDN with VIN. Clarification: carrier info may not be displayed on data usage screens. |
|  | WFHS-REQ-191877/B-Initiating a call to the carrier hotline | | jshelby5: Change: the WifiHotspotOnBoardClient shall determine which carrier hotline number to dial. Updated HMI example. Clarification: Click to call button may not be on the data usage screens. |
|  | WFHSv1-UC-REQ-191959/B-China customer initiates a call to the carrier hotline though the WifiHotspotOnBoardClient display | | jshelby5: Clarification: either a Ford or Lincoln hotline number is dialed depending on the vehicle brand. Replaced MSISDN with VIN |
|  | WFHSv1-UC-REQ-191960/B-China customer purchases data/activates trial period through the carrier hotline | | jshelby5: Change: replaced MSISDN with VIN |
|  | WFHSv1-UC-REQ-191961/B-Customer purchases data/activates free trial period through connected device | | jshelby5: Change: replaced MSISDN with VIN |
|  | WFHSv1-UC-REQ-194537/B-User accesses the mobile app while WifiHotspotServer is not authorized | | jshelby5: Change: replaced MSISDN with VIN |
|  | WFHSv1-ACT-REQ-167114/B-Carrier Info Changes From Backend | | MBORREL4: Updated to clarify that multiple phone numbers will be received. |
|  | WFHSv1-SD-REQ-167131/B-Carrier Info Changes From Backend | | MBORREL4: Updated to clarify that multiple phone numbers will be received. |
|  | WFHS-REQ-191862/B-Reporting out a Wi-Fi Hotspot reset | | jshelby5: Change: Changed not available to Null |
|  | WFHS-REQ-191863/B-Wi-Fi Hotspot reset settings | | jshelby5: Clarification: Some columns were changed from "restore customer setting" to "restore last saved values" to clarify that the customer was not responsible for changing the values. Clarification: all parameters and settings mentioned throughout this document were compiled into a single table. Note: any parameter that is configurable via EOL or via software changes prior to production are not included in the table. Clarification: The "Wi-Fi\_Enabled" parameter name was changed to "Wi-Fi\_Hotspot\_Feature\_Enabled" Clarification: deleted the blacklisted devices parameter Clarification: added parameter Data\_Usage\_Info\_Request\_Timeout and Data\_Usage\_Info\_Refresh\_Timeout. Clarification: Data\_Usage\_Info\_Request\_Timeout parameter was deleted. Clarification: Deleted CarrierDataNotification parameter and added TrialEligible. Added Data\_Usage\_Reception\_Time.  Change: Updated entire table. Combined WFHS-REQ-191784-Initial Wi-Fi Hotspot Settings in with this requirement. |
|  | WFHSv1-UC-REQ-191967/B-User performs a reset but does not deactivate their Wi-Fi Hotspot data plan | | jshelby5: Clarification: deleted blacklist. Refresh button may not be disabled. |
|  | WFHSv1-UC-REQ-191968/B-Dealer replaces WifiHotspotServer while a Wi-Fi Hotspot data plan is active | |  |
|  | WFHSv1-FUN-REQ-195287/A-Transferring MAC Address | | MBORREL4: New Function |
|  | WFHS-REQ-194536/B-Reporting out the Wi-Fi chipset MAC address | | jshelby5: Clarification: the note stating the CAN signals were still undefined was deleted. Clarification: If WifiHotspotServer cannot read the MAC address, it shall send NULL values. A reference was added to the requirement. If feature is disabled, it shall still transmit MAC address. |
|  | WFHSv1-ACT-REQ-195130/A-Transmitting Wi-Fi Chipset MAC Address | | MBORREL4: New Requirement |
|  | WFHSv1-SD-REQ-195131/A-Transmitting Wi-Fi Chipset MAC Address | | MBORREL4: New Requirement |
|  |  |  |  |
| **January 14, 2016** | **1.2** | **Updated Release** |  |
|  | WFHS-REQ-191887/D-Configurable parameters | | jshelby5: Change: updated table. |
|  | WFHS-REQ-194001/C-WifiHotspotServer EOL configuration for determining Wi-Fi Hotspot feature enablement | | jshelby5: Change: deleted the requirement to check enablement status every ignition cycle and report it to the WifiHotspotOffBoardClient. |
|  | WFHS-REQ-191868/C-Request from WifiHotspotOnBoardClient to refresh the data usage values | | jshelby5: Change: added requirement if overage flag is set, set data used percent to invalid |
|  | WFHS-REQ-191882/C-Triggering free trial period reminders | | jshelby5: Deleted requirement for the trial eligible parameter to be configurable via EOL. |
|  |  |  |  |
| **February 19, 2016** | **1.3** | **Updated Release** | **Bundle #2 Updates** |
|  | STR-294566/B-Architectural Design | | MBORREL4: Added REQ-207990 |
|  | STR-294566/C-Architectural Design | | MBORREL4: Updated to replace STR-286735 with new REQ-210528 for Logical Signal Mapping |
|  | WFHS-CLD-REQ-207990/A-Wifi Hotspot Mobile Client | | MBORREL4: New CLD for wifi hotspot connected/disconnected devices |
|  | WFHS-REQ-210528/A-Logical Signal Mapping | | MBORREL4: New req to replace STR (last rev comment from old STR located below) jshelby5: CarMode\_St and PowerMode\_St changed to CarMode and PowerMode. |
|  | MD-REQ-179310/C-DeviceList\_Rsp | | MBORREL4: Increased DeviceName from 17 to 19 characters. Updated ListSize from 20 to 31. |
|  | STR-285877/C-Requirements | | MBORREL4: Removed Req-191887 |
|  | WFHS-REQ-191640/C-WifiHotspotOnBoardClient identifies the vehicle brand | | jshelby5: clarification: generalized the IDS spec name. |
|  | WFHS-REQ-191641/C-WifiHotspotOnBoardClient identifies the vehicle region | | jshelby5: clarification: generalized IDS spec name. |
|  | WFHS-REQ-191705/E-Monitoring Wi-Fi Hotspot feature availability | | jshelby5: added requirement for the hotspot capable modem DID. Lost\_CAN\_Communication shall not be an EOL configurable DID. |
|  | WFHS-REQ-191714/D-Displaying the dedicated WifiHotspotServer icon on the WifiHotspotOnBoardClient display | | jshelby5: Maximum number of devices DID is not needed. |
|  | WFHS-REQ-191712/B-Converting and reporting out the number of WifiHotspotServer signal strength bars | | jshelby5: Clarification: if WiFi APN is not connected, TCU shall report out 0 bars. Updated table to show how each technology shall be measured. |
|  | WFHS-REQ-191713/D-Reporting out technology used to connect to the cellular network | | jshelby5: Clarification: TCU shall report out the technology it is using ONLY if Wi-Fi APN is connected. |
|  | WFHS-REQ-191653/D-Managing the connected devices list | | jshelby5: change: number of connected devices shall not be configurable and it shall have a new default value. |
|  | WFHS-REQ-191696/C-Managing the blocked devices list | | jshelby5: change: number of blocked devices shall not be configurable and it shall have a new default value. |
|  | WFHSv1-ACT-REQ-167115/C-Connect A Device | | MBORREL4: Changed WifHotSpotOffBoardClient to WifiHotSpotMobileClient |
|  | WFHSv1-ACT-REQ-167124/B-User Disconnects Device From Hotspot through the Device | | MBORREL4: Changed WifHotSpotOffBoardClient to WifiHotSpotMobileClient |
|  | WFHSv1-SD-REQ-167138/C-Connect A Device | | MBORREL4: Changed WifHotSpotOffBoardClient to WifiHotSpotMobileClient |
|  | WFHSv1-SD-REQ-167141/B-User Disconnects Device From Hotspot through the Device | | MBORREL4: Changed WifHotSpotOffBoardClient to WifiHotSpotMobileClient |
|  | WFHS-REQ-191872/G-Displaying data usage information | | jshelby5: clarification: generalized the IDS name. |
|  | WFHS-REQ-191874/D-User refreshes data usage screen | | jshelby5: clarification: data usage refresh timer shall not be EOL configurable. |
|  | WFHSv1-FUN-REQ-140759/B-Wi-Fi Hotspot Reset | | jshelby5: deleted CAN signal and FTCP references. |
|  | WFHS-REQ-191863/C-Wi-Fi Hotspot reset settings | | jshelby5: deleted reference to configurable parameters requirement. Blocked devices shall be restored during ignition cycle. Added reference to another requirement. |
|  |  |  |  |
| **March 29, 2016** | **1.4** | **Updated Release** |  |
|  | STR-285874/B-Overview+ | | jshelby5: Bundle 3 update: added CHR |
|  | WFHS-IIR-REQ-179285/C-WifiHotspotServer\_Tx | | MBORREL4: Removed REQ-179303-TCUTechnologyUsed\_St and added REQ-212571-TCUTechnologyUsed2\_St. Added REQ-180729-NumberOfConnectedDevices\_St |
|  | MD-REQ-212571/A-TCUTechnologyUsed2\_St | | MBORREL4: New signal |
|  | MD-REQ-179309/C-DataUsage\_Rsp | | MBORREL4: Updated to include UserID |
|  | WFHS-IIR-REQ-179315/C-WifiHotspotServer\_Rx | | MBORREL4: Added REQ-212570 - HotspotTrialReminderSelection\_Rq |
|  | MD-REQ-212570/A-HotspotTrialReminderSelection\_Rq | | MBORREL4: New signal |
|  | WFHS-REQ-191640/B-WifiHotspotOnBoardClient identifies the vehicle brand+ | | jshelby5: Bundle 3 update: added part II reference. |
|  | WFHS-REQ-191640/D-WifiHotspotOnBoardClient identifies the vehicle brand | | jshelby5: bundle 3 update, added CHR spec reference. |
|  | WFHS-REQ-191641/B-WifiHotspotOnBoardClient identifies the vehicle region+ | | jshelby5: Bundle 3 update: added Europe and added Part II spec reference. |
|  | WFHS-REQ-191641/D-WifiHotspotOnBoardClient identifies the vehicle region | | jshelby5: bundle 3 update, added CHR diagnostic spec reference. |
|  | WFHS-REQ-191639/C-WifiHotspotServer identifies the vehicle region | | jshelby5: bundle 3 update, added EU. |
|  | WFHS-REQ-191705/D-Monitoring Wi-Fi Hotspot feature availability+ | | jshelby5: Bundle 3 update: added CHR requirement. |
|  | WFHS-REQ-191705/F-Monitoring Wi-Fi Hotspot feature availability | | jshelby5: Bundle 3 update. Added CHR requirements. |
|  | WFHS-REQ-191710/D-Disabling driver restricted screens | | jshelby5: bundle 3 update. Added reference to SDM4 spec. |
|  | WFHS-REQ-191896/B-FCC and international radio regulatory requirements | | jshelby5: Bundle 3 update: added European regulations. |
|  | WFHS-REQ-194010/D-Wi-Fi Hotspot parameters transmitted during provisioning | | jshelby5: bundle 3 update. Added EU. |
|  | WFHSv1-UC-REQ-191983/C-User wakes WifiHotspotOnBoardClient up before WifiHotspotServer wakes up | | jshelby5: Bundle 3 update: referenced another HMI spec. |
|  | WFHSv1-UC-REQ-191984/B-User is navigating in the Wi-Fi Hotspot screens when WifiHotspotOnBoardClient loses communication with WifiHotspotServer | | jshelby5: Bundle 3 update: referenced another HMI spec. |
|  | WFHSv1-UC-REQ-191986/B-User is navigating in the Wi-Fi Hotspot screens when a Wi-Fi error occurs | | jshelby5: Bundle 3 updates: added HMI spec reference. |
|  | WFHSv1-FUN-REQ-191999/C-Displaying WifiHotspotServer icon | | jshelby5: bundle 3 update. Wi-Fi Hotspot feature shall have its own icon, independent of the WifiHotspotServer icon. |
|  | STR-285755/C-Requirements | | added WFHS-REQ-212165 and WFHS-REQ-191711 |
|  | WFHS-REQ-191713/C-Reporting out technology used to connect to the cellular network+ | | jshelby5: Bundle 3 update: added Europe. |
|  | WFHS-REQ-191713/E-Reporting out technology used to connect to the cellular network | | jshelby5: bundle 3 update: deleted table. CAN signal can support all states and no mapping is needed to be done. Updated technology used logical name. |
|  | WFHS-REQ-191712/C-Converting and reporting out the number of WifiHotspotServer signal strength bars | | jshelby5: bundle 3 update. Updated the technology names. |
|  | WFHS-REQ-191714/C-Displaying the dedicated WifiHotspotServer icon on the WifiHotspotOnBoardClient display+ | | jshelby5: Bundle 3 update: added HMI reference and CHR part II spec reference. |
|  | WFHS-REQ-191714/E-Displaying the dedicated WifiHotspotServer icon on the WifiHotspotOnBoardClient display | | jshelby5: bundle 3 update. Added HMI spec reference. Number of devices connected to the hotspot shall also be displayed. Updated technology used logical name. |
|  | WFHS-REQ-191708/C-Displaying the Wi-Fi Hotspot's enablement state on the WifiHotspotOnBoardClient display | | jshelby5: Bundle 3 update: added HMI reference. |
|  | WFHSv1-UC-REQ-191925/B-User turns Wi-Fi Hotspot On | | jshelby5: Bundle 3 update: added HMI reference. |
|  | WFHSv1-UC-REQ-191926/B-User turns Wi-Fi Hotspot Off | | jshelby5: Bundle 3 updates: added HMI reference. |
|  | WFHSv1-UC-REQ-191927/B-User attempts to turn the Wi-Fi Hotspot on when the Wi-Fi Hotspot enablement conditions are not met | | jshelby5: Bundle 3 update: added HMI reference. |
|  | WFHSv1-UC-REQ-191928/C-Wi-Fi Hotspot in On-disabled state when the Wi-Fi Hotspot enablement conditions become met | | jshelby5: Bundle 3 update: added HMI reference. |
|  | WFHSv1-UC-REQ-191929/B-Wi-Fi Hotspot is on when the Wi-Fi Hotspot enablement conditions become not met | | jshelby5: Bundle 3 update: added HMI reference. |
|  | WFHSv1-UC-REQ-191916/C-User turns ignition to Run while the Wi-Fi Hotspot is on-disabled | | jshelby5: Bundle 3 update: added HMI reference. |
|  | WFHSv1-UC-REQ-191920/C-User turns vehicle completely off and exits the vehicle | | jshelby5: Bundle 3 update: added HMI reference. |
|  | WFHSv1-UC-REQ-191921/C-User enters vehicle and turns ignition to accessory | | jshelby5: Bundle 3 updates: added HMI reference. |
|  | WFHSv1-UC-REQ-191922/B-User turns the engine off when enhanced hotspot enablement mode is off | | jshelby5: Bundle 3 updates: added HMI reference. |
|  | WFHSv1-UC-REQ-191923/C-Vehicle enters transport mode | | jshelby5: Bundle 3 updates: added HMI reference. |
|  | WFHSv1-UC-REQ-191924/C-Battery is used excessively | | jshelby5: Bundle 3 updates: added HMI reference. |
|  | WFHS-REQ-191634/C-Displaying the SSID on the WifiHotspotOnBoardClient display | | jshelby5: Bundle 3 update: added HMI reference. |
|  | WFHS-REQ-191629/B-Keyboard used to edit the SSID through WifiHotspotOnBoardClient display | | jshelby5: Bundle 3 updates: added HMI reference. |
|  | WFHS-REQ-191635/B-Excepting and updating user SSID configurations | | jshelby5: Bundle 3 updates: added HMI reference. |
|  | WFHSv1-UC-REQ-191936/C-E5 User attempts to view SSID/password through WifiHotspotOnBoardClient while under driver restriction | | jshelby5: Bundle 3 update: added HMI reference. |
|  | WFHS-REQ-191633/C-Displaying the password on the WifiHotspotOnBoardClient display | | jshelby5: Bundle 3 updates: added HMI reference. |
|  | WFHS-REQ-191632/B-Keyboard used to edit the password through WifiHotspotOnBoardClient display | | jshelby5: Bundle 3 updates: added HMI reference. |
|  | WFHS-REQ-191636/B-Excepting and updating user password configurations | | jshelby5: Bundle 3 updates: added HMI reference. |
|  | WFHSv1-UC-REQ-191937/D-User enters into the Wi-Fi Hotspot screen that displays the SSID and password | | jshelby5: Bundle 3 update: added HMI reference. |
|  | WFHSv1-FUN-REQ-140745/B-Changing Security Algorithm | | jshelby5: Bundle 3 update: added Europe. |
|  | WFHS-REQ-191642/C-Security algorithm offerings per region | | jshelby5: Bundle 3 update: Added Europe. |
|  | WFHS-REQ-191644/B-Displaying the security type | | jshelby5: Bundle 3 update: added HMI reference. |
|  | WFHS-REQ-191645/B-Displaying the option to configure the security type | | jshelby5: Bundle 3 update: added HMI reference. |
|  | WFHSv1-UC-REQ-191942/B-User changes security encryption through WifiHotspotOnBoardClient | | jshelby5: Bundle 3 update: added HMI reference. |
|  | WFHS-REQ-191650/B-Displaying the status of the visibility feature | | jshelby5: Bundle 3 update: added HMI reference. |
|  | WFHSv1-UC-REQ-191943/B-User turns the Wi-Fi Hotspot visibility on | | jshelby5: Bundle 3 update: added HMI reference. |
|  | WFHSv1-UC-REQ-191944/B-User turns Wi-Fi Hotspot visibility off | | jshelby5: Bundle 3 updates: added HMI reference. |
|  | WFHS-REQ-191653/C-Managing the connected devices list+ | | jshelby5: Bundle 3 update: Device name characters length shall be equal to the length defined in the referenced requirements. |
|  | WFHS-REQ-191701/C-Displaying the connected devices list on the WifiHotspotOnBoardClient display+ | | jshelby5: Bundle 3 update: Max device name char length shall be equal to that listed in the referenced requirement. |
|  | WFHS-REQ-191701/D-Displaying the connected devices list on the WifiHotspotOnBoardClient display | | jshelby5: Bundle 3 update: added HMI reference. |
|  | WFHS-REQ-191654/B-Reporting the connected devices list | | jshelby5: Bundle 3 update: deleted the 17 char default for device name. |
|  | WFHS-REQ-191702/C-Updating the connected devices screen while the user is in the screen | | jshelby5: Bundle 3 update: added HMI reference. |
|  | WFHS-REQ-191696/B-Managing the blocked devices list+ | | jshelby5: Bundle 3 update: deleted 17 char default for device name. |
|  | WFHS-REQ-191694/B-User requests to block a device from the hotspot through WifiHotspotOnBoardClient display | | jshelby5: Bundle 3 update: added HMI reference. |
|  | WFHS-REQ-191703/C-Displaying the blocked devices list on the WifiHotspotOnBoardClient display | | jshelby5: Bundle 3 update: added HMI reference. |
|  | WFHS-REQ-191704/C-User requests to unblock a device from the blocked list through WifiHotspotOnBoardClient display | | jshelby5: Bundle 3 update: added HMI reference. |
|  | WFHSv1-FUN-REQ-140754/D-Reporting Data Used | | jshelby5: bundle 3 update. Added User ID. |
|  | STR-207794/C-Requirements+ | | jshelby5: Bundle 3 update for CHR: added req WFHSv2-REQ-206087 |
|  | STR-207794/D-Requirements | | jshelby5: bundle 3 update. Added WFHS-REQ-212822. |
|  | WFHS-REQ-191871/D-WifiHotspotOnBoardClient initiates data usage request due to user entering into Wi-Fi Hotspot menu | | jshelby5: Bundle 3 update: added HMI reference. |
|  | WFHS-REQ-191864/C-Request to refresh data usage info without a response required | | jshelby5: Bundle 3 update: Added Europe. |
|  | WFHS-REQ-191872/E-Displaying data usage information+ | | jshelby5: Bundle 3 update: added HMI reference and added Europe requirements. |
|  | WFHS-REQ-191872/I-Displaying data usage information | | jshelby5: added bundle 3 requirements. |
|  | WFHSv2-REQ-206087/B-Displaying data usage information | | jshelby5: deleted table. Added mobile app name disclaimer. |
|  | WFHS-REQ-197429/C-Displaying elapsed time since a data usage update | | jshelby5: Bundle 3 updates: added HMI reference. |
|  | WFHS-REQ-191873/D-Rounding data usage values | | jshelby5: Bundle 3 update: added HMI reference. |
|  | WFHS-REQ-191874/C-User refreshes data usage screen+ | | jshelby5: Bundle 3 update: added HMI reference. |
|  | WFHS-REQ-191874/D-User refreshes data usage screen+ | | jshelby5: clarification: data usage refresh timer shall not be EOL configurable. |
|  | WFHS-REQ-191874/E-User refreshes data usage screen | | jshelby5: Bundle 3 update. Added HMI spec reference. Added default timer of 30 seconds. |
|  | WFHS-REQ-191868/D-Request from WifiHotspotOnBoardClient to refresh the data usage values | | jshelby5: Bundle 3 update: added Europe requirement. |
|  | WFHSv1-SD-REQ-167143/C-User Refreshes Data Usage Values From Centerstack | | MBORREL4: Updated diagram to reflect changes to DataUsage\_Rsp |
|  | WFHSv1-FUN-REQ-140748/C-Carrier Data Notification+ | | jshelby5: Bundle 3 update: low duration notifications shall be added. |
|  | WFHSv1-FUN-REQ-140748/D-Carrier Data Notification | | jshelby5: bundle 3 update: deleted low duration notification. Changed 2 seconds to 1 second. |
|  | WFHS-REQ-191882/D-Triggering free trial period reminders+ | | jshelby5: Bundle 3 update: added HMI reference. Added default values for EU. |
|  | WFHS-REQ-191882/E-Triggering free trial period reminders | | jshelby5: bundle 3 update: deleted repetition DID and added a Reminder delay DID. WifiHotspotServer shall only continue notifying WifiHotspotOnBoardClient of trial reminders if user chooses the Remind me later option. |
|  | WFHS-REQ-191881/D-Displaying critical data plan related popups+ | | jshelby5: Bundle 3 updates: added HMI reference. |
|  | WFHS-REQ-191881/E-Displaying critical data plan related popups | | jshelby5: bundle 3 updates. Trial reminder popup shall include the option to remind the customer later. |
|  | WFHSv1-UC-REQ-191963/D-The vehicle's Wi-Fi Hotspot data plan changes to a low balance, low duration, expired or trial period waiting status+ | | jshelby5: Bundle 3 update: added HMI reference. |
|  | WFHSv1-UC-REQ-191963/E-The vehicle's Wi-Fi Hotspot data plan changes to a low balance or expired or trial period waiting status | | jshelby5: bundle 3: deleted low duration notification. |
|  | STR-266643/B-Activity Diagrams | | MBORREL4: Added REQ-212880 |
|  | WFHSv1-ACT-REQ-167116/D-Carrier Data Notification Received | | MBORREL4: Updated diagram to remove the Carrier Info request/response interaction as this was removed from the HMI screen for this item. |
|  | WFHSv1-ACT-REQ-212880/A-Free Trial Period Reminders | | MBORREL4: New Req. |
|  | STR-266644/B-Sequence Diagrams | | MBORREL4: Added REQ-212881 |
|  | WFHSv1-SD-REQ-167139/D-Carrier Data Notification Received | | MBORREL4: Updated diagram to remove the Carrier Info request/response interaction as this was removed from the HMI screen for this item. |
|  | WFHSv1-SD-REQ-212881/A-Free Trial Period Reminders | | MBORREL4: New Req. |
|  | WFHSv1-FUN-REQ-192000/D-Managing Carrier Information | | jshelby5: bundle 3 updated. Added EU. |
|  | WFHS-REQ-191726/D-Updating the carrier landing page URL | | jshelby5: added EU. |
|  | WFHS-REQ-191875/C-Requesting for carrier information due to the user entering a specific screen | | jshelby5: Bundle 3 update: added HMI reference. |
|  | WFHS-REQ-191729/D-Reporting out the carrier information to the WifiHotspotOnBoardClient | | jshelby5: added EU req. |
|  | WFHS-REQ-191876/D-Displaying carrier information+ | | jshelby5: Bundle 3 updates: added HMI reference. |
|  | WFHS-REQ-191876/E-Displaying carrier information | | jshelby5: All fields in the Carrier Info response CAN signal may be populated. This should not affect the WifiHotspotOnBoardClient. |
|  | WFHS-REQ-191877/D-Initiating a call to the carrier hotline | | jshelby5: Bundle 3 update: added HMI reference. |
|  | WFHSv1-UC-REQ-191961/C-Customer purchases data/activates free trial period through connected device | | jshelby5: clarification: china vehicles and EU vehicles do not need to identify their vehicle. |
|  | WFHSv1-UC-REQ-194539/B-User accesses the landing page from the mobile app when WifiHotspotServer is authorized | | jshelby5: bundle 3 updates: use case only applies to NA and China. |
|  | WFHS-REQ-191785/C-Triggering a Wi-Fi Hotspot reset | | jshelby5: bundle 3 update. Different CAN signal may be used for CHR master reset. |
|  | WFHS-REQ-191863/D-Wi-Fi Hotspot reset settings | | jshelby5: bundle 3 update. Deleted Wi-Fi\_Trial\_Reminder\_Repetition from table and added Wi-Fi\_Trial\_Reminder\_Delay. Added Display\_Carrier\_UserID parameter. Edited first paragraph (table does not list default values). |
|  | WFHSv1-UC-REQ-191967/C-User performs a reset but does not deactivate their Wi-Fi Hotspot data plan | | jshelby5: Bundle 3 update: added HMI reference. |
|  | WFHSv1-UC-REQ-191968/C-Dealer replaces WifiHotspotServer while a Wi-Fi Hotspot data plan is active | | jshelby5: bundle 3 update. Added EU scenario. |
|  |  |  |  |
| **June 22, 2016** | **1.5** | **Updated Release** |  |
|  | WFHS-REQ-210528/B-Logical Signal Mapping | | jshelby5: bundle 3 update: clarification: updated technology used CAN siganl name and logical name. Added number of devices CAN signal and trial reminder selection CAN signal. Added CAN signal for DTCs, data usage and APN connection. Removed security request signal. |
|  | WFHS-IIR-REQ-179285/D-WifiHotspotServer\_Tx | | MBORREL4: Added new REQ-222048, REQ-222050, REQ-222051 |
|  | MD-REQ-222048/A-TelematicsDTC\_St | | MBORREL4: New signal |
|  | MD-REQ-222050/A-DataUsageFeature\_St | | MBORREL4: New signal |
|  | MD-REQ-222051/A-HotspotAPNConnection\_St | | MBORREL4: New signal |
|  | WFHS-IIR-REQ-179315/D-WifiHotspotServer\_Rx | | MBORREL4: Removed REQ-179289 |
|  | STR-207834/B-General Requirements | | MBORREL4: Added REQ-226336 and REQ-226337 |
|  | WFHS-REQ-226336/A-HMI Specification References | | MBORREL4: New Req. for spec referencing |
|  | WFHS-REQ-226337/A-Diagnostic Specification References | | MBORREL4: New Req. for spec referencing |
|  | WFHS-REQ-191640/E-WifiHotspotOnBoardClient identifies the vehicle brand | | jshelby5: Updated reference. |
|  | WFHS-REQ-191641/E-WifiHotspotOnBoardClient identifies the vehicle region | | jshelby5: Updated reference. |
|  | WFHS-REQ-191639/D-WifiHotspotServer identifies the vehicle region | | jshelby5: updated reference. Added requirement for country code. |
|  | WFHS-REQ-191705/G-Monitoring Wi-Fi Hotspot feature availability+ | | jshelby5: Bundle 3 update: added CAN signal name for DTCs. |
|  | WFHS-REQ-191705/H-Monitoring Wi-Fi Hotspot feature availability | | jshelby5: updated reference. |
|  | WFHS-REQ-191710/E-Disabling driver restricted screens | | jshelby5: updated reference. |
|  | WFHS-REQ-191899/B-Reporting out diagnostics+ | | jshelby5: added CAN signal for informing WifiHotspotOnBoardClient of a Wi-Fi DTC. |
|  | WFHS-REQ-191899/C-Reporting out diagnostics | | jshelby5: updated reference. |
|  | WFHS-REQ-191902/C-APN connections | | jshelby5: EU APN shall be written at EOL. APN updates OTA shall follow specific procedure. |
|  | WFHS-REQ-191903/C-Wi-Fi Hotspot feature dependency on the WifiHotspotServer authorization state | | jshelby5: added Privacy Mode requirements. |
|  | WFHS-REQ-191906/B-AP connection rules | | jshelby5: removed WAPI. |
|  | WFHS-REQ-192111/C-Wi-Fi Chipset AP and STA mode | | jshelby5: carry-over change from bundle 2. Part of Wi-Fi provisioning DCR for bundle 2. WiFi chipset shall be enabled for STA mode if WifiHotspotServer is configured to provision over Wi-Fi. |
|  | WFHS-REQ-194010/E-Wi-Fi Hotspot parameters transmitted during provisioning | | jshelby5: IMSI and country code are required. |
|  | WFHS-REQ-194471/C-WifiHotspotServer becomes not authorized | | jshelby5: added privacy mode. |
|  | WFHSv1-UC-REQ-191983/D-User wakes WifiHotspotOnBoardClient up before WifiHotspotServer wakes up | | jshelby5: updated reference. |
|  | WFHSv1-UC-REQ-191984/C-User is navigating in the Wi-Fi Hotspot screens when WifiHotspotOnBoardClient loses communication with WifiHotspotServer | | jshelby5: updated reference. |
|  | WFHSv1-UC-REQ-191986/C-User is navigating in the Wi-Fi Hotspot screens when a Wi-Fi error occurs | | jshelby5: updated reference. |
|  | WFHSv1-FUN-REQ-191999/D-Displaying WifiHotspotServer icon | | jshelby5: number of connected devices shall not be displayed on the WifiHotspotServer icon. |
|  | STR-285755/D-Requirements | | jshelby5: added WFHS-REQ-222428 & WFHS-REQ-222469. |
|  | WFHS-REQ-191713/F-Reporting out technology used to connect to the cellular network | | jshelby5: connection status shall not be tied to WiFi APN only. |
|  | WFHS-REQ-191712/D-Converting and reporting out the number of WifiHotspotServer signal strength bars | | jshelby5: connection status shall not relay on the Wi-Fi APN only. |
|  | WFHS-REQ-191714/F-Displaying the dedicated WifiHotspotServer icon on the WifiHotspotOnBoardClient display+ | | jshelby5: WifiHotspotServer icon is no longer used to represent Wi-Fi Hotspot. It does not show number of connected devices. |
|  | WFHS-REQ-191714/G-Displaying the dedicated WifiHotspotServer icon on the WifiHotspotOnBoardClient display | | jshelby5: updated reference. |
|  | WFHS-REQ-212165/B-Displaying the Wi-Fi Hotspot icon+ | | jshelby5: number of connected devices no longer matters when displaying the icon. |
|  | WFHS-REQ-212165/C-Displaying the Wi-Fi Hotspot icon | | jshelby5: updated reference. |
|  | WFHS-REQ-222469/B-Displaying the number of connected devices | | jshelby5: updated references. |
|  | WFHS-REQ-191706/C-Wi-Fi Hotspot enablement condition checks | | jshelby5: updated reference. |
|  | WFHS-REQ-191708/D-Displaying the Wi-Fi Hotspot's enablement state on the WifiHotspotOnBoardClient display | | jshelby5: updated reference. |
|  | WFHSv1-UC-REQ-191925/C-User turns Wi-Fi Hotspot On | | jshelby5: updated reference. |
|  | WFHSv1-UC-REQ-191926/C-User turns Wi-Fi Hotspot Off | | jshelby5: updated reference. |
|  | WFHSv1-UC-REQ-191927/C-User attempts to turn the Wi-Fi Hotspot on when the Wi-Fi Hotspot enablement conditions are not met | | jshelby5: updated reference. |
|  | WFHSv1-UC-REQ-191928/D-Wi-Fi Hotspot in On-disabled state when the Wi-Fi Hotspot enablement conditions become met | | jshelby5: updated reference. |
|  | WFHSv1-UC-REQ-191929/C-Wi-Fi Hotspot is on when the Wi-Fi Hotspot enablement conditions become not met | | jshelby5: updated reference. |
|  | WFHSv1-UC-REQ-191916/D-User turns ignition to Run while the Wi-Fi Hotspot is on-disabled | | jshelby5: updated reference. |
|  | WFHSv1-UC-REQ-191920/D-User turns vehicle completely off and exits the vehicle | | jshelby5: updated reference. |
|  | WFHSv1-UC-REQ-191921/D-User enters vehicle and turns ignition to accessory | | jshelby5: updated reference. |
|  | WFHSv1-UC-REQ-191922/C-User turns the engine off when enhanced hotspot enablement mode is off | | jshelby5: updated reference. |
|  | WFHSv1-UC-REQ-191923/D-Vehicle enters transport mode | | jshelby5: updated reference. |
|  | WFHSv1-UC-REQ-191924/D-Battery is used excessively | | jshelby5: updated reference. |
|  | WFHS-REQ-191634/D-Displaying the SSID on the WifiHotspotOnBoardClient display | | jshelby5: updated reference. |
|  | WFHS-REQ-191629/C-Keyboard used to edit the SSID through WifiHotspotOnBoardClient display | | jshelby5: updated reference. |
|  | WFHS-REQ-191635/C-Excepting and updating user SSID configurations+ | | jshelby5: clarification: wrong screen ID was referenced. |
|  | WFHS-REQ-191635/D-Excepting and updating user SSID configurations | | jshelby5: updated reference. |
|  | WFHSv1-UC-REQ-191936/D-E5 User attempts to view SSID/password through WifiHotspotOnBoardClient while under driver restriction | | jshelby5: updated reference. |
|  | WFHS-REQ-191633/D-Displaying the password on the WifiHotspotOnBoardClient display | | jshelby5: updated reference. |
|  | WFHS-REQ-191632/C-Keyboard used to edit the password through WifiHotspotOnBoardClient display | | jshelby5: updated reference. |
|  | WFHS-REQ-191636/C-Excepting and updating user password configurations | | jshelby5: updated reference. |
|  | WFHSv1-UC-REQ-191937/E-User enters into the Wi-Fi Hotspot screen that displays the SSID and password | | jshelby5: updated reference. |
|  | WFHSv1-FUN-REQ-140745/C-Changing Security Algorithm | | jshelby5: there shall be one security encryption used for all regions. MBORREL4: Removed Use Cases and Whitebox Views sections (containing REQ-191942, 167119, 167134) |
|  | STR-207806/B-Requirements | | jshelby5: removed WFHS-REQ-191645, WFHS-REQ-191646, WFHS-REQ-191643 |
|  | WFHS-REQ-191642/D-Security algorithm offerings per region | | jshelby5: carry-over from bundle 2. Only one security algorithm shall be used. |
|  | WFHS-REQ-191644/C-Displaying the security type | | jshelby5: updated reference. |
|  | WFHS-REQ-191650/C-Displaying the status of the visibility feature | | jshelby5: updated reference. |
|  | WFHSv1-UC-REQ-191943/C-User turns the Wi-Fi Hotspot visibility on | | jshelby5: updated reference. |
|  | WFHSv1-UC-REQ-191944/C-User turns Wi-Fi Hotspot visibility off | | jshelby5: updated reference. |
|  | WFHS-REQ-191701/E-Displaying the connected devices list on the WifiHotspotOnBoardClient display | | jshelby5: updated reference. |
|  | WFHS-REQ-191702/D-Updating the connected devices screen while the user is in the screen | | jshelby5: updated reference. |
|  | WFHS-REQ-191694/C-User requests to block a device from the hotspot through WifiHotspotOnBoardClient display | | jshelby5: updated reference. |
|  | WFHS-REQ-191703/D-Displaying the blocked devices list on the WifiHotspotOnBoardClient display | | jshelby5: updated reference. |
|  | WFHS-REQ-191704/D-User requests to unblock a device from the blocked list through WifiHotspotOnBoardClient display | | jshelby5: updated reference. |
|  | WFHSv1-FUN-REQ-140754/E-Reporting Data Used | | jshelby5: Data Usage shall not work if privacy mode is On. |
|  | STR-207794/E-Requirements | | jshelby5: added WFHS-REQ-222037, removed WFHS-REQ-212822 |
|  | WFHS-REQ-222045/B-Hiding data usage screen based on data usage feature flag | | jshelby5: New requirement |
|  | WFHS-REQ-191871/E-WifiHotspotOnBoardClient initiates data usage request due to user entering into Wi-Fi Hotspot menu | | jshelby5: WifiHotspotOnBoardClient shall check the data usage timer before determining whether to request for a data usage refresh upon entering into the main menu. Updated reference. |
|  | WFHS-REQ-191864/D-Request to refresh data usage info without a response required | | jshelby5: bundle 3 clarification: clarifies how WifiHotspotServer shall react if it receives a data usage response after the timer expires. Data usage queries shall not be allowed if privacy mode is on. |
|  | WFHS-REQ-191872/J-Displaying data usage information | | jshelby5: clarification: updated screen ID references. WifiHotspotOnBoardClient shall check the data usage timer. WifiHotspotOnBoardClient shall check Privacy mode. Updated reference. |
|  | WFHSv2-REQ-206087/C-Displaying data usage information | | jshelby5: WifiHotspotOnBoardClient shall check the data usage timer before determining whether to request for the current data. WifiHotspotOnBoardClient shall check privacy mode. Updated reference. |
|  | WFHS-REQ-197429/D-Displaying elapsed time since a data usage update | | jshelby5: updated reference. |
|  | WFHS-REQ-191873/E-Rounding data usage values | | jshelby5: updated reference. |
|  | WFHS-REQ-191874/F-User refreshes data usage screen | | jshelby5: WifiHotspotOnBoardClient shall refer to its data usage timeout timer to determine if it shall inform the user of an update in progress. |
|  | WFHS-REQ-191868/E-Request from WifiHotspotOnBoardClient to refresh the data usage values | | jshelby5: Bundle 3 clarification: clarifies how the WifiHotspotServer shall react if it receives a data usage response after the timer expires. Data Usage is not allowed if Privacy Mode is On. |
|  | WFHS-REQ-199543/B-Monitoring elapsed time since the data usage update | | jshelby5: updated reference. |
|  | STR-207793/B-Use Cases | | MBORREL4: Added new use case REQ-222995 |
|  | WFHSv1-UC-REQ-191945/D-User accesses the data usage screen in a good network coverage area | | jshelby5: Privacy mode is off |
|  | WFHSv1-UC-REQ-191946/D-User accesses the data usage screen in a no network coverage area | | jshelby5: privacy mode is off. |
|  | WFHSv1-UC-REQ-191947/B-User enters into the Wi-Fi Hotspot menu and refreshes the data usage screen immediately | | jshelby5: updating popup shall not be displayed. Privacy Mode is off. |
|  | WFHSv1-UC-REQ-191948/C-User refreshes the data usage values from the WifiHotspotOnBoardClient | | jshelby5: no updating popup shall be displayed. User shall not be locked out. Privacy mode is off. |
|  | WFHSv1-UC-REQ-191949/C-User refreshes data usage values from WifiHotspotOnBoardClient when vehicle is in a no coverage area | | jshelby5: privacy mode is off. |
|  | WFHSv1-UC-REQ-191950/B-User refreshes data usage values from WifiHotspotOnBoardClient when vehicle is in a poor coverage area | | jshelby5: updating popup shall not be displayed. Privacy mode is off. |
|  | WFHSv1-UC-REQ-191951/B-User refreshes the data usage values on the mobile app in a good coverage area | | jshelby5: privacy mode must be off |
|  | WFHSv1-UC-REQ-191952/B-User refreshes the data usage values on the mobile app in a no coverage area | | jshelby5: privacy mode is off |
|  | WFHSv1-UC-REQ-191953/C-User refreshes the data usage values on the mobile app while in the Wi-Fi Hotspot screen on the WifiHotspotOnBoardClient display | | jshelby5: privacy mode is off. |
|  | WFHSv1-UC-REQ-194537/C-User accesses the mobile app while WifiHotspotServer is not authorized | | jshelby5: privacy mode may be on. |
|  | WFHSv1-UC-REQ-194540/C-User accesses the data usage screen while WifiHotspotServer is un-authorized | | jshelby5: privacy mode is off. |
|  | WFHS-UC-REQ-222995/A-User accesses the data usage screen while Privacy Mode is On | | jshelby5: new use case. |
|  | WFHSv1-FUN-REQ-140748/E-Carrier Data Notification | | jshelby5: Privacy Mode must be checked. |
|  | WFHS-REQ-191880/C-Receiving carrier data notifications and data usage updates | | jshelby5: bundle 3 update: notifications shall not be accepted if data usage feature DID is set to Off. |
|  | WFHS-REQ-191882/F-Triggering free trial period reminders+ | | jshelby5: clarification: updated the note at the end of the requirement. |
|  | WFHS-REQ-191882/G-Triggering free trial period reminders | | jshelby5: updated reference. |
|  | WFHS-REQ-191881/F-Displaying critical data plan related popups | | jshelby5: updated references. |
|  | WFHSv1-UC-REQ-191963/F-The vehicle's Wi-Fi Hotspot data plan changes to a low balance or expired or trial period waiting status | | jshelby5: Privacy mode must be off. Updated reference. |
|  | WFHS-REQ-191875/D-Requesting for carrier information due to the user entering a specific screen | | jshelby5: updated reference. |
|  | WFHS-REQ-191876/F-Displaying carrier information | | jshelby5: updated reference. |
|  | WFHS-REQ-191877/E-Initiating a call to the carrier hotline | | jshelby5: updated reference. |
|  | WFHSv1-UC-REQ-191959/C-China customer initiates a call to the carrier hotline though the WifiHotspotOnBoardClient display | | jshelby5: updated reference. |
|  | WFHSv1-UC-REQ-194537/C-User accesses the mobile app while WifiHotspotServer is not authorized | | jshelby5: privacy mode may be on. |
|  | WFHS-REQ-191785/D-Triggering a Wi-Fi Hotspot reset | | jshelby5: CHR shall use same CAN signal for a master reset. |
|  | WFHS-REQ-191863/E-Wi-Fi Hotspot reset settings | | jshelby5: deleted Display Carrier User ID parameter. |
|  | WFHSv1-UC-REQ-191967/D-User performs a reset but does not deactivate their Wi-Fi Hotspot data plan | | jshelby5: user shall be informed that their subscription may not be cancelled. Updated reference. |
|  |  |  |  |
| **June 28, 2016** | **1.6** | **Updated Release** |  |
|  | STR-207834/C-General Requirements | | MBORREL4: Added new REQ-227355 & REQ-226998 |
|  | WFHSv2-SR-REQ-227355/A-Request/Response return to Null/NoRequest state | | MBORREL4: New req. for B3 |
|  | WFHS-TMR-REQ-226998/A-T\_ReturnToNull\_NoRequest | | MBORREL4: New req. |
|  |  |  |  |
| **August 5, 2016** | **1.7** | **Updated Release** | **Removal of Privacy Mode** |
|  | WFHS-REQ-191903/D-Wi-Fi Hotspot feature dependency on the WifiHotspotServer authorization state | | jshelby5: privacy mode removed. |
|  | WFHS-REQ-194471/D-WifiHotspotServer becomes not authorized | | jshelby5: privacy mode removed. |
|  | WFHS-REQ-191706/D-Wi-Fi Hotspot enablement condition checks | | jshelby5: WiFi Hotspot enablement shall always be allowed to be on when ignition status is in Run, regardless of the BSBattSOC signal. |
|  | WFHSv1-UC-REQ-191916/E-User turns ignition to Run while the Wi-Fi Hotspot is on-disabled | | jshelby5: Enhanced hotspot enablement mode and BSBattSOC checks not needed in pre-condition. |
|  | WFHSv1-UC-REQ-191924/E-Battery is used excessively | | jshelby5: Engine shall be off, enhanced hotspot enablement mode shall be on. OR logic used instead of AND logic. |
|  | WFHSv1-FUN-REQ-140754/F-Reporting Data Used | | jshelby5: privacy mode removed. |
|  | WFHS-REQ-191864/E-Request to refresh data usage info without a response required | | jshelby5: Privacy mode removed. |
|  | WFHS-REQ-191872/K-Displaying data usage information | | jshelby5: Privacy Mode removed. |
|  | WFHSv2-REQ-206087/D-Displaying data usage information | | jshelby5: privacy mode removed. |
|  | WFHS-REQ-191868/F-Request from WifiHotspotOnBoardClient to refresh the data usage values | | jshelby5: privacy mode removed. |
|  | STR-207793/C-Use Cases | | jshelby5: removed WFHS-UC-REQ-222995 |
|  | WFHSv1-UC-REQ-191945/E-User accesses the data usage screen in a good network coverage area | | jshelby5: privacy mode removed. |
|  | WFHSv1-UC-REQ-191946/E-User accesses the data usage screen in a no network coverage area | | jshelby5: privacy mode removed. |
|  | WFHSv1-UC-REQ-191947/C-User enters into the Wi-Fi Hotspot menu and refreshes the data usage screen immediately | | jshelby5: privacy mode removed. |
|  | WFHSv1-UC-REQ-191948/D-User refreshes the data usage values from the WifiHotspotOnBoardClient | | jshelby5: privacy mode removed. |
|  | WFHSv1-UC-REQ-191949/D-User refreshes data usage values from WifiHotspotOnBoardClient when vehicle is in a no coverage area | | jshelby5: privacy mode removed. |
|  | WFHSv1-UC-REQ-191950/C-User refreshes data usage values from WifiHotspotOnBoardClient when vehicle is in a poor coverage area | | jshelby5: privacy mode removed. |
|  | WFHSv1-UC-REQ-191951/C-User refreshes the data usage values on the mobile app in a good coverage area | | jshelby5: privacy mode removed. |
|  | WFHSv1-UC-REQ-191952/C-User refreshes the data usage values on the mobile app in a no coverage area | | jshelby5: privacy mode removed. |
|  | WFHSv1-UC-REQ-191953/D-User refreshes the data usage values on the mobile app while in the Wi-Fi Hotspot screen on the WifiHotspotOnBoardClient display | | jshelby5: privacy mode removed. |
|  | WFHSv1-UC-REQ-194537/D-User accesses the mobile app while WifiHotspotServer is not authorized | | jshelby5: privacy mode removed. |
|  | WFHSv1-UC-REQ-194540/D-User accesses the data usage screen while WifiHotspotServer is un-authorized | | jshelby5: privacy mode removed. |
|  | WFHSv1-FUN-REQ-140748/F-Carrier Data Notification | | jshelby5: privacy mode removed. |
|  | WFHS-REQ-191880/D-Receiving carrier data notifications and data usage updates | | jshelby5: privacy mode removed. |
|  | WFHSv1-UC-REQ-191963/G-The vehicle's Wi-Fi Hotspot data plan changes to a low balance or expired or trial period waiting status | | jshelby5: privacy mode removed. |
|  | WFHSv1-UC-REQ-194537/D-User accesses the mobile app while WifiHotspotServer is not authorized | | jshelby5: privacy mode removed. |
|  |  |  |  |
| **April 25, 2017** | **1.8** | **Updated Release** |  |
|  | WFHS-REQ-210528/C-Logical Signal Mapping | | MBORREL4: Removed FactoryReset\_Rq |
|  | WFHS-IIR-REQ-179315/E-WifiHotspotServer\_Rx | | MBORREL4: Removed REQ-031265/A-FactoryReset\_Rq (captured in EMR SPSS) |
|  | WFHS-REQ-191708/E-Displaying the Wi-Fi Hotspot's enablement state on the WifiHotspotOnBoardClient display | | jshelby5: Clarification: Deleted picture of on-disabled screen. |
|  | WFHS-REQ-191635/E-Accepting and updating user SSID configurations | | jshelby5: Updated title, added requirement for the WifiHotspotOnBoardClient to re-request for the SSID/psswd if it is updated while the user is on the screen. |
|  | WFHSv1-ACT-REQ-167121/B-User Changes SSID From Centerstack | | MBORREL4: Updated to include a read request for the saved SSID if the SSID is currently being displayed. |
|  | WFHSv1-SD-REQ-167136/B-User Changes SSID From Centerstack | | MBORREL4: Updated to include a read request for the saved SSID if the SSID is currently being displayed. |
|  | WFHS-REQ-191636/D-Accepting and updating user password configurations | | jshelby5: Updated title, added requirement for the WifiHotspotOnBoardClient to re-request for the SSID/psswd if it is updated while the user is on the screen. |
|  | WFHSv1-ACT-REQ-167117/B-User Changes Password From Centerstack | | MBORREL4: Updated to include a read request for the saved Password if the Password is currently being displayed. |
|  | WFHSv1-SD-REQ-167132/B-User Changes Password From Centerstack | | MBORREL4: Updated to include a read request for the saved Password if the Password is currently being displayed. |
|  | WFHS-REQ-191872/L-Displaying data usage information | | jshelby5: Clarification: Updated table to take out screen IDs. Made the description more generic. |
|  | WFHS-REQ-191868/G-Request from WifiHotspotOnBoardClient to refresh the data usage values | | jshelby5: Clarification: added spec clarification to inform WifiHotspotServer how to respond to an FTCP data usage response when not all fields are populated. |
|  | WFHS-REQ-191882/H-Triggering free trial period reminders | | jshelby5: Clarification: if WifiHotspotServer does not receive a command to update the trial reminder trigger, it shall not update this value. |
|  | WFHS-REQ-191785/E-Triggering a Wi-Fi Hotspot reset | | jshelby5: clarification: updated requirement to align with the Embedded Modem Reset SPSS update. |
|  |  |  |  |
| **April 28, 2017** | **1.9** | **Updated Release** |  |
|  | WFHS-REQ-210528/D-Logical Signal Mapping | | jshelby5: removed delay accessory, power mode, battery SOC and added frequency band rq, frequency band st, available band. |
|  | WFHS-IIR-REQ-179285/E-WifiHotspotServer\_Tx | | MBORREL4: Added REQ-263183, REQ-263184 |
|  | MD-REQ-263183/A-HotspotAvailableBands\_St | | MBORREL4: New signal |
|  | MD-REQ-263184/A-HotspotFrequencyBand\_St | | MBORREL4: New signal |
|  | WFHS-IIR-REQ-179315/F-WifiHotspotServer\_Rx | | MBORREL4: Added REQ-263185, removed REQ-077420, REQ-199634, REQ-201601 |
|  | MD-REQ-263185/A-HotspotFrequencyBand\_Rq | | MBORREL4: New signal |
|  | WFHSv2-SR-REQ-227355/B-Request/Response return to Null/NoRequest state | | MBORREL4: Added HotspotFrequencyBand\_Rq |
|  | STR-207866/D-Functional Definition | | MBORREL4: Added New Function: REQ-263189-Switching Frequency Bands |
|  | STR-285877/D-Requirements | | jshelby5: added REQ-263049, REQ-263050, REQ-263051, REQ-263052 |
|  | WFHS-REQ-191889/B-Wi-Fi signal strength | | jshelby5: removed old requirement. New req is still pending. |
|  | WFHS-REQ-191890/C-Wi-Fi throughput | | jshelby5: updated throughput values and added fairness model. |
|  | WFHS-REQ-191891/B-Modulation scheme | | jshelby5: updated req as modulation coding scheme is still in development. |
|  | WFHS-REQ-192117/C-Operating on the 2.4 GHz band in AP mode | | jshelby5: frequency band can be switched from a CAN signal request. |
|  | WFHS-REQ-263049/A-Broadcasting as a Vehicular AP | | jshelby5: New Req. |
|  | WFHS-REQ-263050/A-Broadcasting as a metered account | | jshelby5: New Req. |
|  | WFHS-REQ-263051/A-Metering each connection | | jshelby5: New Req. |
|  | WFHS-REQ-263052/A-Throttling data consumption | | jshelby5: New Req. |
|  | WFHS-REQ-191706/E-Wi-Fi Hotspot enablement condition checks | | jshelby5: removed dependency on battery state of charge, delayed accessory and 30 min timer. |
|  | STR-207797/B-Use Cases | | jshelby5: deleted REQ-191916, REQ-191917, REQ-191920, REQ-191921, REQ-191922, REQ-191924 |
|  | WFHS-REQ-191610/C-Generating the initial password | | jshelby5: password cannot use i or L. |
|  | WFHS-REQ-191653/E-Managing the connected devices list | | jshelby5: number of allowed devices shall be 20 and configurable. |
|  | WFHS-REQ-191701/F-Displaying the connected devices list on the WifiHotspotOnBoardClient display | | jshelby5: WifiHotspotOnBoardClient shall specify how it wants the list to be sent. |
|  | WFHS-REQ-191654/C-Reporting the connected devices list | | jshelby5: WifiHotspotOnBoardClient shall specify how it wants the device list to be sent and WifiHotspotServer shall respond accordingly. |
|  | WFHS-REQ-191696/D-Managing the blocked devices list | | jshelby5: blocked device list size shall be a configurable value. |
|  | WFHS-REQ-191703/E-Displaying the blocked devices list on the WifiHotspotOnBoardClient display | | jshelby5: WifiHotspotOnBoardClient shall specify how to request for the list. |
|  | WFHS-REQ-191698/B-Reporting the blocked devices list | | jshelby5: WifiHotspotOnBoardClient shall specify how the list shall be requested and the WifiHotspotServer shall respond accordingly. |
|  | WFHS-REQ-191863/F-Wi-Fi Hotspot reset settings | | jshelby5: added estimated location |
|  | WFHSv1-FUN-REQ-263189/A-Switching Frequency Bands | | MBORREL4: New Function |
|  | WFHS-REQ-263084/A-Estimating current vehicle location | | jshelby5: New Req. |
|  | WFHS-REQ-263085/A-Restricting frequency channels | | jshelby5: New Req. |
|  | WFHS-REQ-263087/A-Reporting available bands | | jshelby5: New Req. |
|  | WFHS-REQ-263088/A-Reporting the frequency band | | jshelby5: New Req. |
|  | WFHS-REQ-263089/A-Displaying the frequency band | | jshelby5: New Req. |
|  | WFHS-REQ-263090/A-User changes the frequency band on WifiHotspotOnBoardClient | | jshelby5: New Req. |
|  | WFHS-REQ-263091/A-Frequency band change request from WifiHotspotOnBoardClient | | jshelby5: New Req. |
|  | WFHSv1-UC-REQ-263187/A-User changes frequency band | | MBORREL4: New usecase |
|  | WFHSv1-UC-REQ-263186/A-User attempts to change to restricted frequency band | | MBORREL4: New usecase |
|  | WFHSv1-ACT-REQ-263190/A-User Changes Frequency Band From Centerstack | | MBORREL4: New Req. |
|  | WFHSv1-SD-REQ-263192/A-User Changes Frequency Band From Centerstack | | MBORREL4: New Req. |

**Table of Contents**

[Revision History 2](#_Toc481159352)

[1 Architectural Design 21](#_Toc481159353)

[1.1 Overview 21](#_Toc481159354)

[1.2 WFHS-CLD-REQ-191762/A-Wifi Hotspot Server 22](#_Toc481159355)

[1.3 WFHS-CLD-REQ-191763/A-Wifi Hotspot On Board Client 22](#_Toc481159356)

[1.4 WFHS-CLD-REQ-191764/A-Wifi Hotspot Off Board Client 22](#_Toc481159357)

[1.5 WFHS-CLD-REQ-207990/A-Wifi Hotspot Mobile Client 22](#_Toc481159358)

[1.6 WFHS-REQ-210528/D-Logical Signal Mapping 22](#_Toc481159359)

[1.7 WifiHotspotServer Interface 23](#_Toc481159360)

[1.7.1 WFHS-IIR-REQ-179285/E-WifiHotspotServer\_Tx 23](#_Toc481159361)

[1.7.2 WFHS-IIR-REQ-179315/F-WifiHotspotServer\_Rx 31](#_Toc481159362)

[2 General Requirements 36](#_Toc481159363)

[2.1 WFHS-HMI-REQ-192248/A-WifiHotspotOnBoardClient Transport Protocol Data Request 36](#_Toc481159364)

[2.2 WFHS-REQ-226336/A-HMI Specification References 36](#_Toc481159365)

[2.3 WFHS-REQ-226337/A-Diagnostic Specification References 36](#_Toc481159366)

[2.4 WFHSv2-SR-REQ-227355/B-Request/Response return to Null/NoRequest state 36](#_Toc481159367)

[2.5 WFHS-TMR-REQ-226998/A-T\_ReturnToNull\_NoRequest 37](#_Toc481159368)

[3 Functional Definition 38](#_Toc481159369)

[3.1 WFHSv1-FUN-REQ-192079/A-Wi-Fi General Usage 38](#_Toc481159370)

[3.1.1 Requirements 38](#_Toc481159371)

[3.1.2 Use Cases 46](#_Toc481159372)

[3.2 WFHSv1-FUN-REQ-191999/D-Displaying WifiHotspotServer icon 50](#_Toc481159373)

[3.2.1 Requirements 50](#_Toc481159374)

[3.3 WFHSv1-FUN-REQ-140757/A-Turning Wi-Fi Hotspot On or Off 53](#_Toc481159375)

[3.3.1 Requirements 53](#_Toc481159376)

[3.3.2 Use Cases 58](#_Toc481159377)

[3.3.3 White Box Views 62](#_Toc481159378)

[3.4 WFHSv1-FUN-REQ-140746/C-Managing SSID 64](#_Toc481159379)

[3.4.1 Requirements 64](#_Toc481159380)

[3.4.2 Use Cases 66](#_Toc481159381)

[3.4.3 White Box Views 68](#_Toc481159382)

[3.5 WFHSv1-FUN-REQ-140744/B-Managing Password 70](#_Toc481159383)

[3.5.1 Requirements 70](#_Toc481159384)

[3.5.2 Use Cases 72](#_Toc481159385)

[3.5.3 White Box Views 74](#_Toc481159386)

[3.6 WFHSv1-FUN-REQ-140745/C-Changing Security Algorithm 76](#_Toc481159387)

[3.6.1 Requirements 76](#_Toc481159388)

[3.7 WFHSv1-FUN-REQ-140758/A-Turning Visibility On or Off 77](#_Toc481159389)

[3.7.1 Requirements 77](#_Toc481159390)

[3.7.2 Use Cases 78](#_Toc481159391)

[3.7.3 White Box Views 79](#_Toc481159392)

[3.8 WFHSv1-FUN-REQ-140752/B-Manage Devices 81](#_Toc481159393)

[3.8.1 Requirements 81](#_Toc481159394)

[3.8.2 Use Cases 87](#_Toc481159395)

[3.8.3 White Box Views 90](#_Toc481159396)

[3.9 WFHSv1-FUN-REQ-140754/F-Reporting Data Used 97](#_Toc481159397)

[3.9.1 Requirements 97](#_Toc481159398)

[3.9.2 Use Cases 108](#_Toc481159399)

[3.9.3 White Box Views 113](#_Toc481159400)

[3.10 WFHSv1-FUN-REQ-140748/F-Carrier Data Notification 116](#_Toc481159401)

[3.10.1 Requirements 116](#_Toc481159402)

[3.10.2 Use Cases 120](#_Toc481159403)

[3.10.3 White Box Views 120](#_Toc481159404)

[3.11 WFHSv1-FUN-REQ-192000/D-Managing Carrier Information 124](#_Toc481159405)

[3.11.1 Requirements 124](#_Toc481159406)

[3.11.2 Use Cases 127](#_Toc481159407)

[3.11.3 White Box Views 130](#_Toc481159408)

[3.12 WFHSv1-FUN-REQ-140759/C-Wi-Fi Hotspot Reset 132](#_Toc481159409)

[3.12.1 Requirements 132](#_Toc481159410)

[3.12.2 Use Cases 134](#_Toc481159411)

[3.13 WFHSv1-FUN-REQ-195287/A-Transferring MAC Address 136](#_Toc481159412)

[3.13.1 Requirements 136](#_Toc481159413)

[3.13.2 White Box Views 136](#_Toc481159414)

[3.14 WFHSv1-FUN-REQ-263189/A-Switching Frequency Bands 138](#_Toc481159415)

[3.14.1 Requirements 138](#_Toc481159416)

[3.14.2 Use Cases 140](#_Toc481159417)

[3.14.3 White Box Views 141](#_Toc481159418)

[4 Appendix: Reference Documents 143](#_Toc481159419)

# Architectural Design

## Overview



The Wi-Fi (Wireless Fidelity) Hotspot feature allows Wi-Fi enabled devices to connect to the vehicle’s embedded telematics control unit (TCU) and stream data from the internet using the TCU’s 4G LTE MIMO (multiple in multiple out) antenna setup and modem. Vehicles equipped with SYNC or CHR (Connected HMI Radio) shall have a Wi-Fi Hotspot HMI that allows the user to interact with the Wi-Fi Hotspot feature. All data transmitted between the TCU and SYNC/CHR shall be through the vehicle’s CAN (controller area network) bus. Ford shall also offer a mobile app that may be used for subscription purposes. The NG-SDN (next generation service delivery network; contained within the Ford infrastructure) shall interface with the TCU, the mobile app and the wireless carrier’s backend. The carrier backend shall provide essential information to the NG-SDN regarding activation of hotspot data plans, data usage information and more.

The TCU shall be the sole server of the feature and shall be referred to as the WifiHotspotServer throughout this document. The WifiHotspotServer shall be responsible for controlling, transmitting and saving all Wi-Fi Hotspot settings. The NG-SDN and APIM shall act as the clients to the feature.  The NG-SDN, which shall be referred to as the WifiHotspotOffBoardClient in this document, shall store Wi-Fi Hotspot settings and shall route traffic between the WifiHotspotServer, mobile app and carrier backend. The mobile app shall store and display Wi-Fi Hotspot subscription information and accept customer input. The SYNC module or CHR module, which shall be referred to as the WifiHotspotOnBoardClient in this document, shall not be responsible for storing Wi-Fi Hotspot settings and shall only be used to accept customer input and display the Wi-Fi Hotspot settings by monitoring Wi-Fi Hotspot statuses and requesting for appropriate information when needed.

The use cases included in this document refer to command/control failures. The user may experience failures while attempting to utilize the WifiHotspotOnBoardClient or mobile app interface due to:

a.            Mobile app failure

b.            WifiHotspotServer failure

c.            WifiHotspotOnBoardClient failure

d.            CAN failure

e.            WifiHotspotOffBoardClient failure

f.             Cellular network failure

g.            Carrier backend failure

The example WifiHotspotOnBoardClient screens, popups and icons displayed throughout this document are example images and shall not be interpreted as the final implementation. Also, the screen names mentioned throughout this document are subject to change. Refer to the appropriate specifications identified in each requirement for the final implementation of WifiHotspotOnBoardClient screens, popups, screen names and icons.

## WFHS-CLD-REQ-191762/A-Wifi Hotspot Server

Responsibility: The Wifi Hotspot Server is responsible for storing Wifi content and providing that content to the display module when requested.

## WFHS-CLD-REQ-191763/A-Wifi Hotspot On Board Client

Responsibility: The Wifi Hotspot On Board Client is responsible for displaying the Wifi information to the vehicle user. The Wifi Hotspot On Board Client is also responsible for allowing the in vehicle user to adjust the Wifi settings.

## WFHS-CLD-REQ-191764/A-Wifi Hotspot Off Board Client

Responsibility: The Wifi Hotspot Off Board Client is responsible for supplying carrier information related to Wifi usage to the Wifi Hotspot Server.

## WFHS-CLD-REQ-207990/A-Wifi Hotspot Mobile Client

Responsibility: The Wifi Hotspot Mobile Client is a user’s Wi-Fi enabled device responsible for providing the user with a method to connect to and disconnect from the Wifi Hotspot (in STA mode).

## WFHS-REQ-210528/D-Logical Signal Mapping

The CAN signals mentioned throughout this document shall refer to the CAN signal’s logical name. The logical names shall be mapped to their actual CAN signal names. Please use the table below to perform the mapping. The InfoCAN database file is the master file for the actual CAN signal names. Note: some CAN signals referenced throughout this document may use the logical name while some may use the actual CAN signal name.

|  |  |
| --- | --- |
| **Logical Name** | **CAN Signal Name** |
| HotspotEnablement\_St | WifiHtsptEnbl\_D\_Stat |
| HotspotSecurity\_St | WifiHtsptScrty\_D\_Stat |
| HotspotVisibility\_St | WifiHtsptVisbl\_D\_Stat |
| NewDeviceList\_St | WifiDevcListNew\_B\_Stat |
| TCUSignalStrength\_St | ModemSigStren\_D\_Stat |
| TCUTechnologyUsed2\_St | ModemTechnology\_D2\_Stat |
| CarrierDataNotification\_St | WifiDataUsage\_D\_Stat |
| WifiDataUsage\_Pc\_Actl |
| TCUAvailability\_St | WifiEnbl\_D\_Stat |
| HotspotEnablement\_Rq | WifiHtsptEnbl\_D\_Rq |
| HotspotVisibility\_Rq | WifiHtsptVisbl\_D\_Rq |
| CarrierInfo\_Rq | WifiCarrierInfo\_B\_Rq |
| DataUsage\_Rq | WifiDataUsage\_D\_Rq |
| DeviceList\_Rq | WifiDevcList\_D\_Rq |
| WifiDevcListIndx\_No\_Rq |
| WifiDevcListSize\_D\_Rq |
| RemoveDevice\_Rq | WifiRemoveDevc\_D\_Rq |
| WifiRemoveIndx\_No\_Rq |
| IgnitionStatus\_St | Ignition\_Status |
| VehicleSpeed\_St | Veh\_V\_ActlEng |
| CarMode\_St | LifeCycMde\_D\_Actl (CGEA1.3) |
| CarMode\_St | CarMode (C1MCA) |
| OdometerMasterValue | OdometerMasterValue |
| HotspotFrequencyBand\_Rq | TBD |
| HotspotFrequencyBand\_St | TBD |
| HMIMode\_St | HMI\_HMIMode\_St |
| WifiHotspotMAC\_Rq | WifiHtsptMacAddr\_B\_Rq |
| HotspotAvailableBand\_St | TBD |
| VehicleGGCCData | VehicleGGCCData |
| TelematicsService\_St | TelematicsSrvc\_D\_St |
| NumberOfConnectedDevices\_St | WifiNoDevcCnnct\_No\_Actl |
| HotspotTrialReminderSelection\_Rq | WifiHtsptTrial\_D\_RqDrv |
| TelematicsDTC\_St | Telematics\_D\_Falt |
| DataUsageFeature\_St | WifiDataUsageOn\_D\_Stat |
| HotspotAPNConnection\_St | WifiHtsptCnnct\_D\_Stat |

Table. Logical name/CAN signal mapping

## WifiHotspotServer Interface

### WFHS-IIR-REQ-179285/E-WifiHotspotServer\_Tx

#### MD-REQ-179284/A-HotspotEnablement\_St

Message Type: Status

This signal is used to inform the WifiHotSpotOnBoardClient the current state of the Hotspot Enablement

|  |  |  |  |
| --- | --- | --- | --- |
| **Name** | **Literals** | **Value** | **Description** |
| Type | - | - | Wi-Fi chipset transmission status of Wi-Fi signal |
|  | Null | 0x0 |  |
|  | Off | 0x1 | No Wi-Fi signal transmission on Wi-Fi chipset |
|  | On | 0x2 | Wi-Fi chipset is transmitting Wi-Fi signal |
|  | On-Disabled | 0x3 | Wi-Fi chipset shall transmit Wi-Fi signal once other defined conditions are met |

#### MD-REQ-179291/A-HotspotSecurity\_St

Message Type: Status

This signal is used to inform the WifiHotSpotOnBoardClient the current state of the Hotpot Security Algorithm

|  |  |  |  |
| --- | --- | --- | --- |
| **Name** | **Literals** | **Value** | **Description** |
| Type | - | - | Current Security Algorithm in use |
|  | Null | 0x0 |  |
|  | WPA2-WPA | 0x1 |  |
|  | WAPI | 0x2 |  |

#### MD-REQ-179293/A-HotspotVisibility\_St

Message Type: Status

This signal is used to inform the WifiHotSpotOnBoardClient the current state of the Hotpot Visibility

|  |  |  |  |
| --- | --- | --- | --- |
| **Name** | **Literals** | **Value** | **Description** |
| Type | - | - | Wi-Fi chipset SSID transmission status |
|  | Null | 0x0 |  |
|  | Off | 0x1 | Wi-Fi chipset excludes SSID in its beacon frames |
|  | On | 0x2 | Wi-Fi chipset transmits SSID in its beacon frames |

#### MD-REQ-179299/A-NewDeviceList\_St

Message Type: Status

This signal is used to inform the WifiHotSpotOnBoardClient a new device has been added/removed to/from the WifiHotSpotServer

|  |  |  |  |
| --- | --- | --- | --- |
| **Name** | **Literals** | **Value** | **Description** |
| Type | - | - | Status bit to indicate a device has connected/disconnected to the hotspot's network |
|  | NotAvailable | 0x0 |  |
|  | Available | 0x1 |  |

#### MD-REQ-179301/A-TCUSignalStrength\_St

Message Type: Status

This signal is used to inform the WifiHotSpotOnBoardClient the status of the TCU signal strength

|  |  |  |  |
| --- | --- | --- | --- |
| **Name** | **Literals** | **Value** | **Description** |
| Type | - | - | Quality of TCU's signal strength |
|  | 0 Bars | 0x00 |  |
|  | 1 Bar | 0x01 |  |
|  | 2 Bars | 0x02 |  |
|  | 3 Bars | 0x03 |  |
|  | 4 Bars | 0x04 |  |
|  | 5 Bars | 0x05 |  |
|  | NotDetermined | 0x06 |  |

#### MD-REQ-212571/A-TCUTechnologyUsed2\_St

Message Type: Status

This signal is used to inform the WifiHotSpotOnBoardClient the current state of the TCU technology being used (ver2).

|  |  |  |  |
| --- | --- | --- | --- |
| **Name** | **Literals** | **Value** | **Description** |
| Type | - | - | Current TCU technology in use |
|  | Null | 0x00 |  |
|  | No Network | 0x01 |  |
|  | GSM | 0x02 |  |
|  | GPRS | 0x03 |  |
|  | EDGE | 0x04 |  |
|  | UMTS | 0x05 |  |
|  | HSPA+ | 0x06 | (includes HSPA, HSDPA and HSUPA) |
|  | LTE | 0x07 |  |

#### MD-REQ-179304/B-CarrierDataNotification\_St

Message Type: Status

This signal is used to inform the WifiHotSpotOnBoardClient the current state of the connected data plan's data availability.

|  |  |  |  |
| --- | --- | --- | --- |
| **Name** | **Literals** | **Value** | **Description** |
| NotificationType | - | - | State of the hotspot's current data plan |
|  | Null | 0x00 |  |
|  | Free Trial Period Waiting | 0x01 |  |
|  | Percent Data Used | 0x02 |  |
| Percent | - | - | Percent data left on hotspot's current data plan |
|  | 50 percent | 0x00 |  |
|  | 55 percent | 0x01 |  |
|  | 60 percent | 0x02 |  |
|  | 65 percent | 0x03 |  |
|  | … | … |  |
|  | 100 Percent | 0xA |  |
|  | Reserved | 0xB-0xF |  |

#### MD-REQ-179305/B-TCUAvailability\_St

Message Type: Status

This signal is used to inform the WifiHotSpotOnBoardClient the current state of the Wi-Fi Hotspot feature

|  |  |  |  |
| --- | --- | --- | --- |
| **Name** | **Literals** | **Value** | **Description** |
| Type | - | - | Wi-Fi feature readiness status |
|  | Null | 0x0 |  |
|  | Disable | 0x1 |  |
|  | Enable | 0x2 |  |

#### MD-REQ-179307/A-WifiInfo\_Rsp

Message Type: Response

This signal is used to respond to the WifiHotSpotOnBoardClient with the SSID or Password upon a Read operation, or the successful/failed result of the Write operation.

|  |  |  |  |
| --- | --- | --- | --- |
| **Name** | **Literals** | **Value** | **Description** |
| Response Code | - | - | Response code being sent |
|  | Reserved | 0x0 |  |
|  | Data | 0x1 | Response used to provide both SSID & Password |
|  | SSIDWritten | 0x2 | Response used to indicate SSID was written (CES to state success/fail) |
|  | PasswordWritten | 0x3 | Response used to indicate Password was written (CES to state success/fail) |
|  | Reserved | 0x4-0xFF |  |
| Password | - | - | Data array that consists of textual information up to 64 characters in length, plus end of string |
| SSID | - | - | Data array that consists of textual information up to 32 characters in length, plus end of string |

#### MD-REQ-179308/C-CarrierInfo\_Rsp

Message Type: Response

This signal is used to respond to the WifiHotSpotOnBoardClient with a Ford or Lincoln Landing URL and Ford or Lincoln Hotline Phone Number upon request.

|  |  |  |  |
| --- | --- | --- | --- |
| **Name** | **Literals** | **Value** | **Description** |
| Ford Landing page URL | - | - | Ford website displayed to update plan based on data availability and region.  Data array that consists of textual information up to 192 characters in length, plus end of string |
| Lincoln Landing page URL | - | - | Lincoln website displayed to update plan based on data availability and region. Data array that consists of textual information up to 192 characters in length, plus end of string |
| Ford Phone Number | - | - | Ford specific phone number displayed to update plan. Data array that consists of textual information up to 24 characters in length, plus end of string |
| Lincoln Phone Number | - | - | Lincoln specific phone number displayed to update plan. Data array that consists of textual information up to 24 characters in length, plus end of string |

#### MD-REQ-179309/C-DataUsage\_Rsp

Message Type: Response

This signal is used to respond to the WifiHotSpotOnBoardClient with the current state of the connected plans data usage variables.

|  |  |  |  |
| --- | --- | --- | --- |
| **Name** | **Literals** | **Value** | **Description** |
| CounterHour | - | - | Hour of the current data usage counter |
|  | Hour | 0x00-0x17 |  |
|  | Reserved | 0x18-0xFE |  |
|  | Invalid | 0xFF |  |
| CounterMinute | - | - | Minute of the current data usage counter |
|  | Minute | 0x00-0x3B |  |
|  | Reserved | 0x3C-0xFE |  |
|  | Invalid | 0xFF |  |
| CounterSecond | - | - | Second of the current data usage counter |
|  | Second | 0x00-0x3B |  |
|  | Reserved | 0x3C-0xFE |  |
|  | Invalid | 0xFF |  |
| PlanType | - | - | Plan type being used |
|  | Invalid | 0x0 |  |
|  | Shared | 0x1 |  |
|  | Session | 0x2 |  |
| Expiry/RenewalDate | - | - | The text used to differentiate between an Expiry and Renewal Date |
|  | Invalid | 0x0 |  |
|  | Expiry Date | 0x1 |  |
|  | Renewal Date | 0x2 |  |
| Expiry/RenewalMonth | - | - | Month of the next Expiry/Renewal Date |
|  | Invalid | 0x00 |  |
|  | January | 0x01 |  |
|  | February | 0x02 |  |
|  | March | 0x03 |  |
|  | April | 0x04 |  |
|  | May | 0x05 |  |
|  | June | 0x06 |  |
|  | July | 0x07 |  |
|  | August | 0x08 |  |
|  | September | 0x09 |  |
|  | October | 0x0A |  |
|  | November | 0x0B |  |
|  | December | 0x0C |  |
|  | Reserved | 0x0D-0xFF |  |
| Expiry/RenewalDay | - | - | Day of the next Expiry/Renewal Date |
|  | Invalid | 0x00 |  |
|  | Day | 0x01-0x1F |  |
|  | Reserved | 0x20-0xFF |  |
| Expiry/RenewalYear | - | - | Year of the next Expiry/Renewal Date. Offset of 2000 |
|  | Year | 0x00-0xFE |  |
|  | Invalid | 0xFF |  |
| Expiry/RenewalHour | - | - | Hour of the Expiry/Renewal Date |
|  | Hour | 0x00-0x17 |  |
|  | Reserved | 0x18-0xFE |  |
|  | Invalid | 0xFF |  |
| Expiry/RenewalMinute | - | - | Minute of the Expiry/Renewal Date |
|  | Minute | 0x00-0x3B |  |
|  | Reserved | 0x3C-0xFE |  |
|  | Invalid | 0xFF |  |
| Expiry/RenewalSecond | - | - | Second of the Expiry/Renewal Date |
|  | Second | 0x00-0x3B |  |
|  | Reserved | 0x3C-0xFE |  |
|  | Invalid | 0xFF |  |
| DataUsed | - | - | Data used since start of last Renewal Date. Use HEX encoding here. Data values are in steps of 0.01 decimal units (ex. 0x08707 = 34567 = 345.67 Mb (or Kb or Gb) |
|  | Data | 0x000000-0x01869F |  |
|  | Reserved | 0x0186A0-0xFFFFFE |  |
|  | Invalid | 0xFFFFFF |  |
| DataUsedUnits | - | - | Units of measure used to report the data used |
|  | Invalid | 0x0 |  |
|  | KB | 0x1 |  |
|  | MB | 0x2 |  |
|  | GB | 0x3 |  |
| TotalData | - | - | Total data available in current Renewal Date. Use HEX encoding here. Data values are in steps of 0.01 decimal units (ex. 0x08707 = 34567 = 345.67 Mb (or Kb or Gb) |
|  | Data | 0x000000-0x01869F |  |
|  | Unlimited | 0x0186A0 |  |
|  | Reserved | 0x0186A1-0xFFFFFE |  |
|  | Invalid | 0xFFFFFF |  |
| TotalDataUnits | - | - | Units of measure used to report the total data |
|  | Invalid | 0x0 |  |
|  | KB | 0x1 |  |
|  | MB | 0x2 |  |
|  | GB | 0x3 |  |
| DataUsedPercent | - | - | Data used (in percent) in current Renewal Date. Use HEX encoding here |
|  | Data | 0x00-0x64 |  |
|  | Reserved | 0x65-0xFE |  |
|  | Invalid | 0xFF |  |
| OverageFlag | - | - | Overage Flag status |
|  | Invalid | 0x0 |  |
|  | No | 0x1 |  |
|  | Yes | 0x2 |  |
| DataPlanStatus | - | - | Status of the Carrier's Data Plan |
|  | Invalid | 0x0 |  |
|  | Free Trial Period Waiting | 0x1 |  |
|  | Free Trial Period Active | 0x2 |  |
|  | No Active Subscription | 0x3 |  |
|  | Active Subscription | 0x4 |  |
| UserID | - | - | Data array that consists of textual information up to 50 characters in length, plus end of string |

#### MD-REQ-179310/C-DeviceList\_Rsp

Message Type: Response

This signal is used to respond to the WifiHotSpotOnBoardClient with the current list of connected or blocked devices.

|  |  |  |  |
| --- | --- | --- | --- |
| **Name** | **Literals** | **Value** | **Description** |
| ListType | - | - | List type being sent |
|  | Reserved | 0x00 |  |
|  | ConnectedList | 0x01 | Devices currently connected |
|  | BlockedList | 0x02 | Devices actively blocked by driver |
|  | Reserved | 0x03-0x06 |  |
|  | NoEntry | 0x07 |  |
| ListSize | - | - | Number of items in List |
|  | Inactive | 0x00 |  |
|  | List Size 1 | 0x01 |  |
|  | List Size 2 | 0x02 |  |
|  | … | … |  |
|  | List Size 31 | 0x1F |  |
|  | NoEntry | 0xFF |  |
| TotalNumberOf  DevicesAvailable | - | - | Total number of devices available for given list |
|  | Inactive | 0x00 |  |
|  | 1 Device Available | 0x01 |  |
|  | 2 Devices Available | 0x02 |  |
|  | … | … |  |
|  | 254 Devices Available | 0xFE |  |
|  | NoEntry | 0xFF |  |
| Vector |  |  | Array (1…N) of record (IndexNumber, DeviceName, MAC) with TotalNumberOfDevices defined in ListSize |
| IndexNumber | - | - |  |
|  | Inactive | 0x00 |  |
|  | Index 1 | 0x01 |  |
|  | Index 2 | 0x02 |  |
|  | … | … |  |
|  | Index 255 | 0xFF |  |
| MAC | - | - | Data array that consists of textual information fixed to 17 characters in length, NO END OF STRING. |
| DeviceName | - | - | Data array that consists of textual information up to 19 characters in length, plus end of string |

#### MD-REQ-195174/A-WifiHotspotMAC\_Rsp

Message Type: Response

This signal is used to respond to the WifiHotSpotOnBoardClient with the MAC Address.

|  |  |  |  |
| --- | --- | --- | --- |
| **Name** | **Literals** | **Value** | **Description** |
| MAC | - | - | Media Access Control address used to differentiate TCU hotspot from all other hotspots. Data array that consists of textual information up to 17 characters in length, plus end of string |

#### MD-REQ-028115/A-TelematicsService\_St (TcSE ROIN-221143-2)

Message Type: Status

Represents the status of Telematics Service.

|  |  |  |  |
| --- | --- | --- | --- |
| **Name** | **Literals** | **Value** | **Description** |
| Type | - | - | Used to tell the system the status of the service. |
|  | Null | 0x0 |  |
|  | Active | 0x1 |  |
|  | ExpiringSoon | 0x2 |  |
|  | Expired | 0x3 |  |
|  | NotifyExpired | 0x4 |  |
|  | NotActivatedYet | 0x5 |  |
|  | NotifyNotActivatedYet | 0x6 |  |

#### MD-REQ-180729/A-NumberOfConnectedDevices\_St

Message Type: Status

This signal is used to inform the WifiHotSpotOnBoardClient the number of devices currently connected

|  |  |  |  |
| --- | --- | --- | --- |
| **Name** | **Literals** | **Value** | **Description** |
| Type | - | - | Status bit to indicate the number of devices currently connected |
|  | 0 Devices | 0x00 |  |
|  | 1 Device | 0x01 |  |
|  | 2 Devices | 0x02 |  |
|  | … | … |  |
|  | 255 Devices | 0xFF |  |

#### MD-REQ-222048/A-TelematicsDTC\_St

Message Type: Status

This signal is used to inform the WifiHotSpotOnBoardClient any currently active telematics DTCs.

|  |  |  |  |
| --- | --- | --- | --- |
| **Name** | **Literals** | **Value** | **Description** |
| Type | - | - | Currently active Telematics DTC |
|  | Null | 0x000 |  |
|  | Chipset Init. Failure | 0x001 |  |
|  | Runtime Error | 0x002 |  |
|  | Reserved | 0x003 - 0xFFF |  |

#### MD-REQ-222050/A-DataUsageFeature\_St

Message Type: Status

This signal is used to inform the WifiHotSpotOnBoardClient whether the Data Usage functionality is to be supported and shown to the customer.

|  |  |  |  |
| --- | --- | --- | --- |
| **Name** | **Literals** | **Value** | **Description** |
| Type | - | - | Data Usage functionality status |
|  | Null | 0x00 |  |
|  | Off | 0x01 |  |
|  | On | 0x02 |  |

#### MD-REQ-222051/A-HotspotAPNConnection\_St

Message Type: Status

This signal is used to inform the WifiHotSpotOnBoardClient of the WifiHotspot APN connection status.

|  |  |  |  |
| --- | --- | --- | --- |
| **Name** | **Literals** | **Value** | **Description** |
| Type | - | - | Hotspot APN connection status |
|  | Null | 0x00 |  |
|  | NotConnected | 0x01 |  |
|  | Connected | 0x02 |  |

#### MD-REQ-263183/A-HotspotAvailableBands\_St

Message Type: Status

This signal is used to inform the WifiHotSpotOnBoardClient which Hotspot Frequency Bands are available for use.

|  |  |  |  |
| --- | --- | --- | --- |
| **Name** | **Literals** | **Value** | **Description** |
| Type | - | - | Available Frequency Band |
|  | Null | 0x0 |  |
|  | All Restricted | 0x1 |  |
|  | Band 1 only | 0x2 | (2.4GHz available) |
|  | Band 2 only | 0x3 | (5GHz available) |
|  | All Available | 0x4 |  |

#### MD-REQ-263184/A-HotspotFrequencyBand\_St

Message Type: Status

This signal is used to inform the WifiHotSpotOnBoardClient the current state of the Hotspot Frequency Band.

|  |  |  |  |
| --- | --- | --- | --- |
| **Name** | **Literals** | **Value** | **Description** |
| Type | - | - | Current Frequency Band in use |
|  | Null | 0x0 |  |
|  | Band 1 | 0x1 | (2.4GHz) |
|  | Band 2 | 0x2 | (5GHz) |

### WFHS-IIR-REQ-179315/F-WifiHotspotServer\_Rx

#### MD-REQ-179288/A-HotspotEnablement\_Rq

Message Type: Request

This signal is used to request a change to the Hotspot Enablement from the WifiHotSpotOnBoardClient

|  |  |  |  |
| --- | --- | --- | --- |
| **Name** | **Literals** | **Value** | **Description** |
| Type | - | - | Request to change the hotspot's transmission of Wi-Fi signals status |
|  | Null | 0x0 |  |
|  | Off | 0x1 |  |
|  | On | 0x2 |  |

#### MD-REQ-179292/A-HotspotVisibility\_Rq

Message Type: Request

This signal is used to request a change to the Hotpot Visibility from the WifiHotSpotOnBoardClient

|  |  |  |  |
| --- | --- | --- | --- |
| **Name** | **Literals** | **Value** | **Description** |
| Type | - | - | Request to change the hotspot's transmission of SSID status |
|  | Null | 0x0 |  |
|  | Off | 0x1 |  |
|  | On | 0x2 |  |

#### MD-REQ-179294/A-CarrierInfo\_Rq

Message Type: Request

This signal is used to request the Carrier Information from the WifiHotSpotServer

|  |  |  |  |
| --- | --- | --- | --- |
| **Name** | **Literals** | **Value** | **Description** |
| Type | - | - | Carrier Info request from center stack |
|  | NoRequest | 0x0 |  |
|  | Request | 0x1 |  |

#### MD-REQ-179296/B-DataUsage\_Rq

Message Type: Request

This signal is used for the WifiHotSpotOnBoardClient to request the current data usage variables from the WifiHotSpotServer, to request a refresh of this data from the WifiHotSpotOffBoardClient with an expected response, or to request a refresh of this data from the WifiHotSpotOffBoardClient without an expected response.

|  |  |  |  |
| --- | --- | --- | --- |
| **Name** | **Literals** | **Value** | **Description** |
| Type | - | - | Data Usage request from center stack |
|  | Null | 0x0 |  |
|  | CurrentData | 0x1 |  |
|  | RefreshData | 0x2 |  |
|  | RefreshDataNoResponse | 0x3 |  |

#### MD-REQ-179298/B-DeviceList\_Rq

Message Type: Request

This signal is used to request from the WifiHotSpotServer the current list of connected or blocked devices.

|  |  |  |  |
| --- | --- | --- | --- |
| **Name** | **Literals** | **Value** | **Description** |
| ListType | - | - | Type of List being requested |
|  | Null | 0x00 |  |
|  | ConnectedList | 0x01 |  |
|  | BlockedList | 0x02 |  |
|  | NotEntry | 0x03 |  |
|  | NotUsed | 0x04-0x07 |  |
| StartingIndex | - | - | Starting point for the list |
|  | Null | 0x00 |  |
|  | Start Index 1 | 0x01 |  |
|  | Start Index 2 | 0x02 |  |
|  | … | … |  |
|  | Start Index 255 | 0xFF |  |
| ListSize | - | - | Size of the list |
|  | Null | 0x00 |  |
|  | List Size 1 | 0x01 |  |
|  | List Size 2 | 0x02 |  |
|  | … | … |  |
|  | List Size 31 | 0x1F |  |
|  |  |  |  |

#### MD-REQ-179302/A-RemoveDevice\_Rq

Message Type: Request

This signal is used to request a removal of a device from the Connected or Blocked List from the WifiHotSpotServer

|  |  |  |  |
| --- | --- | --- | --- |
| **Name** | **Literals** | **Value** | **Description** |
| ListType | - | - | Type of List being requested |
|  | Null | 0x00 |  |
|  | FromConnectedList | 0x01 |  |
|  | FromBlockedList | 0x02 |  |
| IndexNumber | - | - | What Index to remove |
|  | Null | 0x00 |  |
|  | Index 1 | 0x01 |  |
|  | Index 2 | 0x02 |  |
|  | … | … |  |
|  | Index 255 | 0xFF |  |

#### MD-REQ-179306/A-WifiInfo\_Rq

Message Type: Request

This signal is used to request a Read/Write operation of the Password or SSID from/to the WifiHotSpotServer

|  |  |  |  |
| --- | --- | --- | --- |
| **Name** | **Literals** | **Value** | **Description** |
| OpCode | - | - | Signifies whether the request is to receive or modify Wi-Fi HotSpot Info parameters |
|  | Reserved | 0x0 |  |
|  | Read | 0x1 | Request used to read the current Password and SSID |
|  | WriteSSID | 0x2 | Request used to create a new SSID |
|  | WritePassword | 0x3 | Request used to create a new Password |
|  | Reserved | 0x4-0xFF |  |
| Password | - | - | Data array that consists of textual information up to 64 characters in length, plus end of string |
| SSID | - | - | Data array that consists of textual information up to 32 characters in length, plus end of string |

#### MD-REQ-027149/A-IgnitionStatus\_St (TcSE ROIN-225464-1)

Message Type: Status

Signal used to indicate ignition state.

|  |  |  |  |
| --- | --- | --- | --- |
| **Name** | **Literals** | **Value** | **Description** |
| Type | - | - | Indicates ignition state |
|  | Unknown | 0x0 |  |
|  | Off | 0x1 |  |
|  | Accessory | 0x2 |  |
|  | Run | 0x4 |  |
|  | Start | 0x8 |  |
|  | Invalid | 0xF |  |

#### MD-REQ-086348/A-CarMode\_St

Message Type: Status

|  |  |  |  |
| --- | --- | --- | --- |
| Name | Literals | Value | Description |
| Type | - | - | Defines what car mode state is active. |
|  | Normal | 0x0 |  |
|  | Factory | 0x1 |  |
|  | NotUsed | 0x2 |  |
|  | Transportation | 0x3 |  |

#### MD-REQ-048716/B-OdometerMasterValue (TcSE ROIN-305984)

Message Type: Status

This signal is used to report the odometer value in KM’s.

|  |  |  |  |
| --- | --- | --- | --- |
| Name | Literals | Value | Description |
| Type | - | - | Vehicle Odometer reading in KMs |
|  | 0-16777214 | 0x0-0xFFFFFE |  |
|  | Invalid | 0xFFFFFF |  |

#### MD-REQ-027937/A-HMIMode\_St (TcSE ROIN-229453-1)

Message Type: Status

This method holds the information about the HMI state of the multimedia system.

This attribute shows the HMI mode. The HMI mode is defined in the Network Management Strategy.

|  |  |  |  |
| --- | --- | --- | --- |
| **Name** | **Literals** | **Value** | **Description** |
| Mode | - | - | Signal is used to indicate HMI state. |
|  | Invalid | 0x0 |  |
|  | OffMode | 0x1 |  |
|  | On | 0x2 |  |
|  | Phone | 0x3 |  |
|  | Climate | 0x4 |  |
|  | Load\_Shed\_Active | 0x5 |  |

#### MD-REQ-195171/A-WifiHotspotMAC\_Rq

Message Type: Request

This signal is used to request the MAC Address from the WifiHotSpotServer

|  |  |  |  |
| --- | --- | --- | --- |
| **Name** | **Literals** | **Value** | **Description** |
| Type | - | - | Wi-Fi Hotspot MAC address request from center stack |
|  | NoRequest | 0x0 |  |
|  | Request | 0x1 |  |

#### MD-REQ-212570/A-HotspotTrialReminderSelection\_Rq

Message Type: Request

This signal is sent from the WifiHotspotOnBoardClient to the WifiHotspotServer to request to either continue the Wifi Hotspot Trial reminders or stop them.

|  |  |  |  |
| --- | --- | --- | --- |
| **Name** | **Literals** | **Value** | **Description** |
| Type | - | - | Request from the vehicle occupant to either stop trial reminders or to continue reminding them |
|  | Null | 0x00 |  |
|  | Remind Me Later | 0x01 |  |
|  | Stop Reminders | 0x02 |  |

#### MD-REQ-263185/A-HotspotFrequencyBand\_Rq

Message Type: Request

This signal is used to request a change to the Hotspot Frequency Band from the WifiHotSpotOnBoardClient

|  |  |  |  |
| --- | --- | --- | --- |
| **Name** | **Literals** | **Value** | **Description** |
| Type | - | - | Frequency Band request from WifiHotSpotOnBoardClient |
|  | Null | 0x0 |  |
|  | Band 1 | 0x1 | (2.4GHz) |
|  | Band 2 | 0x2 | (5GHz) |

# General Requirements

## WFHS-HMI-REQ-192248/A-WifiHotspotOnBoardClient Transport Protocol Data Request

The WifiHotspotOnBoardClient shall request all Transport Protocol data required for a given WifiHotspot screen upon entry.

Example: When the user requests the Connected Device List screen, the WifiHotspotOnBoardClient shall make a request for the Device List from the WifiHotspotServer using DeviceList\_Rq. The WifiHotspotServer shall respond with DeviceList\_Rsp.

## WFHS-REQ-226336/A-HMI Specification References

The HMI specifications may vary per module. Refer to the HMI specifications below per module for the actual implementation of screens, popups, screen names and icons.

|  |  |
| --- | --- |
| **Module** | **HMI Specification** |
| APIM | H31i\_SYNC\_Gen3\_Wi-Fi\_Settings (non 4 inch display) and  SDM4\_RELEASE (4 inch display). |
| CHR | SDM4\_RELEASE. |
| CTR | TBD (actual name of the specification may be added to this document at a later time). |

## WFHS-REQ-226337/A-Diagnostic Specification References

The Diagnostics Part 2 specification may vary per module. Refer to the Diagnostic Part 2 specification below per module for relevant DID (diagnostic ID) values, DTC values, and address spaces.

|  |  |
| --- | --- |
| **Module** | **Diagnostic Part 2 Specification** |
| APIM | Infotainment Diagnostics Specification |
| CHR | DS-H1BT-18D832-AB specification |
| CTR | TBD (actual name of the specification may be added to this document at a later time) |
| TCU | TCU Subsystem Specification Diagnostic Specification (Part 2) |

## WFHSv2-SR-REQ-227355/B-Request/Response return to Null/NoRequest state

When updating on event, the following event-periodic signals listed below shall hold there signal encoding values for a period of time defined by T\_ReturnToNull\_NoRequest and then shall transit back to Null or NoRequest as shown in the sequence diagrams (TBD - diagrams will be updated at a later time):

* HotspotEnablement\_Rq
* HotspotVisibility\_Rq
* CarrierInfo\_Rq
* DataUsage\_Rq
* DeviceList\_Rq
* RemoveDevice\_Rq
* WifiHotspotMAC\_Rq
* HotspotTrialReminderSelection\_Rq
* HotspotFrequencyBand\_Rq

The receiving modules of these signals shall act upon the event signal and shall not wait for the “Null” to act upon the signal request.

## WFHS-TMR-REQ-226998/A-T\_ReturnToNull\_NoRequest

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Name** | **Description** | **Units** | **Range** | **Resolution** | **Default** |
| T\_ReturnToNull\_NoRequest | The nominal hold time before returning to a Null or NoRequest state. Use the default value +/- 10%. | sec | 0.5-2 | 0.5 | 1 |

# Functional Definition

## WFHSv1-FUN-REQ-192079/A-Wi-Fi General Usage

### Requirements

#### WFHS-REQ-191640/E-WifiHotspotOnBoardClient identifies the vehicle brand

The WifiHotspotOnBoardClient shall be responsible for determining whether the vehicle brand is Ford or Lincoln. Refer to WFHS-REQ-226337-Diagnostic Specification Reference. The WifiHotspotOnBoardClient shall apply this information to other requirements defined throughout this document in order to fulfill the objectives of those requirements.

#### WFHS-REQ-191641/E-WifiHotspotOnBoardClient identifies the vehicle region

The WifiHotspotOnBoardClient shall be responsible for determining whether the vehicle region is NA (United States or Canada), China or Europe. Refer to WFHS-REQ-226337-Diagnostic Specification Reference. The WifiHotspotOnBoardClient shall apply this information to other requirements defined throughout this document in order to fulfill the objectives of those requirements.

#### WFHS-REQ-191639/D-WifiHotspotServer identifies the vehicle region

The WifiHotspotServer shall determine the vehicle region. The WifiHotspotServer shall be capable of determining if the vehicle is destined for NA (United States or Canada), China or Europe. The WifiHotspotServer shall also know the vehicle’s destination country code. Refer to WFHS-REQ-226337-Diagnostic Specification Reference. The WifiHotspotServer shall apply this information to other requirements defined throughout this document in order to fulfill the objectives of those requirements.

#### WFHS-REQ-191705/H-Monitoring Wi-Fi Hotspot feature availability

The WifiHotspotOnBoardClient shall be able to determine if the vehicle is equipped with a Wi-Fi Hotspot capable modem. If so, the vehicle has the Wi-Fi Hotspot feature. If the vehicle has a hotspot capable modem, the WifiHotspotOnBoardClient shall be required to display the Wi-Fi Hotspot HMI screens (all screens contained in the HMI specification; Refer to WFHS-REQ-226336/A-HMI Specification References) and shall be responsible for complying with the requirements in the rest of this specification. If the vehicle is not equipped with a Wi-Fi Hotspot capable modem, the vehicle does not have the Wi-Fi Hotspot feature and the WifiHotspotOnBoardClient shall not be required to comply with any of the requirements in this specification. The WifiHotspotOnBoardClient shall contain a Hotspot capable modem DID that shall be used to determine if the vehicle has a hotspot capable modem or not. Refer to WFHS-REQ-226337-Diagnostic Specification Reference.

Although a vehicle may be Wi-Fi Hotspot capable, the feature may not be enabled. The Wi-Fi Hotspot feature may be enabled or disabled depending on the configuration on the WifiHotspotServer. The Wi-Fi Hotspot feature may be enabled/disabled at EOL or through an OTA update. The WifiHotspotOnBoardClient shall monitor the TCUAvailability\_St CAN signal in order to determine if the Wi-Fi Hotspot feature is enabled or not.

If the Wi-Fi Hotspot feature is disabled (TCUAvailability\_St = Disable), the WifiHotspotOnBoardClient shall not allow the vehicle occupant to navigate through the Wi-Fi Hotspot screens and shall not be required to monitor/transmit any of the CAN signals defined in this document (except TCUAvailability\_St and other select signals depending on the WifiHotspotOnBoardClient module, see below), unless separate features require the WifiHotspotOnBoardClient to and specify so in separate documents.

1. WifiHotspotOnBoardClient = SYNC: If the Wi-Fi Hotspot feature is disabled, the WifiHotspotOnBoardClient shall, however, be required to monitor the CAN signal TCUAvailability\_St in order to determine if the feature becomes enabled again. The WifiHotspotOnBoardClient shall also be required to transmit the CAN signal WifiHotspotMAC\_Rq and monitor the response signal WifiHotspotMAC\_Rsp (refer to WFHS-REQ-195287-Transferring MAC Address). If the WifiHotspotServer changes its status to indicate the Wi-Fi Hotspot feature is Disabled while the vehicle occupant is in any Wi-Fi Hotspot screen, the WifiHotspotOnBoardClient shall exit the Wi-Fi Hotspot screens immediately and provide a popup. The Wi-Fi Hotspot menu shall not be accessible and any attempts from the vehicle occupant to enter into the Wi-Fi Hotspot menu shall trigger the same popup.
2. WifiHotspotOnBoardClient = CHR: If the Wi-Fi Hotspot feature is disabled, the WifiHotspotOnBoardClient shall, however, be required to monitor the CAN signal TCUAvailability\_St in order to determine if the feature becomes enabled again. If the WifiHotspotServer changes its status to indicate the Wi-Fi Hotspot feature is Disabled while the vehicle occupant is in any Wi-Fi Hotspot screen, the WifiHotspotOnBoardClient shall exit the Wi-Fi Hotspot screens immediately and provide a popup. The Wi-Fi Hotspot menu shall not be accessible and any attempts from the vehicle occupant to enter into the Wi-Fi Hotspot menu shall trigger the same popup.

If the Wi-Fi Hotspot feature is Enabled (TCUAvailability\_St = Enable), the WifiHotspotOnBoardClient shall display the Wi-Fi Hotspot feature screens and shall be required to monitor/transmit all client specified CAN signals defined in this document.

The vehicle occupant shall have access to the Wi-Fi Hotspot screens when the Wi-Fi Hotspot feature is available and enabled (except if vehicle is under driver restrictions, refer to WFHS-REQ-191710-Disabling driver restricted screens). If the feature is unavailable (TCUAvailability\_St=NULL) or disabled (TCUAvailability\_St=Disable) when the WifiHotspotOnBoardClient is active the WifiHotspotOnBoardClient shall disable the Wi-Fi Hotspot screens. The Wi-Fi Hotspot feature may be unavailable due to any of the following:

* 1. WifiHotspotServer is asleep when WifiHotspotOnBoardClient is active due to lack of power mode synchronization,
  2. Lost communication with WifiHotspotServer over CAN,
  3. WifiHotspotServer reset and
  4. Wi-Fi Hotspot errors.

The WifiHotspotOnBoardClient shall monitor the CAN signal TCUAvailability\_St and treat it as a heartbeat to determine whether to allow the user in the Wi-Fi Hotspot screens or not.

1. If the WifiHotspotServer reports that Wi-Fi is Enabled using the CAN signal TCUAvailability\_St. the user shall be able to freely navigate through the Wi-Fi Hotspot screens.
2. If the WifiHotspotServer changes its status to “NULL” while the vehicle occupant is in any Wi-Fi Hotspot screen, the WifiHotspotOnBoardClient shall exit the Wi-Fi Hotspot screens immediately and provide a popup. The Wi-Fi Hotspot menu shall not be accessible and any attempts from the vehicle occupant to enter into the Wi-Fi Hotspot menu shall trigger the same popup.
3. If the CAN signal TCUAvailability\_St is missing on the bus for 5 seconds (Lost CAN Communication timer) or more while the vehicle occupant is in any Wi-Fi Hotspot screen, the WifiHotspotOnBoardClient shall exit the Wi-Fi Hotspot screens immediately and provide a popup. The Wi-Fi Hotspot menu shall not be accessible and any attempts from the vehicle occupant to enter into the Wi-Fi Hotspot menu shall trigger the same popup when the TCUAvailability\_St CAN signal is missing on the bus. If the WifiHotspotOnBoardClient detects TCUAvailability\_St CAN signal is missing on the bus and has started the Lost CAN Communication timer and the timer has not yet expired when the vehicle occupant attempts to enter into the Wi-Fi Hotspot menu, the WifiHotspotOnBoardClient shall display a waiting symbol and lock the user out of the Wi-Fi screens.

The following popups are example WifiHotspotOnBoardClient popups that would be displayed if scenario (b) or (c) were to occur.



Figure. Settings not able to be displayed popup.



Figure. Waiting symbol.

If the Wi-Fi Hotspot feature is enabled, the WifiHotspotOnBoardClient shall monitor for Wi-Fi Hotspot related DTCs to determine if there are any errors with the Wi-Fi system. The WifiHotspotOnBoardClient shall monitor the CAN signal TelematicsDTC\_St to determine if any DTCs are set that indicate a Wi-Fi chipset initialization failure or a runtime error.

1. If the CAN signal mentioned above is set to indicate a Wi-Fi error exists while the vehicle occupant is in any Wi-Fi Hotspot screen, the WifiHotspotOnBoardClient shall exit the Wi-Fi Hotspot screens immediately and provide a popup. The Wi-Fi Hotspot menu shall not be accessible and any attempts from the vehicle occupant to enter into the Wi-Fi Hotspot menu shall trigger the same popup while Wi-Fi Hotspot errors exist.

The following popup is an example WifiHotspotOnBoardClient popup that would be displayed if any of the Wi-Fi related DTCs mentioned above were set.



Figure. Technical error popup

#### WFHS-REQ-191710/E-Disabling driver restricted screens

The WifiHotspotOnBoardClient shall monitor the CAN signal VehicleSpeed\_St to determine the speed of the vehicle. If the vehicle travels above a certain speed, the WifiHotspotOnBoardClient shall disable the Wi-Fi Hotspot driver restricted screens. If the vehicle travels at or below a certain speed, the WifiHotspotOnBoardClient shall enable all Wi-Fi Hotspot driver restricted screens.

* WifiHotspotOnBoardClient = APIM module: Refer H21j for a list of all Wi-Fi Hotspot driver restricted screens. This spec shall also identify the triggers that enable and disable the driver restrictions.
* WifiHotspotOnBoardClient = CHR module or 4inch SYNC module: Refer to the HMI specification (refer to WFHS-REQ-226336/A-HMI Specification References) for a list of all driver restricted screens. This spec shall also identify the triggers that enable and disable the driver restrictions.

#### WFHS-REQ-191715/A-Responding to multiple requests

The WifiHotspotServer shall respond to Wi-Fi related requests in FIFO order.

#### WFHS-REQ-191778/A-CAN message requirements

The WifiHotspotServer and WifiHotspotOnBoardClient shall receive and transmit CAN messages as specified in the CAN database from FORD for Wi-Fi Hotspot feature.

#### WFHS-REQ-191779/A-CAN message retries

CAN message signals shall always reflect the current state of the WifiHotspotServer. In case of message transmission failures the WifiHotspotServer and WifiHotspotOnBoardClient shall retry for a maximum number of 5 retries. This number shall be configurable.

#### WFHS-REQ-191888/A-Wi-Fi chipset

The Wi-Fi chipset shall support 802.11 a/b/g/n and shall support both STA and AP mode.

#### WFHS-REQ-192131/A-Wi-Fi Hotspot traffic model

In order to define a set of Wi-Fi chipset performance requirements, Ford Motor Company has defined two traffic models as a baseline for testing. Traffic model A shall test all 7 devices performing the most throughput and RSSI intensive activity and model B shall test 7 devices performing a combination of different activities. Both models are expected to meet the Wi-Fi performance requirements (WFHS-REQ-191889/A-Wi-Fi signal strength, WFHS-REQ-191890/A-Wi-Fi throughput, WFHS-REQ-191891/A-Modulation scheme and WFHS-REQ-191892/A-Wi-Fi range).

Model A:

a) 7 devices performing Wi-Fi activities such as HD streaming in real time.

Model B:

a) 4 devices streaming HD video

b) 2 devices using email

c) 1 device playing video games

#### WFHS-REQ-191889/B-Wi-Fi signal strength

The RSSI values needed to obtain maximum throughput on each of the frequency bands have not yet been finalized. The WifiHotspotServer hardware team and Feature Owners shall work together to define this requirement.

#### WFHS-REQ-191890/C-Wi-Fi throughput

The Wi-Fi design shall perform at a minimum throughput of 165 Mbps (300 Mbps data rate) on the 2.4GHz band and a minimum throughput of 477 Mbps (867 Mbps data rate) on the 5GHz band. The Wi-Fi chipset shall never be the bottleneck of the system.

The WifiHotspotServer shall implement a fairness model to control the distribution of its throughput. This model shall ensure that all connected clients performing the same application type receives equal throughput.

Example)

* 6 devices are connected.
* 4 are streaming HD video (assumption: HD video requires ~4 Mbps).
* 2 are using email (assumption: email requires ~500 Kbps).
* The 4 streaming YouTube shall each receive ~4 Mbps.
* The 2 using email shall each receive ~500 Kbps.

#### WFHS-REQ-191891/B-Modulation scheme

The WifiHotspotServer shall dynamically adjust the modulation coding scheme depending on the measured SNR. The modulation coding scheme needed is not yet finalized. The WifiHotspotServer hardware team and Feature Owners shall work together to define this requirement.

#### WFHS-REQ-191892/A-Wi-Fi range

The Wi-Fi Hotspot feature shall meet its minimum throughput (WFHS-REQ-191890-Wi-Fi throughput), RSSI (WFHS-REQ-191889-Wi-Fi Signal strength) and MCS requirements (WFHS-REQ-191891-Modulation scheme) up to 50 ft away from the vehicle, 360 degrees around. The RSSI and throughput shall be measured at 50 ft away from the vehicle and at 22 degree increments. The devices used to measure the throughput and RSSI may vary, but shall be kept consistent across all testing.

#### WFHS-REQ-191894/A-Wi-Fi certification

The supplier shall be responsible for certifying the Wi-Fi feature in the following areas as defined by the Wi-Fi alliance certification programs:

* 1. Access point and STA mode for:
     1. 802.11n
     2. WMM
     3. WPA2/WPA
     4. Tx and Rx on 2.4 GHz band & 5 GHz band

Ford Motor Company shall own the Wi-Fi certification in the areas mentioned above.

#### WFHS-REQ-191895/A-Quality of Service on the Wi-Fi chipset

The Wi-Fi chipset shall have Quality of Service enabled for WMM (wireless multimedia) and for Wi-Fi protocol.

#### WFHS-REQ-191896/B-FCC and international radio regulatory requirements

The Wi-Fi Hotspot shall meet all applicable FCC and international radio regulatory requirements. The Wi-Fi Hotspot shall also meet all Chinese and European radio regulatory requirements.

#### WFHS-REQ-191897/A-Wi-Fi chipset and NAD communication interface

The interface between the access point and the NAD shall provide error recovery strategies to enable a robust system where the customer experiences no errors.

The Wi-Fi access point shall have a data communication interface to the NAD that shall allow it to receive Wi-Fi data at a minimum data rate that is greater than the Wi-Fi throughput. The suggested interface allows for a maximum data rate of 200 Mbps running at a clock of 25 MHz.

#### WFHS-REQ-191898/A-Logging Wi-Fi debug messages

The Wi-Fi access point application and Wi-Fi NAD application shall log Wi-Fi debug messages such as Wi-Fi configurations, Wi-Fi parameters and other Wi-Fi data relevant to each station. Parameters such as RSSI, SNR, BER, MCS, number of devices connected, number of devices dropped and the traffic model indicating which device was performing what activity may be captured, for example. The debugging state shall be capable of being turned on or off.

#### WFHS-REQ-191899/C-Reporting out diagnostics

The WifiHotspotServer shall support Wi-Fi diagnostics messages for the Wi-Fi chipset and internal antenna. The diagnostics messages exchanged between the WifiHotspotServer processor and Wi-Fi chipset shall test the health of the Wi-Fi chipset software and hardware and shall also test the internal antenna. The WifiHotspotServer shall set DTCs that identify Wi-Fi related errors (refer to WFHS-REQ-226337-Diagnostic Specification Reference).

The WifiHotspotServer shall inform the WifiHotspotOnBoardClient when Wi-Fi Hotspot related DTCs are set by using the CAN signal TelematicsDTC\_St. If the WifiHotspotServer sets a Wi-Fi Hotspot related DTC, it shall also set the CAN signal to its appropriate state based on the DTC that was set. The CAN signal shall remain set until the DTC is cleared. The two Wi-Fi Hotspot related DTCs include the chipset initialization failure and the runtime error. If both DTCs are set, the CAN signal shall be set to the DTC that is more detrimental to the system.

#### WFHS-REQ-191900/B-Maximum Wi-Fi initialization time

If the WifiHotspotServer begins its initialization process, it shall also initialize the Wi-Fi chipset. The Wi-Fi initialization process, including initialization of the Wi-Fi chipset\SDIO\Wi-Fi antenna\Wi-Fi application, shall not exceed a maximum initialization limit of 12 seconds. After the initialization is complete the Wi-Fi functionality shall be available to the Wi-Fi stations that constitute the hotspot.

#### WFHS-REQ-191901/A-Wi-Fi initialization failure

In case of a Wi-Fi initialization failure, the Wi-Fi application shall implement a Wi-Fi power up recovery strategy such as resetting the Wi-Fi chipset, the SDIO or any appropriate function that may correct the error code.

#### WFHS-REQ-191902/C-APN connections

The Wi-Fi Hotspot feature shall utilize two APNs on the WifiHotspotServer. The first APN shall be referred to as the Ford APN, which is used for Ford-paid services such as remote features, OTA updates, etc. All Wi-Fi Hotspot related FTCP messages shall utilize the Ford APN.

The second APN, referred to as the Wi-Fi APN, shall never communicate with the WifiHotspotOffBoardClient and shall only be used to stream data to the outside Internet. Thus, only data streamed through the Wi-Fi access point shall use the Wi-Fi APN. This APN shall be stored in the WifiHotspotServer and shall be updateable via OTA or EOL.

The NA and China production Wi-Fi APN addresses shall already be written to the WifiHotspotServer when the modules are delivered to Ford. In EU, the country-specific Wi-Fi APN shall be written to the WifiHotspotServer at Ford Motor Company’s EOL once the vehicle’s destination country has been assigned to the vehicle.

If a request to update the Wi-Fi APN is received OTA from the WifiHotspotOffBoardClient, the WifiHotspotServer shall perform a specific procedure to update the Wi-Fi APN. Refer to the 4G TCU Connection Management Flows document for more information.

If no data plan is active on the hotspot, the vehicle occupant shall still be able to connect to the Wi-Fi Hotspot. If the user attempts to stream data through their web browser while no data plan is active, the customer device shall be re-directed to a carrier provided landing page. The carrier shall be responsible for the landing page redirection. The landing page redirection shall utilize the Wi-Fi APN.

#### WFHS-REQ-191903/D-Wi-Fi Hotspot feature dependency on the WifiHotspotServer authorization state

The user shall be able to activate a Wi-Fi Hotspot data plan through the carrier when the WifiHotspotServer is in Waiting for Auth or Authorized state (refer to TCU Provisioning Systems Engg Spec for more information on WifiHotspotServer states). Thus, the WifiHotspotServer shall allow connected clients to stream Internet data if a plan is active, even while the WifiHotspotServer is not authorized.

However, the WifiHotspotServer shall not request or receive any data usage information (refer to WFHSv1-FUN-REQ-140754-Reporting Data Used and WFHSv1-FUN-REQ-140748-Carrier Data Notification) from the WifiHotspotOffBoardClient if the WifiHotspotServer state is NOT equal to “authorized”. The table below reflects the WifiHotspotServer states and Wi-Fi Hotspot feature readiness.

|  |  |
| --- | --- |
| **WifiHotspotServer State** | **Wi-Fi Hotspot Feature Functionality** |
| Factory Mode | Not authorized |
| Unprovisioned | Not authorized |
| Waiting for provisioning Ack | Not authorized |
| Waiting for Home URL | Not authorized |
| Waiting for Auth | Not authorized |
| Authorized | Authorized |

No data usage information shall be required to be transmitted at the time the WifiHotspotServer becomes authorized. If the WifiHotspotServer becomes authorized, data usage information shall be transmitted upon a notification that is triggered from the carrier or from a request from the WifiHotspotServer.

If the WifiHotspotServer is authorized, but becomes not authorized, there shall be no interruption to the customer’s Wi-Fi Hotspot data plan or Wi-Fi service.

#### WFHS-REQ-191904/B-Shutting down and powering up the Wi-Fi chipset and WifiHotspotServer

If the Wi-Fi Hotspot feature is disabled (refer to WFHS-REQ-194001/B-WifiHotspotServer EOL configuration for determining Wi-Fi Hotspot feature enablement), the WifiHotspotServer shall set the CAN signal TCUAvailability\_St= Disable. If the WifiHotspotServer is powering up or down and unable to determine if the feature is enabled or disabled, the WifiHotspotServer shall default the CAN signal TCUAvailability\_St=NULL.

If Wi-Fi Hotspot feature is enabled, follow the requirements below:

When the term “fully functional” is used within this requirement, it implies the WifiHotspotServer is capable of accessing and transmitting its stored Wi-Fi Hotspot settings and is capable of processing Wi-Fi Hotspot related requests from the WifiHotspotOnBoardClient. Note: the WifiHotspotServer shall be capable of updating settings in memory, but may not necessarily need to be capable of updating the Wi-Fi chipset, in order to be deemed “fully functional”. The status of the cellular connection, APN initialization and Wi-Fi chipset connectivity and availability shall not be taken into consideration when determining if the WifiHotspotServer is “fully functional”. For example, if the WifiHotspotServer has a dropped cellular connection it shall not be deemed “not fully functional”. Also, if the Wi-Fi chipset has not yet initialized, the WifiHotspotServer may still be considered “fully functional”.

If the WifiHotspotServer is beginning to transition to low power registered mode, the Wi-Fi manager shall gracefully disconnect all clients and shutdown the Wi-Fi component, clear any unused memory and save any persistent memory. Once the WifiHotspotServer becomes “not fully functional” during the power down process, the WifiHotspotServer shall set the CAN signal TCUAvailability\_St to “NULL” until it fully powers down.

If the WifiHotspotServer is powering up to any full power mode and the WifiHotspotServer is not fully functional, the WifiHotspotServer shall set the CAN signal TCUAvailability\_St status to “NULL”. Once the WifiHotspotServer is fully functional, the WifiHotspotServer shall update its CAN signal TCUAvailability\_St = Enable.

#### WFHS-REQ-191905/A-Wi-Fi networking rules

The WifiHotspotServer shall implement a set of networking and firewall rules to generally restrict external network access while allowing users connected to the Wi-Fi network to access the public Internet. These requirements shall be defined in Internet Gateway Specification.

#### WFHS-REQ-191906/B-AP connection rules

WEP shall not be supported. Wi-Fi should default to operate with WPA2 security enabled. Only if the WifiHotspotServer is configured to enable WPA/WPA2 and detects a legacy device that does not support WPA2 shall the WifiHotspotServer fall back onto WPA.

#### WFHS-REQ-192111/C-Wi-Fi Chipset AP and STA mode

The WifiHotspotServer shall configure the Wi-Fi chipset to be off, in STA mode or in access point mode depending on the WifiHotspotServer state and the configuration method. AP mode shall be enabled to allow the WifiHotspotServer to act as a hotspot. STA mode shall be enabled to support provisioning over Wi-Fi. The table below indicates which mode the WifiHotspotServer shall enable the Wi-Fi chipset to be in (refer to TCU Provisioning Systems Engg Spec for more information on WifiHotspotServer states).

|  |  |
| --- | --- |
| **WifiHotspotServer State** | **Wi-Fi Chipset Mode** |
| Factory Mode | Wi-Fi Chipset Off/STA mode |
| Unprovisioned | Wi-Fi Chipset Off/STA mode |
| Waiting for provisioning Ack | Wi-Fi Chipset Off/STA mode |
| Waiting for Home URL | Wi-Fi Chipset Off/STA mode |
| Waiting for Auth | Access Point mode |
| Authorized | Access Point mode |

If the WifiHotspotServer’s Provisioning Method DID is set to Cellular, the Wi-Fi chipset shall be Off during Factory Mode through Waiting for Home URL states. Refer to the WiFi Provisioning Product Requirement Document for more information on the Provisioning Method DID.

If the WifiHotspotServer’s Provisioning Method DID is set to WiFi, the Wi-Fi chipset shall be configured to STA Mode during Factory Mode through Waiting for Home URL states.

#### WFHS-REQ-192117/C-Operating on the 2.4 GHz band in AP mode

The Wi-Fi chipset shall support both current and legacy Wi-Fi devices while in AP mode.

The WifiHotspotServer shall operate on the 2.4 GHz band and 5 GHz band simultaneously while in AP mode (refer to WFHS-REQ-192111-Wi-Fi Chipset AP and STA mode) to support all devices.

If the WifiHotspotServer is limited to operate on one band only, the WifiHotspotServer shall default to operate on the 5 GHz band while in AP mode. The WifiHotspotServer shall be capable of receiving an OTA update or a request via CAN messaging to switch the Wi-Fi chipset from operating on the 2.4 GHz band to the 5 GHz band and vice versa (parameter Hotspot\_Operational\_Band). This parameter shall also be configurable via EOL.

#### WFHS-REQ-192124/A-Number of key strokes on WifiHotspotOnBoardClient display needed to view the Wi-Fi Hotspot feature

The vehicle occupant shall be able to locate the Wi-Fi Hotspot feature in the WifiHotspotOnBoardClient display in no more than 2 key strokes.

#### WFHS-REQ-194001/D-WifiHotspotServer EOL configuration for determining Wi-Fi Hotspot feature enablement

The parameter Wi-Fi\_Hotspot\_Feature\_Enabled shall be configurable via Ford Motor Company’s EOL process or by an OTA update. The WifiHotspotServer shall be able to detect if it is Wi-Fi capable or not (i.e. by a part number or by detecting if there is a Wi-Fi chipset populated or not, etc.). Thus, a WifiHotspotServer may be Wi-Fi capable, but may have its Wi-Fi Hotspot feature not enabled.

If the Wi-Fi\_Hotspot\_Feature\_Enabled configuration is set to No, the WifiHotspotServer shall disable the feature and shall not be required to monitor/transmit any of the CAN signals (except TCUAvailability\_St, WifiHotspotMAC\_Rq and WifiHotspotMAC\_Rsp) defined in this document, unless separate features require the WifiHotspotServer to and specify so in separate documents. The WifiHotspotServer shall always transmit the TCUAvailability\_St CAN signal regardless of the Wi-Fi Hotspot feature enablement state. The WifiHotspotServer shall also be required to monitor the CAN signal WifiHotspotMAC\_Rq and transmit the response signal WifiHotspotMAC\_Rsp (refer to WFHS-REQ-195287-Transferring MAC Address). The Wi-Fi chipset shall be turned off and kept off, not allowing any transmission of Wi-Fi signals, while the feature is disabled. The WifiHotspotServer shall set the CAN signal TCUAvailability\_St=Disable.

If the configuration is set to Yes, the WifiHotspotServer shall enable the feature and meet all of the requirements in this document and shall be required to monitor/transmit all server specified CAN signals defined in this document. The WifiHotspotServer shall set the CAN signal TCUAvailability\_St = Enable.

A WifiHotspotServer shall never be allowed to have its Wi-Fi Hotspot feature enabled if it is not Wi-Fi capable. If the WifiHotspotServer is NOT Wi-Fi capable but was mistakenly configured as Wi-Fi enabled via Ford’s EOL process or via OTA, the WifiHotspotServer shall override the enabled configuration with the capable configuration.

If the WifiHotspotServer is configured as Wi-Fi capable but does not have its Wi-Fi Hotspot feature enabled, the WifiHotspotServer shall set the Wi-Fi\_Hotspot\_Feature\_Enabled field as NOT Wi-Fi enabled.

If the WifiHotspotServer is configured as Wi-Fi capable AND Wi-Fi Hotspot enabled, the WifiHotspotServer shall set the Wi-Fi\_Hotspot\_Feature\_Enabled field to Wi-Fi enabled.

The Wi-Fi\_Hotspot\_Feature\_Enabled parameter shall be defaulted to Yes. The parameter shall also be configurable via OTA.

#### WFHS-REQ-191783/B-WifiHotspotServer over-the-air software updates

The Wi-Fi Hotspot feature shall be made up of different pieces of software components that may reside on the WifiHotspotServer processor as a Wi-Fi application manager, on the Wi-Fi chipset, SDIO drivers, etc. The OTA update process shall flash all Wi-Fi hotspot software components. There are two implementations for the Wi-Fi OTA updates:

The first approach that shall be implemented is:

1. The Wi-Fi OTA update shall be tied to the OTA update of the WifiHotspotServer software and they shall share the same part number

The second approach that shall be considered for future implementation is:

1. The Wi-Fi OTA update may be separate from the WifiHotspotServer software update where each may have its own software part number. This approach shall be considered for later WifiHotspotServer generations

If the WifiHotspotServer re-flashes its software due to an OTA SW update it shall gracefully disconnect all Wi-Fi clients. When the WifiHotspotServer finishes re-flashing its software, it shall restore all previous Wi-Fi settings listed in WFHS-REQ-191863-Wi-Fi Hotspot reset.

#### WFHS-REQ-192622/A-FTCP messaging between WifiHotspotServer and WifiHotspotOffBoardClient

All interactions between the WifiHotspotServer and WifiHotspotOffBoardClient shall follow the Ford Telematics Control Protocol (FTCP). The Wi-Fi Hotspot FTCP messaging spec shall define all the messaging needed for this feature.

#### WFHS-REQ-194010/E-Wi-Fi Hotspot parameters transmitted during provisioning

In order for the Wi-Fi Hotspot feature to function, certain parameters shall be transmitted from the vehicle to the WifiHotspotOffBoardClient. The following parameters per region shall be transmitted from the WifiHotspotServer to the WifiHotspotOffBoardClient during the provisioning process:

* NA (United States and Canada)

1. VIN

* China

1. VIN

* Europe

1. VIN
2. IMSI
3. Country code

If any of these fields are blank in the provisioning message, the WifiHotspotOffBoardClient shall fail the provisioning process.

#### WFHS-REQ-194471/D-WifiHotspotServer becomes not authorized

If the WifiHotspotServer becomes not authorized, refer to WFHS-REQ-191903/A-Wi-Fi Hotspot feature dependency on the WifiHotspotServer authorization state, the WifiHotspotServer shall clear all data usage information that is typically received in the FTCP data usage notification/response message (refer to WFHSv1-FUN-REQ-140754-Reporting Data Used and WFHSv1-FUN-REQ-140748-Carrier Data Notification). The parameter TrialEligible shall retain its current state and not reset it to “NULL” (i.e. if TrialEligible parameter=”Yes”, after the TCU becomes not authorized, the parameter shall still equal “Yes”).

There shall be no interruption to the customer’s Wi-Fi Hotspot service if the WifiHotspotServer becomes not authorized.

#### WFHS-REQ-263049/A-Broadcasting as a Vehicular AP

The WifiHotspotServer shall advertise its hotspot as being a vehicular AP. It shall broadcast this indicator using the Interworking Element, which includes:

* Venue Group Code = 10 (automotive)
* Venue Type Code = 1 (automotive or truck).

#### WFHS-REQ-263050/A-Broadcasting as a metered account

The WifiHotspotServer shall advertise its hotspot as being a metered account. It shall broadcast this indicator using the Interworking Element, which includes:

* Access Network Type = 2 (Chareable Public Network).

Note: this requirement is still under investigation and may be removed later if deemed not needed.

#### WFHS-REQ-263051/A-Metering each connection

The WifiHotspotServer shall be capable of metering the data consumption of each connected client per session.

#### WFHS-REQ-263052/A-Throttling data consumption

The WifiHotspotServer shall have the ability to throttle a connected client’s throughput. Identification of a client may be done by MAC address or some other identifiable parameter. If the WifiHotspotServer is throttling a particular device, then the fairness model defined in WFHS-REQ-191890-Wi-Fi throughput would not apply to that device.

### Use Cases

#### WFHSv1-UC-REQ-191983/D-User wakes WifiHotspotOnBoardClient up before WifiHotspotServer wakes up

|  |  |
| --- | --- |
| **Actors** | WifiHotspotServer  WifiHotspotOnBoardClient  User |
| **Pre-conditions** | WifiHotspotOnBoardClient is awake  WifiHotspotServer is off |
| **Scenario Description** | User attempts to enter into Wi-Fi Hotspot screens in the in-vehicle WifiHotspotOnBoardClient |
| **Post-conditions** | User is presented either a waiting symbol or a popup and locked out of the screens until the Wi-Fi feature is functioning properly  Any attempts the user makes to enter the Wi-Fi Hotspot screens shall be denied and shall trigger a popup  (refer to WFHS-REQ-226336/A-HMI Specification References) |
| **List of Exception Use Cases** |  |
| **Interfaces** | WifiHotspotServer  WifiHotspotOnBoardClient  CAN |

#### WFHSv1-UC-REQ-191984/C-User is navigating in the Wi-Fi Hotspot screens when WifiHotspotOnBoardClient loses communication with WifiHotspotServer

|  |  |
| --- | --- |
| **Actors** | WifiHotspotServer  WifiHotspotOnBoardClient |
| **Pre-conditions** | WifiHotspotOnBoardClient is awake  WifiHotspotServer is on and reporting statuses on the CAN bus  User is in the Wi-Fi Hotspot screens |
| **Scenario Description** | WifiHotspotOnBoardClient loses communication with WifiHotspotServer over CAN |
| **Post-conditions** | User is presented a popup and locked out of the screens until the WifiHotspotOnBoardClient establishes communication with the WifiHotspotServer  Any attempts the user makes to enter the Wi-Fi Hotspot screens shall be denied and shall trigger a popup  (refer to WFHS-REQ-226336/A-HMI Specification References) |
| **List of Exception Use Cases** |  |
| **Interfaces** | WifiHotspotServer  WifiHotspotOnBoardClient  CAN |

#### WFHSv1-UC-REQ-191986/C-User is navigating in the Wi-Fi Hotspot screens when a Wi-Fi error occurs

|  |  |
| --- | --- |
| **Actors** | WifiHotspotServer  WifiHotspotOnBoardClient |
| **Pre-conditions** | WifiHotspotOnBoardClient is awake  WifiHotspotServer is on  User is in the Wi-Fi Hotspot screens |
| **Scenario Description** | Wi-Fi chipset experiences errors |
| **Post-conditions** | User is presented a popup indicating the WifiHotspotServer is experiencing technical errors and the user is locked out of the screens until the Wi-Fi errors are resolved  Any attempts the user makes to enter the Wi-Fi Hotspot screens shall be denied and shall trigger a popup  (refer to WFHS-REQ-226336/A-HMI Specification References) |
| **List of Exception Use Cases** |  |
| **Interfaces** | WifiHotspotServer  WifiHotspotOnBoardClient  CAN |

#### WFHSv1-UC-REQ-191988/A-Customer puts their vehicle in Valet Mode

|  |  |
| --- | --- |
| **Actors** | WifiHotspotServer  WifiHotspotOnBoardClient  User |
| **Pre-conditions** | WifiHotspotServer is On |
| **Scenario Description** | User puts their vehicle in Valet Mode |
| **Post-conditions** | Wi-Fi Hotspot password may not be viewed on WifiHotspotOnBoardClient display |
| **List of Exception Use Cases** |  |
| **Interfaces** | WifiHotspotOnBoardClient |

#### WFHSv1-UC-REQ-191989/A-Customer sells their vehicle and a new customer takes ownership of the vehicle

|  |  |
| --- | --- |
| **Actors** | WifiHotspotServer  WifiHotspotOnBoardClient  New owner |
| **Pre-conditions** | WifiHotspotServer is On  Vehicle is sold  Previous owner used the free trial period up |
| **Scenario Description** | New vehicle owner purchases the vehicle and accesses the landing page or call center and identifies their vehicle |
| **Post-conditions** | The landing page or carrier hotline operator instructs the new owner to purchase a data plan  Vehicle is not eligible for a free trial period |
| **List of Exception Use Cases** |  |
| **Interfaces** | WifiHotspotOnBoardClient  WifiHotspotServer |

#### WFHSv1-UC-REQ-191990/A-Customer does not activate their free trial period

|  |  |
| --- | --- |
| **Actors** | WifiHotspotServer  WifiHotspotOnBoardClient  User |
| **Pre-conditions** | WifiHotspotServer is On  Free trial period is waiting to be activated |
| **Scenario Description** | New vehicle owner purchases the vehicle and does not activate the trial period right away |
| **Post-conditions** | Customer is presented a free trial period popup reminder in the in-vehicle WifiHotspotOnBoardClient |
| **List of Exception Use Cases** |  |
| **Interfaces** | WifiHotspotOnBoardClient  WifiHotspotServer |

#### WFHSv1-UC-REQ-191932/B-User enters a Wi-Fi Hotspot screen and the text display is delayed

|  |  |
| --- | --- |
| **Actors** | User  System |
| **Pre-conditions** | WifiHotspotServer is on |
| **Scenario Description** | User enters into Wi-Fi SSID/password screen, Connected Devices screen, Blocked devices screen or Data Usage screen |
| **Post-conditions** | The WifiHotspotOnBoardClient displays a blank screen that allows the user to exit out  Text/images may become populated or screen may remain blank |
| **List of Exception Use Cases** |  |
| **Interfaces** | WifiHotspotOnBoardClient  WifiHotspotServer  CAN |

## WFHSv1-FUN-REQ-191999/D-Displaying WifiHotspotServer icon

The WifiHotspotServer shall have a designated icon that shall be displayed on the in-vehicle WifiHotspotOnBoardClient display. The icon shall represent the cellular connection that the modem has with the network. It shall display the technology used to connect to the cellular network (i.e. 3G or 4G) and shall also display the WifiHotspotServer’s signal strength by showing either 1-5 bars or “no service”.

The Wi-Fi Hotspot feature shall also have a designated icon, independent of the WifiHotspotServer icon, that shall be displayed on the in-vehicle WifiHotspotOnBoardClient display. This icon shall be used to indicate whether the Wi-Fi Hotspot service is available or not.

The WifiHotspotServer Wi-Fi Hotspot feature, SYNC Wi-Fi feature and any other Wi-Fi related features existing in the vehicle shall be displayed to the customer in the WifiHotspotOnBoardClient display in a way such that the customer experiences minimum to no confusion. Distinct differentiation between the Wi-Fi features shall be made and customer education on all Wi-Fi features shall be achieved through the in-vehicle WifiHotspotOnBoardClient display.

### Requirements

#### WFHS-REQ-191713/F-Reporting out technology used to connect to the cellular network

The WifiHotspotServer shall detect the technology it is using to connect to the cellular network and transmit this using the CAN signal TCUTechnologyUsed2\_St. If the WifiHotspotServer does not have a connection established with the network (neither the Ford APN nor the Wi-Fi APN are connected), the WifiHotspotServer shall report out “no network”.

If the WifiHotspotServer is unable to detect the technology being used to connect to the network, it shall set the CAN signal to NULL.

#### WFHS-REQ-191711/A-Reporting out the number of devices connected to the Wi-Fi Hotspot

The WifiHotspotServer shall monitor the number of clients connected to the hotspot and transmit this number in the CAN signal NumberOfConnectedDevices\_St. If the number of connected devices increases or decreases the WifiHotspotServer shall update the CAN signal accordingly.

If the WifiHotspotServer cannot detect how many devices are connected, the WifiHotspotServer shall default the CAN signal to 0 devices.

#### WFHS-REQ-191712/D-Converting and reporting out the number of WifiHotspotServer signal strength bars

The WifiHotspotServer shall be responsible for detecting its current signal strength in:

* 1. RSRP (dBm) for LTE
  2. RSCP (dBm) for UMTS and HSPA+
  3. RSSI (dBm) for GSM, GPRS and EDGE.

The WifiHotspotServer shall transmit the number of bars depending on the current signal strength of the network connection using the CAN signal TCUSignalStrength\_St. Refer to the conversion tables below. If the WifiHotspotServer is not connected to the network (neither the Ford APN nor the Wi-Fi APN are connected), the WifiHotspotServer shall report out 0 bars.

1. If the WifiHotspotServer is using the LTE network it shall convert the RSRP values to number of bars using the conversion table below.

|  |  |
| --- | --- |
| **LTE** | |
| **RSRP Thresholds (dBm)** | **Signal Bar Strength Indicator** |
| RSRP ˃ -85 | 5 bars |
| -85 ≥ RSRP ˃ -95 | 4 bars |
| -95 ≥ RSRP ˃ -105 | 3 bars |
| -105 ≥ RSRP ˃ -115 | 2 bars |
| RSRP ≤ -115 | 1 bar |
| No reference signals | No service (0 bars) |

1. If the WifiHotspotServer is using UMTS or HSPA+ it shall convert the RSCP values to number of bars using the conversion table below.

|  |  |
| --- | --- |
| **UMTS, HSPA+ (includes HSPA, HSDPA & HSUPA)** | |
| **RSCP Thresholds (dBm)** | **Signal Bar Strength Indicator** |
| RSCP ˃ -80 | 5 bars |
| -80 ≥ RSCP ˃ -90 | 4 bars |
| -90 ≥ RSCP ˃ -100 | 3 bars |
| -100 ≥ RSCP ˃ -106 | 2 bars |
| RSCP ≤ -106 | 1 bar |
| No reference signals | No service (0 bars) |

1. If the WifiHotspotServer is using GSM, GPRS or EDGE it shall convert the RSSI values to number of bars using the conversion table below.

|  |  |
| --- | --- |
| **GSM, GPRS, EDGE** | |
| **RSSI Thresholds (dBm)** | **Signal Bar Strength Indicator** |
| RSSI ˃ -80 | 5 bars |
| -80 ≥ RSSI ˃ -89 | 4 bars |
| -89 ≥ RSSI ˃ -98 | 3 bars |
| -98 ≥ RSSI ˃ -104 | 2 bars |
| RSSI ≤ -104 | 1 bar |
| No reference signals | No service (0 bars) |

#### WFHS-REQ-191714/G-Displaying the dedicated WifiHotspotServer icon on the WifiHotspotOnBoardClient display

The WifiHotspotServer icon shall represent the status of the cellular connection of the WifiHotspotServer. The icon shall display the number of signal strength bars and the technology in use. The icon below is an example icon. Refer to the HMI specifications to view the actual icon and view the location of the icon (refer to WFHS-REQ-226336/A-HMI Specification References).




Figure. WifiHotspotServer icon

The WifiHotspotOnBoardClient shall display the current signal strength in number of bars based on the status of the CAN signal TCUSignalStrength\_St.

The WifiHotspotOnBoardClient shall also display the technology used (i.e. 3G or 4G) to connect to the cellular network based on the status of the CAN signal TCUTechnologyUsed2\_St. Refer to the Technology Used table within the HMI specs to determine what to display based on the state of the TCUTechnologyUsed2\_St CAN signal.

#### WFHS-REQ-212165/C-Displaying the Wi-Fi Hotspot icon

There may be instances when the WifiHotspotServer is not connected to a network at all or it is connected but the Wi-Fi service is not available because the Wi-Fi channel connection failed due to multiple reasons. Therefore, the in-vehicle occupant shall be informed when the Wi-Fi Hotspot service is and is not available. The Wi-Fi Hotspot icon shall be used to inform the customer when the Wi-Fi Hotspot is:

* On and Wi-Fi service is available,
* On and Wi-Fi service is NOT available and
* Off or On-disabled

Refer to the HMI specifications to view the actual icon, view the different icon states and view the location of the icon (refer to WFHS-REQ-226336/A-HMI Specification References).

The WifiHotspotOnBoardClient shall monitor the CAN signal HotspotEnablement\_St to determine if the Wi-Fi Hotspot is On, On-disabled or Off.

The WifiHotspotOnBoardClient shall monitor the CAN signal HotspotAPNConnection\_St to determine when the Wi-Fi service is and is not available. If the CAN signal is equal to NULL or Not Connected, the Wi-Fi service is NOT available. If the CAN signal is equal to Connected, the Wi-Fi service IS available.

#### WFHS-REQ-222428/A-Reporting out the Wi-Fi APN connectivity status

The WifiHotspotServer shall inform the WifiHotspotOnBoardClient of the Wi-Fi’s APN connectivity status using the CAN signal HotspotAPNConnection\_St. If the Wi-Fi APN is NOT connected to the network, the WifiHotspotServer shall set the CAN signal to Not Connected. If the Wi-Fi APN IS connected to the network, the WifiHotspotServer shall set the CAN signal to Connected. If the WifiHotspotServer is unable to determine the connection status, it shall set the CAN signal to Null.

#### WFHS-REQ-222469/B-Displaying the number of connected devices

The WifiHotspotOnBoardClient shall display the number of devices connected to the hotspot. The CAN signal NumberOfConnectedDevices\_St shall be monitored to determine the number to display. Refer to the HMI specifications to determine where this is displayed (refer to WFHS-REQ-226336/A-HMI Specification References).

## WFHSv1-FUN-REQ-140757/A-Turning Wi-Fi Hotspot On or Off

Users may turn the hotspot on or off through the in-vehicle WifiHotspotOnBoardClient. If the Wi-Fi Hotspot is off, no Wi-Fi enabled devices may connect to the Wi-Fi Hotspot, and if the Wi-Fi Hotspot is on, a set amount of Wi-Fi enabled devices shall be allowed to connect to the Wi-Fi Hotspot (requirement WFHS-REQ-191653-Managing the connected devices list defines the max number of devices).

If the user turns the Wi-Fi Hotspot on or off from the WifiHotspotOnBoardClient display, the WifiHotspotServer shall receive a CAN signal, check the Wi-Fi Hotspot enablement conditions, if necessary, save and update the Wi-Fi Hotspot’s setting and respond to the WifiHotspotOnBoardClient by updating its status on a designated CAN signal.

### Requirements

#### WFHS-REQ-191706/E-Wi-Fi Hotspot enablement condition checks

The WifiHotspotServer shall report the Wi-Fi Hotspot in one of three enablement states through the CAN signal HotspotEnablement\_St:

|  |  |
| --- | --- |
| **Wi-Fi Hotspot Enablement State** | **Functionality** |
| on | The WifiHotspotServer shall provide a Wi-Fi signal and enable clients to connect to the hotspot. This state can only be active when the Wi-Fi Hotspot enablement conditions are met. |
| on-disabled | The WifiHotspotServer shall provide no Wi-Fi signal which shall prohibit clients from connecting to the hotspot. If on-disabled state is active, the WifiHotspotServer shall turn the hotspot to on state as soon as the Wi-Fi Hotspot enablement conditions are all met. |
| off | The WifiHotspotServer shall provide no Wi-Fi signal which shall prohibit clients from connecting to the hotspot. This state can be active regardless of if the Wi-Fi Hotspot enablement conditions are met or not. |

If the WifiHotspotServer is unable to detect the current enablement state of the Wi-Fi Hotspot, the WifiHotspotServer shall set the CAN signal HotspotEnablement\_St to NULL.

The WifiHotspotServer may be required to check the Wi-Fi Hotspot enablement conditions to determine if a specific state can be achieved. If all Wi-Fi Hotspot enablement conditions are met the hotspot is allowed to be turned on.

The on-disabled state implies the hotspot shall turn on as soon as the Wi-Fi Hotspot enablement conditions are met. The table below demonstrates how the WifiHotspotServer shall respond to requests according to different scenarios.

|  |  |  |
| --- | --- | --- |
| **WifiHotspotOnBoardClient Request** | **WifiHotspotServer Response to a Request** | |
|  | Wi-Fi Hotspot enablement conditions not met at time of request | Wi-Fi Hotspot enablement conditions become met at time of request or at a later time |
| Hotspot off | Hotspot is turned to off state | Hotspot remains in off state |
| Hotspot on | Hotspot is turned to on-disabled state | Hotspot is turned to on state |
| Wi-Fi Hotspot Reset (refer to WFHS-REQ-191863-Wi-Fi Hotspot reset) | Hotspot is turned to on-disabled state | Hotspot is turned to on state |

Table. Hotspot enablement state response from a request

* 1. Transport mode condition: The WifiHotspotServer shall be responsible for determining when the vehicle is in transport mode via the CAN signal CarMode\_St. If the vehicle enters Transport mode, the WifiHotspotServer shall gracefully disconnect any connected clients and power down the Wi-Fi chipset. The Wi-Fi chipset shall remain powered off during Transport mode. If the vehicle exits out of Transport mode, the WifiHotspotServer shall power up the Wi-Fi chipset and default the enablement state to on or on-disabled, depending on the status of the Wi-Fi Hotspot enablement conditions.
  2. Ignition Status condition
     1. Ignition= Off: If IgnitionStatus\_St = Off, the WifiHotspotServer shall NOT allow the hotspot to be On. If the hotspot was On when the ignition transitions to Off, the WifiHotspotserver shall turn the hotspot to On-disabled until the ignition transitions to Run, Start or Accessory, at which point it shall turn back to On. If the hotspot is Off and the ignition status is Off when a user requests to turn the hotspot On, the WifiHotspotServer shall turn the hotspot to On-disabled.
     2. Ignition= Run, Start or Accessory: If IgnitionStatus\_St=Run, Start or Accessory the hotspot shall always be allowed to be on unless the WifiHotspotServer is required to turn Off due to a load shed event, etc. (refer to the 4G Telematics Control Unit Power Management Requirements specification for more information) at which point the WifiHotspotServer shall turn the hotspot to On-disabled.

The WifiHotspotServer shall perform the checks displayed in the figures below.



Figure. Wi-Fi Hotspot enablement condition checks needed if the hotspot shall be off



Figure. Wi-Fi Hotspot enablement condition checks needed if the hotspot shall be turned on



Figure. Wi-Fi Hotspot enablement condition checks needed if the hotspot is currently on

#### WFHS-REQ-191708/E-Displaying the Wi-Fi Hotspot's enablement state on the WifiHotspotOnBoardClient display

The WifiHotspotOnBoardClient shall display the current status of the Wi-Fi Hotspot’s enablement state (CAN signal HotspotEnablement\_St). Refer to WFHS-REQ-226336/A-HMI Specification References). The following screens are example WifiHotspotOnBoardClient screens.




Figure. Wi-Fi Hotspot on screen




Figure. Wi-Fi Hotspot off screen

#### WFHS-REQ-191709/A-User requests to turn the Wi-Fi Hotspot on or off through the WifiHotspotOnBoardClient display

If the user requests to turn the Wi-Fi Hotspot on or off from the WifiHotspotOnBoardClient display, the WifiHotspotOnBoardClient shall transmit this request to the WifiHotspotServer using the CAN signal HotspotEnablement\_Rq.

#### WFHS-REQ-191707/A-Request from WifiHotspotOnBoardClient to turn the Wi-Fi Hotspot on or off

If the WifiHotspotServer receives a request from the WifiHotspotOnBoardClient to turn the Wi-Fi Hotspot off (CAN signal HotspotEnablement\_Rq), the WifiHotspotServer shall turn the Wi-Fi Hotspot enablement state to off.

If the WifiHotspotServer receives a request from the WifiHotspotOnBoardClient to turn the Wi-Fi Hotspot on (CAN signal HotspotEnablement\_Rq), the WifiHotspotServer shall check the Wi-Fi Hotspot enablement conditions and configure the Wi-Fi Hotspot to the appropriate enablement state.

### Use Cases

#### WFHSv1-UC-REQ-191925/C-User turns Wi-Fi Hotspot On

|  |  |
| --- | --- |
| **Actors** | User  System  Cell phone |
| **Pre-conditions** | WifiHotspotServer is on  Wi-Fi Hotspot enablement conditions as defined in WFHS-REQ-191706-Wi-Fi Hotspot enablement condition checks are met  Wi-Fi Hotspot is off |
| **Scenario Description** | User turns the Wi-Fi Hotspot on through WifiHotspotOnBoardClient display |
| **Post-conditions** | Wi-Fi Hotspot is on and available  Vehicle occupant may now connect a device to the Wi-Fi Hotspot  WifiHotspotOnBoardClient shall update as defined in the HMI spec (refer to WFHS-REQ-226336/A-HMI Specification References). |
| **List of Exception Use Cases** | WFHSv1-UC-REQ-191931-E4 Wi-Fi Hotspot configuration through WifiHotspotOnBoardClient fails  WFHSv1-UC-REQ-191973-E11 WifiHotspotOnBoardClient update failed |
| **Interfaces** | WifiHotspotOnBoardClient  WifiHotspotServer  CAN |

#### WFHSv1-UC-REQ-191926/C-User turns Wi-Fi Hotspot Off

|  |  |
| --- | --- |
| **Actors** | User  System  Cell phone |
| **Pre-conditions** | Hotspot on  Up to Number\_Hotspot\_Connected\_Devices devices connected to the Wi-Fi Hotspot |
| **Scenario Description** | User turns Wi-Fi Hotspot off through WifiHotspotOnBoardClient display |
| **Post-conditions** | Wi-Fi Hotspot is off  All connected devices become disconnected from Wi-Fi Hotspot  WifiHotspotOnBoardClient display shall update as defined in the HMI spec (refer to WFHS-REQ-226336/A-HMI Specification References). |
| **List of Exception Use Cases** | WFHSv1-UC-REQ-191931-E4 Wi-Fi Hotspot configuration through WifiHotspotOnBoardClient fails  WFHSv1-UC-REQ-191973-E11 WifiHotspotOnBoardClient update failed |
| **Interfaces** | WifiHotspotOnBoardClient  WifiHotspotServer  CAN |

#### WFHSv1-UC-REQ-191927/C-User attempts to turn the Wi-Fi Hotspot on when the Wi-Fi Hotspot enablement conditions are not met

|  |  |
| --- | --- |
| **Actors** | User  System  Cell phone |
| **Pre-conditions** | WifiHotspotServer is on  Wi-Fi Hotspot is off  Wi-Fi Hotspot enablement conditions are not met (refer to WFHS-REQ-191706-Wi-Fi Hotspot enablement conditions check) |
| **Scenario Description** | User turns Wi-Fi Hotspot on through WifiHotspotOnBoardClient |
| **Post-conditions** | Wi-Fi Hotspot is turned to on-disabled  Devices may not connect to Wi-Fi Hotspot  WifiHotspotOnBoardClient shall update as defined in the HMI spec (refer to WFHS-REQ-226336/A-HMI Specification References). |
| **List of Exception Use Cases** | WFHSv1-UC-REQ-191931-E4 Wi-Fi Hotspot configuration through WifiHotspotOnBoardClient fails  WFHSv1-UC-REQ-191973-E11 WifiHotspotOnBoardClient update failed |
| **Interfaces** | WifiHotspotOnBoardClient  WifiHotspotServer  CAN |

#### WFHSv1-UC-REQ-191928/D-Wi-Fi Hotspot in On-disabled state when the Wi-Fi Hotspot enablement conditions become met

|  |  |
| --- | --- |
| **Actors** | System  Cell phone |
| **Pre-conditions** | Wi-Fi Hotspot is on-disabled  Wi-Fi Hotspot enablement conditions as defined in WFHS-REQ-191706-Wi-Fi Hotspot enablement condition checks are not met |
| **Scenario Description** | Wi-Fi Hotspot enablement conditions become met |
| **Post-conditions** | Wi-Fi Hotspot is automatically turned to on  Vehicle occupant may now connect a device to the Wi-Fi Hotspot  WifiHotspotOnBoardClient display shall update as defined in the HMI spec (refer to WFHS-REQ-226336/A-HMI Specification References). |
| **List of Exception Use Cases** | WFHSv1-UC-REQ-191973-E11 WifiHotspotOnBoardClient update failed |
| **Interfaces** | WifiHotspotOnBoardClient  WifiHotspotServer  CAN |

#### WFHSv1-UC-REQ-191929/C-Wi-Fi Hotspot is on when the Wi-Fi Hotspot enablement conditions become not met

|  |  |
| --- | --- |
| **Actors** | System  Cell phone |
| **Pre-conditions** | Wi-Fi Hotspot is on  Wi-Fi Hotspot enablement conditions as defined in WFHS-REQ-191706-Wi-Fi Hotspot enablement condition checks are met  Up to Number\_Hotspot\_Connected\_Devices devices connected to the Wi-Fi Hotspot |
| **Scenario Description** | Hotspot enablement conditions are no longer met |
| **Post-conditions** | Wi-Fi Hotspot is automatically turned to on-disabled  All connected devices are disconnected  WifiHotspotOnBoardClient shall update as defined in the HMI spec (refer to WFHS-REQ-226336/A-HMI Specification References) |
| **List of Exception Use Cases** | WFHSv1-UC-REQ-191973-E11 WifiHotspotOnBoardClient update failed |
| **Interfaces** | WifiHotspotOnBoardClient  WifiHotspotServer  CAN |

#### WFHSv1-UC-REQ-191923/D-Vehicle enters transport mode

|  |  |
| --- | --- |
| **Actors** | System |
| **Pre-conditions** | Engine is on/off  Vehicle is not in transport mode  Enhanced hotspot enablement mode is on (refer to WFHS-REQ-191706-Wi-Fi Hotspot enablement mode condition checks)  Wi-Fi Hotpot is on |
| **Scenario Description** | Vehicle enters transport mode |
| **Post-conditions** | Wi-Fi Hotspot turns off until the vehicle leaves transport mode  WifiHotspotOnBoardClient display shall update as defined in the HMI spec (refer to WFHS-REQ-226336/A-HMI Specification References). |
| **List of Exception Use Cases** | WFHSv1-UC-REQ-191973-E11 WifiHotspotOnBoardClient update failed |
| **Interfaces** | WifiHotspotOnBoardClient  WifiHotspotServer  BCM  CAN |

#### WFHSv1-UC-REQ-191930/A-E3 Wi-Fi Hotspot command through mobile app fails

|  |  |
| --- | --- |
| **Actors** | User  Mobile app |
| **Pre-conditions** | Same as normal use case |
| **Scenario Description** | The user’s command through mobile app fails due to command/control failures defined in the Overview section of this document |
| **Post-conditions** | Page shows pending request until timed out  Mobile app page indicates an unsuccessful attempt and returns to previous display |
| **List of Exception Use Cases** |  |
| **Interfaces** | Mobile app  Ford infrastructure  Carrier infrastructure |

#### WFHSv1-UC-REQ-191931/A-E4 Wi-Fi Hotspot configuration through WifiHotspotOnBoardClient fails

|  |  |
| --- | --- |
| **Actors** | User  WifiHotspotOnBoardClient  WifiHotspotServer |
| **Pre-conditions** | Same as normal use case |
| **Scenario Description** | The user’s configuration through the WifiHotspotOnBoardClient failed due to command/control failures defined in the Overview section of this document |
| **Post-conditions** | Old Hotspot settings are restored and displayed to the customer |
| **List of Exception Use Cases** |  |
| **Interfaces** | WifiHotspotOnBoardClient  WifiHotspotServer  CAN |

#### WFHSv1-UC-REQ-191973/A-E11 WifiHotspotOnBoardClient update failed

|  |  |
| --- | --- |
| **Actors** | User  System  Cell phone |
| **Pre-conditions** | Same as normal use case |
| **Scenario Description** | Wi-Fi Hotspot settings are updated by WifiHotspotServer or carrier and WifiHotspotOnBoardClient update failed due to command/control failures defined in the Overview section of this document |
| **Post-conditions** | WifiHotspotOnBoardClient displays old settings |
| **List of Exception Use Cases** |  |
| **Interfaces** | Ford infrastructure  Carrier infrastructure  Mobile app  WifiHotspotServer  WifiHotspotOnBoardClient  CAN |

#### WFHSv1-UC-REQ-191974/A-E12 Mobile app update failed

|  |  |
| --- | --- |
| **Actors** | User  System  Cell phone |
| **Pre-conditions** | Same as normal use case |
| **Scenario Description** | Wi-Fi Hotspot settings are updated by carrier, and mobile app update failed due to command/control failures defined in the Overview section of this document |
| **Post-conditions** | Mobile app WifiHotspotOnBoardClient displays old settings |
| **List of Exception Use Cases** |  |
| **Interfaces** | Ford infrastructure  Carrier infrastructure  Mobile app |

### White Box Views

#### Activity Diagrams

##### WFHSv1-ACT-REQ-167127/A-User Turns Wi-Fi Hotspot On From Centerstack



#### Sequence Diagrams

##### WFHSv1-SD-REQ-167144/A-User Turns Wi-Fi Hotspot On Off From Centerstack



## WFHSv1-FUN-REQ-140746/C-Managing SSID

The Wi-Fi Hotspot must have an SSID used to differentiate one WLAN from another. The SSID must be between 1-32 ASCII characters and may be configurable by the user from the in-vehicle WifiHotspotOnBoardClient. The WifiHotspotOnBoardClient shall be responsible for verifying that the customer input does not violate the SSID character length. Each WifiHotspotServer shall come with a default SSID.

If the user enters into a screen that displays the SSID, the WifiHotspotOnBoardClient shall transmit a Wi-Fi Info request to the WifiHotspotServer, and in turn, the WifiHotspotServer shall respond with the appropriate SSID and password characters.

### Requirements

#### WFHS-REQ-162363/A-Assigning the SSID to each frequency band

The WifiHotspotServer shall assign the same SSID to both the 2.4 and 5 GHz band.

#### WFHS-REQ-191596/B-Generating the default SSID

Each WifiHotspotServer shall be delivered to Ford with a unique default SSID in the format below:

|  |  |
| --- | --- |
| **Default SSID** | HotspotXXXX |

The XXXX shall be four ASCII characters, randomly generated by the WifiHotspotServer. The same number generator used to generate the password may be used to generate the last four characters. Refer to WFHS-REQ-191610-Generating the initial password. The SSID shall also be updateable via EOL.

#### WFHS-REQ-191634/D-Displaying the SSID on the WifiHotspotOnBoardClient display

If the user enters into any screen that requires the WifiHotspotOnBoardClient to display the SSID characters, the WifiHotspotOnBoardClient shall send a request to the WifiHotspotServer to read the current SSID and password using the CAN signal WifiInfo\_Rq. Once the WifiHotspotOnBoardClient receives a response (CAN signal WifiInfo\_Rsp) from the WifiHotspotServer it shall populate the screen with the corresponding SSID, but keep the password hidden. Refer to WFHS-REQ-191633-Displaying the password on the in-vehicle WifiHotspotOnBoardClient for more information on when to display the password. Refer to WFHS-REQ-226336/A-HMI Specification References. The following screen is an example WifiHotspotOnBoardClient screen.




Figure. Screen Displaying the SSID and Password Characters

#### WFHS-REQ-191629/C-Keyboard used to edit the SSID through WifiHotspotOnBoardClient display

The Wi-Fi Hotspot SSID keyboard provided through the in-vehicle WifiHotspotOnBoardClient screen shall include only ASCII characters for all regions: NA (United States and Canada), China and Europe. Refer to WFHS-REQ-226336/A-HMI Specification References. The SSID keyboard shall inform the user of the appropriate SSID length (1-32 characters). The following screen is an example WifiHotspotOnBoardClient screen.




Figure. Wi-Fi Hotspot SSID Keyboard

#### WFHS-REQ-191635/E-Accepting and updating user SSID configurations

If the vehicle occupant updates the SSID through the WifiHotspotOnBoardClient the WifiHotspotOnBoardClient shall confirm the SSID is between 1-32 ASCII characters. The keyboard shall not allow the user to enter the SSID if it does not meet the required length. If the vehicle occupant has entered an SSID of the appropriate length the WifiHotspotOnBoardClient shall send this update to the WifiHotspotServer using the CAN signal WifiInfo\_Rq and wait for a response in the CAN signal WifiInfo\_Rsp. If the WifiHotspotServer sends back an unsuccessful response the WifiHotspotOnBoardClient shall notify the user and keep the user in the SSID keyboard screen. If the WifiHotspotServer sends back a successful response the WifiHotspotOnBoardClient shall notify the user and exit out of the keyboard screen.

If the vehicle occupant is on a screen that displays the SSID when the WifiHotspotOnBoardClient receives a WifiInfo\_Rsp response = SSIDWritten, the WifiHotspotOnBoardClient shall request for the new data using WifiInfo\_Rq = Read. Once the WifiHotspotOnBoardClient receives the updated SSID it shall reflect the update on the SSID screen.

Refer WFHS-REQ-226336/A-HMI Specification References. The following screens are example WifiHotspotOnBoardClient popups.



Figure. Unsuccessful SSID Update



Figure. Successful SSID Update

#### WFHS-REQ-191628/A-SSID update request from WifiHotspotOnBoardClient

If the WifiHotspotServer receives a request from the WifiHotspotOnBoardClient to change the SSID (CAN signal WifiInfo\_Rq), the WifiHotspotServer shall update and store the new SSID. Once the WifiHotspotServer has successfully updated the SSID, it shall transmit a successful response to the WifiHotspotOnBoardClient (CAN signal WifiInfo\_Rsp). In case of an unsuccessful attempt, the WifiHotspotServer shall send an unsuccessful response.

#### WFHS-REQ-191630/A-Disconnecting clients due to an SSID update

If the WifiHotspotServer changes the hotspot’s SSID, the WifiHotspotServer shall gracefully disconnect all connected clients. Each user shall be required to search for the Wi-Fi Hotspot’s new SSID on their client device and enter in the password in order to re-connect.

### Use Cases

#### WFHSv1-UC-REQ-191933/B-User changes SSID from WifiHotspotOnBoardClient

|  |  |
| --- | --- |
| **Actors** | User  System |
| **Pre-conditions** | WifiHotspotServer is on  SSID/password screen is not driver restricted  Up to Number\_Hotspot\_Connected\_Devices devices connected to the hotspot  User is in the SSID edit screen |
| **Scenario Description** | User enters new SSID from WifiHotspotOnBoardClient that is between 1-32 characters long |
| **Post-conditions** | WifiHotspotOnBoardClient shall display a successful message and the new SSID shall be displayed on the appropriate screen  All connected devices are disconnected |
| **List of Exception Use Cases** | WFHSv1-UC-REQ-191936-E5 User attempts to view SSID/password through WifiHotspotOnBoardClient while under driver restriction  WFHSv1-UC-REQ-191934-E7 User attempts to enter SSID not between 1-32 characters long  WFHSv1-UC-REQ-191931-E4 Wi-Fi Hotspot configuration through WifiHotspotOnBoardClient fails  WFHSv1-UC-REQ-191935-E6 SSID update from WifiHotspotOnBoardClient failed |
| **Interfaces** | WifiHotspotServer  WifiHotspotOnBoardClient  CAN |

#### WFHSv1-UC-REQ-191936/D-E5 User attempts to view SSID/password through WifiHotspotOnBoardClient while under driver restriction

|  |  |
| --- | --- |
| **Actors** | Vehicle occupant  WifiHotspotServer  In-vehicle WifiHotspotOnBoardClient |
| **Pre-conditions** | User is viewing the SSID/password screen on the WifiHotspotOnBoardClient display  SSID/password screen is not under driver restriction |
| **Scenario Description** | Vehicle occupant drives the vehicle over a certain speed and the screen is placed under driver restriction |
| **Post-conditions** | The WifiHotspotOnBoardClient exits the SSID/password screen  The user shall not be allowed back into the screen that displays the SSID and password  WifiHotspotOnBoardClient shall follow the driver restriction (H21j) (Refer to WFHS-REQ-226336/A-HMI Specification References) |
| **List of Exception Use Cases** |  |
| **Interfaces** | WifiHotspotOnBoardClient  CAN  PCM |

#### WFHSv1-UC-REQ-191935/A-E6 SSID update from WifiHotspotOnBoardClient failed

|  |  |
| --- | --- |
| **Actors** | User  System |
| **Pre-conditions** | Same as normal use case |
| **Scenario Description** | User enters new SSID from WifiHotspotOnBoardClient that is between 1-32 characters long but the WifiHotspotServer was unable to successfully change the SSID |
| **Post-conditions** | An error message is displayed to the user  The SSID is not changed |
| **List of Exception Use Cases** |  |
| **Interfaces** | WifiHotspotServer  WifiHotspotOnBoardClient  CAN |

#### WFHSv1-UC-REQ-191934/A-E7 User attempts to enter SSID not between 1-32 characters long

|  |  |
| --- | --- |
| **Actors** | User  System  Cell phone |
| **Pre-conditions** | Same as normal use case |
| **Scenario Description** | User types an SSID into the keyboard on the WifiHotspotOnBoardClient that is longer than 32 characters or less than 1 character |
| **Post-conditions** | Keyboard does not allow the user to enter the request  The SSID is not changed |
| **List of Exception Use Cases** |  |
| **Interfaces** | WifiHotspotOnBoardClient |

### White Box Views

#### Activity Diagrams

##### WFHSv1-ACT-REQ-167121/B-User Changes SSID From Centerstack



#### Sequence Diagrams

##### WFHSv1-SD-REQ-167136/B-User Changes SSID From Centerstack



## WFHSv1-FUN-REQ-140744/B-Managing Password

The Wi-Fi Hotspot shall always be password protected to provide security to the network. The WifiHotspotServer shall come equipped with a randomly generated 12 ASCII character password. Users may view and change the password on the in-vehicle WifiHotspotOnBoardClient. The password may be changed, but it must be 8-63 ASCII characters, and the WifiHotspotOnBoardClient shall be responsible for verifying that the customer input does not violate this password character length.

If the user enters a screen that allows the password to be displayed, the WifiHotspotOnBoardClient shall transmit a Wi-Fi Info request to the WifiHotspotServer, and in turn, the WifiHotspotServer shall respond with the appropriate SSID and password characters.

### Requirements

#### WFHS-REQ-191598/A-Assigning the password to each frequency band

The WifiHotspotServer shall assign the same password to both the 2.4 and 5 GHz band.

#### WFHS-REQ-191610/C-Generating the initial password

Each WifiHotspotServer shall be delivered to Ford with a password created for its hotspot. Each WifiHotspotServer shall randomly generate and store a 12 ASCII character string for its first password. The generated passwords shall be created using a quality random number generator. The supplier shall meet the requirements defined in A51t\_Supplier\_Feed\_Specification\_080.pdf spec, section 1.9.9 Requirements for Key Generation. Each password that the WifiHotspotServer randomly generates for the hotspot to use shall not include the lowercase “l” (L) or the capital “I” (i) due to their similar appearance. Therefore, the WifiHotspotServer shall implement an algorithm that can exclude these two particular characters while generating.

#### WFHS-REQ-191633/D-Displaying the password on the WifiHotspotOnBoardClient display

If the user enters into any screen that requires the WifiHotspotOnBoardClient to display the password characters, the WifiHotspotOnBoardClient shall send a request to the WifiHotspotServer to read the current SSID and password using the CAN signal WifiInfo\_Rq. Once the WifiHotspotOnBoardClient receives a response (CAN signal WifiInfo\_Rsp) from the WifiHotspotServer it shall populate the screen with the corresponding SSID, but keep the password hidden. The WifiHotspotOnBoardClient shall display asterisks in place of the password. The number of asterisks shall equal 12. The screen shall provide the customer with a way to view and hide the password. The password shall always be hidden until the customer manually requests to view it. Should the customer choose to display the password, the WifiHotspotOnBoardClient shall display it until either the customer chooses to hide the password or exits the screen. Refer to WFHS-REQ-226336/A-HMI Specification References. The screen below is an example WifiHotspotOnBoardClient screen.




Figure. Screen Displaying the SSID and Password Characters

#### WFHS-REQ-191637/A-Hiding the password while vehicle is in Valet Mode

If the vehicle is in Valet Mode the WifiHotspotOnBoardClient shall hide the password and NOT allow the password to be viewable in the in-vehicle WifiHotspotOnBoardClient. If the vehicle is NOT in Valet Mode the password may be viewed upon the vehicle occupant’s request (refer to WFHS-REQ-191633-Displaying the password on the in-vehicle WifiHotspotOnBoardClient).

#### WFHS-REQ-191627/A-Reporting the SSID and password

If the WifiHotspotServer receives a request from the WifiHotspotOnBoardClient to read the current SSID and password (CAN signal WifiInfo\_Rq), the WifiHotspotServer shall transmit the SSID and password characters using the CAN signal WifiInfo\_Rsp.

Note: the Wi-Fi Hotspot password (CAN signal WifiInfo\_Rsp) shall not be routed out through the SDLC to the OBD-II connector.

#### WFHS-REQ-191632/C-Keyboard used to edit the password through WifiHotspotOnBoardClient display

The Wi-Fi Hotspot password keyboard provided through the in-vehicle WifiHotspotOnBoardClient screen shall include only ASCII characters for all regions: NA (United States and Canada), China and Europe. Refer to WFHS-REQ-226336/A-HMI Specification References. The password keyboard shall inform the user of the appropriate password lengths (8-63 characters). The following screen is an example WifiHotspotOnBoardClient screen.




Figure. Wi-Fi Hotspot Password Keyboard

#### WFHS-REQ-191636/D-Accepting and updating user password configurations

If the vehicle occupant updates the password through the WifiHotspotOnBoardClient, the WifiHotspotOnBoardClient shall confirm the password is between 8-63 characters. The keyboard shall not allow the user to enter the password if it does not meet the required length. If the vehicle occupant has entered a password of the appropriate length the WifiHotspotOnBoardClient shall send this update to the WifiHotspotServer using the CAN signal WifiInfo\_Rq and wait for a response in the CAN signal WifiInfo\_Rsp. If the WifiHotspotServer sends back an unsuccessful response the WifiHotspotOnBoardClient shall notify the user and keep the user in the password keyboard screen. If the WifiHotspotServer sends back a successful response the WifiHotspotOnBoardClient shall notify the user and exit out of the keyboard screen.

If the vehicle occupant is on a screen that displays the password when the WifiHotspotOnBoardClient receives a WifiInfo\_Rsp response = PasswordWritten, the WifiHotspotOnBoardClient shall request for the new data using WifiInfo\_Rq = Read. Once the WifiHotspotOnBoardClient receives the updated password it shall reflect the update on the password screen.

Refer to WFHS-REQ-226336/A-HMI Specification References. The following screens are example WifiHotspotOnBoardClient popups.



Figure. Unsuccessful Password Update



Figure. Successful Password Update

#### WFHS-REQ-191638/A-Password update request from WifiHotspotOnBoardClient

If the WifiHotspotServer receives a request from the WifiHotspotOnBoardClient to change the password (CAN signal WifiInfo\_Rq), the WifiHotspotServer shall update and store the new password. Once the WifiHotspotServer has successfully updated the password, it shall transmit a successful response to the WifiHotspotOnBoardClient (CAN signal WifiInfo\_Rsp). In case of an unsuccessful attempt, the WifiHotspotServer shall send an unsuccessful response.

#### WFHS-REQ-191631/A-Disconnecting clients due to a password update

If the WifiHotspotServer changes the hotspot’s password, the WifiHotspotServer shall gracefully disconnect all connected clients. Each user shall be required to search for the Wi-Fi Hotspot’s SSID on their client device and enter in the new password in order to re-connect.

### Use Cases

#### WFHSv1-UC-REQ-191937/E-User enters into the Wi-Fi Hotspot screen that displays the SSID and password

|  |  |
| --- | --- |
| **Actors** | User  System |
| **Pre-conditions** | WifiHotspotServer is on  SSID/password screen is not under driver restriction |
| **Scenario Description** | User enters into the Wi-Fi Hotspot screen that displays the SSID and password |
| **Post-conditions** | The SSID is displayed  The password is hidden, but the WifiHotspotOnBoardClient screen displays the option to view the password  Refer to the HMI spec to see the settings that are displayed |
| **List of Exception Use Cases** |  |
| **Interfaces** | WifiHotspotServer  WifiHotspotOnBoardClient  CAN |

#### WFHSv1-UC-REQ-191938/C-User views the password on the WifiHotspotOnBoardClient

|  |  |
| --- | --- |
| **Actors** | User  System |
| **Pre-conditions** | WifiHotspotServer is on  User is in the Wi-Fi Hotspot screen that displays the password on the WifiHotspotOnBoardClient display  Password is hidden  SSID/password screen is not under driver restriction |
| **Scenario Description** | User requests to view the password |
| **Post-conditions** | The password is displayed until the user exits out of the screen or until the user chooses to hide the password  The option to hide the password is presented |
| **List of Exception Use Cases** |  |
| **Interfaces** | WifiHotspotServer  WifiHotspotOnBoardClient  CAN |

#### WFHSv1-UC-REQ-191939/B-User changes password from WifiHotspotOnBoardClient

|  |  |
| --- | --- |
| **Actors** | User  System |
| **Pre-conditions** | WifiHotspotServer is on  SSID/password screen is not under driver restriction  Up to Number\_Hotspot\_Connected\_Devices devices connected to the Wi-Fi Hotspot  User is in the password edit screen |
| **Scenario Description** | User enters a new password into the keyboard on the WifiHotspotOnBoardClient that is between 8-63 characters long |
| **Post-conditions** | WifiHotspotOnBoardClient displays a successful message and the new password is displayed on the appropriate screen  All connected devices are disconnected |
| **List of Exception Use Cases** | WFHSv1-UC-REQ-191940-E8 User attempts to enter password less than 8 characters long OR longer than 63 characters  WFHSv1-UC-REQ-191941-E9 Password update from WifiHotspotOnBoardClient failed  WFHSv1-UC-REQ-191973-E11 WifiHotspotOnBoardClient update failed |
| **Interfaces** | WifiHotspotServer  WifiHotspotOnBoardClient  CAN |

#### WFHSv1-UC-REQ-191940/A-E8 User attempts to enter password less than 8 characters long OR longer than 63 characters

|  |  |
| --- | --- |
| **Actors** | User  System  Cell phone |
| **Pre-conditions** | Same as normal use case |
| **Scenario Description** | User types in a password into the keyboard on WifiHotspotOnBoardClient that is not between 8-63 characters long |
| **Post-conditions** | The keyboard does not allow the password request to be entered  The password is not changed |
| **List of Exception Use Cases** |  |
| **Interfaces** | WifiHotspotOnBoardClient |

#### WFHSv1-UC-REQ-191941/A-E9 Password update from WifiHotspotOnBoardClient failed

|  |  |
| --- | --- |
| **Actors** | User  System |
| **Pre-conditions** | Same as normal use case |
| **Scenario Description** | User enters new password from WifiHotspotOnBoardClient that is between 8-63 characters long but the WifiHotspotServer was unable to successfully change the password |
| **Post-conditions** | An error message is displayed to the user  The password is not changed |
| **List of Exception Use Cases** |  |
| **Interfaces** | WifiHotspotServer  WifiHotspotOnBoardClient  CAN |

### White Box Views

#### Activity Diagrams

##### WFHSv1-ACT-REQ-167117/B-User Changes Password From Centerstack



#### Sequence Diagrams

##### WFHSv1-SD-REQ-167132/B-User Changes Password From Centerstack



## WFHSv1-FUN-REQ-140745/C-Changing Security Algorithm

The WifiHotspotServer shall enable encryption algorithms for the Wi-Fi feature. The security encryption shall be defaulted to WPA2/WPA for all regions.

### Requirements

#### WFHS-REQ-191642/D-Security algorithm offerings per region

The WifiHotspotServer shall enable WPA/WPA2 security encryption for all regions. The WifiHotspotServer shall report this security encryption using the CAN signal HotspotSecurity\_St.

If the WifiHotspotServer cannot detect the type of security that is enabled, it shall set the CAN signal HotspotSecurity\_St to NULL.

#### WFHS-REQ-191644/C-Displaying the security type

The WifiHotspotOnBoardClient shall display the current security encryption enabled, which is reported by the WifiHotspotServer through the CAN signal HotspotSecurity\_St. Refer to WFHS-REQ-226336/A-HMI Specification References. The following screen is an example WifiHotspotOnBoardClient screen.




Figure. Display of the Current Security Type

## WFHSv1-FUN-REQ-140758/A-Turning Visibility On or Off

The visibility function controls the broadcast of the hotspot’s SSID. If the visibility is set to on, Wi-Fi enabled devices may search for the network without specifying the SSID. If the visibility is off the user must enter the network’s SSID into the Wi-Fi enabled device, before searching, in order to find the network. Once the network is found, the user shall enter the security type and password to connect. The user may turn the visibility on or off through the in-vehicle WifiHotspotOnBoardClient.

If the user changes the visibility from the in-vehicle WifiHotspotOnBoardClient the WifiHotspotServer shall receive a CAN signal, save and update the hotspot’s setting and respond to the WifiHotspotOnBoardClient by updating its status on a designated CAN signal.

### Requirements

#### WFHS-REQ-191647/B-Function of the visibility feature

If the visibility is set to on the WifiHotspotServer shall broadcast the hotspot’s SSID in the beacon frames. If the visibility is set to off the SSID shall not be broadcasted in the beacon frames. The visibility shall be configurable by the customer as well as via EOL.

#### WFHS-REQ-191648/B-Reporting the visibility status

The WifiHotspotServer shall report the current status of the visibility feature using the CAN signal HotspotVisibility\_St. If the WifiHotspotServer cannot detect the current visibility state, it shall set the CAN signal to NULL.

#### WFHS-REQ-191650/C-Displaying the status of the visibility feature

The WifiHotspotOnBoardClient shall display the current status of the hotspot’s visibility feature, which is reported from the WifiHotspotServer through the CAN signal HotspotVisibility\_St (refer to WFHS-REQ-226336/A-HMI Specification References). The following screens are example WifiHotspotOnBoardClient screens.




Figure. Viewing Visibility Status

#### WFHS-REQ-191651/A-User requests to configure visibility feature through WifiHotspotOnBoardClient display

If the user requests to turn the hotspot’s visibility on or off through the in-vehicle WifiHotspotOnBoardClient, the WifiHotspotOnBoardClient shall transmit this request to the WifiHotspotServer using the CAN signal HotspotVisibility\_Rq.

#### WFHS-REQ-191649/A-Visibility update request from WifiHotspotOnBoardClient

If the WifiHotspotServer receives a request from the WifiHotspotOnBoardClient (CAN signal HotspotVisibility\_Rq) to change the visibility status, the WifiHotspotServer shall update and save the visibility status. If the WifiHotspotServer’s attempt was unsuccessful, the WifiHotspotServer shall continue reporting out the current status of the visibility feature using the CAN signal HotspotVisibility\_St.

### Use Cases

#### WFHSv1-UC-REQ-191943/C-User turns the Wi-Fi Hotspot visibility on

|  |  |
| --- | --- |
| **Actors** | User  System  Cell phone |
| **Pre-conditions** | Wi-Fi Hotspot is on  Wi-Fi Hotspot visibility is off |
| **Scenario Description** | User turns Wi-Fi Hotspot visibility on from WifiHotspotOnBoardClient |
| **Post-conditions** | The vehicle’s Wi-Fi hotspot SSID will automatically appear when devices are searching for Wi-Fi networks nearby  User may connect to the Wi-Fi Hotspot by entering the password  WifiHotspotOnBoardClient display shall update as defined in the HMI spec (refer to WFHS-REQ-226336/A-HMI Specification References). |
| **List of Exception Use Cases** | WFHSv1-UC-REQ-191931-E4 Wi-Fi Hotspot configuration through WifiHotspotOnBoardClient fails  WFHSv1-UC-REQ-191973-E11 WifiHotspotOnBoardClient update failed |
| **Interfaces** | WifiHotspotServer  WifiHotspotOnBoardClient  CAN |

#### WFHSv1-UC-REQ-191944/C-User turns Wi-Fi Hotspot visibility off

|  |  |
| --- | --- |
| **Actors** | User  System  Cell phone |
| **Pre-conditions** | Wi-Fi Hotspot is on  Wi-Fi Hotspot visibility is on |
| **Scenario Description** | User turns the visibility off from WifiHotspotOnBoardClient |
| **Post-conditions** | The vehicle’s Wi-Fi Hotspot SSID will NOT appear when devices are searching for Wi-Fi networks nearby  User must manually type SSID, security type, encryption type, & password into device to connect  WifiHotspotOnBoardClient display shall update as defined in the HMI spec (refer to WFHS-REQ-226336/A-HMI Specification References) |
| **List of Exception Use Cases** | WFHSv1-UC-REQ-191931-E4 Wi-Fi Hotspot configuration through WifiHotspotOnBoardClient fails  WFHSv1-UC-REQ-191973-E11 WifiHotspotOnBoardClient update failed |
| **Interfaces** | WifiHotspotServer  WifiHotspotOnBoardClient  CAN |

### White Box Views

#### Activity Diagrams

##### WFHSv1-ACT-REQ-167129/A-Wi-Fi Visibility On From Centerstack



#### Sequence Diagrams

##### WFHSv1-SD-REQ-167146/A-User Turns Wi-Fi Visibility On Off From Centerstack



## WFHSv1-FUN-REQ-140752/B-Manage Devices

The user shall be able to manage devices connected to their hotspot. The user may view the clients connected to the hotspot through the in-vehicle WifiHotspotOnBoardClient screen and disconnect any of the clients listed, placing those clients on the blocked list. The user may also view the blocked clients and delete any client off of the blocked list, allowing that client to connect again.

If the user enters into the Connected Devices or Blocked Devices screen the WifiHotspotOnBoardClient shall transmit a request for the device list and specify whether it is a request for the connected devices or a request for the blocked devices. If the WifiHotspotServer receives this request it shall respond with the appropriate list of devices. If a device connects to or disconnects from the WifiHotspotServer (except if initiated through the in-vehicle WifiHotspotOnBoardClient) the WifiHotspotServer shall set a connected device update bit. The WifiHotspotOnBoardClient shall monitor this bit and, if the user is in the Connected Devices screen when this bit is set, the WifiHotspotOnBoardClient shall request for the device list once again. The WifiHotspotServer may unset the update bit once it responds to the WifiHotspotOnBoardClient’s request.

### Requirements

#### WFHS-REQ-191652/B-Checklist for allowing a device to connect to the Wi-Fi Hotspot

The WifiHotspotServer shall manage two lists (Connected List and Blocked List) in order to determine if it shall allow a device to connect to the Wi-Fi Hotspot. The diagram below displays the checks that shall be performed by the WifiHotspotServer before allowing a device to connect to the Wi-Fi hotspot.



Figure. Checklist before allowing a device to connect to the Wi-Fi Hotspot

#### WFHS-REQ-191653/E-Managing the connected devices list

The WifiHotspotServer shall manage a list called the Connected List. This list shall store all the devices currently connected to the hotspot. The WifiHotspotServer shall limit the number of devices allowed to be connected at one time. This number (Number\_Hotspot\_Connected\_Devices) shall be a configurable DID, defaulted to 20. All devices attempting to connect to the hotspot that violate this number shall be denied access. Once the number of connected devices drops below Number\_Hotspot\_Connected\_Devices, the devices may attempt to connect again.

The WifiHotspotServer shall detect when clients connect and disconnect from the hotspot. The WifiHotspotServer shall detect and store the entire MAC address and up to the first Device\_Name\_Characters\_Length (EOL configurable number) characters of the device name per connected device. The default Device\_Name\_Characters\_Length value shall be equal to the maximum number of allowable characters to be displayed that is listed in the following requirements (refer to the Bluetooth Connectivity SPSS and Media Player SPSS documents):

1. BTC-FUR-REQ-194148-Device Friendly Name
2. MP-FUR-REQ-205797-USB Device Name
3. MP-FUR-REQ-205793-Unnamed USB Device.

The WifiHotspotServer shall attempt to detect all device names in ASCII encoding. If the WifiHotspotServer cannot detect a device name in ASCII characters it shall only store the MAC address of that device. All devices on the connected devices list shall be assigned an index number, starting from index 1 to index N (N = the number of connected devices).

If a device has previously connected to the hotspot and the password remains unchanged, the WifiHotspotServer shall allow the device to automatically connect to the hotspot when in range, assuming the number of connected devices is less than the maximum number allowed.

#### WFHS-REQ-191701/F-Displaying the connected devices list on the WifiHotspotOnBoardClient display

If the user enters into the Connected Devices screen (refer to WFHS-REQ-226336/A-HMI Specification References), the WifiHotspotOnBoardClient shall request for the list of connected devices using the CAN signal DeviceList\_Rq. The WifiHotspotOnBoardClient shall specify how it wants the list to be sent (i.e. entire list, one device at a time, etc.). Refer to WFHS-REQ-191654-Reporting the connected devices list for more information on how to request for the list. The WifiHotspotOnBoardClient shall specify the size of the list and the starting index in its request. The WifiHotspotServer shall respond with the CAN signal DeviceList\_Rsp. Each device shall be assigned an index number, and the WifiHotspotOnBoardClient shall display the list of devices in chronological order. If the WifiHotspotServer does not transmit its response quick enough the WifiHotspotOnBoardClient shall populate the information as it is received and display a popup indicating that it is updating. The user shall not be able to click on the list of devices until the screen has finished updating, at which point the popup shall exit.

The WifiHotspotOnBoardClient shall display the device name and MAC address of each connected device per line. If the device name field was not populated in the CAN signal, the WifiHotspotOnBoardClient shall only display the MAC address. The WifiHotspotOnBoardClient shall limit the number of device name characters that shall be displayed. The maximum device name characters length shall be equal to the maximum number of allowable characters to be displayed that is listed in the following requirements (refer to the Bluetooth Connectivity SPSS and Media Player SPSS documents):

1. BTC-FUR-REQ-194148-Device Friendly Name
2. MP-FUR-REQ-205797-USB Device Name
3. MP-FUR-REQ-205793-Unnamed USB Device.

The following is an example WifiHotspotOnBoardClient screen.




Figure. Screen displaying the list items of the connected devices list.

#### WFHS-REQ-191654/C-Reporting the connected devices list

The WifiHotspotOnBoardClient shall specify how it wants the Connected Devices list to be sent. It may request for the entire connected devices list or just a subset of the list using the CAN signal DeviceList\_Rq. The WifiHotspotServer shall respond with the desired list and include the MAC addresses and device names (up to Device\_Name\_Characters\_Length characters) of all the requested devices currently connected using the CAN signal DeviceList\_Rsp. The connected devices’ index numbers shall be referenced in the CAN signal as well. If the WifiHotspotServer cannot detect the device name of a specific device, the WifiHotspotServer shall not populate the device name field in the CAN signal.

Example 1)

* 10 devices are currently connected to the hotspot and the WifiHotspotOnBoardClient would like to request for the entire list.
* WifiHotspotOnBoardClient uses the DeviceList\_Rq CAN signal and sets the following:
  + ListType = ConnectedList
  + StartingIndex = Start Index 1
  + ListSize = List Size 31
* WifiHotspotServer responds with DeviceList\_Rsp and includes the following:
  + ListType = ConnectedList
  + ListSize = List Size 10
  + TotalNumberOfDevicesAvailable = 10 Devices Available
  + IndexNumber = Index 1
  + MAC = {MAC address of device 1}
  + DeviceName = {Device name of device 1}
  + IndexNumber = Index 2
  + MAC = {MAC address of device 2}
  + DeviceName = {Device name of device 2}
  + …
  + IndexNumber = Index 10
  + MAC = {MAC address of device 10}
  + DeviceName = {Device name of device 10}

Example 2)

* 10 devices are currently connected to the hotspot and the WifiHotspotOnBoardClient would like to request for the first 5 devices (i.e. only 5 devices can be displayed at once).
* WifiHotspotOnBoardClient uses the DeviceList\_Rq CAN signal and sets the following:
  + ListType = ConnectedList
  + StartingIndex = Start Index 1
  + ListSize = List Size 5
* WifiHotspotServer responds with DeviceList\_Rsp and includes the following:
  + ListType = ConnectedList
  + ListSize = List Size 5
  + TotalNumberOfDevicesAvailable = 10 Devices Available
  + IndexNumber = Index 1
  + MAC = {MAC address of device 1}
  + DeviceName = {Device name of device 1}
  + IndexNumber = Index 2
  + MAC = {MAC address of device 2}
  + DeviceName = {Device name of device 2}
  + …
  + IndexNumber = Index 5
  + MAC = {MAC address of device 5}
  + DeviceName = {Device name of device 5}

If the user continues to scroll on the Connected Devices screen, the WifiHotspotOnBoardClient may then wish to request for the next 5 devices, etc. by setting the StartingIndex = 6.

#### WFHS-REQ-191695/B-Setting the connected device update bit

If a device connects to or disconnects from the hotspot (except when initiated by the WifiHotspotServer from a Wi-Fi Hotspot reset (refer to WFHS-REQ-191863-Wi-Fi Hotspot reset settings) or from a request from the WifiHotspotOnBoardClient to block the device (RemoveDevice\_Rq)) the WifiHotspotServer shall set a connected device update bit using the CAN signal NewDeviceList\_St. This bit shall remain set until any of the following scenarios occur:

* 1. the WifiHotspotServer receives a request from the WifiHotspotOnBoardClient for the current list of connected devices through the CAN signal DeviceList\_Rq,
  2. The WifiHotspotServer transitions to low power registered mode (refer to WFHS-REQ-191904-Shutting down and powering up the Wi-Fi Chipset and WifiHotspotServer) or
  3. the WifiHotspotServer performs a Wi-Fi Hotspot reset (refer to WFHS-REQ-191863-Wi-Fi Hotspot reset settings)

at which point the WifiHotspotServer shall unset the bit.

#### WFHS-REQ-191702/D-Updating the connected devices screen while the user is in the screen

If the user is in the Connected Devices screen (refer to WFHS-REQ-226336/A-HMI Specification References) when the WifiHotspotServer indicates there is an update by setting the connected devices update bit (CAN signal NewDeviceList\_St), the WifiHotspotOnBoardClient shall transmit another request for the list of connected devices. Once the WifiHotspotOnBoardClient receives the updated list it shall update the screen to show the new information. If the WifiHotspotOnBoardClient is in the process of updating the Connected Devices screen, the WifiHotspotOnBoardClient shall display a popup indicating that it is updating. The user shall not be able to click on the list of devices until the screen has finished updating, at which point the popup shall exit. The WifiHotspotOnBoardClient shall disregard any updates from the WifiHotspotServer regarding the connected devices list if the user has left the Connected Devices screen.

If the user is NOT in the Connected Devices screen when the WifiHotspotServer indicates there is an update, the WifiHotspotOnBoardClient shall ignore the update bit and not perform any additional actions.

#### WFHS-REQ-191696/D-Managing the blocked devices list

The WifiHotspotServer shall manage a list called the Blocked List. This list shall store all the devices that have been blocked. A device may only be added to the blocked list by the user through the in-vehicle WifiHotspotOnBoardClient. If the user selects a device from the connected devices list and chooses to block it, the device shall be stored on the blocked list and unable to connect to the hotspot until it is deleted from the blocked list. The WifiHotspotServer shall limit the number of devices added to the hotspot’s blocked list. This number (Number\_Blocked\_Devices) shall be a configurable DID and defaulted to 20.

The WifiHotspotServer shall be responsible for saving the MAC addresses and device names (up to Device\_Name\_Characters\_Length characters, configurable) of all the devices currently stored on the blocked list. Each blocked device shall all be assigned an index number, starting from index 1 to index M (M = the number of blocked devices). The hotspot’s blocked list shall be managed in FIFO order. The newest blocked device shall be added to the top of the list and be assigned index 1. If the list becomes full and the WifiHotspotServer receives a request from WifiHotspotOnBoardClient to add a new device to the blocked list (CAN signal RemoveDevice\_Rq), the WifiHotspotServer shall delete the oldest blocked device (device on the bottom of the list with index M) to make room for the new blocked device and assign the newest blocked device index 1.

#### WFHS-REQ-191694/C-User requests to block a device from the hotspot through WifiHotspotOnBoardClient display

If the user selects a device from the Connected Devices list and chooses to block the device, the WifiHotspotOnBoardClient shall transmit a request (using CAN signal RemoveDevice\_Rq) to remove the device by specifying the index number of the device. The WifiHotspotServer shall respond with the updated connected devices list using CAN signal DeviceList\_Rsp. Refer to WFHS-REQ-226336/A-HMI Specification References. The following popup is an example WifiHotspotOnBoardClient popup.



Figure. Popup asking the user if they would like to block the selected device

#### WFHS-REQ-191697/A-Request from the WifiHostpotOnBoardClient to block a device from the Wi-Fi Hotspot

If the WifiHotspotServer receives a request from the WifiHotspotOnBoardClient to remove a device from the connected devices list by using the CAN signal RemoveDevice\_Rq and referencing the device by its index number, the WifiHotspotServer shall gracefully disconnect the connected device from the hotspot, add it onto the hotspot’s blocked list and report back the new list of connected devices (CAN signal DeviceList\_Rsp). In the case of an unsuccessful attempt, the WifiHotspotServer shall report back unsuccessful (CAN signal DeviceList\_Rsp). A device (for example device A) shall remain on the blocked list until:

* 1. a Wi-Fi Hotspot reset (see WFHS-REQ-191863-Wi-Fi Hotspot reset settings),
  2. the WifiHotspotServer receives a command from the WifiHotspotOnBoardClient to remove device A from the blocked list (CAN signal RemoveDevice\_Rq) or
  3. the blocked list becomes full when a request to block a device is received and device A is the oldest blocked device on the list.

#### WFHS-REQ-191703/E-Displaying the blocked devices list on the WifiHotspotOnBoardClient display

If the user enters into the Blocked Devices screen (refer to WFHS-REQ-226336/A-HMI Specification References), the WifiHotspotOnBoardClient shall request for the list of blocked devices using the CAN signal DeviceList\_Rq. The WifiHotspotOnBoardClient shall specify how it wants the list to be sent (i.e. entire list, one device at a time, etc.). Refer to WFHS-REQ-191698/A-Reporting the blocked devices list for more information on how to request for the list. The WifiHotspotOnBoardClient shall specify the size of the list and the starting index in its request. The WifiHotspotServer shall respond with the CAN signal DeviceList\_Rsp. Each device shall be assigned an index number, and the WifiHotspotOnBoardClient shall display the MAC address and device name of each device in the list. The list of devices shall be displayed in chronological order (Index 1, …, Index M (M = total number of blocked devices)).

If the device name field was not populated in the CAN signal the WifiHotspotOnBoardClient shall only display the MAC address. If the WifiHotspotServer does not transmit its response quick enough the WifiHotspotOnBoardClient shall populate the information as it is received and display a popup indicating that it is updating. The user shall not be able to click on the list of devices until the screen has finished updating, at which point the popup shall exit. The following screen is an example WifiHotspotOnBoardClient screen.




Figure. Screen displaying devices that the user has blocked

#### WFHS-REQ-191698/B-Reporting the blocked devices list

The WifiHotspotOnBoardClient shall specify how it wants the Blocked Devices list to be sent. It may request for the entire blocked devices list or just a subset of the list using the CAN signal DeviceList\_Rq. The WifiHotspotServer shall respond with the desired list and include the MAC addresses and device names (up to Device\_Name\_Characters\_Length characters) of all the requested devices currently blocked using the CAN signal DeviceList\_Rsp. The blocked devices’ index numbers shall be referenced in the CAN signal as well. If the WifiHotspotServer cannot detect the device name of a specific device, the WifiHotspotServer shall not populate the device name field in the CAN signal.

Example 1)

* 10 devices are currently blocked from the hotspot and the WifiHotspotOnBoardClient would like to request for the entire list.
* WifiHotspotOnBoardClient uses the DeviceList\_Rq CAN signal and sets the following:
  + ListType = BlockedList
  + StartingIndex = Start Index 1
  + ListSize = List Size 31
* WifiHotspotServer responds with DeviceList\_Rsp and includes the following:
  + ListType = BlockedList
  + ListSize = List Size 10
  + TotalNumberOfDevicesAvailable = 10 Devices Available
  + IndexNumber = Index 1
  + MAC = {MAC address of device 1}
  + DeviceName = {Device name of device 1}
  + IndexNumber = Index 2
  + MAC = {MAC address of device 2}
  + DeviceName = {Device name of device 2}
  + …
  + IndexNumber = Index 10
  + MAC = {MAC address of device 10}
  + DeviceName = {Device name of device 10}

Example 2)

* 10 devices are currently blocked from the hotspot and the WifiHotspotOnBoardClient would like to request for the first 5 devices (i.e. only 5 devices can be displayed at once).
* WifiHotspotOnBoardClient uses the DeviceList\_Rq CAN signal and sets the following:
  + ListType = BlockedList
  + StartingIndex = Start Index 1
  + ListSize = List Size 5
* WifiHotspotServer responds with DeviceList\_Rsp and includes the following:
  + ListType = BlockedList
  + ListSize = List Size 5
  + TotalNumberOfDevicesAvailable = 10 Devices Available
  + IndexNumber = Index 1
  + MAC = {MAC address of device 1}
  + DeviceName = {Device name of device 1}
  + IndexNumber = Index 2
  + MAC = {MAC address of device 2}
  + DeviceName = {Device name of device 2}
  + …
  + IndexNumber = Index 5
  + MAC = {MAC address of device 5}
  + DeviceName = {Device name of device 5}
* If the user continues to scroll on the Blocked Devices screen, the WifiHotspotOnBoardClient may then wish to request for the next 5 devices, etc. by setting the StartingIndex = 6.

#### WFHS-REQ-191704/D-User requests to unblock a device from the blocked list through WifiHotspotOnBoardClient display

If the user selects a device from the Blocked Devices list and chooses to unblock the device, the WifiHotspotOnBoardClient shall transmit a request (using CAN signal RemoveDevice\_Rq) to remove the device by specifying the list type (blocked list) and index number of the device. The WifiHotspotServer shall respond with the updated blocked devices list using the CAN signal DeviceList\_Rsp, at which point the WifiHotspotOnBoardClient shall update the screen. Refer to WFHS-REQ-226336/A-HMI Specification References. The following popup is an example WifiHotspotOnBoardClient popup.



Figure. Popup inquiring if the user would like to unblock a device

#### WFHS-REQ-191699/B-Request from the WifiHotspotOnBoardClient to remove a device from the blocked list

If the WifiHotspotServer receives a request from the WifiHotspotOnBoardClient to remove a device from the blocked list by using the CAN signal RemoveDevice\_Rq and referencing the device by its index number, the WifiHotspotServer shall delete that device from the blocked list and report back the new list of blocked devices (CAN signal DeviceList\_Rsp). If a device is removed from the blocked list, the device shall be required to enter the vehicle’s Wi-Fi Hotspot password before it can connect to the Wi-Fi Hotspot again.

### Use Cases

#### WFHSv1-UC-REQ-191955/A-Vehicle occupant blocks a device from the Wi-Fi Hotspot through the WifiHotspotOnBoardClient

|  |  |
| --- | --- |
| **Actors** | User  WifiHotspotOnBoardClient  WifiHotspotServer |
| **Pre-conditions** | Up to Number\_Hotspot\_Connected\_Devices devices connected to the Wi-Fi Hotspot  Up to (Number\_Blocked\_Devices – 1) devices placed on the Wi-Fi Hotspot’s blocked list |
| **Scenario Description** | Vehicle occupant selects a device from the list of connected devices and chooses to block the device |
| **Post-conditions** | The selected device disconnects from the Wi-Fi Hotspot  The selected device is listed under the blocked devices |
| **List of Exception Use Cases** | WFHSv1-UC-REQ-191931-E4 Wi-Fi Hotspot configuration through WifiHotspotOnBoardClient fails  WFHSv1-UC-REQ-191973-E11 WifiHotspotOnBoardClient update failed |
| **Interfaces** | WifiHotspotServer  WifiHotspotOnBoardClient  CAN |

#### WFHSv1-UC-REQ-191956/A-User blocks a device from the Wi-Fi Hotspot through the WifiHotspotOnBoardClient while the blocked list is full

|  |  |
| --- | --- |
| **Actors** | User  In-vehicle WifiHotspotOnBoardClient  WifiHotspotServer |
| **Pre-conditions** | Up to Number\_Hotspot\_Connected\_Devices devices connected to the Wi-Fi Hotspot  Number\_Blocked\_Devices devices are placed on the hotspot’s blocked list |
| **Scenario Description** | Vehicle occupant selects a device from the list of connected devices and chooses to block the device |
| **Post-conditions** | The oldest device that was placed on the blocked list is removed from the blocked list  The selected device disconnects from the hotspot  The selected device is listed under the blocked devices at the top of the list |
| **List of Exception Use Cases** | WFHSv1-UC-REQ-191931-E4 Wi-Fi Hotspot configuration through WifiHotspotOnBoardClient fails  WFHSv1-UC-REQ-191973-E11 WifiHotspotOnBoardClient update failed |
| **Interfaces** | WifiHotspotServer  WifiHotspotOnBoardClient  CAN |

#### WFHSv1-UC-REQ-191957/A-Vehicle occupant removes a device from the Wi-Fi Hotspot’s blocked list through the WifiHotspotOnBoardClient

|  |  |
| --- | --- |
| **Actors** | User  WifiHotspotOnBoardClient  WifiHotspotServer  Cell phone |
| **Pre-conditions** | WifiHotspotServer is on  Up to (Number\_Hotspot\_Connected\_Devices – 1) devices connected to the Wi-Fi Hotspot  Device(s) is/are listed in the blocked list menu |
| **Scenario Description** | Vehicle occupant selects a device from the list of blocked devices and chooses to remove the device from the list |
| **Post-conditions** | The device is deleted from the list  The device is able to connect to the hotspot if the user enters the Wi-Fi Hotspot password |
| **List of Exception Use Cases** | WFHSv1-UC-REQ-191931-E4 Wi-Fi Hotspot configuration through WifiHotspotOnBoardClient fails  WFHSv1-UC-REQ-191973-E11 WifiHotspotOnBoardClient update failed |
| **Interfaces** | WifiHotspotServer  WifiHotspotOnBoardClient  CAN |

#### WFHSv1-UC-REQ-191975/A-User connects a device

|  |  |
| --- | --- |
| **Actors** | Vehicle occupant  WifiHotspotServer  Wi-Fi device |
| **Pre-conditions** | Wi-Fi Hotspot is on  WifiHotspotServer has good cellular coverage  Less than Number\_Hotspot\_Connected\_Devices devices already connected to vehicle’s Wi-Fi Hotspot  Device A is within the 50 foot Wi-Fi range OR vehicle is traveling up to 70mph |
| **Scenario Description** | User enters vehicle’s SSID/password into device A |
| **Post-conditions** | Device A shows established connection  All connected devices may stream 35 Mbps not including overhead (or more or less depending on their applications) |
| **List of Exception Use Cases** |  |
| **Interfaces** | WifiHotspotServer  Wi-Fi device |

#### WFHSv1-UC-REQ-191979/A-User tries to connect a device that exceeds the allowable number of devices

|  |  |
| --- | --- |
| **Actors** | Vehicle occupant  WifiHotspotServer  User |
| **Pre-conditions** | Wi-Fi Hotspot is on  Number\_Hotspot\_Connected\_Devices devices already connected to vehicle’s Wi-Fi Hotspot |
| **Scenario Description** | User enters vehicle’s SSID/password into a Wi-Fi device |
| **Post-conditions** | Password is rejected |
| **List of Exception Use Cases** |  |
| **Interfaces** | WifiHotspotServer  Wi-Fi device |

#### WFHSv1-UC-REQ-191980/A-Returning device connects to hotspot

|  |  |
| --- | --- |
| **Actors** | WifiHotspotServer  Wi-Fi device |
| **Pre-conditions** | Hotspot is on  Wi-Fi visibility is set to on  Device A has connected to the vehicle’s hotspot before & user chose to have device always automatically connect to hotspot  SSID & password has not been changed since  Up to (Number\_Hotspot\_Connected\_Devices – 1) devices already connected |
| **Scenario Description** | Device A enters the vehicle’s Wi-Fi range |
| **Post-conditions** | Device A automatically connects to the vehicle’s Wi-Fi |
| **List of Exception Use Cases** |  |
| **Interfaces** | WifiHotspotServer  Wi-Fi device |

#### WFHSv1-UC-REQ-191981/A-SSID and/or password is changed

|  |  |
| --- | --- |
| **Actors** | WifiHotspotServer  Wi-Fi device |
| **Pre-conditions** | Hotspot is on  Wi-Fi visibility is set to on  Device A has connected to the vehicle’s hotspot before & user chose to have device always automatically connect to hotspot  SSID and/or password has been changed since |
| **Scenario Description** | Device A enters the vehicle’s Wi-Fi range |
| **Post-conditions** | Device A is unable to connect to the Wi-Fi Hotspot |
| **List of Exception Use Cases** |  |
| **Interfaces** | WifiHotspotServer  Wi-Fi device |

#### WFHSv1-UC-REQ-191982/B-Returning device configured to NOT automatically connect to hotspot

|  |  |
| --- | --- |
| **Actors** | WifiHotspotServer  Wi-Fi device |
| **Pre-conditions** | Hotspot is on  Device A has connected to the vehicle’s hotspot before & user chose to have device NOT automatically connect to hotspot |
| **Scenario Description** | Device A enters the vehicle’s Wi-Fi range |
| **Post-conditions** | Device A does not connect to the vehicle’s hotspot |
| **List of Exception Use Cases** |  |
| **Interfaces** | WifiHotspotServer  Wi-Fi device |

### White Box Views

#### Activity Diagrams

##### WFHSv1-ACT-REQ-167115/C-Connect A Device



##### WFHSv1-ACT-REQ-167123/A-User Disconnects Device From Hotspot through the Centerstack



##### WFHSv1-ACT-REQ-167124/B-User Disconnects Device From Hotspot through the Device



##### WFHSv1-ACT-REQ-167126/A-User Removes Device From Blocked List through Centerstack



#### Sequence Diagrams

##### WFHSv1-SD-REQ-167138/C-Connect A Device



##### WFHSv1-SD-REQ-167140/A-User Disconnects Device From Hotspot through the Centerstack



##### WFHSv1-SD-REQ-167141/B-User Disconnects Device From Hotspot through the Device



##### WFHSv1-SD-REQ-167142/A-User Removes Device From Blocked List through Centerstack



## WFHSv1-FUN-REQ-140754/F-Reporting Data Used

The WifiHotspotServer shall NOT transmit any requests to the WifiHotspotOffBoardClient if it is not authorized (see table below). If the WifiHotspotServer is authorized, the WifiHotspotServer may transmit data usage requests and refreshes to the WifiHotspotOffBoardClient.

|  |  |
| --- | --- |
| **WifiHotspotServer State** | **Authorization state** |
| Factory Mode | Not authorized |
| Unprovisioned | Not authorized |
| Waiting for provisioning Ack | Not authorized |
| Waiting for Home URL | Not authorized |
| Waiting for Auth | Not authorized |
| Authorized | Authorized |

The WifiHotspotOnBoardClient shall be capable of graphically displaying data usage information. The data usage information reflects the data used through the vehicle’s Wi-Fi Hotspot. This information MAY consist of the items listed below:

* 1. Plan type: session or shared
  2. Specify if the plan is unlimited or not
  3. Renewal or expiration date and time
  4. Specify whether the date is a renewal date or an expiration date
  5. Current amount of data used since the beginning of the billing cycle or the beginning of the package (in KB/MB/GB and in percentage). Note: this data amount shall reflect the total amount of data used on the plan, i.e. total amount of data used on a mobile share plan or total amount of data used through the vehicle if on an individual package.
  6. Total amount of data per billing cycle or total amount of data on the package
  7. Unit of measure for data used values (KB, MB or GB)
  8. Unit of measure for total data (KB, MB or GB)
  9. Overage flag
  10. User ID
  11. The current status of the hotspot:
      1. Free trial period waiting to be activated
      2. Free trial period is active
      3. No active subscription
      4. Subscription active

Not all the data usage information listed above may be displayed to the customer. The information displayed depends on the type of data package the vehicle is tied to. The carrier shall decide what values to transmit.

If the user enters into the Wi-Fi Hotspot menu, the WifiHotspotOnBoardClient shall transmit a request to the WifiHotspotServer to refresh the data usage information without sending a response back. Therefore, no data usage response shall be sent from the WifiHotspotServer back to the WifiHotspotOnBoardClient.

If the user enters into the Wi-Fi Hotspot Data Usage screen the WifiHotspotOnBoardClient shall transmit a request to the WifiHotspotServer for the current data, and in turn, the WifiHotspotServer shall respond with its stored data usage information.

If the user chooses to refresh the data usage information the WifiHotspotOnBoardClient shall transmit a data usage refresh request. If the WifiHotspotServer receives a data usage refresh request it shall respond with updating, successful and/or fail. If the update was successful the new data usage info shall also be transmitted to the WifiHotspotOnBoardClient.

### Requirements

#### WFHS-REQ-222037/A-Data usage feature flag

The WifiHotspotServer shall have a DID Data\_Usage\_Feature\_Enablement which shall have two states (On/Off) and shall be defaulted to On. This DID shall be updateable via EOL and OTA. This DID shall be used to determine whether the WifiHotspotServer shall allow data usage queries and notifications to be transmitted to and from the WifiHotspotOnBoardClient and WifiHotspotOffBoardClient.

* Data\_Usage\_Feature\_Enablement flag is set to On: If the Data\_Usage\_Feature\_Enablement flag is set to On, the WifiHotspotServer shall inform the WifiHotspotOnBoardClient by setting the CAN signal DataUsageFeature\_St=On. If the WifiHotspotServer receives data usage queries from the WifiHotspotOnBoardClient, it shall accept and transmit them to the WifiHotspotOffBoardClient, assuming there are no other conditions that prohibit WifiHotspotServer from doing so (i.e. WifiHotspotServer is not authorized). If the WifiHotspotServer receives data usage notifications from the WifiHotspotOffBoardClient, it shall accept them and inform the WifiHotspotOnBoardClient of these notifications (refer to section WFHSv1-FUN-REQ-140748-Carrier Data Notification), assuming there are no other conditions that prohibit WifiHotspotServer from doing so.
* Data\_Usage\_Feature\_Enablement flag is set to Off: If the Data\_Usage\_Feature\_Enablement flag is set to Off, the WifiHotspotServer shall inform the WifiHotspotOnBoardClient by setting the CAN signal DataUsageFeature\_St=Off. The WifiHotspotServer shall not have any data usage information stored if this flag is Off. If the WifiHotspotServer has data usage information stored when the DID is set from On to Off, the WifiHotspotServer shall clear the previously stored data usage information. If the WifiHotspotServer receives a data usage query from the WifiHotspotOnBoardClient, it shall ignore the query and NOT transmit any query to the WifiHotspotOffBoardClient. If the WifiHotspotServer receives a data usage notification from the WifiHotspotOffBoardClient, it shall ignore the notification and NOT inform the WifiHotspotOnBoardClient.

#### WFHS-REQ-222045/B-Hiding data usage screen based on data usage feature flag

The WifiHotspotOnBoardClient shall monitor the CAN signal DataUsageFeature\_St to determine if the Data Usage screens shall be enabled or disabled.

If the CAN signal DataUsageFeature\_St=On, the WifiHotspotOnBoardClient shall allow the user to navigate to the Data Usage screens (refer to WFHS-REQ-226336/A-HMI Specification References).

If the CAN signal DataUsageFeature\_St=Off or Null, the WifiHotspotOnBoardClient shall not present the user the option to access the Data Usage screens. Therefore, the Data Usage screens shall not be accessible or viewable by the user.

#### WFHS-REQ-191871/E-WifiHotspotOnBoardClient initiates data usage request due to user entering into Wi-Fi Hotspot menu

If the user enters into the Wi-Fi Hotspot main menu (refer to WFHS-REQ-226336/A-HMI Specification References) from outside the Wi-Fi Hotspot screens and the Wi-Fi Hotspot Data Usage Refresh Timeout timer is NOT ACTIVE (refer to WFHS-REQ-191874/D-User refreshes data usage screen), the WifiHotspotOnBoardClient shall transmit a request to the WifiHotspotServer to refresh the data usage information without sending a response back (CAN signal DataUsage\_Rq=RefreshDataNoResponse). Note: the request shall only be transmitted if the user enters into the Wi-Fi Hotspot main menu from outside the Wi-Fi Hotspot screens (i.e. If the user navigates to the Wi-Fi Hotspot menu screen from the WifiHotspotOnBoardClient home page, the WifiHotspotOnBoardClient shall transmit a request. If the user entered into the Wi-Fi Hotspot main menu screen and navigates to the Data Usage screen then back to the Wi-Fi Hotspot main menu screen, the WifiHotspotOnBoardClient shall not transmit a request).

If the user enters into the Wi-Fi Hotspot main menu from outside the Wi-Fi Hotspot screens and the Wi-Fi Hotspot Data Usage Refresh Timeout timer is ACTIVE, the WifiHotspotOnBoardClient shall NOT transmit any requests to the WifiHotspotServer to refresh the data usage information.

#### WFHS-REQ-191864/E-Request to refresh data usage info without a response required

If the WifiHotspotServer receives a request from the WifiHotspotOnBoardClient to refresh the data usage values without sending a response (CAN signal DataUsage\_Rq=RefreshDataNoResponse) while the WifiHotspotServer is authorized, the WifiHotspotServer shall transmit an FTCP request to the WifiHotspotOffBoardClient to REFRESH the data usage information (Note: if the WifiHotspotOffBoardClient receives a Refresh request from the WifiHotspotServer, the WifiHotspotOffBoardClient will transmit a data usage refresh request to the carrier). Once the WifiHotspotServer has initiated the data usage request it shall start a data usage timer (Data\_Usage\_Info\_Refresh\_Timeout). If the WifiHotspotServer receives an update from the WifiHotspotOffBoardClient before the timer expires, it shall overwrite the previous data usage information with the new information, store the new information, and clear the timer. If the timer expires before the WifiHotspotServer receives the data usage values, the WifiHotspotServer shall clear the timer and end the updating process. Since the request from the WifiHotspotOnBoardClient was “RefreshDataNoResponse”, the WifiHotspotSever shall NOT transmit a data usage response CAN signal to the WifiHotspotOnBoardClient. If a data usage response is received from the WifiHotspotOffBoardClient AFTER the timer expires, the WifiHotspotServer shall discard the response.

Example 1: WifiHotspotServer transmits data usage request A to WifiHotspotOffBoardClient and starts a timer. Timer expires. Data usage response A is received some time later. WifiHotspotServer shall discard the response.

Example 2: WifiHotspotServer transmits data usage request A to WifiHotspotOffBoardClient and starts a timer. Timer expires without receiving data usage response A. WifiHotspotServer initiates data usage request B and starts a timer. During this window data usage response A is received. WifiHotspotServer shall discard response A and continue waiting for data usage response B.

The data usage timer (Data\_Usage\_Info\_Refresh\_Timeout) shall be configurable via EOL or OTA with a default value of 15 seconds for NA vehicles, a default of 15 seconds for China vehicles and a default value of 15 seconds for European vehicles. Refer to WFHS-REQ-191639-WifiHotspotServer identifies the vehicle region for more information on determining vehicle region.

If the WifiHotspotServer receives a request to refresh the data usage values without sending a response (CAN signal DataUsage\_Rq=RefreshDataNoResponse) while it is not authorized, the WifiHotspotServer shall ignore the request and not transmit any request to the WifiHotspotOffBoardClient.

#### WFHS-REQ-191872/L-Displaying data usage information

If the user requests to enter into the Wi-Fi Hotspot Data Usage screen and the Wi-Fi Hotspot Data Usage Refresh Timeout timer is NOT ACTIVE (refer to WFHS-REQ-191874-User refreshes data usage screen), the WifiHotspotOnBoardClient shall request for the current data usage information from the WifiHotspotServer (CAN signal DataUsage\_Rq=CurrentData) before populating the screen. The WifiHotspotServer shall report back the data usage information through the CAN signal DataUsage\_Rsp, and the WifiHotspotOnBoardClient shall display the appropriate information and screen (refer to WFHS-REQ-226336/A-HMI Specification References). If the user requests to refresh the screen, the WifiHotspotOnBoardClient shall transition to the appropriate screen upon receiving the update from the WifiHotspotServer.

If the user enters into the Wi-Fi Hotspot Data Usage screen and the Wi-Fi Hotspot Data Usage Refresh Timeout timer is ACTIVE, the WifiHotspotOnBoardClient shall NOT transmit a request for the current data. Instead, the WifiHotspotOnBoardClient shall display the previously stored data usage values, if any. The Refresh button shall be disabled while the timer is active.

The WifiHotspotOnBoardClient shall determine which region specific data usage screens to display (refer to WFHS-REQ-191641-WifiHotspotOnBoardClient identifies vehicle region). The WifiHotspotOnBoardClient shall also determine which Data Usage screen to display based on the information within the DataUsage\_Rsp message. Refer to the table below for a mapping of the data usage screens to data usage response (only applicable for H31\_SYNC\_GEN3\_Wi-Fi\_Settings specification). Refer to WFHS-REQ-226336/A-HMI Specification References for other HMI specification references.

|  |  |  |
| --- | --- | --- |
| **Data usage response FTCP message** | **CAN signal DataUsage\_Rsp** | **H31i\_SYNC\_GEN3\_Wi-Fi\_Settings Data Usage screens** |
| No data usage information stored in WifiHotspotServer | Invalid | Data usage error screen |
|
|
| Data plan type: trial; Data plan status: pending | Data plan status: Free trial period waiting | Trial eligible screen |
| Data plan type: trial; Data plan status: active | Data plan status: Free trial period active | Trial active screen |
| Data plan type: trial or paid-session or paid-shared or paid-session-unlimited or paid-shared-unlimited; Data plan status: expired | Data plan status: No subscription active | No active data plan screen |
| Data plan type: trial or paid-session or paid-shared or paid-session-unlimited or paid-shared-unlimited; Data plan status: inactive |
| Data plan type: paid-session or paid-shared; Data plan status: active | Data plan status: Active subscription | Screen may vary depending on the data usage percentage field |
|
| Data plan type: paid-session-unlimited or paid-shared-unlimited; Data plan status: active | Data plan status: Active subscription; Total data: unlimited | Unlimited data usage screen |
| Data plan type: paid-shared; Data plan status: active; Overage flag: yes | Overage flag: yes | Data overage screen |

Table. Data usage/Manage account screen displayed depending on data plan status

The WifiHotspotOnBoardClient shall also determine the vehicle brand in order to determine what specific text to populate within the manage account screens (refer to WFHS-REQ-191640-WifiHotspotOnBoardClient identifies vehicle brand). The vehicle brand shall also be used to determine which app the vehicle is compatible with.

If the vehicle is a Ford vehicle, the vehicle is compatible with the Ford app. If the vehicle is a Lincoln, the vehicle is compatible with the Lincoln app. All Wi-Fi Hotspot popups and screens that reference a mobile app shall refer the customer to one of these apps based on vehicle brand. Refer to the HMI specifications for the final mobile app names.

The screen below is an example WifiHotspotOnBoardClient screen.




Figure. NA, Lincoln screen listing the corresponding app

The WifiHotspotOnBoardClient shall monitor the CAN signal TelematicsService\_St to determine if the WifiHotspotServer is authorized (TelematicsService\_St=Active, ExpiringSoon).

If the CAN signal TelematicsService\_St indicates the WifiHotspotServer is NOT authorized (TelematicsService\_St=Expired, NotifyExpired, NotActivatedYet, NotifyNotActivatedYet), the WifiHotspotOnBoardClient shall NOT allow the user to refresh the data usage screen.

If the WifiHotspotOnBoardClient receives all invalid values in the DataUsage\_Rsp CAN signal, but the CAN signal TelematicsService\_St indicates the WifiHotspotServer is authorized, the WifiHotspotOnBoardClient shall still allow the user to refresh the data usage screen.

The wireless carriers currently do not display the expiration/renewal **time** (hh:mm:ss), but have indicated that this may change in the future. To stay consistent, the WifiHotspotOnBoardClient shall display the expiration/renewal date, but shall NOT display the expiration/renewal time. The time shall, however, be included in the CAN signal DataUsage\_Rsp in order to protect for changes in the future. If the carriers decide to display time as well, this requirement shall be updated to allow the time to be displayed.

#### WFHSv2-REQ-206087/D-Displaying data usage information

If the user requests to enter into the Wi-Fi Hotspot Data Usage screen and the Wi-Fi Hotspot Data Usage Refresh Timeout timer is NOT ACTIVE (refer to WFHS-REQ-191874/D-User refreshes data usage screen), the WifiHotspotOnBoardClient shall request for the current data usage information from the WifiHotspotServer (CAN signal DataUsage\_Rq=CurrentData) before populating the screen. The WifiHotspotServer shall report back the data usage information through the CAN signal DataUsage\_Rsp, and the WifiHotspotOnBoardClient shall display the appropriate information and screen (refer to WFHS-REQ-226336/A-HMI Specification References). If the user requests to refresh the screen, the WifiHotspotOnBoardClient shall transition to the appropriate screen upon receiving the update from the WifiHotspotServer.

If the user enters into the Wi-Fi Hotspot Data Usage screen and the Wi-Fi Hotspot Data Usage Refresh Timeout timer is ACTIVE, the WifiHotspotOnBoardClient shall NOT transmit a request for the current data. Instead, the WifiHotspotOnBoardClient shall display the previously stored data usage values, if any. The Refresh button shall be disabled while the timer is active.

The WifiHotspotOnBoardClient shall determine which region specific data usage screens to display (refer to WFHS-REQ-191641-WifiHotspotOnBoardClient identifies vehicle region). The WifiHotspotOnBoardClient shall also determine which Data Usage screen to display based on the information within the DataUsage\_Rsp message.

The WifiHotspotOnBoardClient shall also determine the vehicle brand in order to determine what specific text to populate within the manage account screens (refer to WFHS-REQ-191640-WifiHotspotOnBoardClient identifies vehicle brand). The vehicle brand shall also be used to determine which app the vehicle is compatible with.

If the vehicle is a Ford vehicle, the vehicle is compatible with the Ford app. If the vehicle is a Lincoln, the vehicle is compatible with the Lincoln app. All Wi-Fi Hotspot popups and screens that reference a mobile app shall refer the customer to either of these apps based on the vehicle brand. Refer to the HMI specification for the final mobile app names.

The screen below is an example WifiHotspotOnBoardClient screen.




Figure. NA, Lincoln screen listing the corresponding app

The WifiHotspotOnBoardClient shall monitor the CAN signal TelematicsService\_St to determine if the WifiHotspotServer is authorized (TelematicsService\_St=Active, ExpiringSoon).

If the CAN signal TelematicsService\_St indicates the WifiHotspotServer is NOT authorized (TelematicsService\_St=Expired, NotifyExpired, NotActivatedYet, NotifyNotActivatedYet), the WifiHotspotOnBoardClient shall NOT allow the user to refresh the data usage screen.

If the WifiHotspotOnBoardClient receives all invalid values in the DataUsage\_Rsp CAN signal, but the CAN signal TelematicsService\_St indicates the WifiHotspotServer is authorized, the WifiHotspotOnBoardClient shall still allow the user to refresh the data usage screen.

The wireless carriers currently do not display the expiration/renewal **time** (hh:mm:ss), but have indicated that this may change in the future. To stay consistent, the WifiHotspotOnBoardClient shall display the expiration/renewal date, but shall NOT display the expiration/renewal time. The time shall, however, be included in the CAN signal DataUsage\_Rsp in order to protect for changes in the future. If the carriers decide to display time as well, this requirement shall be updated to allow the time to be displayed.

#### WFHS-REQ-197429/D-Displaying elapsed time since a data usage update

The WifiHotspotOnBoardClient shall display a time in the Wi-Fi Hotspot Data Usage screens that represents the amount of time that has elapsed since the WifiHotspotServer last received any data usage information (refer to WFHS-REQ-226336/A-HMI Specification References).

If the WifiHotspotOnBoardClient receives a data usage response from the WifiHotspotServer that includes a value for the data usage counter, the WifiHotspotOnBoardClient shall follow the rules below to determine how the elapsed time shall be displayed:

|  |  |
| --- | --- |
| **Counter Value (from DataUsage\_Rsp)** | **Display Text** |
| 00:00:00 ≤ counter value < 00:01:00 | Status as of: Now |
| 00:01:00 ≤ counter value < 00:02:00 | Status as of: 1 minute ago |
| 00:02:00 ≤ counter value < 01:00:00 | Status as of: xx minutes ago (xx = minute value) |
| 01:00:00 ≤ counter value < 02:00:00 | Status as of: 1 hour ago |
| 02:00:00 ≤ counter value ≤ 72:00:00 | Status as of: yy hours ago (yy = hour value) |

The following screens are example WifiHotspotOnBoardClient screens.



Figure. Screen displaying data usage information that was updated between 35 to 36 minutes ago



Figure. Screen displaying data usage information that was updated between 2 to 3 hours ago

#### WFHS-REQ-191873/E-Rounding data usage values

The WifiHotspotOnBoardClient shall receive the amount of data used and the total amount of data on the plan, along with the unit of measure for each (either KB, MB or GB).

The WifiHotspotOnBoardClient shall receive the data used value and total data value with two decimal places. If both decimal places hold zeros, the WifiHotspotOnBoardClient shall drop the zeros.

Example)

* Data used = 1.25, WifiHotspotOnBoardClient shall display “1.25”
* Data used = 1.00, WifiHotspotOnBoardClient shall display “1”

Refer to WFHS-REQ-226336/A-HMI Specification References.

#### WFHS-REQ-191866/B-Request from WifiHotspotOnBoardClient for the WifiHotspotServer's stored data usage information

If the WifiHotspotServer receives a request from the WifiHotspotOnBoardClient for the current data usage information (CAN signal DataUsage\_Rq=CurrentData) the WifiHotspotServer shall respond with its stored data usage information using the CAN signal DataUsage\_Rsp. If the WifiHotspotServer does not have any stored data usage information at the time of the request, the WifiHotspotServer shall transmit Invalid values in the response (CAN signal DataUsage\_Rsp).

#### WFHS-REQ-191867/B-Request from WifiHotspotOnBoardClient for data usage while WifiHotspotServer is updating the data usage information

If the WifiHotspotServer has requested for the data usage information from the WifiHotspotOffBoardClient and is currently waiting for a response when it receives a request from WifiHotspotOnBoardClient for the CURRENT data usage information (CAN signal DataUsage\_Rq=CurrentData), the WifiHotspotServer shall transmit the previously stored data usage information to the WifiHotspotOnBoardClient using the CAN signal DataUsage\_Rsp and continue the updating process. If the WifiHotspotServer does not have any data usage information stored at the time of the request, the WifiHotspotServer shall respond with Invalid values.

#### WFHS-REQ-191874/F-User refreshes data usage screen

If the user requests to refresh the data usage information the WifiHotspotOnBoardClient shall transmit this refresh request to the WifiHotspotServer using the CAN signal DataUsage\_Rq=RefreshData. The WifiHotspotServer may respond with “wait”, “failure” or the data usage values and “success” (CAN signal DataUsage\_Rsp). The WifiHotspotOnBoardClient shall also start a timer (Wi-Fi Hotspot Data Usage Refresh Timeout timer; configurable and defaulted to 30 seconds) once it receives a request from the user to refresh the data usage information. The timer shall remain active until one of the following triggers occur:

1. The WifiHotspotServer sends a successful response using the CAN signal DataUsage\_Rsp.

2. The WifiHotspotServer sends a failure response using the CAN signal DataUsage\_Rsp.

3. The Wi-Fi Hotspot Data Usage Refresh Timeout timer expires.

If the WifiHotspotOnBoardClient’s Wi-Fi Hotspot Data Usage Refresh Timeout timer is active while the user is in the Data Usage screen, the WifiHotspotOnBoardClient shall display an updating message to the user and the refresh button shall be disabled. If a successful message is received, the WifiHotspotOnBoardClient shall refresh the screen with the new data usage values. If a failure response is received while the user is still in the Data Usage screen, the screen shall inform the user of the failure and remain displaying the old data usage information. If the Wi-Fi Hotspot Data Usage Refresh Timeout timer expires while the user is still in the Data Usage screen, the screen shall inform the user of the failure and remain displaying the old data usage information. If the timer expires or a failure message is received while the user is NOT in the Data Usage screen, the user shall not be informed of the failure.

#### WFHS-REQ-191868/G-Request from WifiHotspotOnBoardClient to refresh the data usage values

The WifiHotspotServer shall check its authorization state and indicate whether it is authorized or not authorized in the CAN signal TelematicsService\_St by referring to the table below.

|  |  |
| --- | --- |
| **WifiHotspotServer State** | **Indication within DataUsage\_Rsp** |
| Factory Mode | Not authorized |
| Unprovisioned | Not authorized |
| Waiting for provisioning Ack | Not authorized |
| Waiting for Home URL | Not authorized |
| Waiting for Auth | Not authorized |
| Authorized | Authorized |

If the WifiHotspotServer receives a request from the WifiHotspotOnBoardClient to Refresh the data usage information (CAN signal DataUsage\_Rq=RefreshData) and the WifiHotspotServer is authorized, the WifiHotspotServer shall send an FTCP Refresh request to the WifiHotspotOffBoardClient for data usage information. The WifiHotspotServer shall also start a timer (Data\_Usage\_Info\_Refresh\_Timeout configurable with a default value of 15 seconds for NA vehicles, a default of 15 seconds for China vehicles and a default value of 15 seconds for European vehicles, refer to WFHS-REQ-191639-WifiHotspotServer identifies the vehicle region for more information on determining vehicle region) once it receives this request from the WifiHotspotOnBoardClient. Because the request from the WifiHotspotOnBoardClient was a Refresh request, the WifiHotspotServer shall transmit a “wait” response to the WifiHotspotOnBoardClient using the CAN signal DataUsage\_Rsp while it is finishing the updating process. Note: if the WifiHotspotOffBoardClient receives a Refresh request from the WifiHotspotServer, the WifiHotspotOffBoardClient will transmit a data usage refresh request to the carrier.

If the WifiHotspotServer receives the data usage information response from the WifiHotspotOffBoardClient before the timer expires, the WifiHotspotServer shall save and send over the data usage information to the WifiHotspotOnBoardClient (CAN signal DataUsage\_Rsp).

If the timer expires before the WifiHotspotServer receives a response from the WifiHotspotOffBoardClient the WifiHotspotServer shall send a failure message (CAN signal DataUsage\_Rsp) and end the data usage updating process. If a data usage response is received from the WifiHotspotOffBoardClient AFTER the timer expires, the WifiHotspotServer shall discard the response.

Example 1: WifiHotspotServer transmits data usage request A to WifiHotspotOffBoardClient and starts a timer. Timer expires. Data usage response A is received some time later. WifiHotspotServer shall discard the response.

Example 2: WifiHotspotServer transmits data usage request A to WifiHotspotOffBoardClient and starts a timer. Timer expires without receiving data usage response A. WifiHotspotServer initiates data usage request B and starts a timer. During this window data usage response A is received. WifiHotspotServer shall discard response A and continue waiting for data usage response B.

If the WifiHotspotServer does not have a connection established with the WifiHotspotOffBoardClient at the time it receives a request from the WifiHotspotOnBoardClient to update the data usage information (CAN signal DataUsage\_Rq=RefreshData), the WifiHotspotServer shall immediately respond with a failure message (CAN signal DataUsage\_Rsp) and end the updating process.

If the WifiHotspotServer receives a request to Refresh the data usage information (CAN signal DataUsage\_Rq=RefreshData) and the WifiHotspotServer is NOT authorized, the WifiHotspotServer shall ignore the request and NOT transmit a request to the WifiHotspotOffBoardClient. The WifiHotspotServer shall instead respond with “Failure” using the CAN signal DataUsage\_Rsp (note: all data usage information shall be invalid if WifiHotspotServer is unauthorized).

The WifiHotspotServer shall not expect all fields within the data usage FTCP message to be populated. Therefore, the WifiHotspotServer shall not reject a message if some data usage fields are missing. Fields may be missing because the active plan does not support a specific field, there is no active plan so all other fields do not apply, etc. For example, if the FTCP message indicates a Paid Session Plan is Inactive, then data used, % used, etc. would not apply and would therefore not be populated.

If the WifiHotspotServer is required to transmit a data usage response to the WifiHotspotOnBoardClient due to a request for its stored data usage information or due to a refresh request, the WifiHotspotServer shall populate the data plan status field in the CAN signal DataUsage\_Rsp based on the mapping defined in the table below. All other fields within the DataUsage\_Rsp CAN signal shall be populated based on the information stored in the WifiHotspotServer that was received by a data usage FTCP response or a carrier data notification. If the WifiHotspotServer does not have any data usage information stored, it shall set all fields in the DataUsage\_Rsp CAN signal as invalid. If the overage flag is set to Yes, the WifiHotspotServer shall set the data used percent value to Invalid. If the WifiHotspotServer does not have a complete set of data usage information to report in the DataUsage\_Rsp TP message, it shall set the missing data to Invalid in the TP response message.

Example: The WifiHotspotServer receives an FTCP data usage message that contains the following:

• Data plan type = Trial

• Data plan status = Pending

• No other fields are populated.

The WifiHotspotServer shall:

• Populate the counter fields in the TP message.

• Populate DataPlanStatus to "Free trial period waiting".

• All other fields within the TP message shall be set to “Invalid”.

|  |  |  |  |
| --- | --- | --- | --- |
| **Data usage response/carrier data notification FTCP message: data plan type field** | **Data usage responsecarrier data notification FTCP message: data plan status field** | **CAN signal DataUsage\_Rsp; data plan status field** |  |
| No data usage information stored in WifiHotspotServer | No data usage information stored in WifiHotspotServer | Invalid |  |
| trial | pending | Free trial period waiting |  |
| trial | active | Free trial period active |  |
| trial or paid-session or paid-shared or paid-session-unlimited or paid-shared-unlimited | expired | No subscription active |  |
| trial or paid-session or paid-shared or paid-session-unlimited or paid-shared-unlimited | inactive |  |
| paid-session or paid-shared | active | Active subscription |  |
|  |
| paid-session-unlimited or paid-shared-unlimited | active | Active subscription (total data field shall be set to unlimited) |  |

#### WFHS-REQ-191869/C-Request from WifiHotspotOnBoardClient for a data usage refresh while WifiHotspotServer is updating the data usage information

If the WifiHotspotServer is in the process of updating its data usage values (due to user entering into the Wi-Fi Hotspot main menu, refer to WFHS-REQ-191864-Request to refresh data usage info without a response required) when it receives a Refresh data usage command from the WifiHotspotOnBoardClient (CAN signal DataUsage\_Rq=RefreshData), the WifiHotspotServer shall respond with a “wait” status in the CAN signal DataUsage\_Rsp and continue the updating process. The WifiHotspotServer shall not initiate a new data usage request to the WifiHotspotOffBoardClient. If the WifiHotspotServer receives the data usage FTCP response, it shall send this information along with a success response to the WifiHotspotOnBoardClient. If the Data\_Usage\_Info\_Refresh\_Timeout (refer to WFHS-REQ-191864-Request to refresh data usage info without a response required) expires before the WifiHotspotServer received a data usage update, the WifiHotspotServer shall transmit a fail response to the WifiHotspotOnBoardClient.

#### WFHS-REQ-191865/A-Receiving a full data usage response

The WifiHotspotServer Wi-Fi application shall manage the data usage plan information for the Wi-Fi Hotspot received from the WifiHotspotOffBoardClient through a FTCP Ford cloud message exchange. The Wi-Fi subsystem shall manage two buffers. The active data usage buffer that contains the most recent copy last received from the WifiHotspotOffBoardClient and another buffer that is dedicated to receive the data plan usage information updates in real time via FTCP exchange. The active data usage buffer shall only be updated by the FTCP received data when integrity of the data is confirmed by the WifiHotspotServer FTCP component. Otherwise the received data shall be ignored and the active data buffer shall retain its content.

#### WFHS-REQ-199543/B-Monitoring elapsed time since the data usage update

If the WifiHotspotServer receives a carrier data notification (refer to WFHSv1-FUN-REQ-140748-Carrier Data Notification) or data usage response FTCP message, the WifiHotspotServer shall note the time of when the message was received and start a counter. The WifiHotspotServer shall monitor this data usage counter to determine how long ago (in hour, minutes and seconds) the data usage message was received. If the WifiHotspotServer is required to transmit the data usage information (using CAN signal DataUsage\_Rsp) due to a refresh request or a current data request from the WifiHotspotOnBoardClient, the WifiHotspotServer shall include the value of the data usage counter in its response.

Example) The user enters into the Wi-Fi Hotspot main menu and the WifiHotspotOnBoardClient transmits a request to the WifiHotspotServer to refresh the data usage information without sending a response back. The WifiHotspotServer transmits this request to the WifiHotspotOffBoardClient at 4:53:52 PM and receives a data usage response at 4:54:00 PM. The user stays within the Wi-Fi menu and eventually navigates to the Wi-Fi Hotspot Data Usage screen. The WifiHotspotOnBoardClient shall transmit a request to the WifiHotspotServer for the current data. The WifiHotspotServer receives this request at 5:00:00 PM. The WifiHotspotServer shall then transmit the data usage response (CAN signal DataUsage\_Rsp). The response shall include all the data usage information and shall also include the data usage counter value, which shall indicate the elapsed time since the data usage information was received. The value of the counter shall be 00:06:00. The user may then see “Status as of: 6 minutes ago”.

If the WifiHotspotServer has an active data usage counter when it receives a new data usage message from the WifiHotspotOffBoardClient, the WifiHotspotServer shall restart the counter. The counter shall only be counting the time from the last received data usage message. If the WifiHotspotServer clears the data usage information (refer to WFHS-REQ-199544-Clearing data usage information), the WifiHotspotServer shall also reset the data usage counter. The counter shall only be active when the WifiHotspotServer has data usage information stored.

The WifiHotspotServer shall store the time (hh:mm:ss) it received a data usage response or notification message from the WifiHotspotOffBoardClient in the DID Data\_Usage\_Reception\_Time (refer to WFHS-REQ-226337-Diagnostic Specification Reference). The DID shall only reflect the time of the LAST received message. If the WifiHotspotServer does not have any data usage information stored, no time shall be reflected in the DID.

#### WFHS-REQ-199544/A-Clearing data usage information

The WifiHotspotServer shall clear any stored data usage information once the ignition transitions to off, the WifiHotspotServer goes into low powered registered (LPR) mode (refer to the WifiHotspotServer Power Management Requirements specification) or the data usage counter reaches 72 hours.

If the WifiHotspotServer has data usage information (received from a data usage response FTCP message or from a carrier data notification FTCP message) stored in memory, the WifiHotspotServer shall:

* monitor the ignition status (IgnitionStatus\_St).
  + IgnitionStatus\_St≠Off: If the ignition status transitions to off from any other state, the WifiHotspotServer shall clear all stored data usage information and clear the data usage counter.
  + IgnitionStatus\_St=Off: If the WifiHotspotServer begins to transition to LPR mode, the WifiHotspotServer shall first clear all stored data usage information and clear the data usage counter.
* monitor the data usage counter (refer to WFHS-REQ-199543-Monitoring elapsed time since the data usage update).
  + If the data usage counter value < 72 hours, the WifiHotspotServer shall continue monitoring the counter and keep all data usage information stored.
  + If the data usage counter value = 72 hours, the WifiHotspotServer shall clear all data usage information from memory and clear the data usage counter.

The WifiHotspotServer shall clear the data usage information and counter as soon as any of the events stated above occurs.

If the WifiHotspotServer does not have any data usage information stored, the data usage counter shall not be active.

### Use Cases

#### WFHSv1-UC-REQ-191945/E-User accesses the data usage screen in a good network coverage area

|  |  |
| --- | --- |
| **Actors** | User  System |
| **Pre-conditions** | WifiHotspotServer is On  WifiHotspotServer has a good connection to the network  WifiHotspotServer is authorized |
| **Scenario Description** | User enters the Wi-Fi Hotspot screen that displays the data usage |
| **Post-conditions** | The data usage information shows it was last updated at either the time:   1. The user last refreshed it from WifiHotspotOnBoardClient during the current ignition cycle 2. The user entered into the Wi-Fi Hotspot main menu screen from outside the Wi-Fi Hotspot screens during the current ignition cycle or 3. A low balance notification was displayed in the vehicle during the current ignition cycle. |
| **List of Exception Use Cases** | WFHSv1-UC-REQ-191931-E4 Wi-Fi Hotspot configuration through WifiHotspotOnBoardClient fails |
| **Interfaces** | Ford infrastructure  Carrier infrastructure  WifiHotspotServer  WifiHotspotOnBoardClient  CAN |

#### WFHSv1-UC-REQ-191946/E-User accesses the data usage screen in a no network coverage area

|  |  |
| --- | --- |
| **Actors** | User  System |
| **Pre-conditions** | WifiHotspotServer is On  WifiHotspotServer has no connection to the network  WifiHotspotServer is authorized |
| **Scenario Description** | User enters the Wi-Fi Hotspot main menu from outside the Wi-Fi Hotspot screens and then into the Data usage screen |
| **Post-conditions** | The data usage information cannot be displayed or old data usage information is displayed |
| **List of Exception Use Cases** | WFHSv1-UC-REQ-191973-E11 WifiHotspotOnBoardClient update failed |
| **Interfaces** | Ford infrastructure  Carrier infrastructure  WifiHotspotServer  In-vehicle WifiHotspotOnBoardClient  CAN |

#### WFHSv1-UC-REQ-191947/C-User enters into the Wi-Fi Hotspot menu and refreshes the data usage screen immediately

|  |  |
| --- | --- |
| **Actors** | User  System |
| **Pre-conditions** | WifiHotspotServer is On  WifiHotspotServer has a connection to the network  WifiHotspotServer initiates its data usage update  WifiHotspotServer is authorized |
| **Scenario Description** | User enters the Wi-Fi Hotspot screen that displays the data usage and refreshes the data usage values before the WifiHotspotServer has completed its data usage update |
| **Post-conditions** | The WifiHotspotOnBoardClient shows an updating popup  When the data usage values are received the WifiHotspotOnBoardClient screen shall update |
| **List of Exception Use Cases** | WFHSv1-UC-REQ-191931-E4 Wi-Fi Hotspot configuration through WifiHotspotOnBoardClient fails  WFHSv1-UC-REQ-191973-E11 WifiHotspotOnBoardClient update failed |
| **Interfaces** | Ford infrastructure  Carrier infrastructure  WifiHotspotServer  WifiHotspotOnBoardClient  CAN |

#### WFHSv1-UC-REQ-191948/D-User refreshes the data usage values from the WifiHotspotOnBoardClient

|  |  |
| --- | --- |
| **Actors** | User  System |
| **Pre-conditions** | WifiHotspotOnBoardClient is available  WifiHotspotServer has a good connection to the network  WifiHotspotServer is authorized |
| **Scenario Description** | User is in the Wi-Fi Hotspot screen that displays the data usage and presses the refresh button |
| **Post-conditions** | The screen informs the user of an update in progress and the refresh button is disabled.  Data usage information is updated once the data is refreshed. |
| **List of Exception Use Cases** | WFHSv1-UC-REQ-191931-E4 Wi-Fi Hotspot configuration through WifiHotspotOnBoardClient fails  WFHSv1-UC-REQ-191973-E11 WifiHotspotOnBoardClient update failed |
| **Interfaces** | Ford infrastructure  Carrier infrastructure  WifiHotspotServer  WifiHotspotOnBoardClient  CAN |

#### WFHSv1-UC-REQ-191949/D-User refreshes data usage values from WifiHotspotOnBoardClient when vehicle is in a no coverage area

|  |  |
| --- | --- |
| **Actors** | User  WifiHotspotOnBoardClient  WifiHotspotServer |
| **Pre-conditions** | WifiHotspotServer is On  Vehicle in a no coverage area  WifiHotspotServer is authorized |
| **Scenario Description** | User enters the Wi-Fi Hotspot screen that displays the data usage and presses the refresh button |
| **Post-conditions** | A popup shall be displayed to the customer notifying them there are issues connecting to the network  After the popup is closed, the screen shall show all the same values as it did prior to the refresh request. |
| **List of Exception Use Cases** | WFHSv1-UC-REQ-191931-E4 Wi-Fi Hotspot configuration through WifiHotspotOnBoardClient fails  WFHSv1-UC-REQ-191973-E11 WifiHotspotOnBoardClient update failed |
| **Interfaces** | WifiHotspotServer  WifiHotspotOnBoardClient  CAN |

#### WFHSv1-UC-REQ-191950/C-User refreshes data usage values from WifiHotspotOnBoardClient when vehicle is in a poor coverage area

|  |  |
| --- | --- |
| **Actors** | User  In-vehicle WifiHotspotOnBoardClient  WifiHotspotServer |
| **Pre-conditions** | WifiHotspotServer is On  Vehicle is in a poor coverage area  WifiHotspotServer is authorized |
| **Scenario Description** | User enters the Wi-Fi Hotspot screen that displays the data usage and presses the refresh button |
| **Post-conditions** | The screen shall inform the user of an update in progress.  The refresh button shall not be accessible.  A popup shall appear notifying the user there were issues connecting to the network  Popup closes and old data usage information is displayed |
| **List of Exception Use Cases** | WFHSv1-UC-REQ-191931-E4 Wi-Fi Hotspot configuration through WifiHotspotOnBoardClient fails |
| **Interfaces** | WifiHotspotServer  WifiHotspotOnBoardClient  CAN  WifiHotspotOffBoardClient  Carrier backend |

#### WFHSv1-UC-REQ-191951/C-User refreshes the data usage values on the mobile app in a good coverage area

|  |  |
| --- | --- |
| **Actors** | User  Mobile App |
| **Pre-conditions** | Mobile app has good cellular coverage  WifiHotspotServer is authorized |
| **Scenario Description** | User refreshes the data usage values from the mobile app |
| **Post-conditions** | The app updates and the new data usage information is displayed |
| **List of Exception Use Cases** | WFHSv1-UC-REQ-191974-E12 Mobile app update failed  WFHSv1-UC-REQ-191930-E3 Wi-Fi Hotspot command through mobile app fails |
| **Interfaces** | Ford infrastructure  Carrier infrastructure  WifiHotspotOnBoardClient display  CAN |

#### WFHSv1-UC-REQ-191952/C-User refreshes the data usage values on the mobile app in a no coverage area

|  |  |
| --- | --- |
| **Actors** | User  Mobile App |
| **Pre-conditions** | Mobile app has no cellular coverage |
| **Scenario Description** | The user refreshes the data usage values from the mobile app  WifiHotspotServer is authorized |
| **Post-conditions** | The app times out, indicates an unsuccessful attempt and displays the previous data usage values |
| **List of Exception Use Cases** | WFHSv1-UC-REQ-191930-E3 Wi-Fi Hotspot command through mobile app fails |
| **Interfaces** | Ford infrastructure  Carrier infrastructure  WifiHotspotOnBoardClient display  CAN |

#### WFHSv1-UC-REQ-191953/D-User refreshes the data usage values on the mobile app while in the Wi-Fi Hotspot screen on the WifiHotspotOnBoardClient display

|  |  |
| --- | --- |
| **Actors** | User  Mobile App  WifiHotspotServer |
| **Pre-conditions** | Mobile app has good cellular coverage  User is in the Wi-Fi Hotspot screens on the WifiHotspotOnBoardClient display  WifiHotspotServer is authorized |
| **Scenario Description** | User refreshes the data usage values from the mobile app |
| **Post-conditions** | The app updates and the new data usage information is displayed  The WifiHotspotOnBoardClient continues to display the old data usage values |
| **List of Exception Use Cases** | WFHSv1-UC-REQ-191974-E12 Mobile app update failed  WFHSv1-UC-REQ-191930-E3 Wi-Fi Hotspot command through mobile app fails |
| **Interfaces** | Ford infrastructure  Carrier infrastructure  WifiHotspotServer  WifiHotspotOnBoardClient display  CAN |

#### WFHSv1-UC-REQ-194537/D-User accesses the mobile app while WifiHotspotServer is not authorized

|  |  |
| --- | --- |
| **Actors** | User  System |
| **Pre-conditions** | WifiHotspotServer is NOT authorized  User has downloaded the Ford/Lincoln Owner App, created an account and associated a VIN to the account |
| **Scenario Description** | User access the mobile app screen |
| **Post-conditions** | No Wi-Fi Hotspot data usage information is displayed in the mobile app  A link to the carrier landing page is displayed or, if the vehicle is a China vehicle, the landing page and the carrier’s hotline number (if vehicle is a Ford then the Ford specific number shall be displayed and if vehicle is a Lincoln then the Lincoln specific number shall be displayed) and vehicle’s VIN are also displayed |
| **List of Exception Use Cases** |  |
| **Interfaces** | WifiHotspotOffBoardClient  Mobile app |

#### WFHSv1-UC-REQ-194540/D-User accesses the data usage screen while WifiHotspotServer is un-authorized

|  |  |
| --- | --- |
| **Actors** | User  System |
| **Pre-conditions** | WifiHotspotServer is authorized  WifiHotspotServer is on  Wi-Fi Hotspot Data Usage screen displayed data usage information last time the user was in the screen |
| **Scenario Description** | User un-authorizes the WifiHotspotServer through WifiHotspotOnBoardClient or mobile app and accesses the Wi-Fi Hotspot Data Usage screen |
| **Post-conditions** | No data usage information is displayed |
| **List of Exception Use Cases** |  |
| **Interfaces** | WifiHotspotServer  WifiHotspotOnBoardClient  WifiHotspotOffBoardClient  Mobile app |

### White Box Views

#### Activity Diagrams

##### WFHSv1-ACT-REQ-167125/A-User Refreshes Data Usage Values From Centerstack



#### Sequence Diagrams

##### WFHSv1-SD-REQ-167143/C-User Refreshes Data Usage Values From Centerstack



## WFHSv1-FUN-REQ-140748/F-Carrier Data Notification

If the WifiHotspotServer is not authorized, the WifiHotspotOffBoardClient shall not transmit any data usage notifications to the WifiHotspotServer. If the WifiHotspotServer becomes authorized (refer to the table below), the WifiHotspotOffBoardClient may start transmitting data usage notifications to the WifiHotspotServer.

|  |  |
| --- | --- |
| **WifiHotspotServer State** | **Indication within DataUsage\_Rsp** |
| Factory Mode | Not authorized |
| Unprovisioned | Not authorized |
| Waiting for provisioning Ack | Not authorized |
| Waiting for Home URL | Not authorized |
| Waiting for Auth | Not authorized |
| Authorized | Authorized |

The carrier shall transmit low balance notifications in real time to the WifiHotspotOffBoardClient (~2 seconds). If the WifiHotspotServer is authorized, the notifications shall be transmitted from the WifiHotspotOffBoardClient to the WifiHotspotServer in real time (~2 seconds), assuming the WifiHotspotServer is awake. The carrier data notification message that is transmitted to the WifiHotspotServer shall utilize the same FTCP response message that the WifiHotspotServer receives from a data usage request (refer to WFHSv1-FUN-REQ-140754-Reporting Data Used). The notification shall include data usage information, but the message shall indicate it is a notification and not a data usage response. The WifiHotspotServer shall store the most recently received data usage information so that the current status stored in the WifiHotspotServer reflects the current status of the data plan. A carrier data notification shall be transmitted whenever a low balance threshold was met. These thresholds shall be pre-defined and communicated to the carrier.

The WifiHotspotServer shall be responsible for updating the WifiHotspotOnBoardClient of these notifications through its event periodic CAN message (CarrierDataNotifications\_St). The WifiHotspotOnBoardClient shall display a popup to the customer if it receives a low balance notification from the WifiHotspotServer.

### Requirements

#### WFHS-REQ-191880/D-Receiving carrier data notifications and data usage updates

The data usage FTCP message shall indicate whether the message is a notification or not. If the WifiHotspotServer receives a data usage FTCP notification, it shall be responsible for notifying the WifiHotspotOnBoardClient of the notification using the CAN signal CarrierDataNotification\_St only when the WifiHotspotOnBoardClient is available.

The WifiHotspotServer shall monitor the CAN signal HMIMode\_St to determine when the WifiHotspotOnBoardClient display is active. The WifiHotspotOnBoardClient screen is active when the CAN signal HMIMode\_St=0x2:On.

The WifiHotspotServer shall transmit the CAN signal CarrierDataNotification\_St in its default state (parameter notification type=“NULL” and percentage=“50 percent”) until the WifiHotspotServer is triggered to set them to a different state.

If the WifiHotspotServer receives a carrier data notification, the WifiHotspotServer shall first store the data usage information transmitted within the notification message and note when the notification was received (refer to WFHS-REQ-199543-Monitoring elapsed time since the data usage update). The WifiHotspotServer shall then check the “data used” field to determine what threshold percentage it shall send to the WifiHotspotOnBoardClient. The WifiHotspotServer shall also check the status of the WifiHotspotOnBoardClient screen to determine if it is active or to determine when it becomes active. Once the WifiHotspotServer confirms the WifiHotspotOnBoardClient screen is active, the WifiHotspotServer shall perform the following two steps:

1. Set the CAN signal CarrierDataNotification\_St to “percent data used” and set the percentage parameter to the data used percentage identified within the notification and transmit both once (note: the notification type and percentage parameters within the CAN signal CarrierDataNotification\_St shall be set to the appropriate states and transmitted at the same time).
2. Unset the CAN signal CarrierDataNotification\_St back to NULL (and set the percentage back to 50%) and continue transmitting.

If the WifiHotspotServer receives multiple carrier data notifications from the WifiHotspotOffBoardClient while the WifiHotspotOnBoardClient display is not active, then once the display becomes active the WifiHotspotServer shall only set the CAN signal CarrierDataNotification\_St once and set the percentage to the data left percentage contained within the last received notification.

Note: WifiHotspotServer shall ignore data usage notifications if the Data\_Usage\_Feature\_Enablement DID is set to Off. Refer to WFHS-REQ-222037-Data usage feature flag. The WifiHotspotServer shall also ignore data usage notifications if the WifiHotspotServer is NOT authorized.

#### WFHS-REQ-191882/H-Triggering free trial period reminders

The WifiHotspotServer shall contain a parameter (TrialEligible) that shall be used to determine if the WifiHotspotServer is trial eligible or not. The WifiHotspotServer shall be delivered to Ford with the initial status of the parameter TrialEligible=Yes.

|  |  |
| --- | --- |
| **Parameter** | **State** |
| TrialEligible | 1. Yes 2. No |

Table. TrialEligible parameter

If the WifiHotspotServer receives a data usage notification or a data usage response from a request that indicates the WifiHotspotServer is no longer trial eligible, the WifiHotspotServer shall update the TrialEligible parameter to “No”. Once the parameter is changed to “No”, the parameter shall not be changed to “Yes” unless the WifiHotspotServer receives a notification or data usage response indicating that the vehicle is trial eligible. If the WifiHotspotServer receives a notification or data usage response with no indication on whether the vehicle is trial eligible or not, the TrialEligble parameter state shall remain in its previous state. If the WifiHotspotServer does not have any data usage information stored, the TrialEligible parameter shall remain in its previous state. Refer to the table below to see which data plan type and status combinations indicate if the TrialEligible parameter shall be changed to Yes or No.

|  |  |  |
| --- | --- | --- |
| **Carrier data notification/data usage response: data plan type** | **Carrier data notification/data usage response: data plan status** | **TrialEligible parameter** |
| WifiHotspotServer has no data usage information stored | WifiHotspotServer has no data usage information stored | Retain previous state |
| trial | pending | Yes |
| trial | active | No |
| trial or paid | expired | No |
| trial or paid | inactive | No |
| paid | active | No |

Each VIN shall be granted ONE free trial period in its lifetime. Certain exceptions may be made (for example, call center operators may choose to reinstate trial periods after receiving customer complaints). To increase the Wi-Fi Hotspot free trial period awareness, free trial period reminders shall be displayed on the WifiHotspotOnBoardClient display. Refer to WFHS-REQ-226336/A-HMI Specification References. The trial period reminder popups shall be displayed at the next ignition cycle after the vehicle has reached a specific mileage. The user shall have the ability to select a “remind me later” option, at which point the popup will exit and will re-populate at a later time.

The WifiHotspotServer shall have an EOL configuration (Wi-Fi\_Trial\_Reminder) that shall set the trial period reminders either Off or On (refer to WFHS-REQ-226337-Diagnostic Specification Reference). Wi-Fi\_Trial\_Reminder parameter shall also be configurable via OTA. If the trial reminders are set to On, the WifiHotspotServer shall follow the requirements stated within this requirement in order to display the trial period reminder popups. If the trial period reminders are set to Off, the WifiHotspotServer shall not follow the requirements stated within this requirement and no trial reminder popups shall be triggered.

Thetrial period reminder shall be triggered once the vehicle has reached a certain mileage. The reminder mileage trigger (Wi-Fi\_Trial\_Reminder\_Trigger, configurable via EOL or OTA) shall be stored in the WifiHotspotServer and defaulted to:

* 1931 km (1200 miles) for NA (United States and Canada) and China and
* 1000 km for Europe (refer to WFHS-REQ-191639-WifiHotspotServer identifies the vehicle region).

Once a trial period reminder popup is triggered, the reminder may be delayed. If the reminder is delayed, the reminder popup shall be re-populated Wi-Fi\_Trial\_Reminder\_Delay kilometers after the last reminder popup was triggered. The Wi-Fi\_Trial\_Reminder\_Delay parameter shall be configurable via EOL or OTA and shall be stored in the WifiHotspotServer and defaulted to:

* 1287 km (800 miles) for NA and China and
* 1000 km for Europe.

The WifiHotspotServer shall monitor the CAN signal HotspotTrialReminderSelection\_Rq to determine if it shall re-trigger the trial reminder popup at a later distance or end the trial reminder triggers altogether.

The WifiHotspotServer shall monitor the CAN signal OdometerMasterValue to determine the current vehicle mileage.

The WifiHotspotServer shall monitor the CAN signal IgnitionStatus\_St to determine when the next ignition cycle occurs (next time IgnitionStatus\_St=Run).

The WifiHotspotServer shall monitor the CAN signal HMIMode\_St to determine when the WifiHotspotOnBoardClient display is active. The WifiHotspotOnBoardClient screen is active when HMIMode\_St=0x2:On.

If the WifiHotspotServer receives a command from the WifiHotspotOnBoardClient to end the trial reminder triggers (CAN signal HotspotTrialReminderSelection\_Rq =StopReminders), the WifiHotspotServer shall not trigger any more trial reminder popups.

If the WifiHotspotServer receives a command from the WifiHotspotOnBoardClient to re-trigger the reminder popup (CAN signal HotspotTrialReminderSelection\_Rq =RemindMeLater), the WifiHotspotServer shall replace the Wi-Fi\_Trial\_Reminder\_Trigger value with the sum of the Wi-Fi\_Trial\_Reminder\_Trigger value plus the Wi-Fi\_Trial\_Reminder\_Delay value (Wi-Fi\_Trial\_Reminder\_Trigger = Wi-Fi\_Trial\_Reminder\_Trigger + Wi-Fi\_Trial\_Reminder\_Delay). If the WifiHotspotServer never receives a command from the WifiHotspotOnBoardClient to re-trigger the popup, the WifiHotspotServer shall not update the Wi-Fi\_Trial\_Reminder\_Trigger value.

If Wi-Fi\_Trial\_Reminder=On and the parameter TrialEligible=”Yes”, the WifiHotspotServer shall monitor the vehicle mileage.

* If OdometerMasterValue < Wi-Fi\_Trial\_Reminder\_Trigger, the WifiHotspotServer shall NOT set the CarrierDataNotification\_St CAN signal bit and it shall remain set to “NULL”.
* If OdometerMasterValue = Wi-Fi\_Trial\_Reminder\_Trigger, the WifiHotspotServer shall wait until the next ignition cycle (next time IgnitionStatus\_St=Run) and then check the status of the WifiHotspotOnBoardClient screen to determine if it is active or to determine when it becomes active. Once the WifiHotspotServer confirms the WifiHotspotOnBoardClient screen is active, the WifiHotspotServer shall perform the following two steps:

1. Set the CAN signal CarrierDataNotification\_St to “free trial period waiting” and transmit it once
2. Unset the CAN signal CarrierDataNotification\_St back to NULL and continue transmitting.

Note: if the TrialEligible parameter’s state is set to “No”, the WifiHotspotServer shall not trigger a trial reminder popup.

#### WFHS-REQ-191881/F-Displaying critical data plan related popups

The WifiHotspotOnBoardClient shall monitor the CAN signal CarrierDataNotification\_St and detect when it changes its status.

* If the status changes to “XX% data used” (note: the WifiHotspotOnBoard client shall only monitor the percentage values within the CarrierDataNotification\_St CAN signal if the CAN signal CarrierDataNotification\_St=Percent data used), the WifiHotspotOnBoardClient shall display a low balance popup. Refer to WFHS-REQ-226336/A-HMI Specification References.

The popup below is an example WifiHotspotOnBoardClient popup.



Figure. XX% data used popup for NA (United States and Canada)

* If the status changes to “free trial period waiting”, the WifiHotspotOnBoardClient shall display a trial reminder popup.

The trial reminder popup shall have two different options listed on it:

**Option 1.** Close: if the customer closes the popup then the popup shall NOT be re-triggered.

**Option 2.** Remind me later: if the customer chooses the “remind me later” option, then the popup shall exit and re-populate at a later time.

If the user selects the “Close” option, the WifiHotspotOnBoardClient shall notify WifiHotspotServer by setting the CAN signal HotspotTrialReminderSelection\_Rq to “StopReminders” once, transmitting, then unsetting back to NULL.

If the user selects the “Remind me later” option, the WifiHotspotOnBoardClient shall notify the WifiHotspotServer by setting the CAN signal HotspotTrialReminderSelection\_Rq to “RemindMeLater” once, transmitting, then unsetting back to NULL.

The trial reminder popups shall be driver restricted. Refer to H21j specification and the HMI specification (refer to WFHS-REQ-226336/A-HMI Specification References). The trial reminder popup shall remain displayed until the user closes the popup or selects the “remind me later” option. If the driver restriction becomes enabled while the popup is displayed, the popup shall be hidden until the driver restriction is disabled, at which point the popup shall be displayed again. If the user has not closed out of the popup or chosen the “remind me later” option, the popup shall survive ignition cycles. The WifiHotspotServer shall only send the notification once at the time of trigger (using CAN signal CarrierDataNotification\_St=Free Trial Period Waiting). The APIM shall be responsible for storing the notification and displaying the popup as long as needed until the user selects either the “Close” or “Remind Me Later” option.

The popup below is an example WifiHotspotOnBoardClient popup.



Figure. Free trial period waiting popup for NA (United States and Canada)

* If the CAN signal CarrierDataNotification\_St changes its status to “NULL”, the WifiHotspotOnBoardClient shall not display a popup nor request for the carrier information.

If the trial reminder or low balance popups are required to display the carrier information (i.e. landing page URL, hotline number, etc.), the WifiHotspotOnBoardClient shall request for and receive the carrier information (CAN signal CarrierInfo\_Rq and CarrierInfo\_Rsp) before displaying the popups. Also, the XX% data used popups shall be dynamic and shall display the actual percentage value stated in the CAN signal CarrierDataNotification\_St. If the popup is required to display the VIN, the WifiHotspotOnBoardClient shall find the VIN contained within the CAN signal VehicleGGCCData. Refer to the HMI specifications to determine which popups need to display what information.

### Use Cases

#### WFHSv1-UC-REQ-191963/G-The vehicle's Wi-Fi Hotspot data plan changes to a low balance or expired or trial period waiting status

|  |  |
| --- | --- |
| **Actors** | User  System |
| **Pre-conditions** | WifiHotspotServer is On  WifiHotspotOnBoardClient display is available and on any screen  WifiHotspotServer is authorized |
| **Scenario Description** | Any of the following scenarios occurred:   * ignition starts when a trial period is waiting to be activated AND the vehicle reached a specified mileage AND driver distraction is not enabled * Low balance notification was triggered from the carrier |
| **Post-conditions** | The user shall be notified of the update via a popup on the WifiHotspotOnBoardClient display (refer to WFHS-REQ-226336/A-HMI Specification References) |
| **List of Exception Use Cases** | WFHSv1-UC-REQ-191973-E11 WifiHotspotOnBoardClient update failed |
| **Interfaces** | WifiHotspotServer  WifiHotspotOnBoardClient  CAN  Ford infrastructure  Carrier infrastructure |

### White Box Views

#### Activity Diagrams

##### WFHSv1-ACT-REQ-167116/D-Carrier Data Notification Received



##### WFHSv1-ACT-REQ-212880/A-Free Trial Period Reminders



#### Sequence Diagrams

##### WFHSv1-SD-REQ-167139/D-Carrier Data Notification Received



##### WFHSv1-SD-REQ-212881/A-Free Trial Period Reminders



## WFHSv1-FUN-REQ-192000/D-Managing Carrier Information

NA (Unites States and Canada), China and Europe customers may subscribe to the hotspot through a carrier provided landing page. The URL for this page shall be displayed to the user through the WifiHotspotOnBoardClient display on NA, China and Europe vehicles. The landing page URL MAY be different, depending on region, for Ford versus Lincoln customers.

Customers in China may also subscribe to the hotspot by calling their carrier’s hotline and providing their vehicle’s VIN. Thus, the hotline’s telephone number and the vehicle’s VIN shall be displayed to the customer on the WifiHotspotOnBoardClient display of China vehicles. The hotline number for Ford customers shall be different than the hotline number for Lincoln customers. The in-vehicle WifiHotspotOnBoardClient screens of China vehicles shall also allow the customer to initiate a call to the hotline through their paired phone in the vehicle.

If a carrier ever decides to update the URL to the landing page or the carrier hotline number, the carrier backend shall transmit these notifications to Ford, via a manual process, and include the new URL characters or phone number included. The URL or hotline numbers shall be transmitted to the WifiHotspotServer via FTCP messages, and the WifiHotspotServer shall overwrite the previously stored parameters with the new ones.

If the user enters into a Wi-Fi Hotspot screen that requires a landing page URL or carrier hotline number to be displayed, the WifiHotspotOnBoardClient shall transmit a request for the carrier information. If the WifiHotspotServer receives this request it shall respond with the appropriate carrier information.

### Requirements

#### WFHS-REQ-191718/B-Initial carrier hotline number

The WifiHotspotServer shall be delivered to Ford with the two initial hotline numbers below (one for Ford customers and one for Lincoln customers) preprogrammed into the WifiHotspotServer (Note: the hotline numbers shall be added to this document at a later time):

|  |  |
| --- | --- |
| **China Carrier Service Hotline Number** | |
| Ford | Lincoln |
| XXXXXXXX | XXXXXXXX |

Each carrier service hotline number may be up to 24 characters in length.

#### WFHS-REQ-191719/B-Updating the carrier service hotline number

The WifiHotspotServer shall be capable of receiving updates to the carrier hotline numbers from the WifiHotspotOffBoardClient regardless of the WifiHotspotServer authorization state. If the WifiHotspotServer receives a command from the WifiHotspotOffBoardClient to update the carrier service hotline numbers, the WifiHotspotServer shall overwrite the previously stored hotline numbers with the new numbers and store them. The updates shall specify which hotline number is the Ford number and which hotline number is the Lincoln number. The carrier hotline numbers shall also be configurable via EOL.

#### WFHS-REQ-191726/D-Updating the carrier landing page URL

The WifiHotspotServer shall be delivered to Ford with the initial region and brand-specific carrier landing page URLs below preprogrammed into the WifiHotspotServer (Note: the URLs shall be added to this document at a later time):

|  |  |  |
| --- | --- | --- |
| **Region** | **Carrier Landing Page URL** | |
| **Ford** | **Lincoln** |
| NA (United States and Canada) |  |  |
| China |  |  |
| Europe |  |  |

Table. Carrier landing page URL lookup table

Each URL may be up to may be up to 192 characters in length.

The WifiHotspotServer shall be capable of receiving updates to the carrier landing page URLs from the WifiHotspotOffBoardClient regardless of the WifiHotspotServer’s authorization state. If the WifiHotspotServer receives a command from the WifiHotspotOffBoardClient to update the carrier landing page URLs the WifiHotspotServer shall first determine which region it is in (refer to WFHS-REQ-191639-WifiHotspotServer identifies the vehicle region) to determine which region-specific landing page URLs to update. The update shall also specify which is the Ford URL and which is the Lincoln URL. The WifiHotspotServer shall then overwrite the previously stored region-specific landing page URLs with the new URLs and store it. The URLs shall also be updateable via EOL.

#### WFHS-REQ-191875/D-Requesting for carrier information due to the user entering a specific screen

If the user enters into a Wi-Fi Hotspot screen that displays the carrier hotline number or landing page URL, the WifiHotspotOnBoardClient shall request for the carrier information using the CAN signal CarrierInfo\_Rq. The WifiHotspotServer shall respond with the CAN signal CarrierInfo\_Rsp. The WifiHotspotOnBoardClient shall only display the information it needs based on the region and vehicle brand (refer to WFHS-REQ-191640-WifiHotspotOnBoardClient identifies vehicle brand and WFHS-REQ-191641-WifiHotspotOnBoardClient identifies vehicle region). If the vehicle is a China variant, the WifiHotspotOnBoardClient shall also display the 17 character VIN on the screens that require the carrier hotline to be displayed. The VIN is contained within the CAN signal VehicleGGCCData. Refer to the HMI specifications to view the screens and different parameters needed depending on the vehicle brand and region (refer to WFHS-REQ-226336/A-HMI Specification References).

#### WFHS-REQ-191729/D-Reporting out the carrier information to the WifiHotspotOnBoardClient

**China:** If the WifiHotspotOnBoardClient requests for the carrier information through the CAN signal CarrierInfo\_Rq, the WifiHotspotServer shall check the vehicle region (refer to WFHS-REQ-191639-WifiHotspotServer identifies the vehicle region). If the vehicle is a Chinese variant, the WifiHotspotServer shall

1. fetch both the stored China Ford and China Lincoln carrier hotline numbers,
2. fetch both the stored China Ford landing page URL and China Lincoln landing page URL from the landing page URL lookup table (refer to WFHS-REQ-191726-Updating the carrier landing page URL) and

populate all the above parameters into the CAN signal CarrierInfo\_Rsp and transmit.

**NA:** If the WifiHotspotOnBoardClient requests for the carrier information through the CAN signal CarrierInfo\_Rq, the WifiHotspotServer shall check the vehicle region (refer to WFHS-REQ-191639-WifiHotspotServer identifies the vehicle region). If the vehicle is a NA (United States and Canada) variant, the WifiHotspotServer shall

1. fetch both the stored NA Ford landing page URL and NA Lincoln landing page URL from the landing page URL lookup table (refer to WFHS-REQ-191726-Updating the carrier landing page URL) and

populate into the CAN signal CarrierInfo\_Rsp and transmit. (Note: the carrier hotline number field shall NOT be populated into the CAN signal.)

**EU:** If the WifiHotspotOnBoardClient requests for the carrier information through the CAN signal CarrierInfo\_Rq, the WifiHotspotServer shall check the vehicle region (refer to WFHS-REQ-191639-WifiHotspotServer identifies the vehicle region). If the vehicle is a EU variant, the WifiHotspotServer shall

1. fetch both the stored EU Ford landing page URL and EU Lincoln landing page URL from the landing page URL lookup table (refer to WFHS-REQ-191726-Updating the carrier landing page URL) and

populate into the CAN signal CarrierInfo\_Rsp and transmit. (Note: the carrier hotline number field shall NOT be populated into the CAN signal.)

|  |  |  |
| --- | --- | --- |
| **Vehicle Region** | **CAN signal CarrierInfo\_Rsp** | |
| **Carrier hotline numbers field** | **Carrier landing page field** |
| China | populate both China Ford and Lincoln numbers | populate both China Ford and Lincoln URLs |
| NA (United States or Canada) | do not populate | populate both NA Ford and Lincoln URLs |
| EU | do not populate | populate both EU Ford and Lincoln URLs |

Table. Populating the CAN signal CarrierInfo\_Rsp

If the WifiHotspotServer does not have a particular hotline number or URL stored, the WifiHotspotServer shall not populate that field in the CarrierInfo\_Rsp message. For example) The WifiHotspotServer is placed on a European Ford vehicle. The WifiHotspotServer has a EU Ford URL stored, but no EU Lincoln URL stored. The WifiHotspotServer shall only populate the Ford URL in the CAN signal. The WifiHotspotOnBoardClient shall automatically select the Ford URL to display since it is a Ford vehicle.

#### WFHS-REQ-191876/F-Displaying carrier information

Depending on the vehicle region (refer to WFHS-REQ-191641-WifiHotspotOnBoardClient identifies vehicle region), the WifiHotspotOnBoardClient may be required to display either the Ford or the Lincoln carrier hotline number (refer to WFHS-REQ-191640-WifiHotspotOnBoardClient identifies the vehicle brand) and the vehicle VIN in certain Wi-Fi Hotspot screens and popups (refer to the HMI specifications (WFHS-REQ-226336/A-HMI Specification References) to determine which regions and which screens or popups require this information). Both Ford and Lincoln hotline numbers may be populated in the response CAN signal CarrierInfo\_Rsp, and it shall be the responsibility of the WifiHotspotOnBoardClient to display the appropriate number depending on the brand.

The WifiHotspotOnBoardClient may also be required to display a landing page URL on certain screens and popups (refer to HMI specifications to determine which regions and which screens or popups require this information). Both Ford and Lincoln URLs may be populated in the response CAN signal CarrierInfo\_Rsp, and it shall be the responsibility of the WifiHotspotOnBoardClient to display the appropriate URL depending on the brand.

The following screen is an example WifiHotspotOnBoardClient screen.




Figure. Screen that makes customer aware of their data usage statistics (vehicle is a China variant).

Note: If the WifiHotspotServer does not have a particular hotline number or URL stored, the WifiHotspotServer shall not populate that field in the CarrierInfo\_Rsp message. For example) The WifiHotspotServer is placed on a European Ford vehicle. The WifiHotspotServer has a EU Ford URL stored, but no EU Lincoln URL stored. The WifiHotspotServer shall only populate the Ford URL in the CAN signal. The WifiHotspotOnBoardClient shall automatically select the Ford URL to display since it is a Ford vehicle. The WifiHotspotServer shall always provide the minimum amount of information required by the WifiHotspotOnBoardClient to be displayed. The WifiHotspotServer MAY provide more information, at which point the WifiHotspotOnBoardClient shall select which information to display.

#### WFHS-REQ-191877/E-Initiating a call to the carrier hotline

The China Wi-Fi Hotspot screens and popups that display either the Ford or the Lincoln hotline number shall provide the user the option to initiate a call to purchase more data for their vehicle’s hotspot. Refer to WFHS-REQ-226336/A-HMI Specification References. If the user selects the dial button the WifiHotspotOnBoardClient shall initiate a call using the customer’s paired cellphone via Bluetooth. The WifiHotspotOnBoardClient shall dial either the Ford or the Lincoln hotline number provided by the WifiHotspotServer inside the CAN signal CarrierInfo\_Rsp. If the vehicle is a Ford, the WifiHotspotOnBoardClient shall dial the Ford specified carrier hotline number and if the vehicle is a Lincoln, the WifiHotspotOnBoardClient shall dial the Lincoln carrier hotline number. If the user selects the end button (populated on the screen after the dial button is pressed) the WifiHotspotOnBoardClient shall end the phone call. The following is an example WifiHotspotOnBoardClient screen.




Figure. Carrier hotline dial screen

### Use Cases

#### WFHSv1-UC-REQ-191959/C-China customer initiates a call to the carrier hotline though the WifiHotspotOnBoardClient display

|  |  |
| --- | --- |
| **Actors** | User  System  Cell phone |
| **Pre-conditions** | WifiHotspotServer is On  No Wi-Fi subscription is active  Cell phone is connected to the vehicle via Bluetooth  The WifiHotspotOnBoardClient is displaying a screen or popup that displays the Ford carrier hotline number if the vehicle is a Ford or a Lincoln carrier hotline number if the vehicle is a Lincoln, vehicle VIN and call button |
| **Scenario Description** | China customer presses the call button on the WifiHotspotOnBoardClient screen |
| **Post-conditions** | The paired phone and hands-free system begins calling the Ford or Lincoln carrier hotline number (depending on the vehicle brand) and the WifiHotspotOnBoardClient screens follow the process listed in the HMI spec (refer to WFHS-REQ-226336/A-HMI Specification References).  The WifiHotspotOnBoardClient screen remains on its current screen or popup in order to display the VIN |
| **List of Exception Use Cases** |  |
| **Interfaces** | WifiHotspotServer  WifiHotspotOnBoardClient  CAN |

#### WFHSv1-UC-REQ-191960/B-China customer purchases data/activates trial period through the carrier hotline

|  |  |
| --- | --- |
| **Actors** | User  System  Cell phone |
| **Pre-conditions** | WifiHotspotServer is On  Up to Number\_Hotspot\_Connected\_Devices devices connected to the hotspot  Customer **may or may not** have created a mobile app account and authorized their WifiHotspotServer |
| **Scenario Description** | China customer calls the carrier hotline, provides the vehicle VIN, agrees to Terms and Conditions, and purchases data/activates a trial period |
| **Post-conditions** | Customer may now browse the internet/stream data on the connected devices |
| **List of Exception Use Cases** | WFHSv1-UC-REQ-191962-E10 Carrier did not add data to the vehicle hotspot |
| **Interfaces** | WifiHotspotServer  WifiHotspotOnBoardClient  CAN  Ford WifiHotspotOffBoardClient  Carrier infrastructure |

#### WFHSv1-UC-REQ-191961/C-Customer purchases data/activates free trial period through connected device

|  |  |
| --- | --- |
| **Actors** | User  System  Cell phone |
| **Pre-conditions** | Vehicle’s hotspot is not tied to a data plan  Hotspot On  Device is connected to the hotspot  Customer **may or may not** have created a mobile app account and authorized their WifiHotspotServer |
| **Scenario Description** | User accesses the internet browser and is re-directed to the carrier’s landing page where the customer activates the trial period/purchases data by agreeing to a set of Terms and Conditions. The vehicle occupant is not required to identify their vehicle. |
| **Post-conditions** | The user may browse the internet/stream data |
| **List of Exception Use Cases** | E10 Carrier did not add data to the vehicle hotspot |
| **Interfaces** | WifiHotspotServer  Carrier infrastructure  Ford Infrastructure  WifiHotspotOnBoardClient  CAN |

#### WFHSv1-UC-REQ-191962/A-E10 Carrier did not add data to the Wi-Fi Hotspot

|  |  |
| --- | --- |
| **Actors** | User  System  Cell phone |
| **Pre-conditions** | Same as normal use case |
| **Scenario Description** | User purchases more data for the hotspot or activates the free trial period but the carrier did not process the request correctly |
| **Post-conditions** | No data can be streamed through the hotspot  User is redirected to a landing page |
| **List of Exception Use Cases** |  |
| **Interfaces** | WifiHotspotServer  WifiHotspotOnBoardClient  CAN |

#### WFHSv1-UC-REQ-194537/D-User accesses the mobile app while WifiHotspotServer is not authorized

|  |  |
| --- | --- |
| **Actors** | User  System |
| **Pre-conditions** | WifiHotspotServer is NOT authorized  User has downloaded the Ford/Lincoln Owner App, created an account and associated a VIN to the account |
| **Scenario Description** | User access the mobile app screen |
| **Post-conditions** | No Wi-Fi Hotspot data usage information is displayed in the mobile app  A link to the carrier landing page is displayed or, if the vehicle is a China vehicle, the landing page and the carrier’s hotline number (if vehicle is a Ford then the Ford specific number shall be displayed and if vehicle is a Lincoln then the Lincoln specific number shall be displayed) and vehicle’s VIN are also displayed |
| **List of Exception Use Cases** |  |
| **Interfaces** | WifiHotspotOffBoardClient  Mobile app |

#### WFHSv1-UC-REQ-194538/B-User accesses the landing page from the mobile app when WifiHotspotServer is not authorized

|  |  |
| --- | --- |
| **Actors** | User  System |
| **Pre-conditions** | WifiHotspotServer is NOT authorized  Vehicle is a NA or China variant  User has downloaded the Ford/Lincoln Owner App, created an account and associated a VIN to the account |
| **Scenario Description** | User clicks on the landing page link |
| **Post-conditions** | The user’s device re-directs them to the landing page  Customer does not need to enter VIN. |
| **List of Exception Use Cases** |  |
| **Interfaces** | Mobile app  Landing page |

#### WFHSv1-UC-REQ-194539/B-User accesses the landing page from the mobile app when WifiHotspotServer is authorized

|  |  |
| --- | --- |
| **Actors** | User  System |
| **Pre-conditions** | WifiHotspotServer is authorized  User has downloaded the Ford/Lincoln Owner App, created an account and associated a VIN to the account  Vehicle is a NA or China variant. |
| **Scenario Description** | User clicks on the landing page link |
| **Post-conditions** | The user’s device re-directs them to the landing page  Some customer information, including VIN, is pre-populated in the customer information fields |
| **List of Exception Use Cases** |  |
| **Interfaces** | WifiHotspotOffBoardClient  Carrier infrastructure  Mobile app  Landing page |

### White Box Views

#### Activity Diagrams

##### WFHSv1-ACT-REQ-167114/C-Carrier Info Changes From Backend



#### Sequence Diagrams

##### WFHSv1-SD-REQ-167131/C-Carrier Info Changes From Backend



## WFHSv1-FUN-REQ-140759/C-Wi-Fi Hotspot Reset

The user may reset its Wi-Fi Hotspot settings by performing a Master Reset from the in-vehicle WifiHotspotOnBoardClient or by removing a VIN from their mobile app. If either of these scenarios occurs, the WifiHotspotServer shall initiate a Wi-Fi Hotspot reset.

### Requirements

#### WFHS-REQ-191785/E-Triggering a Wi-Fi Hotspot reset

If the WifiHotspotServer receives any of the following:

* A Master Reset CAN signal from the WifiHotspotOnBoardClient,
* A Master Reset FTCP command from the WifiHotspotOffBoardClient or
* A Wi-Fi-Hotspot specific reset CAN signal from the WifiHotspotOnBoardClient,

the WifiHotspotServer shall perform a Wi-Fi Hotspot reset (refer to WFHS-REQ-191863-Wi-Fi Hotspot reset settings). Refer to the Embedded Modem Reset APIM Subsystem Part Specific Specification for all relevant requirements and information regarding the above mentioned CAN signals, etc.

#### WFHS-REQ-191862/B-Reporting out a Wi-Fi Hotspot reset

If the WifiHotspotServer performs a Wi-Fi Hotspot reset it shall update its status in the CAN signal TCUAvailability\_St to “NULL” until the reset is complete.

#### WFHS-REQ-191863/F-Wi-Fi Hotspot reset settings

The WifiHotspotServer shall be delivered to Ford with all of its Wi-Fi Hotspot settings and parameters set to their default values. The default values for each parameter may be found in separate sections within this specification. Note: The Wi-Fi Hotspot settings and parameters shall only be applied when the WifiHotspotServer enables access point mode (refer to WFHS-REQ-192111-Wi-Fi Chipset AP and STA mode).

If the WifiHotspotServer changes any of the hotspot settings and parameters listed in the table below it shall overwrite the previously stored settings/parameters with the new modified settings/parameters and save them.

If the WifiHotspotServer performs a Wi-Fi Hotspot reset (refer to WFHS-REQ-191785-Triggering a Wi-Fi Hotspot Reset), the WifiHotspotServer shall gracefully disconnect all connected clients and reset the Wi-Fi chipset. After the reset is completed all previously connected clients shall be required to enter the newly-generated password if they wish to connect. The WifiHotspotServer shall reset all the Wi-Fi Hotspot settings and parameters to the values listed in the table below.

|  |  |  |
| --- | --- | --- |
| **Parameter Name** | **TCU power cycle, TCU OTA SW update, power reset, running reset and diagnostic reset settings** | **Wi-Fi Hotspot reset settings** |
| Wi-Fi Hotspot enablement state | Restore customer modified setting | Factory setting: On |
|
|
| Wi-Fi visibility state | Restore customer modified setting | Factory setting: On |
|
| Wi-Fi SSID | Restore customer modified setting | Factory default SSID HotspotXXXX (refer to WFHS-REQ-191596-Generating the default SSID) |
| Wi-Fi password | Restore customer modified setting | XXXXXXXXXXXX (refer to WFHS-REQ-191610-Generating the initial password) |
| Wi-Fi security algorithm | Restore customer modified setting | Factory setting: WPA/WPA2 |
|
| TrialEligible parameter | Restore last saved value | Restore last saved value |
|
| Blocked clients list | Restore last saved values | Factory setting: NULL |
| Landing page URLs | Restore last saved values | Restore last saved values |
| Ford/Lincoln carrier hotline numbers | Restore last saved values | Restore last saved values |
| Wi-Fi data usage | NULL | Factory setting: NULL |
| Hotspot\_Enablement\_Timer timer | Reset timer | Reset timer |
| Wi-Fi APN | Restore last saved values | Restore last stored values |
| Wi-Fi\_Trial\_Reminder\_Trigger | Restore last stored value | Restore last stored value |
| Wi-Fi\_Trial\_Reminder\_Delay | Restore last stored value | Restore last stored value |
| Wi-Fi\_Hotspot\_Feature\_Enabled | Restore last stored value | Restore last stored value |
|
| Data\_Usage\_Info\_Refresh\_Timeout timer | Reset timer | Reset timer |
| Data\_Usage\_Reception\_Time | 0:00:00 | 0:00:00 |
| Enhanced\_Hotspot\_Enablement\_Mode | Restore last stored value | Restore last stored value |
| Wi-Fi\_Trial\_Reminder | Restore last stored value | Restore last stored value |
| Hotspot\_Operational\_Band | Restore last saved value | Factory setting: 5GHz |
|
| Estimated location | Restore last saved value | Factory setting: Null |

Table. Wi-Fi Hotspot Default Settings

Note:

* 1. The WifiHotspotServer shall default the Wi-Fi Hotspot enablement state to on ONLY if all Wi-Fi Hotspot enablement conditions are met. If the conditions are not met the WifiHotspotServer shall set the Wi-Fi Hotspot enablement state to on-disabled (refer to WFHS-REQ-191706-Wi-Fi Hotspot enablement condition checks).
  2. The SSID shall be reset to the default SSID that the WifiHotspotServer was delivered to Ford with (refer to WFHS-REQ-191596-Generating the default SSID).
  3. The password shall be randomly re-generated to a 12 ASCII character password. The generated passwords shall be created using a quality random number generator. The supplier shall meet the requirements defined in A51t\_Supplier\_Feed\_Specification\_080.pdf spec, section 1.9.9 Requirements for Key Generation.
  4. All blocked devices shall be deleted from the blocked list and shall be allowed to connect by entering the newly generated password.
  5. All data usage information shall be cleared. If the WifiHotspotServer is in the process of updating the data usage values and waiting for a response from the WifiHotspotOffBoardClient when a request for a Wi-Fi Hotspot reset is received the WifiHotspotServer shall immediately initiate the reset. If the request for a data usage update was initiated by the WifiHotspotOnBoardClient (refer to WFHS-REQ-191868-Request from WifiHotspotOnBoardClient to refresh the data usage values) the WifiHotspotServer shall send an unsuccessful response (CAN signal DataUsage\_Rsp). The WifiHotspotServer shall not restart the updating process once the reset is complete.

### Use Cases

#### WFHSv1-UC-REQ-191967/D-User performs a reset but does not deactivate their Wi-Fi Hotspot data plan

|  |  |
| --- | --- |
| **Actors** | User  WifiHotspotOnBoardClient  WifiHotspotServer |
| **Pre-conditions** | WifiHotspotServer is on  Customer has a data plan active on their vehicle |
| **Scenario Description** | Customer performs a Master reset from the WifiHotspotOnBoardClient or decommissions their VIN from their Owner App account |
| **Post-conditions** | The customer shall be locked out of the Wi-Fi Hotspot screens  Any attempts the customer makes to enter the Wi-Fi Hotspot screens shall be denied and shall trigger a popup while the WifiHotspotServer is resetting  (refer to WFHS-REQ-226336/A-HMI Specification References)  WifiHotspotOnBoardClient display shall update according to the HMI spec.  The user shall be informed through the WifiHotspotOnBoardClient display that their subscriptions MAY not be cancelled.  All connected devices shall be disconnected from the Wi-Fi Hotspot and required to enter the new, randomly generated password  Blocked devices shall be able to connect by entering the new, randomly generated password  Vehicle shall remain tied to the customer’s data plan  No data usage information shall be displayed on the Wi-Fi Hotspot Data Usage screens in-vehicle or on the mobile app until the WifiHotspotServer/mobile app receives new data usage information from the WifiHotspotOffBoardClient (if authorized) |
| **List of Exception Use Cases** | E3 Wi-Fi Hotspot command through mobile app fails  E4 Wi-Fi Hotspot configuration through WifiHotspotOnBoardClient fails  E11 WifiHotspotOnBoardClient update failed |
| **Interfaces** | WifiHotspotOnBoardClient  WifiHotspotServer  CAN  Mobile App  Ford infrastructure |

#### WFHSv1-UC-REQ-191968/C-Dealer replaces WifiHotspotServer while a Wi-Fi Hotspot data plan is active

|  |  |
| --- | --- |
| **Actors** | User  WifiHotspotOnBoardClient  WifiHotspotServer |
| **Pre-conditions** | User has personalized their Wi-Fi Hotspot settings (such as SSID, on/off, etc.)  WifiHotspotServer has malfunctioned  Customer **may or may not** have created a mobile app account and authorized their WifiHotspotServer  A Wi-Fi data plan is active (trial or retail) |
| **Scenario Description** | Dealer replaces the old WifiHotspotServer with a new one and completes the provisioning process as defined in the WifiHotspotServer Provisioning spec |
| **Post-conditions** | If the vehicle is NA or China, the customer’s data plan is active on the new WifiHotspotServer (trial or retail; if the trial period was already used up, the new WifiHotspotServer will not offer a new trial period)  If the vehicle is EU, the customer shall be required to pair their account to the vehicle in order to utilize their data plan (if the trial period was already used up, the customer shall not be offered a new trial on the vehicle).  No data usage information shall be displayed on the Wi-Fi Hotspot Data Usage screens in-vehicle or on the mobile app until the WifiHotspotServer/mobile app receives new data usage information from the WifiHotspotOffBoardClient (if authorized)  The Wi-Fi Hotspot settings are defaulted back to their default states |
| **List of Exception Use Cases** |  |
| **Interfaces** | WifiHotspotOnBoardClient  WifiHotspotServer  CAN  Ford WifiHotspotOffBoardClient  Carrier WifiHotspotOffBoardClient  Mobile App |

## WFHSv1-FUN-REQ-195287/A-Transferring MAC Address

The WifiHotspotOnBoardClient has a Wi-Fi chipset configured in client mode. The WifiHotspotOnBoardClient Wi-Fi chipset shall never connect to the WifiHotspotServer’s Wi-Fi AP. To prevent this, the WifiHotspotOnBoardClient shall detect the WifiHotspotServer Wi-Fi chipset’s MAC address and never allow its chipset to connect.

The WifiHotspotOnBoardClient shall transmit a request for the MAC address every ignition cycle, and in turn, the WifiHotspotServer shall respond with the MAC address of its Wi-Fi chipset.

Refer to the Feature-WiFi Settings Max Level Infotainment Subsystem Part Specification (SPSS) to for more information on this requirement.

### Requirements

#### WFHS-REQ-194536/B-Reporting out the Wi-Fi chipset MAC address

The WifiHotspotServer shall monitor the CAN signal WifiHotspotMAC\_Rq. If the WifiHotspotServer receives a request for its Wi-Fi chipset’s MAC address (WifiHotspotMAC\_Rq), the WifiHotspotServer shall populate the MAC address of its Wi-Fi chipset into the CAN signal WifiHotspotMAC\_Rsp and transmit. If the Wi-Fi Hotspot feature is disabled, the WifiHotspotServer shall still respond to the request and populate the Wi-Fi chipsets MAC address. If the WifiHotspotServer is unable to read the Wi-Fi chipset’s MAC address, it shall transmit a NULL response. Refer to the Feature-WiFi Settings Max Level Infotainment Subsystem Part Specification (SPSS) to for more information on how the WifiHotspotOnBoardClient processes the response.

### White Box Views

#### Activity Diagrams

##### WFHSv1-ACT-REQ-195130/A-Transmitting Wi-Fi Chipset MAC Address



#### Sequence Diagrams

##### WFHSv1-SD-REQ-195131/A-Transmitting Wi-Fi Chipset MAC Address



## WFHSv1-FUN-REQ-263189/A-Switching Frequency Bands

If the vehicle is in a location that allows more than one frequency band to be used, the customer shall have the ability to select which frequency band they would like the Wi-Fi Hotspot feature to operate on. Therefore, the WifiHotspotOnBoardClient shall display the current frequency band in use, as well as provide the option of changing the band, assuming the hotspot is allowed to operate on more than one frequency band.

If the user changes the frequency band from the WifiHotspotOnBoardClient, the WifiHotspotServer shall receive a CAN signal, save and update the hotspot’s setting, and respond to the WifiHotspotOnBoardClient by updating its status on a designated CAN signal.

### Requirements

#### WFHS-REQ-263084/A-Estimating current vehicle location

The WifiHotspotServer shall contain an algorithm that estimates the vehicle’s current location based on data it has available. Example) The WifiHotspotServer may reference the MCC in order to identify the location. The software development group shall create this algorithm and it shall be reviewed by the Feature Owner.

If there is no current data available for the WifiHotspotServer to utilize, it shall refer to the last estimated location. If there is no previously stored data to reference, the WifiHotspotServer shall reference its country configuration DID (refer to WFHS-REQ-191639/D-WifiHotspotServer identifies the vehicle region) to estimate the location.

The WifiHotspotServer shall use its estimated vehicle location in order to determine whether any frequency channels are required to be restricted or not. For more information, refer to WFHS-REQ-263085-Restricting frequency channels.

The estimated vehicle location shall be stored in a DID (Estimated\_Location).

#### WFHS-REQ-263085/A-Restricting frequency channels

Each region may have its own local regulatory restrictions on the 5 GHz frequency band that may be subject to change with time. Some examples of restrictions that may be placed on a particular channel include:

* No broadcasting at all
* Dynamic Frequency Selection shall be enabled
* Transmit Power Control shall be enabled
* AP can only broadcast indoors, etc.

The WifiHotspotServer shall utilize its estimated current vehicle location (refer to WFHS-REQ-263084-Estimating current vehicle location) in order to determine which frequency channels or entire band it is and is not allowed to operate on.

The WifiHotspotServer shall contain a lookup table that determines which frequency channels it is allowed to operate on per country. The software development group shall define the frequency restriction lookup table and it shall be reviewed by the Feature Owner. The table may be subject to change based on the fluctuating local regulations.

If the WifiHotspotServer’s hotspot is turned On and configured to operate on the 5 GHz band or it receives a request to change to the 5 GHz band, it shall:

* Confirm the vehicle’s current estimated location allows for 5 GHz operation,
* Reference the frequency restriction lookup table,
* Perform auto-channel selection on the allowed frequency channels and
* Select the least congested channel to operate on.

If the WifiHotspotServer is operating on the 5 GHz band when it detects a country change, it shall refer to the frequency restriction lookup table to determine if it needs to change the frequency channel or band.

#### WFHS-REQ-263087/A-Reporting available bands

The WifiHotspotServer shall monitor its current estimated vehicle location and determine whether an entire frequency band shall be restricted or not based on the frequency restriction table. The WifiHotspotServer shall then report the frequency bands available for use with the CAN signal HotspotAvailableBands\_St. If the WifiHotspotServer cannot detect which frequency bands are available for use, it shall set the CAN signal to NULL.

Note: The CAN signal uses generic literals, so refer to the following:

* Band1 = 2.4 GHz
* Band2 = 5 GHz

Example 1) The WifiHotspotServer detects the vehicle is in a country where all frequency channels on the 5 GHz band are restricted. It shall therefore set HotspotAvailableBands\_St = Band1.

Example 2) If the WifiHotspotServer is in a country where there are available channels to use on both the 2.4 GHz band and the 5 GHz band, it shall set HotspotRestrictedBand\_St = All available.

#### WFHS-REQ-263088/A-Reporting the frequency band

The WifiHotspotServer shall report the current frequency band that the hotspot is operating on using the CAN signal HotspotFrequencyBand\_St. If the WifiHotspotServer cannot detect the current frequency band that it is configured for, it shall set the CAN signal to NULL.

Note: The CAN signal uses generic literals, so refer to the following:

* Band1 = 2.4 GHz
* Band2 = 5 GHz

#### WFHS-REQ-263089/A-Displaying the frequency band

The WifiHotspotOnBoardClient shall display the frequency band in use, which is reported from the WifiHotspotServer through the CAN signal HotspotFrequencyBand\_St.

The WifiHotspotServer may disable certain frequency bands from being used based on the vehicle’s location. Therefore, the WifiHotspotOnBoardClient shall display the available frequency band options to the customer. If there is more than one option available for use, the WifiHotspotOnBoardClient shall allow the user to select which frequency band to use. The WifiHotspotOnBoardServer shall monitor the CAN signal HotspotAvailableBands\_St to determine which bands are available.

Note: The CAN signal uses generic literals, so refer to the following:

* Band1 = 2.4 GHz
* Band2 = 5 GHz

Example 1) The vehicle is in a location where the entire 5 GHz band is restricted and only the 2.4 GHz band is available. The WifiHotspotServer shall set the CAN signal HotspotAvailableBands\_St = Band1 and HotspotFrequencyBand\_St = Band1. The WifiHotspotOnBoardClient shall not allow the user to select the 5 GHz band.

Example 2) The vehicle is in a location where there are available channels to use on both the 2.4 GHz band and the 5 GHz band. The hotspot is currently using the 5 GHz band. The WifiHotspotServer shall set the CAN signal HotspotAvailableBands\_St = All available and HotspotFrequencyBand\_St = Band2. The WifiHotspotOnBoardClient shall inform the user that the 5 GHz band is in use and it shall also provide the user the option to select the 2.4 GHz band.

Refer to WFHS-REQ-226336/A-HMI Specification References for how this shall be displayed to the customer.

#### WFHS-REQ-263090/A-User changes the frequency band on WifiHotspotOnBoardClient

If the user requests to change the frequency band through the in-vehicle WifiHotspotOnBoardClient (assuming the WifiHotspotOnBoardClient is allowed to display multiple options to the user), the WifiHotspotOnBoardClient shall transmit this request to the WifiHotspotServer using the CAN signal HotspotFrequencyBand\_Rq.

Note: The CAN signal uses generic literals, so refer to the following:

* Band1 = 2.4 GHz
* Band2 = 5 GHz

#### WFHS-REQ-263091/A-Frequency band change request from WifiHotspotOnBoardClient

If the WifiHotspotServer receives a request from the WifiHotspotOnBoardClient (CAN signal HotspotFrequencyBand\_Rq) to change the frequency band, the WifiHotspotServer shall ensure the frequency band is allowed based on the vehicle’s estimated location. If it is supported, the WifiHotspotServer shall immediately switch the AP’s frequency to the desired band and update the CAN signal HotspotFrequencyBand\_St and corresponding Diagnostic ID (Hotspot\_Operational\_Band) when the transition is complete. If the WifiHotspotServer’s attempt was unsuccessful, the WifiHotspotServer shall continue reporting out the current frequency band in use.

All user configurable Wi-Fi Hotspot parameters (i.e. SSID, password, etc.) shall remain the same once the WifiHotspotServer is operating on the new frequency band. The WifiHotspotServer shall keep as many of the AP parameters the same as possible in order to allow client devices to automatically reconnect to the new band.

Note: The CAN signal uses generic literals, so refer to the following:

* Band1 = 2.4 GHz
* Band2 = 5 GHz

### Use Cases

#### WFHSv1-UC-REQ-263187/A-User changes frequency band

|  |  |
| --- | --- |
| **Actors** | User  System  Cell phone |
| **Pre-conditions** | WifiHotspotServer is on  Vehicle is in a location that allows multiple frequency bands to be used  Wi-Fi Hotspot is On and operating on the 5GHz band  The SSID = 123  The Password = 12345678  Up to Number\_Hotspot\_Connected\_Devices devices are connected |
| **Scenario Description** | User changes the frequency band from 5GHz to 2.4GHz band through the WifiHotspotOnBoardClient display |
| **Post-conditions** | Wi-Fi Hotspot is On and operating on the 2.4GHz band  The SSID = 123  The Password = 12345678  All previously connected devices may automatically reconnect  All other Wi-Fi Hotspot configurable parameters remain the same as before the frequency band switch (i.e. visibility status) |
| **List of Exception Use Cases** | WFHSv1-UC-REQ-191931-E4 Wi-Fi Hotspot configuration through WifiHotspotOnBoardClient fails  WFHSv1-UC-REQ-191973-E11 WifiHotspotOnBoardClient update failed |
| **Interfaces** | WifiHotspotOnBoardClient  WifiHotspotServer  CAN |

#### WFHSv1-UC-REQ-263186/A-User attempts to change to restricted frequency band

|  |  |
| --- | --- |
| **Actors** | User  System  Cell phone |
| **Pre-conditions** | WifiHotspotServer is on  Wi-Fi Hotspot is On and operating on the 2.4 GHz band  The vehicle is in an area where the 5 GHz band is completely restricted |
| **Scenario Description** | User accesses the Vehicle Hotspot page where the frequency band would normally be displayed |
| **Post-conditions** | The user is NOT able to change the frequency to the 5 GHz band (not displayed, or interface is disabled, etc.) |
| **List of Exception Use Cases** |  |
| **Interfaces** | WifiHotspotOnBoardClient  WifiHotspotServer  CAN |

### White Box Views

#### Activity Diagrams

##### WFHSv1-ACT-REQ-263190/A-User Changes Frequency Band From Centerstack



#### Sequence Diagrams

##### WFHSv1-SD-REQ-263192/A-User Changes Frequency Band From Centerstack



# Appendix: Reference Documents

|  |  |
| --- | --- |
| Reference # | Document Title |
| 1 |  |
| 2 |  |
| 3 |  |
| 4 |  |
| 5 |  |