

**Research & Vehicle Technology**

**“Infotainment Systems Product Development”**

**Feature – Rocket Setup Server**

**Infotainment Subsystem Part Specific Specification (SPSS)**

Version 1.3

**UNCONTROLLED COPY IF PRINTED**

**Version Date: July 13, 2020**

**FORD CONFIDENTIALF**

**Revision History**

|  |  |  |  |
| --- | --- | --- | --- |
| **Date** | **Ver** | **Notes** | |
| **Aug. 29, 2019** | **1.0** | **Initial Release** |  |
|  |  |  |  |
| **December 20, 2019** | **1.1** |  | |
|  | STR-679269/B-Overview | | MBORREL4: Added "if applicable" for Work. Removed Ambient Lighting |
|  | STR-679275/B-Terms and Definitions | | MBORREL4: Added Final Purchase Flag |
|  | RKS-IIR-REQ-354840/B-RSServer\_Rx | | MBORREL4: Added REQ-370458 |
|  | RKS-IIR-REQ-354841/B-RSServer\_Tx | | MBORREL4: Added REQ-370458 |
|  | MD-REQ-370458/A-saveNavLocation | | MBORREL4: New API |
|  | STR-668798/B-General Requirements | | MBORREL4: Added REQ-364451 |
|  | RKS-REQ-361373/B-FTCP Specification References | | MBORREL4: Corrected the Class name |
|  | RKS-REQ-361339/B-Security Specification Reference | | MBORREL4: Updated title |
|  | RKS-REQ-361338/B-Feature Configuration | | MBORREL4: Added the default config. value |
|  | RKS-REQ-362420/B-RS Settings – RSServer Module Swap | | MBORREL4: Added VehicleGGCCData message and startup condition |
|  | RKS-REQ-362421/B-RS Settings – Rocket Setup Disabled on RSServer | | MBORREL4: Added reference to config req. |
|  | RKS-REQ-364451/A-RS Settings Feature Numbers/Structure | | MBORREL4: New req. |
|  | STR-680484/B-Use Cases | | MBORREL4: Removed REQ-361472 |
|  | RKS-UC-REQ-361470/B-User selects and submits RS Settings on RSOffBoardClient | | MBORREL4: Updated preconditions |
|  | RKS-UC-REQ-361471/B-RS Settings downloaded to RSServer when awake | | MBORREL4: Updated usecase |
|  | RKS-UC-REQ-361473/B-RS Settings payload fails Payload Check(s) | | MBORREL4: Updated usecase and title |
|  | STR-680483/B-Requirements | | MBORREL4: Added REQ-364357, REQ-367354 |
|  | RKS-REQ-361342/B-RS Settings Download – RSCommand | | MBORREL4: Added req references |
|  | RKS-REQ-361344/B-RS Settings Download – Persistence | | MBORREL4: Removed yellow text. No alert needed, no need to save URL |
|  | RKS-REQ-361345/B-RS Settings Download – Persistence Timer | | MBORREL4: Updated "max time" |
|  | RKS-TMR-REQ-361379/B-T\_Persist | | MBORREL4: Updated Range |
|  | RKS-REQ-361346/B-RS Settings Download – Payload Timestamp | | MBORREL4: Updated timestamp format to ISO 8601 |
|  | RKS-REQ-362418/B-RS Settings Download – Failure | | MBORREL4: Changed "download" to "persist" |
|  | RKS-REQ-364357/A-RS Settings Download - Failure Retry | | MBORREL4: New req. |
|  | RKS-REQ-361348/B-RS Settings Download – RSCommandResponse | | MBORREL4: Updated |
|  | RKS-REQ-361349/B-RS Settings Download – RSAlert | | MBORREL4: Updated |
|  | RKS-REQ-367354/A-RS Settings Download - Rejecting RSCommand | | MBORREL4: New req. |
|  | RKS-UC-REQ-361474/B-User accepts and continues RS process on RSServer | | MBORREL4: Updated precondition |
|  | RKS-UC-REQ-361475/B-User accepts and fails to complete RS process on RSServer | | MBORREL4: Updated precondition |
|  | RKS-UC-REQ-361476/B-User denies RS process on RSServer | | MBORREL4: Updated precondition |
|  | RKS-UC-REQ-361477/B-User postpones RS process on RSServer | | MBORREL4: Updated precondition |
|  | RKS-UC-REQ-361478/B-User postpones RS process on RSServer (last retry) | | MBORREL4: Updated precondition |
|  | RKS-UC-REQ-361480/B-RS & Master Reset – After RS Settings applied | | MBORREL4: Updated precondition |
|  | STR-680487/B-Requirements | | MBORREL4: Removed REQ-361359. Added REQ-372250 |
|  | RKS-REQ-361351/B-Validate Identified User | | MBORREL4: Updated req. |
|  | RKS-REQ-372250/A-RS Process Pause | | MBORREL4: New req. |
|  | RKS-REQ-361356/B-RS Process - Accept | | MBORREL4: Updated req. |
|  | RKS-REQ-361357/B-RS Process - Deny | | MBORREL4: Updated req. |
|  | RKS-REQ-361360/B-RS Process – Postpone Retry | | MBORREL4: Added validation requirement before showing welcome screen |
|  | RKS-REQ-362419/B-RS Process – Rocket Setup Complete Flag | | MBORREL4: Updated req. |
|  | RKS-REQ-361362/B-Master Reset before RS Process Success | | MBORREL4: Updated req. |
|  | RKS-REQ-361363/B-Master Reset after RS Process Success | | MBORREL4: Updated req. |
|  | STR-680489/B-Requirements | | MBORREL4: Removed REQ-362422 (settings are applied in parallel, not sequential). Removed Ambient Lighting section and all subsequent requirements. Added Drive Mode section and all subsequent requirements. |
|  | RKS-REQ-362424/B-RS Settings – Profile Name Format | | MBORREL4: Updated table |
|  | RKS-REQ-362425/B-RS Settings – Profile Name Usage | | MBORREL4: Added feature number & data value |
|  | RKS-REQ-362427/B-RS Settings – Failure to Apply Profile Name | | MBORREL4: Updated default value |
|  | RKS-REQ-362428/B-RS Settings – Profile Photo Format | | MBORREL4: Changed compression to encoding, updated table |
|  | RKS-REQ-362429/B-RS Settings – Profile Photo Usage | | MBORREL4: Added feature number & data value |
|  | RKS-REQ-362431/B-RS Settings – Failure to Apply Profile Photo | | MBORREL4: Updated default photo |
|  | STR-680495/B-Navigation Favorites | | MBORREL4: Added REQ-367359 |
|  | RKS-REQ-361366/B-RS Settings – Navigation Favorites | | MBORREL4: Added "if applicable" for Work |
|  | RKS-REQ-362432/B-RS Settings – Navigation Favorites Parameters/Format | | MBORREL4: Updated table |
|  | RKS-REQ-362433/B-RS Settings – Required Navigation Favorite Parameters | | MBORREL4: Updated table |
|  | RKS-REQ-362434/B-RS Settings – Applying the Navigation Favorites | | MBORREL4: Updated req. |
|  | RKS-REQ-362436/B-RS Settings – Multiple Addresses Found for a Navigation Favorite | | MBORREL4: Removed "TBD" |
|  | RKS-REQ-367359/A-RS Settings – Max Saved Locations Occupied | | MBORREL4: New req. |
|  | STR-680496/B-Radio Presets | | MBORREL4: Added REQ-372296 |
|  | RKS-REQ-372296/A-RS Settings - NA vs EU Preset Determination | | MBORREL4: New req. |
|  | RKS-REQ-362446/B-RS Settings – Radio Presets Parameters/Format | | MBORREL4: Updated table |
|  | RKS-REQ-362447/B-RS Settings - Required NA AM/FM Radio Preset Parameters | | MBORREL4: Updated table |
|  | RKS-REQ-362448/B-RS Settings - Required NA SDARS Radio Preset Parameters | | MBORREL4: Updated table |
|  | RKS-REQ-362449/B-RS Settings - Required EU FM/DAB Radio Preset Parameters | | MBORREL4: Updated table |
|  | RKS-REQ-362453/B-RS Settings – Applying NA AM/FM Radio Presets | | MBORREL4: Added feature number & data value |
|  | RKS-REQ-362454/B-RS Settings – Applying NA SDARS Radio Presets | | MBORREL4: Added feature number & data value |
|  | RKS-REQ-362455/B-RS Settings – Applying EU FM/DAB Radio Presets | | MBORREL4: Updated req. |
|  | RKS-REQ-362438/B-RS Settings – Departure Times Parameters/Format | | MBORREL4: Updated table |
|  | RKS-REQ-362439/B-RS Settings – Applying the Departure Times | | MBORREL4: Added feature number & data value |
|  | RKS-REQ-362440/B-RS Settings – Failure to Apply Departure Times | | MBORREL4: Removed TBD note |
|  | STR-688823/A-Drive Mode | | MBORREL4: New req. |
|  | RKS-REQ-364513/A-RS Settings – Drive Mode | | MBORREL4: New req. |
|  | RKS-REQ-364514/A-RS Settings – Drive Mode Parameters/Format | | MBORREL4: New req. |
|  | RKS-REQ-364515/A-RS Settings – Applying the Drive Mode Setting | | MBORREL4: New req. |
|  | RKS-REQ-364516/A-RS Settings – Failure to Apply Drive Mode Setting | | MBORREL4: New req. |
|  | STR-668800/B-Appendix: Reference Documents | | MBORREL4: Updated references |
|  |  |  |  |
| **April 1, 2020** | **1.2** |  | |
|  | DOC-668801/B-Physical Mapping of Classes | | MBORREL4: Removed BCM |
|  | RKS-IIR-REQ-354840/C-RSServer\_Rx | | MBORREL4: Added REQ-384392, Removed REQ-086348 |
|  | MD-REQ-370458/B-saveNavLocation | | MBORREL4: Updated R/O fields |
|  | MD-REQ-384392/A-setDriveMode | | MBORREL4: New API |
|  | RKS-IIR-REQ-354841/C-RSServer\_Tx | | MBORREL4: Added REQ-384392 |
|  | MD-REQ-370458/B-saveNavLocation | | MBORREL4: Updated R/O fields |
|  | MD-REQ-384392/A-setDriveMode | | MBORREL4: New API |
|  | RKS-REQ-362420/C-RS Settings – RSServer Module Swap | | MBORREL4: Removed second bullet point |
|  | STR-668799/B-Functional Definition | | MBORREL4: Added REQ-384393 |
|  | RKS-FUN-REQ-384393/A-BLE Download | | MBORREL4: New function for BLE Key |
|  | STR-743013/A-Use Cases | | MBORREL4: New STR |
|  | RKS-UC-REQ-384394/A-User submits RS Settings on RSOffBoardClient – BLE Payload | | MBORREL4: New req. |
|  | RKS-UC-REQ-384395/A-BLE Payload downloaded to RSServer when awake | | MBORREL4: New req. |
|  | RKS-UC-REQ-384396/A-BLE Payload fails Payload Check(s) | | MBORREL4: New req. |
|  | STR-743014/A-Requirements | | MBORREL4: New STR |
|  | RKS-REQ-384397/A-BLE Payload Download – RSCommand | | MBORREL4: New req. |
|  | RKS-REQ-384398/A-BLE Payload Download – SyncP Wrapped | | MBORREL4: New req. |
|  | RKS-REQ-384399/A-BLE Payload Download – Persistence | | MBORREL4: New req. |
|  | RKS-REQ-384400/A-BLE Payload Download – Persistence Timer | | MBORREL4: New req. |
|  | RKS-REQ-384401/A-BLE Payload Download – Payload Timestamp | | MBORREL4: New req. |
|  | RKS-REQ-384402/A-BLE Payload Download – Timestamp Check | | MBORREL4: New req. |
|  | RKS-REQ-384403/A-BLE Payload Download – Payload Check | | MBORREL4: New req. |
|  | RKS-REQ-384404/A-BLE Payload Download – Failure | | MBORREL4: New req. |
|  | RKS-REQ-384405/A-BLE Payload Download – Failure Retry | | MBORREL4: New req. |
|  | RKS-REQ-384406/A-BLE Payload Download – RSCommandResponse | | MBORREL4: New req. |
|  | RKS-REQ-384408/A-BLE Payload MAI and RS Payload Profile ID Check | | MBORREL4: New req. |
|  | RKS-UC-REQ-361471/C-RS Settings downloaded to RSServer when awake | | MBORREL4: Removed one postcondition |
|  | STR-680486/B-Use Cases | | MBORREL4: Removed REQ-361478 |
|  | RKS-UC-REQ-361479/B-RS & Master Reset – Before RS Settings applied | | MBORREL4: Updated usecase |
|  | RKS-UC-REQ-361480/C-RS & Master Reset – After RS Settings applied | | MBORREL4: Updated usecase |
|  | RKS-REQ-361351/C-Validate Identified User | | MBORREL4: Updated req. |
|  | RKS-REQ-361355/B-RS Process Abort - Retry Strategy | | MBORREL4: Updated req. |
|  | RKS-REQ-361363/C-Master Reset after RS Process Success | | MBORREL4: Updated req. |
|  | RKS-REQ-362428/C-RS Settings – Profile Photo Format | | MBORREL4: Updated req. |
|  | RKS-REQ-362432/C-RS Settings – Navigation Favorites Parameters/Format | | MBORREL4: Updated Feature Numbers |
|  | RKS-REQ-362433/C-RS Settings – Required Navigation Favorite Parameters | | MBORREL4: Updated Required fields |
|  | RKS-REQ-362434/C-RS Settings – Applying the Navigation Favorites | | MBORREL4: Added clarification |
|  | RKS-REQ-362446/C-RS Settings – Radio Presets Parameters/Format | | MBORREL4: Changed ChannelID to integer (to match proto). Added Presets 11-15 |
|  | RKS-REQ-362447/C-RS Settings - Required NA AM/FM Radio Preset Parameters | | MBORREL4: Updated radio preset number in table |
|  | RKS-REQ-362448/C-RS Settings - Required NA SDARS Radio Preset Parameters | | MBORREL4: Updated radio preset number in table |
|  | RKS-REQ-362449/C-RS Settings - Required EU FM/DAB Radio Preset Parameters | | MBORREL4: Updated radio preset number in table |
|  | RKS-REQ-362450/B-RS Settings – Muting while Applying Radio Presets | | MBORREL4: Updated req. |
|  | RKS-REQ-362451/B-RS Settings – UnMuting after Applying Radio Presets | | MBORREL4: Updated req. |
|  | RKS-REQ-362453/C-RS Settings – Applying NA AM/FM Radio Presets | | MBORREL4: Updated CurrentPreset2.St with CurrMixPreset\_St. Added REQ-192639 reference |
|  | RKS-REQ-362454/C-RS Settings – Applying NA SDARS Radio Presets | | MBORREL4: Updated CurrentPreset2.St with CurrMixPreset\_St. Added REQ-192639 reference |
|  | RKS-REQ-362455/C-RS Settings – Applying EU FM/DAB Radio Presets | | MBORREL4: Updated CurrentPreset2.St with CurrMixPreset\_St. Added REQ-192639 reference |
|  | RKS-REQ-362438/C-RS Settings – Departure Times Parameters/Format | | MBORREL4: Updated Feature Numbers |
|  | RKS-REQ-364515/B-RS Settings – Applying the Drive Mode Setting | | MBORREL4: Updated to include API |
|  |  |  |  |
| **July 13, 2020** | **1.3** |  | |
|  | STR-679269/C-Overview | | MBORREL4: Added Avatar Selection |
|  | STR-743013/B-Use Cases | | MBORREL4: Removed REQ-384394 |
|  | RKS-UC-REQ-384395/B-BLE Payload downloaded to RSServer when awake | | MBORREL4: Updated/corrected usecase |
|  | RKS-UC-REQ-384396/B-BLE Payload fails Payload Check(s) | | MBORREL4: Updated/corrected usecase |
|  | STR-743014/B-Requirements | | MBORREL4: Added REQ-388562 |
|  | RKS-REQ-384397/B-BLE Payload Download – BLECommand | | MBORREL4: Corrected title. Updated req to delete old payload upon reception. Updated for multiple payloads |
|  | RKS-REQ-384406/B-BLE Payload Download – BLECommandResponse | | MBORREL5: Updated title. |
|  | RKS-REQ-384408/B-BLE Payload MAI and RS Payload Profile ID Check | | MBORREL4: Updated req to delete payloads on mismatch |
|  | RKS-REQ-388562/A-BLE Payload Download - Rejecting BLECommand | | MBORREL4: New req. |
|  | STR-680484/C-Use Cases | | MBORREL4: Removed REQ-361470 |
|  | RKS-UC-REQ-361471/D-RS Settings downloaded to RSServer when awake | | MBORREL4: Updated/corrected usecase |
|  | RKS-UC-REQ-361473/C-RS Settings payload fails Payload Check(s) | | MBORREL4: Updated/corrected usecase |
|  | RKS-REQ-361342/C-RS Settings Download – RSCommand | | MBORREL4: Updated req to delete old payload upon reception. Updated for multiple payloads |
|  | RKS-REQ-367354/B-RS Settings Download - Rejecting RSCommand | | MBORREL4: Updated for multiple payloads |
|  | RKS-UC-REQ-361475/C-User accepts and fails to complete RS process on RSServer | | MBORREL4: Updated postcondition for "Abort is not a Postpone" |
|  | RKS-UC-REQ-361476/C-User denies RS process on RSServer | | MBORREL4: Updated Postcondition |
|  | RKS-UC-REQ-361477/C-User postpones RS process on RSServer | | MBORREL4: Updated postcondition for "Abort is not a Postpone" |
|  | RKS-REQ-361355/C-RS Process Abort - Retry Strategy | | MBORREL4: Updated for "Abort is not a Postpone" |
|  | RKS-REQ-361356/C-RS Process - Accept | | MBORREL4: Updated for "Avatar Selection" |
|  | STR-680489/C-Requirements | | MBORREL4: Added "Avatar Selection" section and all supporting reqs. |
|  | RKS-REQ-362428/D-RS Settings – Profile Photo Format | | MBORREL4: Added PNG format |
|  | RKS-REQ-362429/C-RS Settings – Profile Photo Usage | | MBORREL4: Removed req to show photo during welcome screen |
|  | STR-761509/A-Avatar Selection | | MBORREL4: New section for Avatar Selection |
|  | RKS-REQ-388450/A-RS Settings – Avatar Selection | | MBORREL4: New req. for Avatar Selection |
|  | RKS-REQ-388451/A-RS Settings – Avatar Selection Format | | MBORREL4: New req. for Avatar Selection |
|  | RKS-REQ-388452/A-RS Settings – Avatar Selection Usage | | MBORREL4: New req. for Avatar Selection |
|  | RKS-REQ-388453/A-RS Settings – Avatar Selection Edit | | MBORREL4: New req. for Avatar Selection |
|  | RKS-REQ-388454/A-RS Settings – Failure to Apply Avatar Selection | | MBORREL4: New req. for Avatar Selection |
|  | RKS-REQ-361367/B-RS Settings – Radio Presets | | MBORREL4: Updated number of presets to 15 |
|  | RKS-REQ-362446/D-RS Settings – Radio Presets Parameters/Format | | MBORREL4: Added ECC |
|  | RKS-REQ-362447/D-RS Settings - Required NA AM/FM Radio Preset Parameters | | MBORREL4: Added ECC |
|  | RKS-REQ-362448/D-RS Settings - Required NA SDARS Radio Preset Parameters | | MBORREL4: Added ECC |
|  | RKS-REQ-362449/D-RS Settings - Required EU FM/DAB Radio Preset Parameters | | MBORREL4: Added ECC |
|  | RKS-REQ-362453/D-RS Settings – Applying NA AM/FM Radio Presets | | MBORREL4: Removed CurrMixPreset\_St from step 4 |
|  | RKS-REQ-362454/D-RS Settings – Applying NA SDARS Radio Presets | | MBORREL4: Removed CurrMixPreset\_St from step 4 |
|  | RKS-REQ-362455/D-RS Settings – Applying EU FM/DAB Radio Presets | | MBORREL4: Updated per EU implementation |
|  | RKS-REQ-362439/C-RS Settings – Applying the Departure Times | | MBORREL4: Corrected Feature numbers. |
|  |  | | XGU14: Modified for China. |

**Table of Contents**

[Revision History 2](#_Toc45552544)

[1 Overview 10](#_Toc45552545)

[1.1 Terms and Definitions 10](#_Toc45552546)

[2 Architectural Design 11](#_Toc45552547)

[2.1 Boundary Diagram 11](#_Toc45552548)

[2.1.1 RKS-BD-REQ-360828/A-RS Boundary Diagram 11](#_Toc45552549)

[2.2 RKS-CLD-REQ-354834/A-Rocket Setup Server 11](#_Toc45552550)

[2.3 RKS-CLD-REQ-354836/A-Rocket Setup OffBoard Client 11](#_Toc45552551)

[2.4 RKS-CLD-REQ-354835/A-Rocket Setup Client 11](#_Toc45552552)

[2.5 Physical Mapping of Classes 11](#_Toc45552553)

[2.6 RSServer Interface 12](#_Toc45552554)

[2.6.1 RKS-IIR-REQ-354840/C-RSServer\_Rx 12](#_Toc45552555)

[2.6.2 RKS-IIR-REQ-354841/C-RSServer\_Tx 15](#_Toc45552556)

[3 General Requirements 18](#_Toc45552557)

[3.1 RKS-REQ-361373/B-FTCP Specification References 18](#_Toc45552558)

[3.2 RKS-REQ-361339/B-Security Specification Reference 18](#_Toc45552559)

[3.3 RKS-REQ-361338/B-Feature Configuration 18](#_Toc45552560)

[3.4 RKS-REQ-362420/C-RS Settings – RSServer Module Swap 18](#_Toc45552561)

[3.5 RKS-REQ-362421/B-RS Settings – Rocket Setup Disabled on RSServer 18](#_Toc45552562)

[3.6 RKS-REQ-364451/A-RS Settings Feature Numbers/Structure 18](#_Toc45552563)

[4 Functional Definition 19](#_Toc45552564)

[4.1 RKS-FUN-REQ-384393/A-BLE Download 19](#_Toc45552565)

[4.1.1 Use Cases 19](#_Toc45552566)

[4.1.2 Requirements 19](#_Toc45552567)

[4.2 RKS-FUN-REQ-361370/A-RS Download 22](#_Toc45552568)

[4.2.1 Use Cases 22](#_Toc45552569)

[4.2.2 Requirements 22](#_Toc45552570)

[4.3 RKS-FUN-REQ-361371/A-RS Process 25](#_Toc45552571)

[4.3.1 Use Cases 25](#_Toc45552572)

[4.3.2 Requirements 26](#_Toc45552573)

[4.4 RKS-FUN-REQ-361374/A-Applying RS Settings 30](#_Toc45552574)

[4.4.1 Use Cases 30](#_Toc45552575)

[4.4.2 Requirements 30](#_Toc45552576)

[5 Appendix: Reference Documents 43](#_Toc45552577)

# Overview

Rocket Setup is a feature that enables customers to select a set of preferences, via a FordPass application, for their recently purchased vehicle before they take ownership. Through Rocket Setup, the vehicle is already setup with the customer’s preferences when they interact with the vehicle for the first time.

The core preferences/settings supported by this feature are:

* Name and Photo
* Avatar Selection
* Navigation Home/Work (if applicable)/Favorites
* EV Charge Departure Times
* Radio Presets (ex. FM/AM/Sirius/DAB)
* Drive Modes
* Apps (Apps Anywhere Phase 1)
* IVI wakeup word
* IVI voice setup
* IVI theme setup

This feature has an objective to improve dealership handover process of new vehicles, increase Ford Pass downloads, increase loyalty/satisfaction of customers and decrease customer complains related to navigation settings and mobile phone-vehicle pairing.

Rocket Setup will allow the customer to use a mobile phone, computer, or Ford kiosk in a dealership to select their preferences. The preferences will only be available to a vehicle after a first time purchase (not available to re-sale vehicles), and they will be sent to the vehicle one-time only (this is not a continuous app experience, app preference management, or preference synchronization).

## Terms and Definitions

|  |  |
| --- | --- |
| **Abbreviation** | **Description** |
| CAN | Controller Area Network |
| CCS | Customer Connectivity Setting |
| DID | Data Identifier |
| FCI | Ford Cloud Interface |
| FNV2.0 | Fully Networked Vehicle 2nd Generation |
| FTCP | Ford Telematics Communication Protocol |
| IPPT | IP pass-through |
| POI | Points of interest |
| PPP | Portable Personal Profiles |
| RS | Rocket Setup |
| SDN | Service Delivery Network |
| SOA | Service Oriented Architecture |
| SPSS | Subsystem Part Specific Specification |
| WIR | Wireless Interface Router |

|  |  |
| --- | --- |
| **Term** | **Description** |
| RS Settings | The settings or preferences selected by the user via the RSOffBoardClient to be loaded in-vehicle |
| RS Settings payload | Specifically referring to the FTCP payload containing the RS Settings |
| SyncP | A Ford standard mechanism for secure communication. |
| Final Purchase Flag | The event/flag used to indicate Final Purchase and transfer of ownership from Ford to the customer |

# Architectural Design

## Boundary Diagram

### RKS-BD-REQ-360828/A-RS Boundary Diagram



## RKS-CLD-REQ-354834/A-Rocket Setup Server

The Rocket Setup Server (RSServer) is responsible for the tasks listed below:

* Receive payload from RSOffBoardClient
* Send acknowledgement to RSOffBoardClient
* Push payload to all RSClients using existing interfaces
* Trigger RS download process once account was logged in China.

Please review the implementation guide/ block diagram to locate the Rocket Setup Server class.

## RKS-CLD-REQ-354836/A-Rocket Setup OffBoard Client

The Rocket Setup OffBoardClient (RSOffBoardClient) is responsible for the tasks listed below:

* Receive user input via FordPass
* Compile user preferences into payload
* Send payload to RSServer
* Receive acknowledgement from RSServer

Please review the implementation guide/ block diagram to locate the Rocket Setup OffBoardClient class.

## RKS-CLD-REQ-354835/A-Rocket Setup Client

The Rocket Setup Client (RSClient) is responsible for the tasks listed below:

* Receive and save settings from RSServer

Please review the implementation guide/ block diagram to locate the Rocket Setup Client class.

## Physical Mapping of Classes

The table below shows an example of how the logical classes that make up the Rocket Setup feature can be mapped into physical modules. This mapping is an example only and does not necessarily carryover to other carlines or vehicle architectures.

|  |  |
| --- | --- |
| **Logical Class** | **Physical Module (ECU)** |
| RSServer | SYNC |
| RSOffBoardClient | SDN |
| RSClient | AHU, HPCM, etc. |

## RSServer Interface

### RKS-IIR-REQ-354840/C-RSServer\_Rx

#### MD-REQ-361425/A-RSCommand

Message Type: FTCP

This message is used to send the RS Settings payload to the RSServer.

**Note:** Refer to the latest “Ford Telematics Communication Protocol Specification” and Protofile for the most up to date FTCP messages/definitions.

|  |  |
| --- | --- |
| **Command** | **Description** |
| RSCommand | Command sent from the RSOffBoardClient to the RSServer including the RS Settings payload. |

#### ~~MD-REQ-361428/A-BLECommand~~

~~Message Type: FTCP~~

~~This message is used to send the BLE auto-pair key the RSServer.~~

**~~Note:~~** ~~Refer to the latest “Ford Telematics Communication Protocol Specification” and Protofile for the most up to date FTCP messages/definitions.~~

|  |  |
| --- | --- |
| **~~Command~~** | **~~Description~~** |
| ~~BLECommand~~ | ~~Command sent from the RSOffBoardClient to the RSServer including the BLE auto-pair key.~~ |

#### MD-REQ-027149/A-IgnitionStatus\_St (TcSE ROIN-225464-1)

Message Type: Status

Signal used to indicate ignition state.

|  |  |  |  |
| --- | --- | --- | --- |
| **Name** | **Literals** | **Value** | **Description** |
| Type | - | - | Indicates ignition state |
|  | Unknown | 0x0 |  |
|  | Off | 0x1 |  |
|  | Accessory | 0x2 |  |
|  | Run | 0x4 |  |
|  | Start | 0x8 |  |
|  | Invalid | 0xF |  |

#### MD-REQ-028253/A-GearLeverPosition\_St (TcSE ROIN-282103-1)

Message Type: Status

Status used to indicate the current gear selected.

|  |  |  |  |
| --- | --- | --- | --- |
| **Name** | **Literals** | **Value** | **Description** |
| Type | - | - | Used to indicate current gear selected. |
|  | Park | 0x0 |  |
|  | Reverse | 0x1 |  |
|  | Neutral | 0x2 |  |
|  | Drive | 0x3 |  |
|  | Sport\_DriveSport | 0x4 |  |
|  | Low | 0x5 |  |
|  | First | 0x6 |  |
|  | Second | 0x7 |  |
|  | Third | 0x8 |  |
|  | Fourth | 0x9 |  |
|  | Fifth | 0xA |  |
|  | Sixth | 0xB |  |
|  | Undefined\_Treat\_as\_Fault | 0xC |  |
|  | Undefined\_Treat\_as\_Fault1 | 0xD |  |
|  | Unknown\_Position | 0xE |  |
|  | Fault | 0xF |  |

#### MD-REQ-014025/A-VehicleSpeed\_St (TcSE ROIN-223023-1)

Message Type: Status

Status used to indicate vehicle speed.

|  |  |  |  |
| --- | --- | --- | --- |
| **Name** | **Literals** | **Value** | **Description** |
| Type | - | - | Indicates vehicle speed.  Unit: kph  Resolution:0.01  Offset:0 |
|  | Kph | 0x0 to 0xFFFF |  |

#### ~~MD-REQ-370458/B-saveNavLocation~~

~~This API is used to request the Nav Vendor to save a Navigation Favorite. The Nav Vendor also uses this API for its response.~~

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | |
| **~~Method Type~~** | | ~~One-Shot (Synch)~~ | | | | | |
| **~~QoS Level~~** | | ~~Default~~ | | | | | |
| **~~Retained~~** | | ~~No~~ | | | | | |
|  | | | | | | | |
| **~~R/O~~** | **~~Name~~** | | **~~Type~~** | **~~Literals~~** | **~~Value~~** | **~~Description~~** |
| **~~Request~~** | | | | | | | |
| ~~R~~ | ~~RequestID~~ | | ~~Int32~~ | ~~-~~ | ~~-2147483648 to +2147483647~~ |  |
| ~~R~~ | ~~Location Name~~ | | ~~String~~ | ~~-~~ | ~~0-200 chars~~ |  |
| ~~O~~ | ~~Phone Number~~ | | ~~String~~ | ~~-~~ | ~~0-20 chars~~ |  |
| ~~O~~ | ~~City~~ | | ~~String~~ | ~~-~~ | ~~0-50 chars~~ | ~~Hypernym for e.g. city/village~~ |
| ~~O~~ | ~~SubCity~~ | | ~~String~~ | ~~-~~ | ~~0-50 chars~~ | ~~Hypernym for e.g. district~~ |
| ~~O~~ | ~~State~~ | | ~~String~~ | ~~-~~ | ~~0-100 chars~~ | ~~Portion of country (e.g. state, province)~~ |
| ~~O~~ | ~~Door Number~~ | | ~~String~~ | ~~-~~ | ~~0-50 chars~~ | ~~Portion of thoroughfare e.g. house number~~ |
| ~~O~~ | ~~Street Name~~ | | ~~String~~ | ~~-~~ | ~~0-100 chars~~ | ~~Hypernym for street, road etc.~~ |
| ~~O~~ | ~~Cross Street Name~~ | | ~~String~~ | ~~-~~ | ~~0-100 chars~~ |  |
| ~~O~~ | ~~ZIP Code~~ | | ~~String~~ | ~~-~~ | ~~0-10 chars~~ | ~~ZIP, PLZ, PIN, CAP, PostalCode, etc.~~ |
| ~~O~~ | ~~Country~~ | | ~~String~~ | ~~-~~ | ~~0-50 chars~~ | ~~Name of country~~ |
| ~~R~~ | ~~Latitude~~ | | ~~Double~~ | ~~-~~ | ~~8 bytes~~ |  |
| ~~R~~ | ~~Longitude~~ | | ~~Double~~ | ~~-~~ | ~~8 bytes~~ |  |
| **~~Response~~** | | | | | | | |
| ~~R~~ | ~~RequestID~~ | | ~~Int32~~ | ~~-~~ | ~~-2147483648 to +2147483647~~ | ~~Corresponding to the RequestID in the request~~ |
| ~~R~~ | ~~Status~~ | | ~~Enum~~ | ~~-~~ | ~~-~~ |  |
|  |  | |  | ~~Success~~ | ~~0x0~~ |  |
|  |  | |  | ~~Reject~~ | ~~0x1~~ |  |

#### MD-REQ-384392/A-setDriveMode

This API is used to request the Drive Mode application to change Drive Modes. The Drive Mode application also uses this API for its response.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | |
| **Method Type** | | One-Shot (Synch) | | | | |
| **QoS Level** | | Default | | | | |
| **Retained** | | No | | | | |
|  | | | | | | |
| **R/O** | **Name** | | **Type** | **Literals** | **Value** | **Description** |
| **Request** | | | | | | |
| R | Drive Mode Request | | Int32 | - | -2147483648 to +2147483647 | Request for a specific drive mode (0-30: SelDrvMde01 - SelDrvMde31) |
| **Response** | | | | | | |
| R | Status | | Enum | - | - | Response to Drive Mode request |
|  |  | |  | Success | 0x0 |  |
|  |  | |  | Fail | 0x1 |  |
|  |  | |  | No Response | 0x2 |  |
|  |  | |  | Invalid Mode | 0x3 |  |

### RKS-IIR-REQ-354841/C-RSServer\_Tx

#### MD-REQ-361426/A-RSCommandResponse

Message Type: FTCP

This message is used to acknowledge the RSOffBoardClient’s command containing the RS Settings payload.

**Note:** Refer to the latest “Ford Telematics Communication Protocol Specification” and Protofile for the most up to date FTCP messages/definitions.

|  |  |
| --- | --- |
| **Command** | **Description** |
| RSCommandResponse | Response sent from the RSServer to the RSOffBoardClient upon receiving the RS Settings payload. |

#### ~~MD-REQ-361429/A-BLECommandResponse~~

~~Message Type: FTCP~~

~~This message is used to acknowledge the RSOffBoardClient’s Command containing the BLE auto-pair key.~~

**~~Note:~~** ~~Refer to the latest “Ford Telematics Communication Protocol Specification” and Protofile for the most up to date FTCP messages/definitions.~~

|  |  |
| --- | --- |
| **~~Command~~** | **~~Description~~** |
| ~~BLECommandResponse~~ | ~~Response sent from the RSServer to the RSOffBoardClient upon receiving the BLE auto-pair key.~~ |

#### MD-REQ-361427/A-RSAlert

Message Type: FTCP

This non correlated alert is used to notify the RSOffBoardClient of different success/failure statuses regarding the RS Settings payload.

**Note:** Refer to the latest “Ford Telematics Communication Protocol Specification” and Protofile for the most up to date FTCP messages/definitions.

|  |  |
| --- | --- |
| **Command** | **Description** |
| RSAlert | Alert sent from the RSServer to the RSOffBoardClient for various RS Settings payload success/failure statuses. |

#### ~~MD-REQ-361430/A-BLEAlert~~

~~Message Type: FTCP~~

~~This non correlated alert is used to notify the RSOffBoardClient of different success/failure statuses regarding the BLE auto-pair key.~~

**~~Note:~~** ~~Refer to the latest “Ford Telematics Communication Protocol Specification” and Protofile for the most up to date FTCP messages/definitions.~~

|  |  |
| --- | --- |
| **~~Command~~** | **~~Description~~** |
| ~~BLEAlert~~ | ~~Alert sent from the RSServer to the RSOffBoardClient for various BLE auto-pair key success/failure statuses.~~ |

#### ~~MD-REQ-370458/B-saveNavLocation~~

~~This API is used to request the Nav Vendor to save a Navigation Favorite. The Nav Vendor also uses this API for its response.~~

|  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | | |
| **~~Method Type~~** | | ~~One-Shot (Synch)~~ | | | | | |
| **~~QoS Level~~** | | ~~Default~~ | | | | | |
| **~~Retained~~** | | ~~No~~ | | | | | |
|  | | | | | | | |
| **~~R/O~~** | **~~Name~~** | | **~~Type~~** | **~~Literals~~** | **~~Value~~** | **~~Description~~** |
| **~~Request~~** | | | | | | | |
| ~~R~~ | ~~RequestID~~ | | ~~Int32~~ | ~~-~~ | ~~-2147483648 to +2147483647~~ |  |
| ~~R~~ | ~~Location Name~~ | | ~~String~~ | ~~-~~ | ~~0-200 chars~~ |  |
| ~~O~~ | ~~Phone Number~~ | | ~~String~~ | ~~-~~ | ~~0-20 chars~~ |  |
| ~~O~~ | ~~City~~ | | ~~String~~ | ~~-~~ | ~~0-50 chars~~ | ~~Hypernym for e.g. city/village~~ |
| ~~O~~ | ~~SubCity~~ | | ~~String~~ | ~~-~~ | ~~0-50 chars~~ | ~~Hypernym for e.g. district~~ |
| ~~O~~ | ~~State~~ | | ~~String~~ | ~~-~~ | ~~0-100 chars~~ | ~~Portion of country (e.g. state, province)~~ |
| ~~O~~ | ~~Door Number~~ | | ~~String~~ | ~~-~~ | ~~0-50 chars~~ | ~~Portion of thoroughfare e.g. house number~~ |
| ~~O~~ | ~~Street Name~~ | | ~~String~~ | ~~-~~ | ~~0-100 chars~~ | ~~Hypernym for street, road etc.~~ |
| ~~O~~ | ~~Cross Street Name~~ | | ~~String~~ | ~~-~~ | ~~0-100 chars~~ |  |
| ~~O~~ | ~~ZIP Code~~ | | ~~String~~ | ~~-~~ | ~~0-10 chars~~ | ~~ZIP, PLZ, PIN, CAP, PostalCode, etc.~~ |
| ~~O~~ | ~~Country~~ | | ~~String~~ | ~~-~~ | ~~0-50 chars~~ | ~~Name of country~~ |
| ~~R~~ | ~~Latitude~~ | | ~~Double~~ | ~~-~~ | ~~8 bytes~~ |  |
| ~~R~~ | ~~Longitude~~ | | ~~Double~~ | ~~-~~ | ~~8 bytes~~ |  |
| **~~Response~~** | | | | | | | |
| ~~R~~ | ~~RequestID~~ | | ~~Int32~~ | ~~-~~ | ~~-2147483648 to +2147483647~~ | ~~Corresponding to the RequestID in the request~~ |
| ~~R~~ | ~~Status~~ | | ~~Enum~~ | ~~-~~ | ~~-~~ |  |
|  |  | |  | ~~Success~~ | ~~0x0~~ |  |
|  |  | |  | ~~Reject~~ | ~~0x1~~ |  |

#### MD-REQ-384392/A-setDriveMode

This API is used to request the Drive Mode application to change Drive Modes. The Drive Mode application also uses this API for its response.

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
|  | | | | | | |
| **Method Type** | | One-Shot (Synch) | | | | |
| **QoS Level** | | Default | | | | |
| **Retained** | | No | | | | |
|  | | | | | | |
| **R/O** | **Name** | | **Type** | **Literals** | **Value** | **Description** |
| **Request** | | | | | | |
| R | Drive Mode Request | | Int32 | - | -2147483648 to +2147483647 | Request for a specific drive mode (0-30: SelDrvMde01 - SelDrvMde31) |
| **Response** | | | | | | |
| R | Status | | Enum | - | - | Response to Drive Mode request |
|  |  | |  | Success | 0x0 |  |
|  |  | |  | Fail | 0x1 |  |
|  |  | |  | No Response | 0x2 |  |
|  |  | |  | Invalid Mode | 0x3 |  |

# General Requirements

## RKS-REQ-361373/B-FTCP Specification References

The following FTCP specifications define the FTCP alerts/commands mentioned in this SPSS, as well as the protocol used to transmit them via the RSServer:

* Ford Telematics Communication Protocol Specification
* FNV2-FCI Protocol SPSS

## RKS-REQ-361339/B-Security Specification Reference

The RSServer shall comply with the security requirements per “Rocket Setup On-Board Security Specification”

## RKS-REQ-361338/B-Feature Configuration

The RSServer shall have a configurable parameter/DID to allow the Rocket Setup feature to be enabled/disabled.

* When the parameter indicates that Rocket Setup is enabled, all the functionality and signals defined in this SPSS shall be supported.
* When the parameter indicates that Rocket Setup is disabled, none of the functionality defined in this SPSS shall be supported.
  + The default value for this parameter shall be Disabled.

## RKS-REQ-362420/C-RS Settings – RSServer Module Swap

If the RSServer detects a new VIN via the VehicleGGCCData message upon an Ignition Cycle (transition from IgnitionStatus = Off to Run), it shall delete the saved RS Settings payload and BLE payload if not yet applied.

## RKS-REQ-362421/B-RS Settings – Rocket Setup Disabled on RSServer

If the Rocket Setup feature is disabled (per REQ-361338) on the RSServer, the RSServer shall delete the saved RS Settings payload if not yet applied.

## RKS-REQ-364451/A-RS Settings Feature Numbers/Structure

The RS Settings are structured as a value pair of ‘Feature Number’ (also called LabelID in the FTCP protofile) and ‘Data Value’ (also called Label Value in the FTCP protofile). Each RS Setting is assigned their own Feature Number per the “Rocket Setup Data Elements” document. The RS Settings payload shall be formatted and received by the RSServer in a .proto structure.

# Functional Definition

## ~~RKS-FUN-REQ-384393/A-BLE Download~~

### ~~Use Cases~~

#### ~~RKS-UC-REQ-384395/B-BLE Payload downloaded to RSServer when awake~~

|  |  |
| --- | --- |
| **~~Actors~~** | ~~Vehicle Purchaser, RSOffBoardClient, RSServer~~ |
| **~~Pre-conditions~~** | ~~Powermode conditions are met~~  ~~VIN added to Garage (manual process) OR Initial Order Complete (auto process)~~ |
| **~~Scenario Description~~** | ~~User selects Rocket Setup tile in the mobile app, personalizes settings, and presses submit. BLE Payload is created and sent to RSServer.~~ |
| **~~Post-conditions~~** | ~~BLE Payload is downloaded to the RSServer.~~ |
| **~~List of Exception Use Cases~~** | ~~REQ-384396-BLE Payload fails Payload Check(s)~~ |
| **~~Interfaces~~** | ~~FTCP, SoA~~ |

#### ~~RKS-UC-REQ-384396/B-BLE Payload fails Payload Check(s)~~

|  |  |
| --- | --- |
| **~~Actors~~** | ~~RSOffBoardClient, RSServer~~ |
| **~~Pre-conditions~~** | ~~Powermode conditions are met~~  ~~BLE payload submitted~~ |
| **~~Scenario Description~~** | ~~BLE Payload is sent to RSServer. BLE Payload is corrupt, or timestamp is old.~~ |
| **~~Post-conditions~~** | ~~BLE payload fails the payload checks and fails to persist on the RSServer. RSServer requests another download.~~ |
| **~~List of Exception Use Cases~~** |  |
| **~~Interfaces~~** | ~~FTCP, SoA~~ |

### ~~Requirements~~

#### ~~RKS-REQ-384397/B-BLE Payload Download – BLECommand~~

~~The RSServer shall receive and save (pending REQ-384402 & REQ-384403) the BLE Payload~~~~contained within the BLECommand from the RSOffBoardClient. The RSServer shall delete any previously saved BLE Payloads or RS Payloads upon reception of the BLECommand.~~

~~The RSOffBoardClient is able to send multiple BLECommands to the RSServer. The RSServer shall perform all checks upon reception of a new BLECommand (as if it was the first one received).~~

#### ~~RKS-REQ-384398/A-BLE Payload Download – SyncP Wrapped~~

~~The RSServer shall receive the BLE payload SyncP wrapped (secured using SyncP v1) within the BLECommand from the RSOffBoardClient. Refer to “S13a SyncP Functional Specification” for more details.~~

#### ~~RKS-REQ-384399/A-BLE Payload Download – Persistence~~

~~The RSServer shall persist the BLE payload until:~~

* ~~The RS Settings have been successfully applied (until the RS Process successfully completes, see REQ-361353), OR~~
* ~~T\_Persist has been reached~~

~~Once the RS Settings have been applied, or if the RS Settings have not been applied within T\_Persist after having received/stored the RS Settings payload, the BLE payload shall be deleted.~~

~~The only exception to the above is the timestamp. The RSServer shall persist the timestamp permanently for use in the timestamp check (see REQ-384402). The BLE payload shall be persisted through ignition cycles, battery disconnects, loss of power, etc.~~

#### ~~RKS-REQ-384400/A-BLE Payload Download – Persistence Timer~~

~~The RSServer shall persist the BLE payload for T\_Persist (REQ-361379).~~

#### ~~RKS-REQ-384401/A-BLE Payload Download – Payload Timestamp~~

~~The BLE payload contains a timestamp to indicate the freshness of the BLE data. The timestamp format shall follow the ISO 8601 standard:~~

* ~~Format (for reference): YYYY-MM-DDThh:mm:ssTZD~~
* ~~Example (for reference) 2019-04-09T19:20:30+01:00~~

#### ~~RKS-REQ-384402/A-BLE Payload Download – Timestamp Check~~

~~The RSServer shall check the timestamp upon reception of the BLECommand. The check shall confirm whether:~~

* ~~The timestamp is valid~~
* ~~The timestamp is newer than that of the last received/saved BLE payload~~

#### ~~RKS-REQ-384403/A-BLE Payload Download – Payload Check~~

~~The RSServer shall check the BLE payload content upon reception of the BLECommand. The check shall confirm whether:~~

* ~~The payload contents are readable~~
* ~~The payload contents have not been modified in transit (per SyncP header)~~

#### ~~RKS-REQ-384404/A-BLE Payload Download – Failure~~

~~The RSServer shall fail and not persist the BLE payload from the BLECommand when:~~

* ~~The BLE payload fails the Payload Check, OR~~
* ~~The BLE payload fails the Timestamp Check, OR~~
* ~~The RocketSetupComplete flag is set “True” when the BLECommand is received~~

#### ~~RKS-REQ-384405/A-BLE Payload Download – Failure Retry~~

~~When the RSServer fails to persist the BLE payload from the BLECommand due to a failed Timestamp or Payload Check, the RSServer shall send a BLEAlert to the RSOffBoardClient indicating “AutoPair Failed” due to “Payload Corrupt” (triggering a redownload).~~

~~This retry shall only occur once.~~

~~If the Timestamp Check fails again (or if both Checks fail):~~

* ~~The RSServer shall discard the BLE Payload~~
* ~~The RSServer shall send a BLEAlert to the RSOffBoardClient indicating “AutoPair Failed” due to “Payload Corrupt” (no re-download)~~

~~If the Payload Check fails again:~~

* ~~The RSServer shall discard the BLE payload~~
* ~~The RSServer shall send a BLEAlert to the RSOffBoardClient indicating “AutoPair Failed” due to “Payload Corrupt” (no re-download)~~

#### ~~RKS-REQ-384406/B-BLE Payload Download – BLECommandResponse~~

~~The RSServer shall send BLECommandResponse to the RSOffBoardClient after reception of the BLECommand, indicating successful reception of the BLECommand.~~

#### ~~RKS-REQ-384408/B-BLE Payload MAI and RS Payload Profile ID Check~~

~~Once both the BLE Payload and RS Settings payload have been received, the RSServer shall check that the MAI in the BLE payload matches the Profile ID (Feature Number 0x0028) provided in the RS Settings payload.~~

* ~~If the two match, no BLEAlert shall be sent.~~
* ~~If the two do not match, the RSServer shall send a BLEAlert to the RSOffBoardClient indicating “AutoPair Failed” due to “Payload Corrupt.” The RSServer shall then delete both the BLE Payload and the RS Payload.~~

#### ~~RKS-REQ-388562/A-BLE Payload Download - Rejecting BLECommand~~

~~The RSServer shall reject any incoming BLECommands while the RS Process is in progress (once the user has been validated and the RS Welcome Screen has been displayed). The RSServer shall send a BLECommandResponse to the RSOffBoardClient indicating “Failed” due to “Command Already In Progress” during this time.~~

~~The RSServer shall accept BLECommands when the RS Process is not in progress, as long as the RocketSetupComplete flag is not set to true (see REQ-362419).~~

## RKS-FUN-REQ-361370/A-RS Download

### Use Cases

#### RKS-UC-REQ-361471/D-RS Settings downloaded to RSServer when awake (China: When account logged in)

|  |  |
| --- | --- |
| **Actors** | Vehicle Purchaser, RSOffBoardClient, RSServer |
| **Pre-conditions** | Powermode conditions are met  VIN added to Garage (manual process) OR Initial Order Complete (auto process) |
| **Scenario Description** | User selects Rocket Setup tile in the mobile app, personalizes settings, and presses submit. RS Settings payload is sent to RSServer.  (China: RS download request was sent from RS server once account was logged in on IVI) |
| **Post-conditions** | RS Settings payload is downloaded to the RSServer. |
| **List of Exception Use Cases** | REQ-361473-RS Settings payload fails Payload Check(s) |
| **Interfaces** | FTCP, SoA |

#### RKS-UC-REQ-361473/C-RS Settings payload fails Payload Check(s)

|  |  |
| --- | --- |
| **Actors** | RSOffBoardClient, RSServer |
| **Pre-conditions** | Powermode conditions are met  RS Settings payload submitted |
| **Scenario Description** | RS Settings are sent to RSServer. RS Settings payload is corrupt, or timestamp is old. |
| **Post-conditions** | RS Settings payload fails the payload checks and fails to persist on the RSServer. RSServer requests another download. |
| **List of Exception Use Cases** |  |
| **Interfaces** | FTCP |

### Requirements

#### RKS-REQ-361342/C-RS Settings Download – RSCommand

The RSServer shall receive and save (pending REQ-361449 & REQ-361347) the RS Settings payload contained within the RSCommand from the RSOffBoardClient. The RSServer shall delete any previously saved RS Payloads or BLE Payloads upon reception of the RSCommand.

The RSOffBoardClient is able to send multiple RSCommands to the RSServer. The RSServer shall reset T\_Persist, reset the Postpone Counter, and perform all checks upon reception of a new RSCommand (as if it was the first one received).

#### RKS-REQ-361343/A-RS Settings Download – SyncP Wrapped

The RSServer shall receive the RS Settings payload SyncP wrapped (**secured using SyncP v1**) within the RSCommand from the RSOffBoardClient. Refer to “S13a SyncP Functional Specification” for more details.

#### RKS-REQ-361344/B-RS Settings Download – Persistence

~~The RSServer shall persist the RS Settings payload until:~~

* ~~The RS Settings have been successfully applied (until the RS Process successfully completes, see REQ-361353), OR~~
* ~~T\_Persist has been reached~~

~~Once the RS Settings have been applied, or if the RS Settings have not been applied within T\_Persist after having received/stored the RS Settings payload, the RS Settings payload shall be deleted.~~ (China: RS setting will not be deleted on IVI)

The only exception to the above is the timestamp. The RSServer shall persist the timestamp permanently for use in the timestamp check (see REQ-361346). The RS Settings payload shall be persisted through ignition cycles, battery disconnects, loss of power, etc.

#### ~~RKS-REQ-361345/B-RS Settings Download – Persistence Timer~~

~~The RSServer shall have a timer to monitor how long it shall persist the RS Settings payload. The timer shall be persisted through ignition cycles, battery disconnects, loss of power, etc. The max time to persist shall be defined by T\_Persist.~~ (China: RSServer don’t need to monitor download timer. )

#### RKS-TMR-REQ-361379/B-T\_Persist

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Name** | **Description** | **Units** | **Range** | **Resolution** | **Default** |
| T\_Persist | The maximum time the RSServer shall persist the RS Settings payload (1 day = 86400 sec)  Note: Use the default value. | sec | 86400-1728000 | 86400 | 864000 |

#### ~~RKS-REQ-361346/B-RS Settings Download – Payload Timestamp~~

~~The RS Settings payload contains a timestamp to indicate the freshness of the RS Settings data. The timestamp format shall follow the ISO 8601 standard:~~

* ~~Format (for reference): YYYY-MM-DDThh:mm:ssTZD~~
* ~~Example (for reference) 2019-04-09T19:20:30+01:00~~

#### ~~RKS-REQ-361449/A-RS Settings Download – Timestamp Check~~

~~The RSServer shall check the timestamp upon reception of the RSCommand. The check shall confirm whether:~~

* ~~The timestamp is valid~~
* ~~The timestamp is newer than that of the last received/saved RS Settings payload~~

#### RKS-REQ-361347/A-RS Settings Download – Payload Check

The RSServer shall check the RS Settings payload content upon reception of the RSCommand. The check shall confirm whether:

* The payload contents are readable
* The payload contents and parameter values are within the bounds identified in this SPSS
* The payload contents have not been modified in transit (per SyncP header)

#### RKS-REQ-362418/B-RS Settings Download – Failure

The RSServer shall fail and not persist the RS Settings payload from the RSCommand when:

* The RS Settings payload fails the Payload Check, OR
* ~~The RS Settings payload fails the Timestamp Check, OR~~ (China: Timestamp check not needed as we directly download profile once user login IVI. There shall be no GAP between download and application.)
* The RocketSetupComplete flag is set “True” when the RSCommand is received

#### RKS-REQ-364357/A-RS Settings Download - Failure Retry

When the RSServer fails to persist the RS Settings payload from the RSCommand due to a failed Timestamp or Payload Check, the RSAlert sent to the RSOffBoardClient shall request a re-download of the RS Settings payload (see REQ-361349).

This retry shall only occur once.

If the Timestamp Check fails again (or if both Checks fail):

* The RSServer shall discard the RS Settings payload
* The RSServer shall send an RSAlert to the RSOffBoardClient indicating “Failed” (no re-download)

If the Payload Check fails again:

* The RSServer shall apply the successful RS Settings in the payload (if any)
  + For the settings that have defaults defined in this SPSS (ex. Profile Name, Photo, etc.), those shall be used if the respective RS Setting failed
  + For the settings that have no defaults defined in this SPSS (ex. Radio Presets, Navigation Locations, etc.), that RS Setting shall be skipped
* The RSServer shall send an RSAlert to the RSOffBoardClient indicating “Applied”

#### RKS-REQ-361348/B-RS Settings Download – RSCommandResponse

The RSServer shall send RSCommandResponse to the RSOffBoardClient after reception of the RSCommand, indicating successful reception of the RSCommand.

#### RKS-REQ-361349/B-RS Settings Download – RSAlert

The RSServer shall send an RSAlert to the RSOffBoardClient to indicate any of the following:

1. That the RS Settings payload has failed to be applied. This may be due to one of the following reasons:
   * The payload is corrupt/invalid or timestamp is old/invalid (“Payload Corrupted”)
     + This shall trigger a re-download from the RSOffBoardClient
   * Master Reset has been performed (“Master Reset Interrupted”)
     + This may trigger a re-download from the RSOffBoardClient
2. That the RS Settings payload has been successfully applied
   * An additional indicator of “No User Response” shall also be sent per REQ-361357

#### RKS-REQ-367354/B-RS Settings Download - Rejecting RSCommand

The RSServer shall reject any incoming RSCommands while the RS Process is in progress (once the user has been validated and the RS Welcome Screen has been displayed). The RSServer shall send an RSCommandResponse to the RSOffBoardClient indicating “Failed” due to “Command Already In Progress”during this time.

The RSServer shall accept RSCommands when the RS Process is not in progress, as long as the RocketSetupComplete flag is not set to true (see REQ-362419).

## RKS-FUN-REQ-361371/A-RS Process

### Use Cases

#### RKS-UC-REQ-361474/B-User accepts and continues RS process on RSServer

|  |  |
| --- | --- |
| **Actors** | Vehicle Occupant, RSOffBoardClient, RSServer |
| **Pre-conditions** | Powermode conditions are met  RS Settings downloaded  User is validated |
| **Scenario Description** | User is presented with RS Welcome screen and presses Accept. (China: User press “Download/apply setting from Cloud” on IVI. |
| **Post-conditions** | RSServer continues RS process and leads user to create a Driver Profile. Upon completion, Driver Profile is created and all RS Settings are applied. (China: RSServer Trigger download/apply process for RS setting. ) |
| **List of Exception Use Cases** |  |
| **Interfaces** | G-HMI, FTCP, CAN, SoA |

#### RKS-UC-REQ-361475/C-User accepts and fails to complete RS process on RSServer

|  |  |
| --- | --- |
| **Actors** | Vehicle Occupant, RSServer |
| **Pre-conditions** | Powermode conditions are met  RS Settings downloaded  User is validated |
| **Scenario Description** | User is presented with RS Welcome screen and presses Accept. RSServer continues RS process and leads user to create a Driver Profile. User leaves/aborts the RS process. |
| **Post-conditions** | RSServer aborts RS process and offers a retry at the next ignition cycle.  Postpone Counter is not incremented. (China: Sync+ will not reload user onboard process again if user quit the process for the first time. ) |
| **List of Exception Use Cases** |  |
| **Interfaces** | G-HMI, FTCP |

#### RKS-UC-REQ-361476/C-User denies RS process on RSServer

|  |  |
| --- | --- |
| **Actors** | Vehicle Occupant, RSServer |
| **Pre-conditions** | Powermode conditions are met  RS Settings downloaded  User is validated |
| **Scenario Description** | User is presented with RS Welcome screen and presses Deny |
| **Post-conditions** | RSServer exits the RS process (the Welcome Screen, at this stage of the process), and deletes the RS Payload and BLE Payload. No retries are given for these payloads. User must re-submit their Settings via the mobile app. (China: user either start the download process or skip the process. There will not be Deny operation.) |
| **List of Exception Use Cases** |  |
| **Interfaces** | G-HMI, FTCP |

#### ~~RKS-UC-REQ-361477/C-User postpones RS process on RSServer~~

|  |  |
| --- | --- |
| **~~Actors~~** | ~~Vehicle Occupant, RSServer~~ |
| **~~Pre-conditions~~** | ~~Powermode conditions are met~~  ~~RS Settings downloaded~~  ~~User is validated~~  ~~Retry counter is not maxed out~~ |
| **~~Scenario Description~~** | ~~User is presented with RS Welcome screen and presses Postpone~~ |
| **Post-conditions** | RSServer exits the RS process and offers a retry at next ignition cycle.  Postpone Counter is incremented. (China: there will not be postpone operation on SYNC+ IVI). |
| **List of Exception Use Cases** |  |
| **Interfaces** | G-HMI, FTCP |

#### ~~RKS-UC-REQ-361479/B-RS & Master Reset – Before RS Settings applied~~

|  |  |
| --- | --- |
| **~~Actors~~** | ~~Vehicle Occupant, RSOffBoardClient, RSServer~~ |
| **~~Pre-conditions~~** | ~~Powermode conditions are met~~  ~~RS Settings downloaded~~ |
| **~~Scenario Description~~** | ~~User navigates to Reset menu and presses Master Reset~~ |
| **~~Post-conditions~~** | ~~RSServer deletes the RS Settings, reboots, and sends RSAlert. RSOffBoardClient determines whether to send another payload.~~ |
| **~~List of Exception Use Cases~~** |  |
| **~~Interfaces~~** | ~~G-HMI, FTCP~~ |

#### RKS-UC-REQ-361480/C-RS & Master Reset – After RS Settings applied

|  |  |
| --- | --- |
| **Actors** | Vehicle Occupant, RSServer, RSOffBoardClient |
| **Pre-conditions** | Powermode conditions are met  RS Settings downloaded and applied |
| **Scenario Description** | User navigates to Reset menu and presses Master Reset |
| **Post-conditions** | RSServer deletes all data per Master Reset, reboots, and sends RSAlert.  RSOffBoardClient does not send another payload. (China: When MR was done, the redownload/application was enabled again. And if user do user account login again on IVI. The download shall be triggered again.) |
| **List of Exception Use Cases** |  |
| **Interfaces** | G-HMI, FTCP |

### Requirements

#### RKS-REQ-361353/A-RS Process

The RSServer shall implement and monitor an “RS Process” which is the in-vehicle procedure (start to finish) required to successfully complete the application of RS Settings. This process shall begin with the offering of the RS Welcome Screen and end with the successful creation of an Enhanced Memory Profile.

#### RKS-REQ-361340/A-Powermode Conditions – RS Settings Application

The RSServer shall allow the RS Settings to be applied only when the following preconditions are met (same preconditions as Enhanced Memory (see ENMEM-REQ-099699):

* IgnitionStatus\_St = Run
* GearPosition = Park
* VehicleSpeed <= Driver Restrictions Threshold

#### RKS-REQ-361350/A-HMI – Display RS Welcome Screen

The RSServer shall display the RS Welcome Screen when the identified user has been validated (by either BLE Auto-pairing or Manual BT pairing). Account login for China.

#### RKS-REQ-361352/A-HMI – RS Welcome Screen Button Selections

The RSServer shall display and allow the user to select one of the below inputs on the RS Welcome Screen (not literal button text):

* Accept
* Deny
* Postpone

(China: RS application welcome screen will be prompted together with “New Customer Onboard Process” on SYNC+)

#### RKS-REQ-361351/C-Validate Identified User

~~The RSServer shall validate the identified user (via BLE) by comparing the MAID from the BLE pairing process (see BT Phone SPSS) against the Profile ID (Feature Number 0x0028) provided in the RS Settings payload.~~

~~If the identified user cannot be validated, the RSServer shall not show the RS Welcome Screen.~~

(China: User was identified/validated via account login process.)

#### RKS-REQ-361354/A-RS Process Abort - Conditions

The RS Process shall utilize the abort conditions of Enhanced Memory (see ENMEM-REQ-116802).

For reference (refer to Enhanced Memory SPSS for the most up to date conditions):

* IgnitionStatus\_St != Run
* GearPosition != Park
* VehicleSpeed > Driver Restrictions threshold
* User initiates an HMI domain change
* Infotainment System Reset

#### RKS-REQ-361355/C-RS Process Abort - Retry Strategy

If the RS Process is aborted any time after the user selects Accept, or if the RS Welcome Screen itself is aborted/closed without user input, the RSServer shall continue to save the RS Settings until a subsequent and successful RS Process attempt is made. The retry strategy for an abort shall follow the same strategy as indicated in REQ-361360. However, an abort event shall not result in an increment of the Postpone Counter.

Note: Upon an abort, any progress made within the Enhanced Memory profile creation process is deleted, a profile will not be created (see ENMEM-REQ-116802).

#### RKS-REQ-372250/A-RS Process Pause

The RSServer shall pause the application process (ex. applying of radio presets) as permitted by Enhanced Memory. One example of this is during an incoming/accepted phone call.

#### RKS-REQ-361356/C-RS Process - Accept

When Accept is selected on the RSServer, the RSServer shall initiate/use the existing Enhanced Memory profile creation process. The RSServer shall:

* Enable the Enhanced Memory feature if no prior profiles have been created
* Parse the RS Settings payload as needed/required
* Preload the Driver Profile Name with that from the RS Settings
* Preload the Photo/Avatar Selection with that from the RS Settings
* If no DSM is present, automatically select and use the next available PersIndex for the remainder of the profile creation process
* Apply the rest of the RS Settings per REQ-362423
* Send the RSAlert to the RSOffBoardClient indicating “Applied”

#### RKS-REQ-361357/B-RS Process - Deny

When Deny is selected on the RSServer, the RSServer shall not apply the RS Settings or create a Driver Profile, but shall instead:

* Delete the saved RS Settings
* Send the RSAlert to the RSOffBoardClient indicating “Failed” due to ”No User Response”

(China: No deny option. If user don’t click “download and apply Setting from cloud” on IVI. The RS download/application will be skipped.)

#### RKS-REQ-361358/A-RS Process - Postpone (under N\_Postpone)

~~When Postpone is selected on the RSServer and N\_Postpone has not been reached, the RSServer shall:~~

* ~~Close the RS Welcome Screen~~
* ~~Increment the Postpone counter~~

(China: No postpone option. If user don’t click “download and apply Setting from cloud” on IVI. The RS download/application will be skipped.)

#### RKS-REQ-361360/B-RS Process – Postpone Retry

When Postpone is selected, a retry strategy shall be performed. The retry strategy is as follows:

1. If the Postpone counter is less than N\_Postpone (Counter < N\_Postpone), the RSServer shall display the RS Welcome Screen to the user at the next Ignition Cycle (transition from IgnitionStatus = Off to Run), so long as the user has first been validated per REQ-361351. If not validated, the RS Welcome Screen shall not be shown.
2. If the Postpone counter is equal to N\_Postpone (Counter = N\_Postpone), the RSServer shall offer the RS Welcome Screen as in #1, but not include/show the Postpone button (only Accept/Deny).

(China: No postpone option. If user don’t click “download and apply Setting from cloud” on IVI. The RS download/application will be skipped.)

#### RKS-REQ-361361/A-RS Process – Postpone Counter

The RSServer shall have a counter to monitor the number of postpone retries the user has completed. The counter shall be persisted through ignition cycles, battery disconnects, loss of power, etc. The number of retries offered shall be defined by N\_Postpone.

(China: No postpone option. If user don’t click “download and apply Setting from cloud” on IVI. The RS download/application will be skipped.)

#### RKS-REQ-361398/A-N\_Postpone

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Name** | **Description** | **Units** | **Range** | **Resolution** | **Default** |
| N\_Postpone | Maximum number of postpone retries offered to the user.  Note: Use the default value. |  | 0-30 | 1 | 20 |

#### RKS-REQ-362419/B-RS Process – Rocket Setup Complete Flag

When the RS Process is complete, the RS Settings have been applied, and an Enhanced Memory Driver Profile has been created, the RSServer shall set a completion flag true, RocketSetupComplete = True. This flag shall be set to False by default until the above has occurred. The RSServer shall persist the flag through ignition cycles, battery disconnects, loss of power, software updates, etc.). This flag shall be cleared (set to False) when a Master Reset is performed.

When the RocketSetupComplete flag is set to True, any subsequent RS Settings payloads and RSCommand’s containing new RS Settings received by the RSServer shall be ignored and not applied. The RSServer shall send an RSCommandResponse indicating “Failed” due to “Command Not Permitted” in this case. Only one profile shall be successfully applied for the life of the RSServer.

#### ~~RKS-REQ-361362/B-Master Reset before RS Process Success~~

~~If a Master Reset occurs before the RSServer has successfully completed the RS Process, the RSServer shall:~~

* ~~Delete the RS Settings payload~~
* ~~Reset all counters and timers specific to this feature (ex. N\_Postpone, T\_Persist)~~
* ~~Send the RSAlert to the RSOffBoardClient indicating “Failed” due to “Master Reset Interrupted”~~

**~~Note~~**~~: The RSOffBoardClient will determine whether a re-download is to be performed or not (this is based on a timer it maintains and initiates when the purchase event occurs).~~

#### RKS-REQ-361363/C-Master Reset after RS Process Success

If a Master Reset occurs any time after the RSServer has successfully completed the RS Process, the RSServer shall:

* Delete the RS Settings payload if it has not yet already been deleted
* Reset all counters and timers specific to this feature (ex. N\_Postpone, T\_Persist)
* Reset the Rocket Setup Complete Flag
* Send the RSAlert to the RSOffBoardClient indicating “Failed” due to “Master Reset Interrupted”

**Note:** The RSAlert is sent anytime a Master Reset is performed (whether the RS Process has been completed or not, see REQ-361362).

## RKS-FUN-REQ-361374/A-Applying RS Settings

### Use Cases

#### RKS-UC-REQ-362592/A-RSServer applies RS Settings

|  |  |
| --- | --- |
| **Actors** | RSServer, RSClient |
| **Pre-conditions** | Powermode conditions are met  RS Settings downloaded  User Accepted RS Welcome screen  RS Process in progress |
| **Scenario Description** | RSServer begins to apply RS Settings within the Enhanced Memory Driver Profile creation process. RSServer steps through each of the RS Settings, requesting to save each either internally or from the applicable RSClient(s). |
| **Post-conditions** | RSServer and RSClient(s) save the requested RS Setting. |
| **List of Exception Use Cases** |  |
| **Interfaces** | G-HMI, CAN, SoA |

### Requirements

#### RKS-REQ-362423/A-RS Settings – Time to Apply the RS Settings

During the RS Process, the RSServer shall only apply the RS Settings after the following has occurred (events from Enhanced Memory):

1. The Copy Operation has been issued (per ENMEM-REQ-198923-Copy Request)
2. All profile data required by Enhanced Memory has been saved (per ENMEM-REQ-198920-Execute Copy Operation)
3. A Recall of the new driver profile has been requested (per ENMEM-REQ-198918B-Recall New Driver Profile After Copy)
4. All profile data for the recalled profile has been loaded (per ENMEM-REQ-099673-Driver Profile Settings Recall)

**Note**: Once the recall is complete, the RS Settings will be applied to the active profile. The newly created profile must be active before applying the RS Settings; otherwise, the RS Settings will be applied to the previously active profile. The RS Settings will then be saved to the active profile when the RSServer and RSClients persist their settings per Enhanced Memory.

#### Profile Name

##### RKS-REQ-361364/A-RS Settings – Profile Name

The RSServer shall receive one Profile Name from the RS Settings payload.

##### RKS-REQ-362424/B-RS Settings – Profile Name Format

The RSServer shall receive the Profile Name in String format and it shall consist of no more than 20 characters.

|  |  |  |  |
| --- | --- | --- | --- |
| **RS Setting** | **RS Setting Payload – Packet Format** | | **Range**  **(in-vehicle)** |
| **Feature Number (FeatNum)** | **Data Value (DatVal)** |
| Profile Name | 0x0024 | String | 0-20 chars |

##### RKS-REQ-362425/B-RS Settings – Profile Name Usage

During the RS Process, the RSServer shall use/preload 0x0024:”DataValue” in:

* the RS Welcome Screen greeting
* the Enhanced Memory Driver Profile Name entry screen

##### RKS-REQ-362426/A-RS Settings – Profile Name Edit

The RSServer shall allow the user to edit the Profile Name in the Enhanced Memory Driver Profile Name entry screen (as per normal Enhanced Memory procedure). If the user decides to change the Profile Name, the new name shall be used for the remainder of the RS Process.

(China: China IVI UX flow does not have profile name edit.)

##### RKS-REQ-362427/B-RS Settings – Failure to Apply Profile Name

If the RSServer cannot save or use the requested Profile Name for whatever reason (parameters invalid, parameters corrupt, etc.), the RSServer shall not display or prepopulate any Profile Name as required in REQ-362425. The RSServer shall instead:

* Display “Welcome” in the RS Welcome Screen
* Not populate a Profile Name in the Enhanced Memory Driver Profile Name entry screen (rely on the user to manually enter a profile name)

#### Profile Photo

##### RKS-REQ-361365/A-RS Settings – Profile Photo

The RSServer shall receive one Profile Photo from the RS Settings payload as well as a URL from which a larger photo/image may be accessed (URL not currently used).

(China: the RS server shall receive one profile photo which is translated and re-translate to image type on IVI.)

##### RKS-REQ-362428/D-RS Settings – Profile Photo Format

The RSServer shall receive the Profile Photo in Bytes and shall be no larger than 80 KB.

* The photo format may be of the following types: Jpeg, PNG
* The photo may be encoded using the following encoding type: Base 64

The RSServer shall receive the Profile Photo URL in String format and shall be no larger than 40 characters (URL not currently used).

|  |  |  |  |
| --- | --- | --- | --- |
| **RS Setting** | **RS Setting Payload – Packet Format** | | **Range**  **(in-vehicle)** |
| **Feature Number (FeatNum)** | **Data Value (DatVal)** |
| Profile Photo | 0x0025 | Bytes | 80kb |
| Profile Photo URL | 0x0026 | String | 0-40 chars |

##### RKS-REQ-362429/C-RS Settings – Profile Photo Usage

During the RS Process, the RSServer shall use/preload the 0x0025:”DataValue” in:

* the Enhanced Memory Driver Profile Photo entry screen

##### RKS-REQ-362430/A-RS Settings – Profile Photo Edit

The RSServer shall allow the user to edit the Profile Photo in the Enhanced Memory Driver Profile Photo entry screen. If the user decides to change the Profile Photo, the new photo shall be used for the remainder of the RS Process.

##### RKS-REQ-362431/B-RS Settings – Failure to Apply Profile Photo

If the RSServer cannot save or use the requested Profile Photo for whatever reason (parameters invalid, parameters corrupt, etc.), the RSServer shall use the “Profile Name Initials” avatar as the default Profile Photo.

#### Avatar Selection

##### RKS-REQ-388450/A-RS Settings – Avatar Selection

The RSServer shall receive one Avatar Selection from the RS Settings payload. The Avatar Selection shall indicate a selection of Profile Name Initials, Profile Photo (see REQ-361365), or an Avatar Image selection of Image 1-6. The Avatar Image selection shall align with the list of Avatars available in the Enhanced Memory Profile Creation Process.

##### RKS-REQ-388451/A-RS Settings – Avatar Selection Format

The RSServer shall receive the Avatar Selection in integer format as described below:

|  |  |  |  |
| --- | --- | --- | --- |
| **RS Setting** | **RS Setting Payload – Packet Format** | | **Range**  **(in-vehicle)** |
| **Feature Number (FeatNum)** | **Data Value (DatVal)** |
| Avatar Selection | 0x0029 | 0x0 – 0x7 | 0x0: Profile Name initials  0x1: Profile Photo  0x2: Avatar Image 1  0x3: Avatar Image 2  …  0x7: Avatar Image 6 |

##### RKS-REQ-388452/A-RS Settings – Avatar Selection Usage

During the RS Process, the RSServer shall use/preload the 0x0029:”DataValue” in the Enhanced Memory Driver Profile Photo entry screen:

* If 0x0029:”DataValue” = 0x0, the Profile Name Initials shall be used
* If 0x0029:”DataValue” = 0x1, the Profile Photo shall be used, as provided in 0x0025:”DataValue”
* If 0x0029:”DataValue” = 0x2-7, the corresponding Avatar Image 1-6 shall be used

##### RKS-REQ-388453/A-RS Settings – Avatar Selection Edit

The RSServer shall allow the user to change Avatar Selection in the Enhanced Memory Driver Profile Photo entry screen. If the user decides to change the Avatar Selection, the new selection shall be used for the remainder of the RS Process.

##### RKS-REQ-388454/A-RS Settings – Failure to Apply Avatar Selection

If the RSServer cannot save or use the requested Avatar Selection for whatever reason (parameters invalid, parameters corrupt, etc.), the RSServer shall use the “Profile Name Initials” avatar as the default Profile Photo.

#### Navigation Favorites

##### RKS-REQ-361366/B-RS Settings – Navigation Favorites

The RSServer shall receive one Home Favorite, one Work Favorite (if applicable), and up to ten additional Favorites from the RS Settings payload.

##### RKS-REQ-362432/C-RS Settings – Navigation Favorites Parameters/Format

The RSServer shall receive the Navigation Favorites as a collection of required and optional data parameters, formatted as indicated below, with their relative max values.

|  |  |  |  |
| --- | --- | --- | --- |
| **RS Setting** | **RS Setting Payload – Packet Format** | | **Range**  **(in-vehicle)** |
| **Feature Number (FeatNum)** | **Data Value (DatVal)** |
| Home - Location Name | 0x0350 | String | 0-200 chars |
| Home - Phone Number | 0x0351 | String | 0-20 chars |
| Home - City | 0x0352 | String | 0-50 chars |
| Home - Subcity | 0x0353 | String | 0-50 chars |
| Home - State/Province | 0x0354 | String | 0-100 chars |
| Home - Door Number | 0x0355 | String | 0-50 chars |
| Home - Street Name | 0x0356 | String | 0-100 chars |
| Home - Cross Street Name | 0x0357 | String | 0-100 chars |
| Home - Zip Code/Postal Code | 0x0358 | String | 0-10 chars |
| Home - Country | 0x0359 | String | 0-50 chars |
| Home - Latitude | 0x035A | Double | 8 bytes |
| Home - Longitude | 0x035B | Double | 8 bytes |
| **>> The set above is repeated for each additional favorite** | | | |
| Work | 0x035C - 0x0367 | - | - |
| Favorite 1 | 0x0368 - 0x0373 | - | - |
| Favorite 2 | 0x0374 - 0x037F | - | - |
| Favorite 3 | 0x0380 - 0x038B | - | - |
| Favorite 4 | 0x038C - 0x0397 | - | - |
| Favorite 5 | 0x0398 - 0x03A3 | - | - |
| Favorite 6 | 0x03A4 - 0x03AF | - | - |
| Favorite 7 | 0x03B0 - 0x03BB | - | - |
| Favorite 8 | 0x03BC - 0x03C7 | - | - |
| Favorite 9 | 0x03C8 - 0x03D3 | - | - |
| Favorite 10 | 0x03D4 - 0x03DF | - | - |

##### RKS-REQ-362433/C-RS Settings – Required Navigation Favorite Parameters

The RS Settings payload includes both optional and required parameters for Navigation Favorites. The minimal parameters required by the RSServer (in order to save a Navigation Favorite) shall be:

|  |  |  |
| --- | --- | --- |
| **Favorite #** | **RS Setting** | **Required/Optional** |
| Home, Work, Favorite 1-10 | Location Name | Required |
| Phone Number | Optional |
| City | Optional |
| Subcity | Optional |
| State/Province | Optional |
| Door Number | Optional |
| Street Name | Optional |
| Cross Street Name | Optional |
| Zip Code/Postal Code | Optional |
| Country | Optional |
| Latitude | Required |
| Longitude | Required |

##### RKS-REQ-362434/C-RS Settings – Applying the Navigation Favorites

The RSServer shall request the Nav Application to save each favorite provided in the RS Settings payload using saveNavLocation.

The RSServer shall request saveNavLocation with the following parameters (as provided in the RS Settings payload) for a given favorite:

* RequestID = any unique int32 value used to correlate the response
* Location Name = “Favorite# - Location Name”:“DataValue”
  + ex. For Home, the value pair is 0x0345: “DataValue”
* Phone Number = “Favorite# - Phone Number”:“DataValue”
  + ex. For Home, the value pair is 0x0346: “DataValue”
* City = “Favorite# - City”:“DataValue”
  + ex. For Home, the value pair is 0x0347: “DataValue”
* SubCity = “Favorite# - SubCity”:“DataValue”
  + ex. For Home, the value pair is 0x0348: “DataValue”
* State = “Favorite# - State”:“DataValue”
  + ex. For Home, the value pair is 0x0349: “DataValue”
* Door Number = “Favorite# - Door Number”:“DataValue”
  + ex. For Home, the value pair is 0x034A: “DataValue”
* Street Name = “Favorite# - Street Name”:“DataValue”
  + ex. For Home, the value pair is 0x034B: “DataValue”
* Cross Street Name = “Favorite# - Cross Street Name”:“DataValue”
  + ex. For Home, the value pair is 0x034C: “DataValue”
* ZIP Code = “Favorite# - ZIP Code”:“DataValue”
  + ex. For Home, the value pair is 0x034D: “DataValue”
* Country = “Favorite# - Location Country”:“DataValue”
  + ex. For Home, the value pair is 0x034E: “DataValue”
* Latitude = “Favorite# - Latitude”:“DataValue”
  + ex. For Home, the value pair is 0x034F: “DataValue”
* Longitude = “Favorite# - Longitude”:“DataValue”
  + ex. For Home, the value pair is 0x0350: “DataValue”

The RSServer may issue requests in parallel or wait for a response before requesting to save subsequent favorites. The response shall indicate either a success or failure along with the correlated RequestID, however the RSServer is not required to take any action on a failed response at this time.

##### RKS-REQ-362435/A-RS Settings – Failure to Apply Navigation Favorites

If the Nav Application cannot save the requested Navigation Favorite for whatever reason (parameters invalid, parameters corrupt, address cannot be found, etc.), the Nav Application shall not perform a retry and shall skip the requested Navigation Favorite.

##### RKS-REQ-362436/B-RS Settings – Multiple Addresses Found for a Navigation Favorite

If the Nav Application finds multiple addresses for the requested Navigation Favorite, the Nav Application shall skip the requested Navigation Favorite.

##### RKS-REQ-367359/A-RS Settings – Max Saved Locations Occupied

If all of the allowable saved locations are occupied, the Nav Application shall overwrite as many locations as requested from the RSServer

##### RKS-REQ-362437/A-RS Settings – Nav Application Welcome Screen

If the Nav Application has a Welcome Screen or any such user interface that asks the user for any of the Navigation Parameters offered by the RocketSetup feature, the following shall be performed:

* If the RS Settings have been applied, the Nav Application shall remove/configure off their Welcome Screen.
* If the RS Settings have not been applied, the Nav Application shall offer their Welcome Screen and user entry per normal operation.

#### Radio Presets

##### RKS-REQ-361367/B-RS Settings – Radio Presets

The RSServer shall receive up to 15 Radio Presets from the RS Settings payload.

(China: will only receive up to 1 Radio Presets from RS Setting Payload.)

##### RKS-REQ-372296/A-RS Settings - NA vs EU Preset Determination

For the preset requirements to follow, the RSServer shall use the below to determine whether the following presets types are available (and therefore which application method to follow) based on the configurations listed:

* **North American AM/FM:** DE00 Byte 2 Bit 6 = “0 – Non RDS Market”
* **North American SDARS:** DE00 Byte 1 Bit 5 = “1 – SDARS HMI and DTCs Enabled”
* **European FM:** DE00 Byte 2 Bit 6 = “1 – RDS Market”
* **European DAB:** DE00 Byte 1 Bit 0 = “1 – Available”

If the RS Settings Payload contains radio preset information for a region that the RSServer is not configured for, the RSServer shall ignore/skip those radio presets.

* Ex. The RS Settings Payload contains European DAB radio presets when the RSServer is configured for North American SDARS.

##### RKS-REQ-362446/D-RS Settings – Radio Presets Parameters/Format

The RSServer shall receive the Radio Presets as a collection of optional and required data parameters, formatted as indicated below, with their relative possible values.

|  |  |  |  |
| --- | --- | --- | --- |
| **RS Setting** | **RS Setting Payload – Packet Format** | | **Range**  **(in-vehicle)** |
| **Feature Number (FeatNum)** | **Data Value**  **(DatVal)** |
| Preset 1 – Frequency | 0x021D | uint (500000 -108100000) | (500000-1600000) and (88100000-108100000) |
| Preset 1 – Band Type | 0x021E | 0x1, 0x5, 0x7, 0x9 | 0x1-0xC (1-FM1, 5-AM, 7-DAB, 9-SAT1) |
| Preset 1 – HDNumber | 0x021F | 0x1-0x7 | 0x1-0x7 (1-MC1, 2-MC2, 3-MC3, etc.) |
| Preset 1 – SID | 0x0220 | 0x0001 – 0xFFFF | 0x0001 – 0xFFFF |
| Preset 1 – ChannelID | 0x0221 | Int (0-9999) | (0-9999) |
| Preset 1 – Station Name | 0x0222 | String | 16 chars |
| Preset 1 – PI Code | 0x0223 | 0x0001 – 0xFFFF | 0x0001 – 0xFFFF |
| Preset 1 – ECC | 0x03E0 | String | 2 chars |
| **>> The set above is repeated for each additional preset** | | | |
| Preset 2 | 0x0224 - 0x022A, 0x03E1 | - | - |
| Preset 3 | 0x022B - 0x0231, 0x03E2 | - | - |
| Preset 4 | 0x0232 - 0x0238, 0x03E3 | - | - |
| Preset 5 | 0x0239 - 0x023F, 0x03E4 | - | - |
| Preset 6 | 0x0240- 0x0246, 0x03E5 | - | - |
| Preset 7 | 0x0247 - 0x024D, 0x03E6 | - | - |
| Preset 8 | 0x024E - 0x0254, 0x03E7 | - | - |
| Preset 9 | 0x0255 - 0x025B, 0x03E8 | - | - |
| Preset 10 | 0x025C - 0x0262, 0x03E9 | - | - |
| Preset 11 | 0x0263 - 0x0269, 0x03EA | - | - |
| Preset 12 | 0x026A - 0x0270, 0x03EB | - | - |
| Preset 13 | 0x0271 - 0x0277, 0x03EC | - | - |
| Preset 14 | 0x0278 - 0x027E, 0x03ED | - | - |
| Preset 15 | 0x027F - 0x0285, 0x03EE | - | - |

##### RKS-REQ-362447/D-RS Settings - Required NA AM/FM Radio Preset Parameters

The RS Settings payload includes both optional and required parameters for Radio Presets. The minimal parameters required by the RSServer (in order to save a North American AM/FM Radio Preset) shall be:

|  |  |  |
| --- | --- | --- |
| **Radio Preset #** | **Parameter** | **Required/Optional** |
| Radio Preset 1-15 | Frequency | Required |
| Band Type | Required |
| HDNumber | Optional |
| SID | N/A |
| ChannelID | N/A |
| Station Name | N/A |
| PI Code | N/A |
| ECC | N/A |

##### RKS-REQ-362448/D-RS Settings - Required NA SDARS Radio Preset Parameters

The RS Settings payload includes both optional and required parameters for Radio Presets. The minimal parameters required by the RSServer (in order to save a North American SDARS Radio Preset) shall be:

|  |  |  |
| --- | --- | --- |
| **Radio Preset #** | **Parameter** | **Required/Optional** |
| Radio Preset 1-15 | Frequency | N/A |
| Band Type | Required |
| HDNumber | N/A |
| SID | Required |
| ChannelID | Required (IP Channels) |
| Station Name | N/A |
| PI Code | N/A |
| ECC | N/A |

##### RKS-REQ-362449/D-RS Settings - Required EU FM/DAB Radio Preset Parameters

The RS Settings payload includes both optional and required parameters for Radio Presets. The minimal parameters required by the RSServer (in order to save a European DAB/FM Radio Preset) shall be:

|  |  |  |
| --- | --- | --- |
| **Radio Preset #** | **Parameter** | **Required/Optional** |
| Radio Preset 1-15 | Frequency | Required (FM only) |
| Band Type | Required |
| HDNumber | N/A |
| SID | Required (DAB only) |
| ChannelID | N/A |
| Station Name | Required |
| PI Code | Required (FM only) |
| ECC | Required |

##### RKS-REQ-362450/B-RS Settings – Muting while Applying Radio Presets

When the RSServer is required to apply the Radio Presets, it shall mute the Media audio by using the SYNC\_Alerts message and setting Attn\_Info\_Audio = “Attenuation\_6” (full mute).

* Follow the attenuation strategy as defined in ALERT-FUN-REQ-014794-Audio Attenuation/Muting Strategy.
* For the attenuation for this feature, follow the Screen Interruption Table entry for Enhanced Memory and only allow interrupt events as required (see H22a\_SYNC\_4\_Screen\_Interruption\_Table).
* The RSServer shall mute as necessary when the application process has resumed after a pause, per REQ-372250.

##### RKS-REQ-362451/B-RS Settings – UnMuting after Applying Radio Presets

When the RSServer has finished applying all of the Radio Presets, it shall unmute the Media audio by using the SYNC\_Alerts message and setting Attn\_Info\_Audio = “No Attenuation of Audio.”

* Follow the attenuation strategy as defined in ALERT-FUN-REQ-014794-Audio Attenuation/Muting Strategy.
* The RSServer shall unmute as necessary when the application process is paused per REQ-372250.

##### RKS-REQ-362452/A-RS Settings – Applying Radio Presets by Band Type

When the RSServer is required to apply the Radio Presets, it shall do so by applying each Radio Preset based on its Band Type, regardless of Preset Position (but still maintaining Preset Position). The RSServer shall apply the Radio Presets by Band Type in the following order:

* AM (analog)
* AM (multicast/HD)
* FM (analog)
* FM (multicast/HD)
* SDARS / DAB
* SDARS (IP Channels)

**Note**: This is done to reduce the number of band/source changes, expediting the process.

##### RKS-REQ-362453/D-RS Settings – Applying NA AM/FM Radio Presets

The RSServer shall utilize the existing AM/FM Radio Preset interfaces per AMFM-IIR-REQ-023795-AMFM Slave CAN Request and AMFM-IIR-REQ-023797-AMFM Slave CAN Status.

If the Radio Preset being requested is an AM or FM station (indicated by Band Type = “0x5 - AM” or “0x1 - FM1”) for a vehicle in North America, the RSServer shall:

1. Direct Tune to the Radio Preset frequency by setting and sending the below signals to the RSClient (see AMFM-SD-REQ-023838-Direct Station Selection):
   1. SetCurrentStat.Rq: Operation = “0x1 - Set Current Frequency”
   2. SetCurrentStat.Rq: Frequency = “Offset”
      1. See “Offset” under SetCurrentStat.Rq in AMFM-IIR-REQ-023797-AMFM Slave CAN Status (RSServer must calculate and use Offset, using the provided “Preset# - Frequency”:“DataValue”)
   3. SetCurrentStat.Rq: PICode = “Preset# - PI Code”:“DataValue”
      1. ex. For Preset1-PI Code, the value pair is 0x0223: “DataValue”
   4. SetCurrentStat.Rq: MCChannel = “Preset# - HDNumber”:“DataValue” (if applicable)
      1. ex. For Preset1-HDNumber, the value pair is 0x021F:“DataValue”
   5. **Note:** if the active band type is different than the one being requested, a SetCurrTUBand.Rq = “Preset# - Band Type”:“DataValue” shall be issued (per above ref. diagram)
2. Wait for the RSClient to respond with the below, indicating the Radio Preset frequency has been tuned to:
   1. CurrentTUBand.St = Band Type
   2. DirectTune.St = “0x2 - Valid Station”
   3. CurrentFreq.St = Offset
      1. See “Offset” under CurrentFreq.St in AMFM-IIR-REQ-023797-AMFM Slave CAN Status
   4. CurrentHDMulticast.St = HDNumber (if applicable)
   5. CurrentPICode.St = PI Code
3. Request a Store Preset operation by settings and sending the below signals to the RSClient (see AMFM-SD-REQ-023861-Store Preset):
   1. StorePreset2.Rq = Preset#
4. Wait for the RSClient to respond with the below, indicating the Radio Preset has been successfully stored:
   1. StorePreset.St = Preset#
5. Repeat steps 1-4 for all AM or FM Radio Presets provided in the RS Settings payload

Reference requirements:

AMFM-IIR-REQ-023795-AMFM Slave CAN Request

AMFM-IIR-REQ-023797-AMFM Slave CAN Status

AMFM-SD-REQ-023838-Direct Station Selection

AMFM-SD-REQ-023861-Store Preset

TU-SR-REQ-192639/B-Mixed Mode Presets Intigration into AMFM/SDARS/DAB Feature

##### RKS-REQ-362454/D-RS Settings – Applying NA SDARS Radio Presets

The RSServer shall utilize the existing SDARS Radio Preset interfaces per AMFM-IIR-REQ-023795-AMFM Slave CAN Request, AMFM-IIR-REQ-023797-AMFM Slave CAN Status, SDARS-IIR-REQ-195704-SDARSClient\_Tx and SDARS-IIR-REQ-210911-SDARSRemoteServer\_Rx.

If the Radio Preset being requested is an SDARS station (indicated by Band Type = “0x9 - SAT1”) for a vehicle in North America, the RSServer shall:

1. Direct Tune to the “Preset# - SID”:“DataValue” or “Preset# - ChannelID”:“DataValue” (see SDARSv2-SD-REQ-195749-Direct Channel Selection).
   1. For SDARSv2, the RSServer tunes internally, therefore, the RSServer shall internally tune to the SID or ChannelID provided.
   2. **Note:** if the active band type is different than the one being requested, a SetCurrTUBand.Rq = “Preset# - Band Type”:“DataValue” shall be issued (per above ref. diagram)
2. The Store Preset operation shall not be issued until the RSServer has updated the below signals after tuning to the SID/ChannelID (per SDARS-FUR-REQ-196124-Presets):
   1. ServiceID2.St
   2. CurrentChanNum2.St
   3. ChannelName.St
3. Request a Store Preset operation by settings and sending the below signals to the RSClient (see SDARSv2-SD-REQ-195723-Store SDARS Preset):
   1. StorePreset2.Rq = Preset#
4. Wait for the RSClient to respond with the below, indicating the Radio Preset has been successfully stored:
   1. StorePreset.St = Preset#
5. Repeat steps 1-4 for all SDARS Radio Presets provided in the RS Settings payload

Reference requirements:

AMFM-IIR-REQ-023795-AMFM Slave CAN Request

AMFM-IIR-REQ-023797-AMFM Slave CAN Status

SDARS-IIR-REQ-195704-SDARSClient\_Tx

SDARS-IIR-REQ-210911-SDARSRemoteServer\_Rx

SDARSv2-FUN-REQ-195747-Direct Tune

SDARSv2-SD-REQ-195749-Direct Channel Selection

SDARS-FUR-REQ-196124-Presets

SDARSv2-SD-REQ-195723-Store SDARS Preset

SDARSv2-FUN-REQ-195721-Store Preset

TU-SR-REQ-192639/B-Mixed Mode Presets Intigration into AMFM/SDARS/DAB Feature

##### RKS-REQ-362455/D-RS Settings – Applying EU FM/DAB Radio Presets

The RSServer shall utilize the existing FM/DAB Radio Preset interfaces per AMFM-IIR-REQ-023795-AMFM Slave CAN Request, AMFM-IIR-REQ-023797-AMFM Slave CAN Status, TU-IIR-REQ-299207-TunerClient-TunerServer, TU-IIR-REQ-299209-TunerServer-TunerClient, TU-FUN-REQ-268693-Station List Selection.

If the Radio Preset being requested is an FM station (indicated by “Preset# - Band Type”: “0x1 - FM1”) for a vehicle in Europe, the RSServer shall:

1. Request a tune to the FM Radio Preset via “Station List Selection” by setting and sending the below signals to the RSClient (see TU-SD-REQ-268244-Select Station From Station List Via Voice Command):
   1. SelectStation\_Rq:RequestSelector = “0x1 - PI-Code”
   2. SelectStation\_Rq:PI-Code = “Preset# - PI Code”:“DataValue”
      1. ex. For Preset1-PI Code, the value pair is 0x0223: “DataValue”
   3. SelectStation\_Rq:SCID = “0x0000 - Inactive”
   4. SelectStation\_Rq:SID = “0x0000 - Inactive”
   5. SelectStation\_Rq:ECC = “Preset# - ECC”:“DataValue”
   6. **Note:** the band type will change automatically if needed.
2. Wait for the RSClient to respond with the below, indicating the FM Radio Preset frequency has been tuned to:
   1. SelectStation\_Rsp:ResponseCode = “0x2 - Accepted”
3. Request a Store Preset operation by settings and sending the below signals to the RSClient (see AMFM-SD-REQ-023861-Store Preset, DAB-SD-REQ-024405-Store Preset):
   1. StorePreset2.Rq = Preset#
4. Wait for the RSClient to respond with the below, indicating the Radio Preset has been successfully stored:
   1. StorePreset.St = Preset#
5. Validate PI Code:
   1. ACU\_CurrentPICode\_St = “Preset# - PI Code”:“DataValue”
6. Repeat steps 1-5 for all FM Radio Presets provided in the RS Settings payload

If the Radio Preset being requested is a DAB station (indicated by “Preset# - Band Type”:“0x7 - DAB1”) for a vehicle in Europe, the RSServer shall:

1. Request a tune to the DAB Radio Preset via “Station List Selection” by setting and sending the below signals to the RSClient (see TU-SD-REQ-268244-Select Station From Station List Via Voice Command):
   1. SelectStation\_Rq:RequestSelector = “0x2 - SCIDI\_SID\_EEC”
   2. SelectStation\_Rq:PI-Code = “0x0000 - Inactive”
   3. SelectStation\_Rq:SCID = RSServer shall obtained this from the Station List
   4. SelectStation\_Rq:SID = “Preset# - SID”:“DataValue”
   5. SelectStation\_Rq:ECC = “Preset# - ECC”:“DataValue”
      1. ex. For Preset1-ECC, the value pair is 0x03E0: “DataValue”
      2. If DataValue = 0x0, RSServer shall obtained this from the Station List
   6. **Note:** the band type will change automatically if needed.
2. Wait for the RSClient to respond with the below, indicating the DAB Radio Preset has been tuned to:
   1. SelectStation\_Rsp:ResponseCode = “0x2 - Accepted”
3. Request a Store Preset operation by settings and sending the below signals to the RSClient (see AMFM-SD-REQ-023861-Store Preset, DAB-SD-REQ-024405-Store Preset):
   1. StorePreset2.Rq = Preset#
4. Wait for the RSClient to respond with the below, indicating the Radio Preset has been successfully stored:
   1. StorePreset.St = Preset#
5. Validate SID & ECC (ignore ECC if DataValue = 0x0):
   1. ACU\_CurrTUSID\_St (Byte 1..2) = “Preset# - SID”:“DataValue”

&&

* 1. ACU\_CurrTUSID\_St (Byte 3) = “Preset# - ECC”:“DataValue”

1. Repeat steps 1-5 for all DAB Radio Presets provided in the RS Settings payload

Reference requirements:

AMFM-IIR-REQ-023795-AMFM Slave CAN Request

AMFM-IIR-REQ-023797-AMFM Slave CAN Status

TU-IIR-REQ-299207-TunerClient-TunerServer

TU-IIR-REQ-299209-TunerServer-TunerClient

DAB-FUN-REQ-024402-Store DAB Preset

AMFM-SD-REQ-023861-Store Preset

DAB-SD-REQ-024405-Store Preset

TU-SD-REQ-268244-Select Station From Station List Via Voice Command

TU-FUN-REQ-268693-Station List Selection

TU-SR-REQ-192639/B-Mixed Mode Presets Intigration into AMFM/SDARS/DAB Feature

##### RKS-REQ-362456/A-RS Settings – Failure to Tune to a Radio Preset

If the RSServer cannot tune to the requested Radio Preset, the RSServer shall:

* For AM/FM HD channels in North America
  + Tune to the analog frequency and store it instead (repeat same process in REQ-362453 but with CurrentHDMulticast.St = “0x0 - 0”)
* For SDARS channels in North America
  + Skip the preset
* For FM/DAB in Europe
  + Store the frequency, regardless of active station

##### RKS-REQ-362457/A-RS Settings – Failure to Apply a Radio Preset

After sending StorePreset2.Rq, if the RSServer receives StorePreset.St set to any value other than the requested preset number, the RSServer shall not perform a retry and shall skip that Radio Preset.

#### Departure Times

##### RKS-REQ-361368/A-RS Settings – Departure Times

The RSServer shall receive up to fourteen Departure Times from the RS Settings payload.

##### RKS-REQ-362438/C-RS Settings – Departure Times Parameters/Format

The RSServer shall receive the Departure Times as a collection of required data parameters, formatted as indicated below, with their relative possible values.

|  |  |  |  |
| --- | --- | --- | --- |
| **RS Setting** | **RS Setting Payload – Packet Format** | | **Range**  **(in-vehicle)** |
| **Feature Number (FeatNum)** | **Data Value (DatVal)** |
| Global Departure Time | 0x0D60 | 0x1, 0x2 | 0x0-0x2 (0-Null, 1-Off, 2-On) |
| Element ID 1 – Hour | 0x0D61 | 0x00-0x17 | 0x00-0x17 (dec: 0-23) |
| Element ID 1 – Minutes | 0x0D62 | 0x0-0xB | 0x0-0xB (dec: 0-55)  (in increments of 5) |
| Element ID 1 – Precondition Setting | 0x0D63 | 0x0-0x3 | 0x0-0x3 (0-Off, 1-Low, 2-Med, 3-High) |
| **>> The set above (Hour/Min/Precondition only) is repeated for each additional Element ID** | | | | |
| Element ID 2 | 0x0D64 - 0x0D66 | - | - |
| Element ID 3 | 0x0D67 - 0x0D69 | - | - |
| Element ID 4 | 0x0D6A - 0x0D6C | - | - |
| Element ID 5 | 0x0D6D - 0x0D6F | - | - |
| Element ID 6 | 0x0D70 - 0x0D72 | - | - |
| Element ID 7 | 0x0D73 - 0x0D75 | - | - |
| Element ID 8 | 0x0D76 - 0x0D78 | - | - |
| Element ID 9 | 0x0D79 - 0x0D7B | - | - |
| Element ID 10 | 0x0D7C - 0x0D7E | - | - |
| Element ID 11 | 0x0D7F - 0x0D81 | - | - |
| Element ID 12 | 0x0D82 - 0x0D84 | - | - |
| Element ID 13 | 0x0D85 - 0x0D87 | - | - |
| Element ID 14 | 0x0D88 - 0x0D8A | - | - |

##### RKS-REQ-362439/C-RS Settings – Applying the Departure Times

The RSServer shall utilize the existing EV Charge Programming interfaces per EVCS-IIR-REQ-250960-APIM Saving of Departure Times.

If the RSServer receives 0x0D60:“0x1 - Off”, the RSServer shall:

1. Request the Global Departure Times be turned Off (if ChrgGoTAllOn\_B\_Stat = “(0x1 - Go Times On)”) via:
   1. OnbChrgGoTOn\_D\_Rq = “0x0 - Go Times Off”
   2. OnbChrgGoTUpdate\_B\_Rq = “0x1 - Request”
2. Wait for the RSClient to respond with the below, indicating the Global Departure Times has been turned Off:
   1. ChrgGoTAllOn\_B\_Stat = “(0x0 - Go Times Off)”
3. Not request any Departure Times.

If the RSServer receives 0x0D60:“0x2 - On”, the RSServer shall:

1. Request the Global Departure Times be turned On (if ChrgGoTAllOn\_B\_Stat = “(0x0 - Go Times Off)”) via:
   1. OnbChrgGoTOn\_D\_Rq = “0x1 - Go Times On”
   2. OnbChrgGoTUpdate\_B\_Rq = “0x1 - Request”
2. Wait for the RSClient to respond with the below, indicating the Global Departure Times has been turned On:
   1. ChrgGoTAllOn\_B\_Stat = “(0x1 - Go Times On)”
3. Request the RSClient save the Departure Times Schedule (collection of all of the provided Departure Times) by setting and sending the following signals:
4. OnbChrgGoTUpdate\_B\_Rq = “0x1 - Request”
   * 1. Hold this signal value until all ElementID’s have been requested
5. OnbChrgGoTElement\_D\_Rq = ElementID
6. OnbChrgGoTHr\_T\_Rq = “Element ID # - Hour”:“DataValue”
7. ex. For Element ID 1, the value pair would be 0x0D61:“DataValue”
8. OnbChrgGoTMnte\_D\_Rq = “Element ID # - Minutes”:“DataValue”
   1. ex. For Element ID 1, the value pair would be 0x0D62:“DataValue”
9. OnbChrgGoTPrcond\_D\_Rq = “Element ID # - Precondition Setting”:“DataValue”
10. ex. For Element ID 1, the value pair would be 0x0D63:“DataValue”
11. Repeat sending the signals in b, c, d, e for every ElementID provided in the RS Settings payload.
12. OnbChrgGoTUpdate\_B\_Rq = “0x0 - No Request”
13. Set this signal value after all ElementID’s have been requested
14. Wait for the RSClient to respond with the below set of signals (repeated for each ElementID), indicating the Departure Times have been saved:
15. ChrgGoTElement\_D\_Stat = ElementID
16. ChrgGoTHr\_T\_Stat = Hour
17. ChrgGoTMnte\_D\_Stat = Minutes
18. ChrgGoTPrcond\_D\_Stat = Precondition Setting

**Note**: The Departure Times are requested by the RSServer as a set of ElementID’s or a “Schedule.” The RSServer must request each ElementID, with the accompanying parameters, using the above signals repeated for each ElementID. During this entire transmission, the Update flag must be sent to “Request” and set back to “No Request” when complete. The RSClient will respond after the Update flag has been cleared with the status of each ElementID, again repeated using the same set of status signals above.

Reference requirements:

EVCS-IIR-REQ-250960-APIM Saving of Departure Times

EVCS-REQ-263405-Communication - Onboard Update Flag - Charge Settings Update

EVCS-REQ-263401-Communication - Onboard Update Flag - No Update

EVCS-FUN-REQ-281551-Charge Schedule

##### RKS-REQ-362440/B-RS Settings – Failure to Apply Departure Times

If the RSServer cannot save the requested Departure Times for whatever reason (failure from OnBoardChargeSchedulerServer, etc.), the RSServer shall not perform a retry and shall skip the requested Departure Time.

#### Drive Mode

##### RKS-REQ-364513/A-RS Settings – Drive Mode

The RSServer shall receive one Drive Mode Setting from the RS Settings payload.

##### RKS-REQ-364514/A-RS Settings – Drive Mode Parameters/Format

The RSServer shall receive the Drive Mode Setting as a single required data parameter, formatted as indicated below, with its relative possible values.

|  |  |  |  |
| --- | --- | --- | --- |
| **RS Setting** | **RS Setting Payload – Packet Format** | | **Range**  **(in-vehicle)** |
| **Feature Number (FeatNum)** | **Data Value (DatVal)** |
| Drive Mode | 0x0E60 | 0x00, 0x01, 0x04 | 0x00-0x1E |

##### RKS-REQ-364515/B-RS Settings – Applying the Drive Mode Setting

The RSServer shall request the Drive Mode application to select the Drive Mode Setting provided in the RS Settings payload using setDriveMode.

The RSServer shall request setDriveMode with the following parameters:

* Drive Mode Request = 0x0E60:“DataValue”

The response shall indicate success, failure, no response, or invalid, however the RSServer is not required to take any action on any of the responses at this time.

##### RKS-REQ-364516/A-RS Settings – Failure to Apply Drive Mode Setting

If the RSServer cannot save the requested Drive Mode Setting for whatever reason (failure from DriveModeServer, etc.), the RSServer shall not perform a retry and shall skip the Drive Mode Setting.

# Appendix: Reference Documents

|  |  |
| --- | --- |
| Reference # | Document Title |
| 1 | Vehicle Settings APIM SPSS |
| 2 | AM\_FM\_HD Tuner APIM SPSS |
| 3 | DAB APIM SPSS |
| 4 | Satellite Radio v2 APIM SPSS |
| 5 | Ev Charge Programming APIM SPSS |
| 6 | Ford Telematics Communication Protocol Specification |
| 7 | FNV2-FCI Protocol SPSS |
| 8 | Rocket Setup On-Board Security Specification |
| 9 | ISO 8601 - <https://www.iso.org/iso-8601-date-and-time-format.html> |
| 10 |  |
| 11 |  |
| 12 |  |
| 13 |  |
| 14 |  |
| 15 |  |
| 16 |  |
| 17 |  |