

**Research & Vehicle Technology**

**“Product Development”**

**Feature – Enhanced Memory**

**IVI Subsystem Part Specific Specification (SPSS)**

Version 1.9

**UNCONTROLLED COPY IF PRINTED**

**Version Date: June 6, 2018**

**FORD CONFIDENTIALF**

**Revision History**

|  |  |  |  |
| --- | --- | --- | --- |
| **Date** | **Version** | **Notes** | |
| **September 17, 2015** | **0.01** | **Draft Release** | **Draft release. Not to have software coded to. That will be when have the official 1.0 release** |
|  |  |  |  |
| **December 14, 2015** | **1.0** | **Initial Release** |  |
|  |  |  |  |
| **February 9, 2016** | **1.1** | **Updated Release** |  |
|  | STR-196365/D-General Requirements | | MBORREL4: Added New Req 206864 & 207325 |
|  | ENMEM-REQ-206864/A-EnhancedMemoryServers to Retain Settings After Software Reflash | | MBORREL4: New req |
|  | ENMEM-SR-REQ-207325/A-Updates to Non-Volatile Memory | | MBORREL4: New Req. |
|  | ENMEM-SR-REQ-136593/K-Network Bus Start-up / Shut-down (EnhancedMemoryServer) | | MBORREL4: Updated to clarify software reflash functionality. |
|  | ENMEM-FUN-REQ-195573/B-EnhancedMemoryInterfaceClient HMI Requirements – APIM | | MBORREL4: Added New Req 207327 |
|  | ENMEM-HMI-REQ-207327/A-Driver Profile Name Restrictions | | cwu3: New for Drive Profile name restrictions |
|  |  |  |  |
| **February 12, 2016** | **1.2** | **Updated Release** |  |
|  | STR-176691/C-Requirements | | MBORREL4: Added req 099763, 099674, 136618 |
|  | ENMEM-SR-REQ-136618/D-Recall Event - Infotainment Audio | | MBORREL4: New Req. |
|  | ENMEM-REQ-099674/B-Requesting Audio Preset Info After Profile Change | | MBORREL4: New Req. |
|  | ENMEM-TMR-REQ-099763/B-T\_PersPresetWait | | MBORREL4: New Req. |
|  | STR-176718/C-Requirements | | MBORREL4: Added Req-099698 |
|  | STR-307926/C-Driver Profile Creation via Copy Operation | | MBORREL4: Added Req-099698 |
|  | ENMEM-REQ-099698/B-Wait Response From AudioServer While Copy Operation is Still in Progress | | MBORREL4: New Req. |
|  |  |  |  |
| **March 18, 2016** | **1.3** | **Updated Release** |  |
|  | ENMEM-IIR-REQ-099360/G-EnhancedMemoryInterfaceClient\_Tx | | MBORREL4: Updated Logical to GSDB Signal Name table to include FactoryReset\_Rq |
|  | ENMEM-IIR-REQ-099371/B-EnhancedMemoryServer\_Rx | | MBORREL4: Added REQ-015018-FactoryReset\_Rq and updated Logical to GSDB Signal Name table to include FactoryReset\_Rq |
|  | ENMEM-UC-REQ-195889/B-Associate a Keyfob with Incorrect Method | | MBORREL4: Fixed spelling error in Notes |
|  | ENMEM-REQ-099685/D-Request Enter Memory Seat Button Association Mode | | MBORREL4: Updated to include re-entry conditions upon unsuccessful pairing attempts. |
|  | ENMEM-REQ-116803/C-Request Exit Memory Seat Button Association Mode | | MBORREL4: Updated the "SET button" condition and added condition for "already associated Driver Memory Seat button press" |
|  | STR-307927/B-Keyfob Association | | MBORREL4: Added ENMEM-FUN-REQ-212303 |
|  | ENMEM-SR-REQ-212303/A-PersIndex used for Keyfob Association | | MBORREL4: New Req. |
|  | ENMEM-SD-REQ-099425/D-Create Driver Profile | | MBORREL4: Updated Feature\_Rq Copy operation for Pers to stay in last known. |
|  | STR-297590/D-Requirements | | MBORREL4: Added REQ-212764 |
|  | ENMEM-HMI-REQ-212764/A-Enhanced Memory HMI Notification of Profile Creation Abort | | MBORREL4: New Req. |
|  |  |  |  |
| **April 11, 2016** | **1.4** | **Updated Release** |  |
|  | ENMEM-FUR-REQ-134134/K-Enhanced Memory Features Supported - APIM | | MBORREL4: Removed 11 features from NAV section per vpatel18 (no longer supported) |
|  | ENMEM-IIR-REQ-099371/B-EnhancedMemoryServer\_Rx | | MBORREL4: Added REQ-015018-FactoryReset\_Rq and updated Logical to GSDB Signal Name table to include FactoryReset\_Rq |
|  | STR-196365/E-General Requirements | | MBORREL4: Removed REQ-198778-T\_ReturnToIdle and REQ-180452-Request/Response return to Idle state, as they are no longer needed/used. |
|  | ENMEM-REQ-099685/E-Request Enter Memory Seat Button Association Mode | | MBORREL4: Updated first paragraph to clarify when button pairing is entered |
|  | ENMEM-SD-REQ-099425/E-Create Driver Profile | | MBORREL4: Removed all instances of T\_ReturnToIdle as it is no longer needed |
|  | ENMEM-SD-REQ-197169/B-User Chooses a Seat Button That is Already Associated to Another Driver Profile | | MBORREL4: Removed all instances of T\_ReturnToIdle as it is no longer needed |
|  | ENMEM-HMI-REQ-207327/B-Driver Profile Name Restrictions | | MBORREL4: Removed Profile Name character limits and details that were moved to the H84a Enhanced Memory HMI Spec in [H84a.R043.xx] |
|  |  |  |  |
| **May 11, 2016** | **1.5** | **Updated Release** |  |
|  | STR-176673/B-Use Cases | | Added REQ-214249, REQ-214250, and REQ-214246 |
|  | ENMEM-UC-REQ-214249/A-Valet Mode enabled with Enhanced Memory On | | New Use Case describing Valet Mode functionality |
|  | ENMEM-UC-REQ-214250/A-Valet Mode disabled with Enhanced Memory On | | New Use Case describing Valet Mode functionality |
|  | ENMEM-UC-REQ-214246/A-Valet Mode disabled with Enhanced Memory Off | | New Use Case describing Valet Mode functionality |
|  | STR-176669/C-Requirements | | MBORREL4: Added REQ-214801 |
|  | ENMEM-SR-REQ-214801/A-Enable/Disable Enhanced Memory in Valet Mode | | MBORREL4: New req. added to cover Valet Mode functionality. |
|  | STR-176692/C-Use Cases | | Added REQ-214249, REQ-214250 |
|  | ENMEM-UC-REQ-214249/A-Valet Mode enabled with Enhanced Memory On | | New Use Case describing Valet Mode functionality |
|  | ENMEM-UC-REQ-214250/A-Valet Mode disabled with Enhanced Memory On | | New Use Case describing Valet Mode functionality |
|  | STR-176691/D-Requirements | | MBORREL4: Added REQ-214221 |
|  | ENMEM-REQ-099673/C-Driver Profile Settings Recall | | MBORREL4: Updated to have HMI sign-in notification shown each time the “Start Screen” is shown as defined by H22g\_SYNC3\_Welcome\_Power\_Modes, as well as during a profile recall. |
|  | ENMEM-SR-REQ-136618/E-Recall Event - Infotainment Audio | | MBORREL4: Updated to describe muting when in a phone call/VR session. |
|  | ENMEM-SR-REQ-214221/A-Recall behavior when Valet Mode Enabled/Disabled | | MBORREL4: New req. added for Valet Mode recall functionality |
|  | ENMEM-REQ-099699/C-Disable Driver Profile Creation and Editing When Key is Not in Run or Vehicle Speed is greater than 5KPH | | MBORREL4: Updated to include condition of Gear Position = Park |
|  | ENMEM-REQ-116802/C-Profile Creation Interruption | | MBORREL4: Updated to include all actions required to be taken when aborted (spec clarification). Added Park condition to the interrupt example |
|  | ENMEM-SR-REQ-198055/B-Enhanced Memory HMI Option for Associated Keyfob | | MBORREL4: Updated signal in last bullet from EnMemKeyPairing\_S\_Rq to EnMemProfilePairing\_Rq (spec correction) |
|  | ENMEM-REQ-198100/B-Overwrite Associated Keyfob | | MBORREL4: Updated signals to EnMemProfilePairing\_Rq (spec correction) |
|  | ENMEM-REQ-116804/D-Keyfob Pairing Error | | MBORREL4: Added Park condition as an interrupt method |
|  | ENMEM-SR-REQ-198055/B-Enhanced Memory HMI Option for Associated Keyfob | | MBORREL4: Updated signal in last bullet from EnMemKeyPairing\_S\_Rq to EnMemProfilePairing\_Rq (spec correction) |
|  |  |  |  |
| **July 18, 2016** | **1.6** | **Updated Release** |  |
|  | ENMEM-SR-REQ-136593/L-Network Bus Start-up / Shut-down (EnhancedMemoryServer) | | MBORREL4: Added clarification for when the last active personality cannot be determined. |
|  | ENMEM-REQ-129547/C-Last Known Driver Profile Applied | | MBORREL4: Added clarification for when the Last Known Driver Profile cannot be determined. |
|  | ENMEM-REQ-198928/B-Button Press in Button Association Mode | | MBORREL4: Removed Memory\_Cmd from req and changed "should" to "shall" in 1st paragraph. |
|  |  |  |  |
| **September 26, 2016** | **1.7** | **Updated Release** |  |
|  | STR-184156/C-Overview | | MBORREL4: Updated to include PaaK |
|  | ENMEM-CLD-REQ-099556/E-Enhanced Memory Profile Server – BCM | | MBORREL4: Updated to include PaaK |
|  | MD-REQ-099304/D-EnMemProfilePairing\_Rq | | MBORREL4: Updated for PaaK. Added EnterPhoneAssoc and DisassociatePhone encodings |
|  | ENMEM-IIR-REQ-099363/F-EnhancedMemoryInterfaceClient\_Rx | | MBORREL4: Updated for PaaK. Added new signal PersPhonePairing\_St |
|  | MD-REQ-099352/C-EnMemKeyPairing\_St | | MBORREL4: Updated for PaaK. Added WrongDeviceSelected encoding |
|  | MD-REQ-233493/A-PersPhonePairing\_St | | MBORREL4: New Method Description |
|  | STR-196365/F-General Requirements | | MBORREL4: Added new REQ-232557 |
|  | ENMEM-REQ-116801/D-Retain Enhanced Memory Settings After Software Reflash | | MBORREL4: Updated to include PaaK |
|  | ENMEM-SR-REQ-136937/E-Enhanced Memory Feature Inclusion Guidelines | | MBORREL4: Updated to include PaaK |
|  | ENMEM-REQ-137867/B-Keyfob/Phone Association Term Consolidation | | MBORREL4: Updated to include PaaK |
|  | ENMEM-REQ-166096/E-Operations Shall Not Recall a Driver Profile | | MBORREL4: Updated to include PaaK |
|  | ENMEM-REQ-232557/A-Phone & Phone-As-A-Key | | MBORREL4: New Req. for PaaK |
|  | STR-310182/B-Recall Function Description | | MBORREL4: Updated to include PaaK |
|  | ENMEM-UC-REQ-095940/D-Sign Into a Driver Profile via Keyfob/Phone | | MBORREL4: Updated to include PaaK |
|  | ENMEM-UC-REQ-162635/C-Sign Into a Driver Profile via Keyfob/Phone Button Press While Vehicle In Motion | | MBORREL4: Updated to include PaaK |
|  | ENMEM-UC-REQ-161547/D-Classic Memory Only Recall via Previously Associated Keyfob/Phone | | MBORREL4: Updated to include PaaK |
|  | ENMEM-UC-REQ-137996/D-Recall Last Known Driver Profile With Keypad Code When A Keyfob/Phone Is Not With The User | | MBORREL4: Updated to include PaaK |
|  | ENMEM-UC-REQ-137858/D-MyKey Overrides Driver Profile Setting | | MBORREL4: Updated to include PaaK |
|  | ENMEM-UC-REQ-162575/C-Admin Key does not restrict Driver Profile associated to MyKey | | MBORREL4: Updated to include PaaK |
|  | ENMEM-REQ-099671/E-Keyfob/Phone Detection for Driver Profile Sign-In | | MBORREL4: Updated to include PaaK |
|  | ENMEM-ACT-REQ-099384/D-Sign Into Driver Profile Via Keyfob/Phone | | MBORREL4: Updated to include PaaK |
|  | ENMEM-SD-REQ-099432/D-Sign Into Driver Profile Via Keyfob/Phone | | MBORREL4: Updated to include PaaK |
|  | STR-176719/C-Use Cases | | MBORREL4: Added REQ-232959 |
|  | ENMEM-UC-REQ-095908/D-Associate Keyfob/Phone to a Driver Profile | | MBORREL4: Updated to include PaaK |
|  | ENMEM-UC-REQ-095925/C-Attempt to Associate Already Associated Keyfob/Phone | | MBORREL4: Updated to include PaaK |
|  | ENMEM-UC-REQ-195889/C-Associate a Keyfob with Incorrect Method | | MBORREL4: Updated to include PaaK |
|  | ENMEM-UC-REQ-095927/C-Disassociate Keyfob/Phone from a Driver Profile | | MBORREL4: Updated to include PaaK |
|  | ENMEM-UC-REQ-232959/A-Disassociate Phone from Driver Profiles after Phone is Erased/Revoked | | MBORREL4: New req. for PaaK |
|  | ENMEM-UC-REQ-095929/C-Delete a Driver Profile | | MBORREL4: Updated to include PaaK |
|  | ENMEM-UC-REQ-195890/B-Delete All Driver Profiles via Master Reset | | MBORREL4: Updated to include PaaK |
|  | ENMEM-UC-REQ-096802/D-User Aborts or System Cancel Event Occurs During Keyfob/Phone Association Process | | MBORREL4: Updated to include PaaK |
|  | STR-176718/D-Requirements | | MBORREL4: Added REQ-232984 & REQ-233009 |
|  | ENMEM-SR-REQ-232984/A-Configurable Parameter to Enable PaaK HMI | | MBORREL4: New req. and config bit for InterfaceClient to support PaaK |
|  | ENMEM-REQ-116801/D-Retain Enhanced Memory Settings After Software Reflash | | MBORREL4: Updated to include PaaK |
|  | ENMEM-REQ-116802/D-Profile Creation Interruption | | MBORREL4: Updated to include PaaK |
|  | ENMEM-HMI-REQ-233009/A-Phone HMI Indication | | MBORREL4: New req. for PaaK |
|  | ENMEM-REQ-198928/B-Button Press in Button Association Mode | | MBORREL4: Removed Memory\_Cmd from req and changed "should" to "shall" in 1st paragraph. |
|  | STR-307927/C-Keyfob/Phone Association | | MBORREL4: Updated to include PaaK, added REQ-233118, REQ-233161, REQ-234278, REQ-234279 |
|  | ENMEM-REQ-099672/C-Configurable Parameter for Key/Phone Pairing | | MBORREL4: Updated to include PaaK |
|  | ENMEM-REQ-233118/A-Phone Pairing Mode | | MBORREL4: New req. for PaaK |
|  | ENMEM-REQ-234278/A-Detection of a Keyfob/Phone in Opposite Pairing Mode | | MBORREL4: New req. for PaaK |
|  | ENMEM-HMI-REQ-234279/A-Wrong Device Detected HMI | | MBORREL4: New req. for PaaK |
|  | ENMEM-REQ-198044/B-Detection of Associated Keyfob/Phone | | MBORREL4: Updated to include PaaK |
|  | ENMEM-SR-REQ-198055/C-Enhanced Memory HMI Option for Associated Keyfob/Phone | | MBORREL4: Updated to include PaaK |
|  | ENMEM-REQ-233161/A-Overwrite Associated Phone | | MBORREL4: New req. for PaaK |
|  | ENMEM-REQ-099690/C-Keyfob/Phone Pairing Failed | | MBORREL4: Updated to include PaaK |
|  | ENMEM-REQ-194169/B-Keyfob/Phone Pairing Timer Expired | | MBORREL4: Updated to include PaaK |
|  | ENMEM-TMR-REQ-194101/C-T\_FobAssocTotal2 | | MBORREL4: Updated to include PaaK |
|  | ENMEM-REQ-116804/E-Keyfob/Phone Pairing Error | | MBORREL4: Updated to include PaaK |
|  | ENMEM-SR-REQ-212303/B-PersIndex used for Keyfob/Phone Association | | MBORREL4: Updated to include PaaK |
|  | STR-307929/B-Delete Driver Profiles | | MBORREL4: Updated to include PaaK |
|  | ENMEM-REQ-134465/D-Delete Driver Profile | | MBORREL4: Updated to include PaaK |
|  | ENMEM-HMI-REQ-197502/B-Enhanced Memory HMI Indications for Delete a Driver Profile | | MBORREL4: Updated to include PaaK |
|  | ENMEM-REQ-105569/D-Driver Profiles Deleted During Master Reset | | MBORREL4: Updated to include PaaK |
|  | STR-307928/C-Keyfob/Phone Disassociation | | MBORREL4: Updated to include PaaK, added RED-233009 |
|  | ENMEM-REQ-233209/A-Disassociate the Phone per User Request | | MBORREL4: New req. for PaaK |
|  | ENMEM-REQ-233210/A-Phone Disassociation Status | | MBORREL4: New req. for PaaK |
|  | ENMEM-HMI-REQ-233009/A-Phone HMI Indication | | MBORREL4: New req. for PaaK |
|  | STR-176721/C-Activity Diagrams | | MBORREL4: Added REQ-233257 |
|  | ENMEM-ACT-REQ-233257/A-Associate Phone To Driver Profile | | MBORREL4: New req. for PaaK |
|  | ENMEM-ACT-REQ-099379/D-Delete Driver Profile | | MBORREL4: Updated to include PaaK |
|  | ENMEM-ACT-REQ-197508/B-Master Reset | | MBORREL4: Updated to include PaaK |
|  | STR-176722/C-Sequence Diagrams | | MBORREL4: Added REQ-233258 & REQ-233259 |
|  | ENMEM-SD-REQ-233258/A-Associate Phone | | MBORREL4: New req. for PaaK |
|  | ENMEM-SD-REQ-233259/A-Disassociate Phone | | MBORREL4: New req. for PaaK |
|  | ENMEM-SD-REQ-099427/D-Delete Driver Profile | | MBORREL4: Updated to include PaaK |
|  | ENMEM-SD-REQ-197509/B-Master Reset | | MBORREL4: Updated to include PaaK |
|  | ENMEM-FUN-REQ-195573/C-EnhancedMemoryInterfaceClient HMI Requirements – APIM | | MBORREL4: Added REQ-233009, REQ-233260, REQ-234279, REQ-233264 |
|  | STR-297590/E-Requirements | | MBORREL4: Added REQ-233009, REQ-233260, REQ-234279, REQ-233264 |
|  | ENMEM-HMI-REQ-195574/B-HMI Timeout for Overall Keyfob/Phone Pairing Process | | MBORREL4: Updated to include PaaK |
|  | ENMEM-TMR-REQ-194098/C-T\_FobAssocTotal | | MBORREL4: Updated to include PaaK |
|  | ENMEM-HMI-REQ-195576/B-HMI Timeout for One Keyfob/Phone Pairing Attempt | | MBORREL4: Updated to include PaaK |
|  | ENMEM-TMR-REQ-194099/C-T\_FobAssocOneTime | | MBORREL4: Updated to include PaaK |
|  | ENMEM-HMI-REQ-195575/B-Number of Retries on HMI for Keyfob/Phone Pairing | | MBORREL4: Updated to include PaaK |
|  | ENMEM-REQ-179346/B-N\_NumberOfRetries | | MBORREL4: Updated to include PaaK |
|  | ENMEM-HMI-REQ-233009/A-Phone HMI Indication | | MBORREL4: New req. for PaaK |
|  | ENMEM-HMI-REQ-197850/B-Enhanced Memory HMI Indications for Driver Profile | | MBORREL4: Updated to include PaaK |
|  | ENMEM-SR-REQ-198055/C-Enhanced Memory HMI Option for Associated Keyfob/Phone | | MBORREL4: Updated to include PaaK |
|  | ENMEM-HMI-REQ-197502/B-Enhanced Memory HMI Indications for Delete a Driver Profile | | MBORREL4: Updated to include PaaK |
|  | ENMEM-HMI-REQ-233260/A-Keyfob & Phone Association During Profile Creation | | MBORREL4: New Req. for PaaK |
|  | ENMEM-HMI-REQ-234279/A-Wrong Device Detected HMI | | MBORREL4: New req. for PaaK |
|  | ENMEM-HMI-REQ-233264/A-Phone Association HMI Option | | MBORREL4: New Req. for PaaK |
|  |  |  |  |
| **February 1, 2017** | **1.8** | **Updated Release** |  |
|  | ENMEM-IIR-REQ-099363/G-EnhancedMemoryInterfaceClient\_Rx | | MBORREL4: Added REQ-238321 and updated table to include PaaKConnection\_St |
| MD-REQ-238321/A-PaakConnection\_St | | wstephe1: Added method description to indicate whether a PaaK device (phone) is connected |
| ENMEM-UC-REQ-095721/C-Create a Driver Profile | | MBORREL4: Updated to include Park as a pre-condition (clarification, no new content) |
|  | ENMEM-UC-REQ-134147/C-Create or Edit Driver Profile Name | | MBORREL4: Updated to include Park as a pre-condition (clarification, no new content) |
|  | ENMEM-UC-REQ-095929/D-Delete a Driver Profile | | MBORREL4: Corrected keyfob/phone disassociation post conditions |
|  | ENMEM-REQ-099686/C-Keyfob Pairing Mode | | MBORREL4: Updated to include Park for exit condition (clarification, no new content) |
|  | ENMEM-REQ-233118/B-Phone Pairing Mode | | MBORREL4: Updated to include Park for exit condition (clarification, no new content) |
|  | ENMEM-REQ-099690/D-Keyfob/Phone Pairing Failed | | MBORREL4: Removed recalls from memory seat button during keyfob or phone association. That is no longer allowed |
|  | ENMEM-SD-REQ-099425/F-Create Driver Profile | | MBORREL4: Updated Precondition to include Park (correction, no new content) |
|  | ENMEM-SD-REQ-099422/D-Associate Key Fob | | MBORREL4: Updated Precondition to include Park (correction, no new content) |
|  | ENMEM-SD-REQ-233258/B-Associate Phone | | MBORREL4: Updated Precondition to include Park (correction, no new content) |
|  | ENMEM-HMI-REQ-233264/B-Phone Association HMI Option | | MBORREL4: Updated to include new signal name |
|  |  |  |  |
| **June 6, 2018** | **1.9** | **Updated Release** |  |
|  | MD-REQ-238321/B-PaaKConnection\_St | | cwu3: change Logic name typo (Paak) to PaaK. No content changes. |
| ENMEM-SR-REQ-136593/M-Network Bus Start-up / Shut-down (EnhancedMemoryServer) | | MBORREL4: Removed line regarding B+ Reset, contradicts REQ-207325 |
| ENMEM-UC-REQ-136944/C-Sign Into a Driver Profile via Memory Seat Button While Vehicle In Motion | | MBORREL4: Clarification (8 KPH, not 5 KPH) |
|  | ENMEM-UC-REQ-095934/C-Memory Seat Button Recall of the Active Driver Profile | | MBORREL4: Clarification (8 KPH, not 5 KPH) |
|  | ENMEM-UC-REQ-095939/C-Sign Into a Driver Profile via HMI Menu | | MBORREL4: Clarification (8 KPH, not 5 KPH) |
|  | ENMEM-REQ-099693/E-Display Data Refresh After Driver Profile Change | | MBORREL4: Updated to clarify that all Clients that display any EnMem settings shall perform refresh. |
|  | ENMEM-SR-REQ-136618/F-Recall Event - Infotainment Audio | | MBORREL4: Updated to include TA. Added detail regarding Feature Volume session behavior |
|  | ENMEM-REQ-099674/C-Requesting Audio Preset Info After Profile Change | | MBORREL4: Updated to include to all Clients that display audio presets |
|  | ENMEM-TMR-REQ-099763/C-T\_PersPresetWait | | MBORREL4: Updated to include to all Clients that display audio presets |
|  | ENMEM-REQ-099699/D-Disable Driver Profile Creation and Editing When Key is Not in Run or Vehicle Speed is greater than 8KPH+ | | MBORREL4: Updated title for clarification (8 KPH, not 5 KPH) |
|  | ENMEM-REQ-099699/E-Disable Driver Profile Creation and Editing When Key is Not in Run or Vehicle Speed is greater than 8KPH | | MBORREL4: Updated to specify that Gear=Park is for Auto Trans vehicles only. |
|  | ENMEM-REQ-116802/E-Profile Creation Interruption+ | | MBORREL4: Clarification (8 KPH, not 5 KPH) |
|  | ENMEM-REQ-116802/F-Profile Creation Interruption | | MBORREL4: Updated to include domain changes |
|  | ENMEM-REQ-116804/F-Keyfob/Phone Pairing Error | | MBORREL4: Updated to include domain changes |
| **Feb, 10 2020** | **1.91** | **Updated Release** |  |
|  | 4.5 Create profile modified | | Modify the profile create logic with the hard button removed |
| 4.7 New added function-dialog | | The IVI need display a dialog after mirror and seat manual moving |
| 4.8 New added function-save from IVI | | The user can choose the save button on the dialog |
|  | 4.9 New added function-restore | | The user can choose the restore button on the dialog |
|  |  | |  |
|  |  | |  |
|  |  | |  |
|  |  | |  |
|  |  | |  |
|  |  | |  |
|  |  | |  |
|  |  | |  |
|  |  | |  |
|  |  | |  |

**Table of Contents**

[Revision History 2](#_Toc36750556)

[1 Overview 10](#_Toc36750557)

[2 Architectural Design 11](#_Toc36750558)

[2.1 ENMEM-CLD-REQ-099554/D-Enhanced Memory Interface Client - APIM 11](#_Toc36750559)

[2.2 ENMEM-CLD-REQ-099555/C-Enhanced Memory Position Client - DSM 11](#_Toc36750560)

[2.3 ENMEM-CLD-REQ-099556/E-Enhanced Memory Profile Server - BCM 11](#_Toc36750561)

[2.4 ENMEM-CLD-REQ-099557/D-Enhanced Memory Server 11](#_Toc36750562)

[2.5 ENMEM-CLD-REQ-134131/B-Enhanced Memory Server - APIM 11](#_Toc36750563)

[2.5.1 ENMEM-FUR-REQ-134134/K-Enhanced Memory Features Supported - APIM 11](#_Toc36750564)

[2.6 EnhancedMemoryInterfaceClient Interface - APIM 14](#_Toc36750565)

[2.6.1 ENMEM-IIR-REQ-099360/G-EnhancedMemoryInterfaceClient\_Tx 14](#_Toc36750566)

[2.6.2 ENMEM-IIR-REQ-099363/G-EnhancedMemoryInterfaceClient\_Rx 17](#_Toc36750567)

[2.7 EnhancedMemoryServer Interface 22](#_Toc36750568)

[2.7.1 ENMEM-IIR-REQ-099371/B-EnhancedMemoryServer\_Rx 22](#_Toc36750569)

[3 General Requirements 24](#_Toc36750570)

[3.1 ENMEM-REQ-116801/Scope of this document 24](#_Toc36750571)

[3.2 ENMEM-REQ-116801/D-Retain Enhanced Memory Settings After Software Reflash 24](#_Toc36750572)

[3.3 ENMEM-REQ-206864/A-EnhancedMemoryServers to Retain Settings After Software Reflash 24](#_Toc36750573)

[3.4 ENMEM-SR-REQ-207325/A-Updates to Non-Volatile Memory 24](#_Toc36750574)

[3.5 ENMEM-REQ-134099/B-MyKey Takes Precedence Over Driver Profile Settings 24](#_Toc36750575)

[3.6 ENMEM-REQ-136642/B-Driver Distraction 24](#_Toc36750576)

[3.7 ENMEM-REQ-198389/B-Enhanced Memory Ignition Restriction 24](#_Toc36750577)

[3.8 ENMEM-REQ-136644/A-Crank Event - Enhanced Memory 25](#_Toc36750578)

[3.9 ENMEM-REQ-136692/C-Enhanced Memory Feature Classification 25](#_Toc36750579)

[3.10 ENMEM-SR-REQ-136936/C-Request/Response return to Null state 25](#_Toc36750580)

[3.11 ENMEM-TMR-REQ-198777/A-T\_ReturnToNull 25](#_Toc36750581)

[3.12 ENMEM-SR-REQ-136937/E-Enhanced Memory Feature Inclusion Guidelines 25](#_Toc36750582)

[3.13 ENMEM-REQ-137866/A-Recall and Sign-In term consolidation 25](#_Toc36750583)

[3.14 ENMEM-REQ-137867/B-Keyfob/Phone Association Term Consolidation 25](#_Toc36750584)

[3.15 ENMEM-REQ-166096/E-Operations Shall Not Recall a Driver Profile 26](#_Toc36750585)

[3.16 ENMEM-REQ-232557/A-Phone & Phone-As-A-Key 26](#_Toc36750586)

[4 Functional Definition 27](#_Toc36750587)

[4.1 ENMEM-FUN-REQ-136591/B-System Start-Up and Shut Down 27](#_Toc36750588)

[4.1.1 Requirements 27](#_Toc36750589)

[4.2 ENMEM-FUN-REQ-095956/A-Enable/Disable Driver Profiles 29](#_Toc36750590)

[4.2.1 Use Cases 29](#_Toc36750591)

[4.2.2 Requirements 30](#_Toc36750592)

[4.2.3 White Box View 32](#_Toc36750593)

[4.3 ENMEM-FUN-REQ-095957/B-Sign-In/Recall Settings 35](#_Toc36750594)

[4.3.1 Recall Function Description 35](#_Toc36750595)

[4.3.2 Use Cases 35](#_Toc36750596)

[4.3.3 Requirements 40](#_Toc36750597)

[4.3.4 White Box View 44](#_Toc36750598)

[4.4 ENMEM-FUN-REQ-095958/A-Store Occupant Position Settings 51](#_Toc36750599)

[4.4.1 Use Cases 51](#_Toc36750600)

[4.4.2 Requirements 52](#_Toc36750601)

[4.4.3 White Box View 52](#_Toc36750602)

[4.5 ENMEM-FUN-REQ-095959/A-Create/Edit Driver Profile 55](#_Toc36750603)

[4.5.1 Use Cases 55](#_Toc36750604)

[4.5.2 Requirements 60](#_Toc36750605)

[4.5.3 White Box View 73](#_Toc36750606)

[4.6 ENMEM-FUN-REQ-195573/C-EnhancedMemoryInterfaceClient HMI Requirements - APIM 88](#_Toc36750607)

[4.6.1 Requirements 88](#_Toc36750608)

[5 Appendix: Reference Documents 102](#_Toc36750609)

# Overview

The Enhanced Memory feature introduces the Driver Profiles concept which extends memory capability of the vehicle. The current memory capability, commonly referred to as “Classic Memory,” only covers things related to driver position such as seat position, exterior mirror position and steering column position. With the addition of a driver profiles the memory capabilities are expanded to include many other settings that may include but are not limited to radio presets, navigation preferences, and drive assist settings.

Enhanced Memory allows a driver to create a unique profile that, when active, will automatically save included settings and keep those settings associated to this profile. The unique profile will be associated to one of the “Classic Memory” driver seat buttons and the driver can use this button to sign into his/her profile. The driver may also elect to associate a keyfob or phone to his/her profile such that when the unlock button of the chosen keyfob or phone is pressed, the driver is automatically signed into his/her associated profile. Additionally the driver has the option to sign-into his/her profile through the infotainment screen HMI.

# Architectural Design

## ENMEM-CLD-REQ-099554/D-Enhanced Memory Interface Client - APIM

The EnhancedMemoryInterfaceClient is responsible for the tasks listed below.

* Offering the user an interface to turn on and off Enhanced Memory feature
* Offering the user an interface to create, edit, delete and change Driver Profiles
* Displaying information related to the active Driver Profile
* Providing indications of changes to the active Driver Profile
* Indicating which Driver Profiles have been created (pers1-4 possible) to the vehicle system interface
* Maintaining the mapping of the created Driver Profile names to the network personality index

Please review the implementation guide/block diagram to locate the EnhanceMemoryInterfaceClient class

## ENMEM-CLD-REQ-099555/C-Enhanced Memory Position Client - DSM

The EnhancedMemoryPositionClient is responsible for the tasks listed below.

* Maintaining the settings related to driver position and its relation to the active personality profile
* Selecting the proper driver position (seat position, exterior mirror position, steering column position) as determined by the active personality profile signal on the vehicle network interface
* Requesting changes the active personality profile when it detects a memory seat button is pressed
* Making changes to the position settings when a setting store operation is detected via a memory seat button

Please review the implementation guide/block diagram to locate the EnhancedMemoryPositionClient object.

## ENMEM-CLD-REQ-099556/E-Enhanced Memory Profile Server - BCM

The EnhancedMemoryProfileServer is responsible for the tasks listed below.

* Determining the active Driver Profile
* Broadcasting the active Driver Profile to vehicle network interface
* Associating or Disassociating a selected keyfob or phone to/from a selected Driver Profile

Review the implementation guide/block diagram to locate the EnhancedMemoryProfileServer class.

## ENMEM-CLD-REQ-099557/D-Enhanced Memory Server

The EnhancedMemoryServer is responsible for the tasks listed below.

* Executing settings for the active Driver Profile as requested by the vehicle system interface
* Maintaining settings for four separate Driver Profiles and one Vehicle Profile

Please review the implementation guide/ block diagram to locate the EnhancedMemoryServer class

## ENMEM-CLD-REQ-134131/B-Enhanced Memory Server - APIM

### ENMEM-FUR-REQ-134134/K-Enhanced Memory Features Supported - APIM

|  |  |  |  |
| --- | --- | --- | --- |
| **Remembered Feature** | **Remembered Settings** | **Affected Module** | **Feature Name** |
| Screen Display Settings & Vehicle Settings | Center Stack Display: Auto Dim, Screen Mode, Brightness, etc  Vehicle Setting |  |  |
|  | Clock Settings | APIM (Internal) | Time Zone |
|  | Display Settings | APIM (Internal) | Screen mode (ie day/night mode) |
|  | Display Settings | APIM (Internal) | Auto Dim |
|  | Display Settings | APIM (Internal) | Screen Brightness |
|  | Touchscreen Settings | APIM (Internal) | Sounds - Touchscreen button beep |
|  | Touchscreen Settings | APIM (Internal) | Sounds - EFP Button Beep |
|  | Language Settings | System interface / APIM (internal) | Language\*\*\* |
|  | Vehicle Settings | System interface | Distance Units |
|  | Vehicle Settings | System interface | Clock (12/24 mode) |
|  | Vehicle Settings | System interface | Temperature Units |
|  | Vehicle Settings | System interface / APIM (internal) | Ambient Lighting\*\* |
|  | Camera Setting | APIM (Internal) | Enhanced Park Aids |
|  | Camera Setting | APIM (Internal) | Rear Camera Delay ON / OFF |
| Audio / Volume Settings | Audio / Volume Settings |  |  |
|  | Volume Settings | System interface | Speed Compensated Volume |
|  | Volume Settings | System interface | Phone Volume |
|  | Volume Settings | System interface | Prompt Volume |
|  | Volume Settings | System interface | Voice Recognition Volume |
|  | Volume Settings | System interface | TA Volume |
|  | Audio Settings | System interface | Equalizer Setting - Bass |
|  | Audio Settings | System interface | Equalizer Setting - Treble |
|  | Audio Settings | System interface | Equalizer Setting - Balance |
|  | Audio Settings | System interface | Equalizer Setting - Fade |
|  | Audio Settings | System interface | Equalizer Setting - Mid |
|  | Audio Settings | System interface | Audio Occupancy Modes |
| Phone | Phone |  |  |
|  | Favorite Phone | APIM (internal) | Favorite Phone  (includes phone settings: ring tone,  Phonebook sorting…) |
| Voice Recognition Settings | Center Stack Display: Interaction Mode, Confirmation Prompts |  |  |
|  | Voice Recognition Settings | APIM (Internal) | Voice Recognition – Advance Mode |
|  | Voice Recognition Settings | APIM (Internal) | Voice Recognition – Phone Confirmation |
|  | Voice Recognition Settings | APIM (Internal) | Voice Recognition – Voice Command List |
| Navigation Preferences and Settings | Center Stack Display: Navigation: Map Preferences, Route Preferences, Navigation Preferences, Traffic Preferences, Avoid Areas. |  |  |
|  | Navigation Settings | APIM (Internal) | Nav Prefs - Guidance Prompts |
|  | Navigation Settings | APIM (Internal) | Nav Prefs - Parking POI Notification |
|  | Navigation Settings | APIM (Internal) | Route Prefs - Preferred Route |
|  | Navigation Settings | APIM (Internal) | Route Prefs - Avoid Freeways |
|  | Navigation Settings | APIM (Internal) | Route Prefs - Avoid Tollroads |
|  | Navigation Settings | APIM (Internal) | Route Prefs - Avoid Ferries / Car trains |
|  | Navigation Settings | APIM (Internal) | Route Preferences - Use HOV Lanes |
|  | Navigation Settings | APIM (Internal) | Route Prefs - Avoid Tunnels |
|  | Navigation Settings | APIM (Internal) | Map Prefs - Map Content - Breadcrumbs |
|  | Navigation Settings | APIM (Internal) | Map Prefs - Map Content - Point of Interest (POI) Icons |
|  | Navigation Settings | APIM (Internal) | POI map overlay |
|  | Navigation Settings | APIM (Internal) | Previous destinations |
|  | Navigation Settings | APIM (Internal) | Traffic Prefs - traffic (map) |
|  | Navigation Settings | APIM (Internal) | Dynamic Route Guidance (On/Off) |

* Note when says “System interface” it can be something as simple as monitoring the status signals which APIM module should be doing already (ex Audio Settings, Vehicle Settings, Volume periodic status messages). See enhanced memory SPSS functional requirements for how this is done
  + If don’t have an \* asterisk(s) next to a feature name marked as System Interface there should be no new requirements that need to be added to the SPSS features/functions.
* \*\* For Ambient Lighting to support enhanced memory see “Ambient Lighting – Variant 2”
* \*\*\* For Language see SPSS updates for Language and enhanced memory

## EnhancedMemoryInterfaceClient Interface - APIM

### ENMEM-IIR-REQ-099360/G-EnhancedMemoryInterfaceClient\_Tx

The EnhancedMemoryInterfaceClient\_Tx represents all the Enhanced Memory feature related signals transmitted by the EnhancedMemoryInterfaceClient object. The below table represents the mapping of the logical signal names (as described in this specification) to the global GSDB signal names.

|  |  |  |
| --- | --- | --- |
| **Logical Signal Name** | **Parameter Name** | **GSDB Signal Name** |
| EnMemProfilePairing\_Rq | PersIndex | EmPrflNo\_D\_Rq |
| ButtonPairing | EmPrflButtnAssoc\_D\_Rq |
| KeyPairing | EmPrflKeyAssoc\_D\_Rq |
| EnhancedMemory\_St | Status | Em\_D\_Stat |
| InfotainmentPersStore\_Rq | PersIndex | PersStore\_D\_Rq |
| InfotainmentRecall\_Rq | PersIndex | CntrStk\_D\_RqRecall |
| PersonalityOptIn\_St | Pers1Status | Pers1OptIn\_B\_Stats |
| Pers2Status | Pers2OptIn\_B\_Stats |
| Pers3Status | Pers3OptIn\_B\_Stats |
| Pers4Status | Pers4OptIn\_B\_Stats |
| Feature\_Rq | Operation | CtrStkDsplyOp\_D\_Rq |
| FeatureID | CtrStkFeatNoActl |
| Configuration | CtrStkFeatConfigActl |
| PersIndex | CtrStkPersIndex\_D\_Actl |
| FactoryReset\_Rq | Type | SDARS\_FactoryReset\_Rq |

Note:  GSDB signal names are reference only.  The Global Signal Database (GSDB) is the master for all signals.  If there is a conflict bring to the module D&R’s attention.

#### MD-REQ-099304/D-EnMemProfilePairing\_Rq

Message Type: Request

The signal is used to request that the Enhanced Memory Position Client or Enhanced Memory Profile Server make a change to the state of memory seat button pairing mode, keyfob pairing mode, or phone pairing mode.

|  |  |  |  |
| --- | --- | --- | --- |
| **Name** | **Literals** | **Value** | **Description** |
| PersIndex | - | - | Indicates which Personality Profile the "Pairing" request is referring to.  Received by Enhanced Memory Profile Server only |
|  | Null | 0x0 |  |
|  | Pers1 | 0x1 |  |
|  | Pers2 | 0x2 |  |
|  | Pers3 | 0x3 |  |
|  | Pers4 | 0x4 |  |
|  | NotUsed | 0x5 |  |
|  | NotUsed | 0x6 |  |
|  | NotUsed | 0x7 |  |
| ButtonPairing | - | - | Indicates the Personality Profile button pairing mode request value. Received by Enhanced Memory Position Client only |
|  | Null | 0x0 |  |
|  | EnterButtonPairing | 0x1 |  |
|  | ExitButtonPairing | 0x2 |  |
|  | NotUsed | 0x3 |  |
| KeyPairing | - | - | Indicates the Personality Profile key fob and phone pairing mode request value. Received by Enhanced Memory Profile Server only |
|  | Null | 0x0 |  |
|  | EnterKeyPairing | 0x1 |  |
|  | ExitKeyPairing | 0x2 |  |
|  | DisassociateKey | 0x3 |  |
|  | OverwriteKey | 0x4 |  |
|  | EnterPhonePairing | 0x5 |  |
|  | DisassociatePhone | 0x6 |  |

#### MD-REQ-099311/B-EnhancedMemory\_St

Message Type: Status

The signal is used to inform the Enhanced Memory System whether the personality profiles feature is currently active or not.

Notes:

Enhanced Memory Active (enabled) means, Pers1/2/3/4 may be the active personality profile.

Enhanced Memory Not Active (disabled) means, only Guest can be the active personality profile.

|  |  |  |  |
| --- | --- | --- | --- |
| **Name** | **Literals** | **Value** | **Description** |
| Status | - | - | Indicates the status of the Enhanced Memory feature as selected by the driver. |
|  | Null | 0x0 |  |
|  | ProfilesOn | 0x1 |  |
|  | ProfilesOff | 0x2 |  |
|  | NotSupported | 0x3 |  |

#### MD-REQ-099305/A-InfotainmentPersStore\_Rq

Message Type: Request

The signal is used by the EnhancedMemoryInterfaceClient to request current Classic Memory settings be stored to the indicated personality profile by the EnhancedMemorySystem parts.

|  |  |  |  |
| --- | --- | --- | --- |
| **Name** | **Literals** | **Value** | **Description** |
| PersIndex | - | - | Indicates the Personality Profile the requested store operation is referring to. |
|  | Null | 0x0 |  |
|  | Pers1 | 0x1 |  |
|  | Pers2 | 0x2 |  |
|  | Pers3 | 0x3 |  |
|  | Pers4 | 0x4 |  |
|  | Vehicle | 0x5 |  |

#### MD-REQ-099308/A-InfotainmentRecall\_Rq

Message Type: Request

The signal is used by the Enhanced Memory Interface Client to change the active personality profile to the personality profile indicated in the request.

|  |  |  |  |
| --- | --- | --- | --- |
| **Name** | **Literals** | **Value** | **Description** |
| PersIndex | - | - | Indicates the Personality Profile being requested. |
|  | Null | 0x0 |  |
|  | Pers1 | 0x1 |  |
|  | Pers2 | 0x2 |  |
|  | Pers3 | 0x3 |  |
|  | Pers4 | 0x4 |  |
|  | Vehicle | 0x5 |  |

#### MD-REQ-099309/A-PersonalityOptIn\_St

Message Type: Status

The signal is used to inform the Enhanced Memory Profile Server which personality profiles have been created (Opted-In).

|  |  |  |  |
| --- | --- | --- | --- |
| **Name** | **Literals** | **Value** | **Description** |
| Pers1Status | - | - | Indicates Personality Profile 1 Opt-In Status. |
|  | NotOptedIn | 0x0 |  |
|  | OptedIn | 0x1 |  |
| Pers2Status | - | - | Indicates Personality Profile 2 Opt-In Status. |
|  | NotOptedIn | 0x0 |  |
|  | OptedIn | 0x1 |  |
| Pers3Status | - | - | Indicates Personality Profile 3 Opt-In Status. |
|  | NotOptedIn | 0x0 |  |
|  | OptedIn | 0x1 |  |
| Pers4Status | - | - | Indicates Personality Profile 4 Opt-In Status. |
|  | NotOptedIn | 0x0 |  |
|  | OptedIn | 0x1 |  |

#### MD-REQ-014068/A-Feature\_Rq (TcSE ROIN-282333-2)

Message Type: Request

Represents the request to command a feature change (select new feature, change feature setting, query features, etc.).

Included Parameters:

Operation

FeatureID

Configuration

PersIndex

|  |  |  |  |
| --- | --- | --- | --- |
| **Name** | **Literals** | **Value** | **Description** |
| Operation | **-** | **-** | Type of operation being requested |
|  | Null | 0x0 |  |
|  | Query | 0x1 |  |
|  | Set | 0x2 |  |
|  | Upload | 0x3 |  |
|  | Restore | 0x4 |  |
|  | Copy | 0x5 |  |
|  | NotUsed | 0x6 – 0x7 |  |
| FeatureID | **-** | **-** | Feature number being requested |
|  |  | 0x0000 – 0xFFFF |  |
| Configuration | **-** | **-** | Configuration value being requested |
|  |  | 0x0000 – 0xFFFF |  |
| PersIndex | **-** | **-** | Indicates which personality profile is being accessed |
|  | PERS\_1 | 0x0 |  |
|  | PERS\_2 | 0x1 |  |
|  | PERS\_3 | 0x2 |  |
|  | PERS\_4 | 0X3 |  |
|  | VEHICLE | 0X4 |  |
|  | Not Used | 0x5 |  |
|  | Not Used | 0x6 |  |
|  | Not Used | 0x7 |  |

#### MD-REQ-015018/A-FactoryReset\_Rq (TcSE ROIN-284876-1)

Message Type: Request

Note: Reset all user adjustable parameters to the factory default setting.

|  |  |  |  |
| --- | --- | --- | --- |
| Name | Literals | Value | Description |
| Type | - | - | Reset all user adjustable parameters to the factory default setting. |
|  | Int Reset |  |  |
|  | Invalid | 0x0 |  |
|  | Reset | 0x1 |  |
|  |  |  |  |

### ENMEM-IIR-REQ-099363/G-EnhancedMemoryInterfaceClient\_Rx

The EnhancedMemoryInterfaceClient\_Rx represents all the Enhanced Memory feature related signals received by the EnhancedMemoryInterfaceClient object. The below table represents the mapping of the logical signal names (as described in this specification) to the global GSDB signal names.

|  |  |  |
| --- | --- | --- |
| **Logical Signal Name** | **Parameter Name** | **GSDB Signal Name** |
| ActivePersonality\_St | PersIndex | PersNo\_D\_Actl |
| EnMemButtonPairing\_St | ButtonPairing | EmButtn\_D\_Stat |
| EnMemKeyPairing\_St | PersIndex | EmPrflNo\_D\_Stat |
| KeyPairing | EmPrflKeyAssoc\_D\_Stat |
| InfotainmentPersStore\_St | Status | PersStore\_D\_Actl |
| PersonalityRecallCount\_St | CountValue | RecallEvent\_No\_Cnt |
| PersKeyPairing\_St | Pers1KeyStatus | Pers1Key\_D\_Stat |
| Pers2KeyStatus | Pers2Key\_D\_Stat |
| Pers3KeyStatus | Pers3Key\_D\_Stat |
| Pers4KeyStatus | Pers4Key\_D\_Stat |
| PersPhonePairing\_St | Pers1PhoneStatus | Pers1Phone\_D\_Stat |
| Pers2PhoneStatus | Pers2Phone\_D\_Stat |
| Pers3PhoneStatus | Pers3Phone\_D\_Stat |
| Pers4PhoneStatus | Pers4Phone\_D\_Stat |
| PaakConnection\_St | Status | PaakCnnct\_D\_Stat |

Note:  GSDB signal names are reference only.  The Global Signal Database (GSDB) is the master for all signals.  If there is a conflict bring to the module D&R’s attention.

#### MD-REQ-099354/E-ActivePersonality\_St

Message Type: Status

The signal is used to inform the Enhanced Memory System which personality profile is currently active.

|  |  |  |  |
| --- | --- | --- | --- |
| **Name** | **Literals** | **Value** | **Description** |
| PersIndex | - | - | Indicates which Personality Profile is currently active. |
|  | Pers1 | 0x0 |  |
|  | Pers2 | 0x1 |  |
|  | Pers3 | 0x2 |  |
|  | Pers4 | 0x3 |  |
|  | Vehicle | 0x4 |  |
|  | NotDetermined | 0x5 |  |
|  | NotUsed | 0x6 |  |
|  | NotUsed | 0x7 |  |

#### MD-REQ-099312/A-EnMemButtonPairing\_St

Message Type: Status

The signal is used to inform the Enhanced Memory Interface Client the status of memory seat button pairing mode.

|  |  |  |  |
| --- | --- | --- | --- |
| **Name** | **Literals** | **Value** | **Description** |
| ButtonPairing | - | - | Indicates the Personality Profile memory seat button pairing mode status value. |
|  | Null | 0x0 |  |
|  | Button1Pressed | 0x1 |  |
|  | Button2Pressed | 0x2 |  |
|  | Button3Pressed | 0x3 |  |
|  | Button4Pressed | 0x4 |  |
|  | ButtonPairingEntered | 0x5 |  |
|  | ButtonPairingExited | 0x6 |  |
|  | ButtonPairingFailed | 0x7 |  |

#### MD-REQ-099352/C-EnMemKeyPairing\_St

Method Type: Status

The signal is used to inform the Enhanced Memory Interface Client the status of key fob and phone pairing modes.

|  |  |  |  |
| --- | --- | --- | --- |
| **Name** | **Literals** | **Value** | **Description** |
| PersIndex | - | - | Indicates which Personality Profile the "Pairing" status is referring to. |
|  | Null | 0x0 |  |
|  | Pers1 | 0x1 |  |
|  | Pers2 | 0x2 |  |
|  | Pers3 | 0x3 |  |
|  | Pers4 | 0x4 |  |
|  | NotUsed | 0x5 |  |
|  | NotUsed | 0x6 |  |
|  | NotUsed | 0x7 |  |
| KeyPairing | - | - | Indicates the Personality Profile key fob and phone pairing mode status value. |
|  | Null | 0x0 |  |
|  | KeyPairingEntered | 0x1 |  |
|  | KeyPairingExited | 0x2 |  |
|  | KeyDisassociated | 0x3 |  |
|  | KeyAlreadyInUse | 0x4 |  |
|  | KeyAssociateSuccess | 0x5 |  |
|  | KeyAssociateFailed | 0x6 |  |
|  | WrongDeviceSelected | 0x7 |  |

#### MD-REQ-099349/A-InfotainmentPersStore\_St

Message Type: Status

The signal is used to inform the Enhanced Memory Interface Client the status of a requested store event.

|  |  |  |  |
| --- | --- | --- | --- |
| **Name** | **Literals** | **Value** | **Description** |
| Status | - | - | Indicates the Personality Profile the store operation completed for. |
|  | Complete | 0x0 |  |
|  | InProgress | 0x1 |  |
|  | Null | 0x2 |  |

#### MD-REQ-099356/A-PersonalityRecallCount\_St

Message Type: Status

The signal is used to inform the Enhanced Memory System a change in personality profile has occurred (counter is incremented each time a profile change occurs).

|  |  |  |  |
| --- | --- | --- | --- |
| **Name** | **Literals** | **Value** | **Description** |
| CountValue | - | - | Increment indicates a change to active personality profile. |
|  | 0 | 0x0 |  |
|  | 1 | 0x1 |  |
|  | … |  |  |
|  | 255 | 0xFF |  |

#### MD-REQ-197231/A-PersKeyPairing\_St

Message Type: Status

The signal is used to inform the EnhancedMemoryInterfaceClient if a personality profile has a keyfob associated to it or not.

|  |  |  |  |
| --- | --- | --- | --- |
| **Name** | **Literals** | **Value** | **Description** |
| Pers1KeyStatus | - | - | Indicates Personality Profile 1 Keyfob Association Status. |
|  | Null | 0x0 |  |
|  | Key Associated | 0x1 |  |
|  | Key Not Associated | 0x2 |  |
|  | Reserved | 0x3 |  |
| Pers2KeyStatus | - | - | Indicates Personality Profile 2 Keyfob Association Status. |
|  | Null | 0x0 |  |
|  | Key Associated | 0x1 |  |
|  | Key Not Associated | 0x2 |  |
|  | Reserved | 0x3 |  |
| Pers3KeyStatus | - | - | Indicates Personality Profile 3 Keyfob Association Status. |
|  | Null | 0x0 |  |
|  | Key Associated | 0x1 |  |
|  | Key Not Associated | 0x2 |  |
|  | Reserved | 0x3 |  |
| Pers4KeyStatus | - | - | Indicates Personality Profile 4 Keyfob Association Status. |
|  | Null | 0x0 |  |
|  | Key Associated | 0x1 |  |
|  | Key Not Associated | 0x2 |  |
|  | Reserved | 0x3 |  |

#### MD-REQ-233493/A-PersPhonePairing\_St

Message Type: Status

The signal is used to inform the EnhancedMemoryInterfaceClient if a personality profile has a phone (or phones) associated to it or not.

|  |  |  |  |
| --- | --- | --- | --- |
| **Name** | **Literals** | **Value** | **Description** |
| Pers1PhoneStatus | - | - | Indicates Personality Profile 1 Phone Association Status. |
|  | No Phones Associated | 0x0 |  |
|  | One Phone Associated | 0x1 |  |
|  | Two Phones Associated | 0x2 |  |
|  | Three Phones Associated | 0x3 |  |
|  | Four Phones Associated | 0x4 |  |
|  | Five Phones Associated | 0x5 |  |
|  | Six Phones Associated | 0x6 |  |
|  | Seven Phones Associated | 0x7 |  |
| Pers2PhoneStatus | - | - | Indicates Personality Profile 2 Phone Association Status. |
|  | No Phones Associated | 0x0 |  |
|  | One Phone Associated | 0x1 |  |
|  | Two Phones Associated | 0x2 |  |
|  | Three Phones Associated | 0x3 |  |
|  | Four Phones Associated | 0x4 |  |
|  | Five Phones Associated | 0x5 |  |
|  | Six Phones Associated | 0x6 |  |
|  | Seven Phones Associated | 0x7 |  |
| Pers3PhoneStatus | - | - | Indicates Personality Profile 3 Phone Association Status. |
|  | No Phones Associated | 0x0 |  |
|  | One Phone Associated | 0x1 |  |
|  | Two Phones Associated | 0x2 |  |
|  | Three Phones Associated | 0x3 |  |
|  | Four Phones Associated | 0x4 |  |
|  | Five Phones Associated | 0x5 |  |
|  | Six Phones Associated | 0x6 |  |
|  | Seven Phones Associated | 0x7 |  |
| Pers4PhoneStatus | - | - | Indicates Personality Profile 4 Phone Association Status. |
|  | No Phones Associated | 0x0 |  |
|  | One Phone Associated | 0x1 |  |
|  | Two Phones Associated | 0x2 |  |
|  | Three Phones Associated | 0x3 |  |
|  | Four Phones Associated | 0x4 |  |
|  | Five Phones Associated | 0x5 |  |
|  | Six Phones Associated | 0x6 |  |
|  | Seven Phones Associated | 0x7 |  |

#### MD-REQ-238321/B-PaaKConnection\_St

Message Type: Status

This signal is used to inform whether a Phone-As-A-Key is currently connected to the vehicle.

|  |  |  |  |
| --- | --- | --- | --- |
| **Name** | **Literals** | **Value** | **Description** |
| Status | - | - | Indicates the connection status of a PaaK. |
|  | Null | 0x0 |  |
|  | NoneConnected | 0x1 |  |
|  | Connected | 0x2 |  |

## EnhancedMemoryServer Interface

### ENMEM-IIR-REQ-099371/B-EnhancedMemoryServer\_Rx

The EnhancedMemoryServer\_Rx represents all the Enhanced Memory feature related signals received by the EnhancedMemoryServer object. The below table represents the mapping of the logical signal names (as described in this specification) to the global GSDB signal names.

|  |  |  |
| --- | --- | --- |
| **Logical Signal Name** | **Parameter Name** | **GSDB Signal Name** |
| ActivePersonality\_St | PersIndex | PersNo\_D\_Actl |
| PersonalityRecallCount\_St | CountValue | RecallEvent\_No\_Cnt |
| Feature\_Rq | Operation | CtrStkDsplyOp\_D\_Rq |
| FeatureID | CtrStkFeatNoActl |
| Configuration | CtrStkFeatConfigActl |
| PersIndex | CtrStkPersIndex\_D\_Actl |
| FactoryReset\_Rq | Type | SDARS\_FactoryReset\_Rq |

Note:  GSDB signal names are reference only.  The Global Signal Database (GSDB) is the master for all signals.  If there is a conflict bring to the module D&R’s attention.

#### MD-REQ-099354/E-ActivePersonality\_St

Message Type: Status

The signal is used to inform the Enhanced Memory System which personality profile is currently active.

|  |  |  |  |
| --- | --- | --- | --- |
| **Name** | **Literals** | **Value** | **Description** |
| PersIndex | - | - | Indicates which Personality Profile is currently active. |
|  | Pers1 | 0x0 |  |
|  | Pers2 | 0x1 |  |
|  | Pers3 | 0x2 |  |
|  | Pers4 | 0x3 |  |
|  | Vehicle | 0x4 |  |
|  | NotDetermined | 0x5 |  |
|  | NotUsed | 0x6 |  |
|  | NotUsed | 0x7 |  |

#### MD-REQ-099356/A-PersonalityRecallCount\_St

Message Type: Status

The signal is used to inform the Enhanced Memory System a change in personality profile has occurred (counter is incremented each time a profile change occurs).

|  |  |  |  |
| --- | --- | --- | --- |
| **Name** | **Literals** | **Value** | **Description** |
| CountValue | - | - | Increment indicates a change to active personality profile. |
|  | 0 | 0x0 |  |
|  | 1 | 0x1 |  |
|  | … |  |  |
|  | 255 | 0xFF |  |

#### MD-REQ-014068/A-Feature\_Rq (TcSE ROIN-282333-2)

Message Type: Request

Represents the request to command a feature change (select new feature, change feature setting, query features, etc.).

Included Parameters:

Operation

FeatureID

Configuration

PersIndex

|  |  |  |  |
| --- | --- | --- | --- |
| **Name** | **Literals** | **Value** | **Description** |
| Operation | **-** | **-** | Type of operation being requested |
|  | Null | 0x0 |  |
|  | Query | 0x1 |  |
|  | Set | 0x2 |  |
|  | Upload | 0x3 |  |
|  | Restore | 0x4 |  |
|  | Copy | 0x5 |  |
|  | NotUsed | 0x6 – 0x7 |  |
| FeatureID | **-** | **-** | Feature number being requested |
|  |  | 0x0000 – 0xFFFF |  |
| Configuration | **-** | **-** | Configuration value being requested |
|  |  | 0x0000 – 0xFFFF |  |
| PersIndex | **-** | **-** | Indicates which personality profile is being accessed |
|  | PERS\_1 | 0x0 |  |
|  | PERS\_2 | 0x1 |  |
|  | PERS\_3 | 0x2 |  |
|  | PERS\_4 | 0X3 |  |
|  | VEHICLE | 0X4 |  |
|  | Not Used | 0x5 |  |
|  | Not Used | 0x6 |  |
|  | Not Used | 0x7 |  |

#### MD-REQ-015018/A-FactoryReset\_Rq (TcSE ROIN-284876-1)

Message Type: Request

Note: Reset all user adjustable parameters to the factory default setting.

|  |  |  |  |
| --- | --- | --- | --- |
| Name | Literals | Value | Description |
| Type | - | - | Reset all user adjustable parameters to the factory default setting. |
|  | Int Reset |  |  |
|  | Invalid | 0x0 |  |
|  | Reset | 0x1 |  |
|  |  |  |  |

# General Requirements

## ENMEM-REQ-116801/Scope of this document

The vehicle shall be equipped with the classic memory which only include the mirrors and seat position (Such as CD542). If the vehicle’s classic memory is also including HUD and Steering column position, the feature spec shall do the specific modification for that.

The vehicle’s memory button configuration shall consist of the Button1/Button2/Button3 (MemorySetSw\_Cfg=Not Present, such as CD542), if the vehicle’s memory button consists of Button1/Button2/Button Set, the feature spec shall do the specific modification for that.

Also, this document only suitable for the program that replace the hard button with soft button on IVI.

## ENMEM-REQ-116801/D-Retain Enhanced Memory Settings After Software Reflash

The EnhancedMemoryInterfaceClient shall retain Driver Profile information and internally managed settings values after a software reflash occurs. This is to prevent the customer from recreating Driver Profiles and associating keyfobs and/or phone’s after a software reflash service is done at dealership.

The information to be retained shall include opted in and opted out (created and deleted) status of all Driver Profiles, Driver Profile’s keyed-in name and the association of Driver Profile name to Memory Seat button number.

## ENMEM-REQ-206864/A-EnhancedMemoryServers to Retain Settings After Software Reflash

The EnhancedMemoryServers shall retain all personalizable settings for each Driver Profile after a software reflash occurs.

This is to prevent the customer from having to reprogram their settings after a software reflash service performed at a dealership or via Wifi Automatic Software Update. For example, the information to be retained may include Language Settings, Climate Control Settings, Navigation Preferences, etc.

## ENMEM-SR-REQ-207325/A-Updates to Non-Volatile Memory

Personalized settings supported by EnhancedMemoryServers shall be stored in those modules’ NVM (Non-Volatile Memory) in order to survive power loss. These settings shall be saved and updated immediately in the NVM as user changes occur. NVM changes shall not be accumulated for later writing.

## ENMEM-REQ-134099/B-MyKey Takes Precedence Over Driver Profile Settings

If a MyKey is the active key in the vehicle, all MyKey restrictions shall remain active regardless of which driver profile is active. In the event of any conflict between a MyKey restriction and an Enhanced Memory personalized setting, the MyKey restriction shall override the personalized setting.

## ENMEM-REQ-136642/B-Driver Distraction

For the purpose of this document if there are any existing driver distraction requirements and / or guidelines those requirements do apply for enhanced memory and supersede any requirements in this specification.

For any conflicts bring to the attention to the Ford D&R.

## ENMEM-REQ-198389/B-Enhanced Memory Ignition Restriction

Enhanced Memory shall impose ignition restriction to the following specific Enhanced Memory operations:

* Create/add Driver Profiles
* Edit Driver Profiles

These two operations shall be allowed only when ignition is in Run.

## ENMEM-REQ-136644/A-Crank Event - Enhanced Memory

For the purposes of this document when a crank event occurs (ex Ignition\_Status = Crank) it is to be considered a don’t care and assume the last state unless noted otherwise.

* For example if Ignition\_Status = Run and a Crank event happens with Ignition\_Status = Crank and then Ignition\_Status goes back to Run then unless noted otherwise it shall be assumed that in the use cases and functional requirements that Ignition remained in Run.

## ENMEM-REQ-136692/C-Enhanced Memory Feature Classification

The feature classification of Enhanced Memory is B per ES1W7T-F407K00-AA. This means that Enhanced Memory is not a safety feature.

## ENMEM-SR-REQ-136936/C-Request/Response return to Null state

When updating on event, the following event-periodic signals listed below shall hold there signal encoding values for a period of time defined by T\_ReturnToNull and then shall transit back to Null as shown in the sequence diagrams:

* InfotainmentRecall\_Rq
* InfotainmentPersStore\_Rq
* EnMemProfilePairing\_Rq
* EnMemKeyPairing\_St
* MemSwitchRecall\_Rq
* InfotainmentPersStore\_St
* Feature\_Rq

The receiving modules of these signals shall act upon the event signal and shall not wait for the “Null” to act upon the signal request.

## ENMEM-TMR-REQ-198777/A-T\_ReturnToNull

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Name** | **Description** | **Units** | **Range** | **Resolution** | **Default** |
| T\_ReturnToNull | The nominal hold time before returning to a Null state. Use the default value +/- 10%. | sec | 0.5-2 | 0.5 | 1 |

## ENMEM-SR-REQ-136937/E-Enhanced Memory Feature Inclusion Guidelines

As a general guideline, the following conditions were considered to determine if a feature shall be included as part of Enhanced Memory:

* If a setting is reset to a default value at every key cycle, then that setting is not included. One example of this type features is Traction Control setting
* MyKey is not included. All MyKey settings remain the same for different keyfobs, phones, and Driver Profiles within a vehicle. For example, the MyKey Max Speed setting for MyKey keyfob1 and MyKey keyfob2 can only be the same.

Exact features included in Enhanced Memory could vary among different programs and different vehicle packages. Information about program specific Enhanced Memory Feature List can be found in Reference section.

## ENMEM-REQ-137866/A-Recall and Sign-In term consolidation

For purposes of this specification the terms "Recall" and "Sign-In" are used interchangeably and have the same meaning.

## ENMEM-REQ-137867/B-Keyfob/Phone Association Term Consolidation

For purposes of this specification the terms "Link," "Pair," and "Associate" are used interchangeably with respect to describing a keyfob’s or phone’s connection to the Enhanced Memory feature, and thus have the same meaning.

## ENMEM-REQ-166096/E-Operations Shall Not Recall a Driver Profile

Enhanced Memory shall not allow the following operations being used to recall a Driver Profile when Enhanced memory is enabled:

* Entering a keypad code
* Starting engine with an associated or an unassociated keyfob or phone
* Storing positional settings via the Classic Memory Method to a button that has not been associated to a Driver Profile. In this case, the saved Classic Memory positional settings shall be recalled and the Vehicle Profile shall be recalled for applicable soft settings.
* Associating a keyfob or phone to a Driver Profile

## ENMEM-REQ-232557/A-Phone & Phone-As-A-Key

The association of a phone to a Driver Profile shall be supported by use of the Phone-As-A-Key (PaaK) feature. The phone must be setup, authorized, and connected as a PaaK before it can be associated to a Driver Profile.

Refer to the PaaK feature specification for detailed information.

# Functional Definition

## ENMEM-FUN-REQ-136591/B-System Start-Up and Shut Down

### Requirements

#### ENMEM-SR-REQ-136592/M-Network Bus Start-up / Shut-down (EnhancedMemoryProfileServer)

The EnhancedMemoryProfileServer shall update the ActivePersonality\_St signal with the active personality (Vehicle, Pers1 – Pers4) used within 500 msec of network bus wake-up.

* If the ActivePersonality\_St signal is published on the network bus before the value of the signal is known then the ActivePersonality\_St signal shall be set to NotDetermined at network bus start-up.
* Exception: If within the first 500 msec of bus wake-up if the value of ActivePersonality\_St is not known because of an error (ie application powered up and still doesn’t know), then the Enhanced Memory Profile Server shall update the ActivePersonality\_St signal with the default value of Vehicle. This could possibly occur for example if the EEPROM was corrupted.

At network bus wake-up/start-up if the EnhancedMemoryProfileServer receives EnhancedMemory\_St =Null then the EnhancedMemoryProfileServer shall assume the last known state (ex if Enhanced Memory was last ON before network shutdown then assume still ON).

At network bus wake-up/start-up if the EnhancedMemoryProfileServer has not received PersonalityOptIn\_St within 500 msec of network bus wake-up then the EnhancedMemoryProfileServer shall assume the last known state (ex if all profiles were opted-in before network shutdown than assume they are still opted-in).

The EnhancedMemoryProfileServer shall remember the last active personality profile between different power mode cycles such as remembering (but not limited to):

* between network bus sleep and wake-up events, and
* between ignition cycles

Responding to request signals at network bus start-up:

The EnhancedMemoryProfileServer and EnhancedMemoryInterfaceClient can be on different network buses such that one bus is asleep while the other is awake (ex. Infotainment System ON when Ignition\_Status = OFF). In order for request signals not to be lost (first change in the request signal encoding value wakes up the other bus) the following shall be supported:

* The EnhancedMemoryProfileServer shall be able to receive enhanced memory request signals such as “InfotainmentRecall = New PersonX” or “EnhancedMemory = ON/OFF” within 200 msec of network bus wake-up. If the application software is not completely powered up after 200 msec those signals shall be stored and processed later by the EnhancedMemoryProfileServer.

#### ENMEM-SR-REQ-136594/I-Network Bus Start-up / Shut-down (EnhancedMemoryInterfaceClient)

The EnhancedMemoryInterfaceClient shall update the “EnhancedMemory\_St” and “PersonalityOptIn\_St : Pers1/2/3/4Status” signals with the last known state within 500 msec of network bus wake-up.

* If the EnhancedMemory\_St signal is published on the network bus before the last known state can be published then the EnhancedMemory\_St signal shall be set to Null at network bus start-up.
* The “PersonalityOptIn\_St : Pers1/2/3/4Status” signals shall not be published on the bus until the last known state is published and shall not publish its CAN init value at CAN bus start-up.
  + Note: The “PersonalityOptIn\_St : Pers1/2/3/4Status” signals shall not be set to the CAN dB Init value at CAN bus start-up since there is no “Null” value and only put on the bus the last value of the OptIn is published (has to be done within 500 msec of network bus wake-up)

The EnhancedMemoryInterfaceClient shall remember the “EnhancedMemory\_St” and “PersonalityOptIn\_St : Pers1/2/3/4Status” signal settings between different power mode cycles such as remembering:

* between network bus sleep and wake-up events, and
* between ignition cycles, and
* after a B+ reset

Note: ActivePersonality\_St = NotDetermined is treated as a don’t care and shall assume the last known state.

Request signals / Status signal update:

The EnhancedMemoryProfileServer and EnhancedMemoryInterfaceClient can be on different network buses such that one bus is asleep while the other is awake (ex Infotainment System ON while Ignition\_Status = OFF). In order for request signals / updated status signals not to be missed (first change in the signal encoding value wakes up the other bus) the following shall be supported:

* When using the request signal “InfotainmentRecall\_Rq = a new Personality” the EnhancedMemoryInterfaceClient shall send the request and re-send the same request 500 msec later without setting to Null between those two requests (the EnhancedMemoryProfileServer will act on the second request if its bus was asleep when the first request was sent).
* When the status signal EnhancedMemory\_St has an encoding value change (ex ProfilesOn changes to ProfilesOff) the EnhancedMemoryInterfaceClient shall send the updated signal and re-send the same signal 500 msec later (the EnhancedMemoryProfileServer will act on the second signal if its bus was asleep when the first updated signal was sent).
* Note: PersonalityOptIn\_St can only be changed when Ignition\_Status = Run. In Run all the network buses are awake and therefore do not need to re-send the signal.

#### ENMEM-SR-REQ-136593/M-Network Bus Start-up / Shut-down (EnhancedMemoryServer)

At network bus wake-up/start-up the EnhancedMemoryServer shall act on the ActivePersonality\_St and PersonalityRecallCounter\_St signals.

* The EnhancedMemoryServer shall remember the last active personality and PersonalityRecallCounter\_St for the following (but not limited to):
  + between network bus sleep and wake-up events, and
  + between ignition cycles
  + when any network communication failure prevents these signals from being transmitted by the EnhancedMemoryProfileServer

Note: If the last active personality cannot be determined, the EnhancedMemoryServer shall

default to the Vehicle level Profile (Guest Profile).

Note: ActivePersonality\_St = NotDetermined is treated as a don’t care and shall assume the last

known state.

Infotainment Only:

At infotainment system start-up the Infotainment System Master (ex SYNC) shall recall the last savable active audio source prior to the last shutdown. The active audio source is not personalizable for different personality profiles.

* For example if Profile 3 was last active at shutdown with CD as the last active source and if personality Profile 1 (last source SDARS) is active at start-up then the System Master shall still activate CD for personality Profile 1.

If a tuner source was the last savable source at shutdown then at system start-up the last known tuner frequency and band shall be activated regardless of personality Profile used at start-up.

## ENMEM-FUN-REQ-095956/A-Enable/Disable Driver Profiles

### Use Cases

#### ENMEM-UC-REQ-095714/B-Enable Driver Profiles Feature

|  |  |
| --- | --- |
| **Actors** | Vehicle Occupant |
| **Pre-conditions** | The Driver Profiles feature is set to Off (i.e. enhanced memory feature is turned Off). |
| **Scenario Description** | The User accesses the Driver Profiles HMI menu and chooses to enable the Driver Profiles feature (set to On) |
| **Post-conditions** | * The Driver Profiles feature is set to *ON* * New Driver Profiles can be added * Existing Driver Profiles now can be recalled and edited |
| **List of Exception Use Cases** |  |
| **Interfaces** | Personalization Interface |
| **Notes** |  |

#### ENMEM-UC-REQ-095715/C-Disable Driver Profiles Feature

|  |  |
| --- | --- |
| **Actors** | Vehicle Occupant |
| **Pre-conditions** | The Driver Profiles feature is set to On.  At least one Driver Profile has been created. |
| **Scenario Description** | The User accesses the Driver Profiles HMI and chooses to disable the Driver Profiles feature (set to Off). |
| **Post-conditions** | * The Driver Profiles feature is now set to *OFF* * The active Driver Profile is set to *Vehicle (i.e. Guest)* * All applicable non-positional settings will be recalled for the Guest profile * Positional settings remains unchanged * New profiles can no longer be added * Created Driver Profiles are not deleted and are temperately not accessible to the user |
| **List of Exception Use Cases** |  |
| **Interfaces** | Personalization Interface |
| **Notes** | When the feature is turned on again, all created profile will be accessible again |

#### ENMEM-UC-REQ-214249/A-Valet Mode enabled with Enhanced Memory On

|  |  |
| --- | --- |
| **Actors** | Vehicle Occupant |
| **Pre-conditions** | The ignition status is in Run.  The vehicle speed is less than 8 KPH  Enhanced Memory is set to On  Valet Mode is Off |
| **Scenario Description** | The user enables Valet Mode from the HMI |
| **Post-conditions** | Active Personality Profile is remembered  Enhanced Memory is set to Off   * By default, the Guest Profile is recalled   Valet Mode is enabled |
| **Interfaces** | Personalization Interface |

#### ENMEM-UC-REQ-214250/A-Valet Mode disabled with Enhanced Memory On

|  |  |
| --- | --- |
| **Actors** | Vehicle Occupant |
| **Pre-conditions** | The ignition status is in Run.  The vehicle speed is less than 8 KPH  Valet Mode is ON  Enhanced Memory is set to Off (was On prior to enabling Valet Mode) |
| **Scenario Description** | The user disables Valet Mode from the HMI |
| **Post-conditions** | Valet Mode is disabled  Enhanced Memory is set to On  The remembered Active Personality Profile is recalled |
| **List of Exception Use Cases** | ENMEM-UC-REQ-214246-Valet Mode disabled with Enhanced Memory Off |
| **Interfaces** | Personalization Interface |

#### ENMEM-UC-REQ-214246/A-Valet Mode disabled with Enhanced Memory Off

|  |  |
| --- | --- |
| **Actors** | Vehicle Occupant |
| **Pre-conditions** | The ignition status is in Run.  The vehicle speed is less than 8 KPH  Enhanced Memory is set to Off (prior to enabling Valet Mode)  Valet Mode is On |
| **Scenario Description** | The user disables Valet Mode from the HMI |
| **Post-conditions** | Valet Mode is disabled  Enhanced Memory remains Off  No recall is performed |
| **Interfaces** | Personalization Interface |

### Requirements

#### ENMEM-SR-REQ-140360/B-Configurable Parameter to Enable Driver Profiles HMI

The EnhancedMemoryInterfaceClient shall have a configurable parameter to determine whether the vehicle supports the Enhanced Memory feature. If the parameter indicates that the vehicle is to support “Enhanced Memory”, then the Driver Profiles HMI shall be enabled and accessible within the existing HMI menu hierarchy.

#### ENMEM-REQ-099679/B-Enhanced Memory Feature Activation Status

The EnhancedMemoryInterfaceClient shall report the activation status of the Driver Profile feature via the EnhancedMemory\_St method:

* If a user opts in Enhanced memory to create the first Driver Profile, the EnhancedMemoryInterfaceClient shall then update the status of the EnhancedMemory\_St method to indicate that the Driver Profiles feature is currently ON
* If a user selects to turn the Enhanced Memory feature on via HMI interface, the EnhancedMemoryInterfaceClient shall report the status of the EnhancedMemory\_St method as ON to indicate that the Driver Profiles feature is currently ON.
* If the Enhanced Memory Feature is OFF or a user selects to turn the Enhanced Memory feature OFF via HMI interface, the EnhancedMemoryInterfaceClient shall report the status of the EnhancedMemory\_St method as OFF to indicate that the Driver Profiles feature is currently OFF.
* If no profiles exist (either because all have been deleted by the user one by one or via Master Reset), the EnhancedMemoryInterfaceClient shall report the status of the EnhancedMemory\_St method as OFF to indicate that the Driver Profiles feature is currently OFF.

#### ENMEM-REQ-134104/B-Recall Vehicle Profile When Enhanced Memory Feature Is Turned Off

When Enhanced Memory feature is turned Off, as indicated via EnhancedMemory\_St(ProfilesOff), the EnhancedMemoryInterfaceClient shall recall Vehicle Profile via InfotainmentRecall\_Rq

#### ENMEM-REQ-197515/A-Driver Profiles Not Deleted When Enhanced Memory Feature OFF

When Enhanced Memory feature is turned off by the user, the EnhancedMemoryInterfaceClient shall NOT delete existing Driver Profiles so that those Driver Profiles can be accessible to the user when Enhanced Memory feature is set back to on.

#### ENMEM-SR-REQ-214801/A-Enable/Disable Enhanced Memory in Valet Mode

If EnhancedMemory\_St = ProfilesOn when Valet Mode is enabled, the EnhancedMemoryInterfaceClient shall temporarily disable the Enhanced Memory feature by setting EnhancedMemory\_St = ProfilesOff.

When Valet Mode is then disabled, the EnhancedMemoryInterfaceClient shall re-enable the Enhanced Memory feature by setting EnhancedMemory\_St = ProfilesOn.

If EnhancedMemory\_St = ProfilesOff when Valet Mode is enabled, the feature status shall remain set as EnhancedMemory\_St = ProfilesOff when Valet Mode is disabled.

All existing Valet Mode requirements/restrictions apply for Enhanced Memory and supersede any requirements in this specification.

For any conflicts bring to the attention of the Ford D&R.

### White Box View

#### Activity Diagrams

##### ENMEM-ACT-REQ-099381/B-Enable/Disable Driver Profiles Feature

Activity Diagram



#### Sequence Diagrams

##### ENMEM-SD-REQ-099429/A-Enable Driver Profiles

Constraints

Pre-Condition

Driver profiles feature is disabled

Scenarios

Normal Usage

The driver chooses to enable the driver profiles feature (set to on).

Post-Condition

The driver profiles feature is enabled (set to on).

Sequence Diagram



##### ENMEM-SD-REQ-099428/B-Disable Driver Profiles

Constraints

Pre-Condition

Driver profiles feature is enabled

Scenarios

Normal Usage

The driver chooses to disable the driver profiles feature (set to off).

Post-Condition

The driver profiles feature is disabled (set to off).

The active personality profile is set to “Guest”.

Positional settings are unaffected

Sequence Diagram



## ENMEM-FUN-REQ-095957/B-Sign-In/Recall Settings

### Recall Function Description

Recall is a function that loads a requested Driver Profile, via a recall request, as the Active Driver Profile. This provides a user with his/her own personal settings to use and edit while in the vehicle.

The Recall function can be initiated by three different user requests and by an Enhanced Memory system request. A user recall request may be sent by a Memory Seat Button press, by Keyfob or Phone detection (via unlock event or remote start event), and by touch screen manual selection. The Enhanced Memory System recall request may occur when the Active or last Driver Profile is deleted, when a Driver Profile is first created, and when the Enhanced Memory feature is turned from On to Off.

### Use Cases

#### ENMEM-UC-REQ-095719/C-Memory Seat Button Recall with Driver Profiles OFF

|  |  |
| --- | --- |
| **Actors** | Vehicle Occupant |
| **Pre-conditions** | The Driver Profiles feature is set to OFF |
| **Scenario Description** | The User presses any Memory Seat button on the driver door panel |
| **Post-conditions** | The positional settings are recalled for that particular button and the user stays signed into the Guest Profile |
| **List of Exception Use Cases** |  |
| **Interfaces** | Personalization Interface |

#### ENMEM-UC-REQ-095930/C-Sign Into a Driver Profile via Memory Seat Button

|  |  |
| --- | --- |
| **Actors** | Vehicle Occupant |
| **Pre-conditions** | The Driver Profiles feature is set to ON |
| **Scenario Description** | The User presses a memory seat button on the driver door panel that is associated to an alternate Driver Profile (other than the active profile.) |
| **Post-conditions** | All applicable user settings including positional settings that tied with Classic Memory are recalled for that particular button and an HMI indication is given that the user has now signed into the associated Driver Profile for that button. |
| **List of Exception Use Cases** | E1 – ENMEM-UC-REQ-136944/A-Sign Into a Driver Profile via Memory Seat Button While Vehicle In Motion |
| **Interfaces** | Personalization Interface |
| **Note:** | The Guest profile would be considered an “alternate Driver Profile” for any buttons that aren’t associated to a created Driver Profile. |

#### ENMEM-UC-REQ-136944/C-Sign Into a Driver Profile via Memory Seat Button While Vehicle In Motion

|  |  |
| --- | --- |
| **Actors** | Vehicle Occupant |
| **Pre-conditions** | The Driver Profiles feature is set to ON |
| **Scenario Description** | The User presses a Memory Seat button on the driver door panel that is associated to an alternate Driver Profile (other than the active profile) while the vehicle is in motion (not in Park or vehicle speed is greater than 8 KPH for a manual transmission) |
| **Post-conditions** | All applicable user settings, excluding positional settings that are tied with Classic Memory, are recalled for that particular button and an HMI indication is given that the user has now signed into the associated Driver Profile for that button |
| **List of Exception Use Cases** |  |
| **Interfaces** | Personalization Interface |

#### ENMEM-UC-REQ-095934/C-Memory Seat Button Recall of the Active Driver Profile

|  |  |
| --- | --- |
| **Actors** | Vehicle Occupant |
| **Pre-conditions** | The vehicle transmission is in Park OR vehicle speed is less than 8 KPH for a manual transmission  The Driver Profiles feature is set to ON |
| **Scenario Description** | The User presses a memory seat button on the driver door panel that is associated to the active Driver Profile. |
| **Post-conditions** | The last saved positional settings are recalled for the active Driver Profile. |
| **List of Exception Use Cases** |  |
| **Interfaces** | Personalization Interface |
| **Notes** | If the current positional settings are the same as the last saved positional settings, then no position change will occur. |

#### ENMEM-UC-REQ-095939/C-Sign Into a Driver Profile via HMI Menu

|  |  |
| --- | --- |
| **Actors** | Vehicle Occupant |
| **Pre-conditions** | The Driver Profiles feature is set to ON |
| **Scenario Description** | The User accesses the Driver Profiles HMI menu and chooses to sign in to a Driver Profile. |
| **Post-conditions** | All applicable user settings are recalled for the chosen Driver Profile and an HMI indication is given that the user has now signed into that Driver Profile. |
| **List of Exception Use Cases** |  |
| **Interfaces** | Personalization Interface |
| **Note** | Positional settings will only be recalled if vehicle is in “Park” OR vehicle speed is less than 8 KPH. |

#### ENMEM-UC-REQ-095940/D-Sign Into a Driver Profile via Keyfob/Phone

|  |  |
| --- | --- |
| **Actors** | Vehicle Occupant |
| **Pre-conditions** | The Driver Profiles feature is set to ON.  The User has chosen to associate their keyfob or phone to their Driver Profile.  Phone is registered, authenticated, and connected as a PaaK (refer to the Phone-As-A-Key SPSS) |
| **Scenario Description** | The User’s keyfob or phone is detected and the associated Driver Profile is signed in automatically. |
| **Post-conditions** | All applicable user settings are recalled for the chosen Driver Profile and an HMI indication is given that the user has now signed into that Driver Profile. |
| **List of Exception Use Cases** |  |
| **Interfaces** | Personalization Interface |
| **Notes** | - Keyfob or phone detection may be the result of an unlock or remote start button press from an associated phone or keyfob (IKT or IA Key) or the result of a PEPS unlock event from an associated passive key. (i.e. Driver door handle unlock with a passive IA key present.) |

#### ENMEM-UC-REQ-162635/C-Sign Into a Driver Profile via Keyfob/Phone Button Press While Vehicle In Motion

|  |  |
| --- | --- |
| **Actors** | Vehicle Occupant |
| **Pre-conditions** | The Driver Profiles feature is set to ON  The User’s keyfob or phone is associated to a Driver Profile  Phone is registered, authenticated, and connected as a PaaK (refer to the Phone-As-A-Key SPSS) |
| **Scenario Description** | The User presses a keyfob or phone unlock button that is associated to an alternate Driver Profile (other than the active profile) while the vehicle is in motion (not in Park or vehicle speed is greater than 8 KPH). |
| **Post-conditions** | No new Driver Profile is recalled |
| **List of Exception Use Cases** |  |
| **Interfaces** | Personalization Interface |

#### ENMEM-UC-REQ-161547/D-Classic Memory Only Recall via Previously Associated Keyfob/Phone

|  |  |
| --- | --- |
| **Actors** | Vehicle Occupant |
| **Pre-conditions** | The User’s keyfob or phone is associated to a Driver Profile  Phone is registered, authenticated, and connected as a PaaK (refer to the Phone-As-A-Key SPSS)  The Driver Profiles feature is set to OFF.  Vehicle is in PARK or less than 8 kph |
| **Scenario Description** | The User’s keyfob or phone is detected and the associated Classic Memory Position is recalled. |
| **Post-conditions** | All Classic Memory position settings are recalled for the associated memory position number and no Driver Profile recall occurs (i.e. Guest profile remains active.) |
| **List of Exception Use Cases** |  |
| **Interfaces** | Personalization Interface |
| **Notes** | - Keyfob or phone detection may be the result of a unlock button press from an associated phone or keyfob (IKT or IA Key) or the result of a PEPS unlock event from an associated passive key. (i.e. Driver door handle unlock with a passive IA key present.)  - No HMI indication is given that the user has signed into the Guest Profile while the Driver Profiles feature is set to OFF. |

#### ENMEM-UC-REQ-137996/D-Recall Last Known Driver Profile With Keypad Code When A Keyfob/Phone Is Not With The User

|  |  |
| --- | --- |
| **Actors** | Vehicle Occupant |
| **Pre-conditions** | * The Driver Profile feature is set to ON * The Vehicle ignition is OFF * The user approaches the vehicle with NO associated keyfob or phone |
| **Scenario Description** | The User unlocks the door via the Vehicle Keypad then opens the door and starts the engine |
| **Post-conditions** | The last known Driver Profile is recalled |
| **Interfaces** | Personalization Interface |
| **Note** | * Because there is no keyfob or phone with the user, opening the door via door handle will not change profile for vehicle with or without Smart Door Handle * Starting the engine is not a method of recall profile |

#### ENMEM-UC-REQ-162841/C-Recall Driver Profile When An IA Key Is With The User

|  |  |
| --- | --- |
| **Actors** | Vehicle Occupant |
| **Pre-conditions** | * The Driver Profile feature is set to ON * The Vehicle ignition is OFF * The Vehicle is equipped with Smart Door Handle * The user approaches the vehicle with an IA Key |
| **Scenario Description** | The User opens the door |
| **Post-conditions** | The last known Driver Profile is recalled if the IA Key is not associated to any Driver Profile.  The Driver Profile associated to the user’s IA Key will be recalled. It could be the last known Driver Profile or any other Driver Profiles. |
| **Interfaces** | Personalization Interface |
| **Note** | Because the vehicle is equipped with Smart Door Handle and the IA Key is with the user, opening the door via door handle will trigger passive key unlock search. Depending on the fob association status, passive key unlock search may or may not recall a Driver Profile different than the last known Driver Profile. |

#### ENMEM-UC-REQ-137858/D-MyKey Overrides Driver Profile Setting

|  |  |
| --- | --- |
| **Actors** | Vehicle Occupant |
| **Pre-conditions** | * The Driver Profiles feature is set to ON * Personality profile X has speed compensated volume set to HIGH * Personality profile Y has speed compensated volume set to Low * Fob A is associated with profile X and is programmed as a MyKey * Volume Limiter is set to ON for MyKey |
| **Scenario Description** | 1. Vehicle is started up with MyKey Fob A and activates Profile X 2. User manually changes to Profile Y via the HMI |
| **Post-conditions** | Speed Compensated Volume is overridden and disabled due to the MyKey restriction on both Profile X and Profile Y |
| **List of Exception Use Cases** |  |
| **Interfaces** | G-HMI  Vehicle System Interface |
| **Note** | - No matter which profile is recalled to be the active profile as long as a MyKey is in the ignition (recognized by vehicle to start engine), MyKey restrictions shall apply.  - Phones associated via PaaK may also be made a MyKey. The same functionality shall apply. |

#### ENMEM-UC-REQ-162575/C-Admin Key does not restrict Driver Profile associated to MyKey

|  |  |
| --- | --- |
| **Actors** | Vehicle Occupant |
| **Pre-conditions** | * The Driver Profiles feature is set to ON * Personality profile X has speed compensated volume set to HIGH * Fob A is associated with profile X and is programmed as a MyKey * Volume Limiter is set to ON for MyKey |
| **Scenario Description** | * Vehicle is started up with Fob B, an Admin Key (a non-MyKey Fob) * The driver recalls profile X after engine started |
| **Post-conditions** | Speed Compensated Volume from Driver Profile X is not overridden and remains HIGH |
| **List of Exception Use Cases** |  |
| **Interfaces** | G-HMI  Vehicle System Interface |
| **Note** | - No matter which profile is recalled to be the active profile (even if associated to a MyKey Keyfob) as long as an Admin Key (non-MyKey Fob) is in ignition (recognized by vehicle to start engine), MyKey restrictions shall not apply  - Phones associated via PaaK may also be made a MyKey. The same functionality shall apply. |

#### ENMEM-UC-REQ-214249/A-Valet Mode enabled with Enhanced Memory On

|  |  |
| --- | --- |
| **Actors** | Vehicle Occupant |
| **Pre-conditions** | The ignition status is in Run.  The vehicle speed is less than 8 KPH  Enhanced Memory is set to On  Valet Mode is Off |
| **Scenario Description** | The user enables Valet Mode from the HMI |
| **Post-conditions** | Active Personality Profile is remembered  Enhanced Memory is set to Off   * By default, the Guest Profile is recalled   Valet Mode is enabled |
| **Interfaces** | Personalization Interface |

#### ENMEM-UC-REQ-214250/A-Valet Mode disabled with Enhanced Memory On

|  |  |
| --- | --- |
| **Actors** | Vehicle Occupant |
| **Pre-conditions** | The ignition status is in Run.  The vehicle speed is less than 8 KPH  Valet Mode is ON  Enhanced Memory is set to Off (was On prior to enabling Valet Mode) |
| **Scenario Description** | The user disables Valet Mode from the HMI |
| **Post-conditions** | Valet Mode is disabled  Enhanced Memory is set to On  The remembered Active Personality Profile is recalled |
| **List of Exception Use Cases** | ENMEM-UC-REQ-214246-Valet Mode disabled with Enhanced Memory Off |
| **Interfaces** | Personalization Interface |

### Requirements

#### ENMEM-REQ-129547/C-Last Known Driver Profile Applied

If upon network wakeup, no sign-in method is detected, the EnhancedMemoryProfileServer shall recall the last known Driver Profile by updating the ActivePersonality\_St method to the last known value. The PersonalityRecallCount\_St shall NOT be incremented.

If the last known Driver Profile cannot be determined, the EnhancedMemoryProfileServer shall recall the Vehicle level Profile (Guest Profile) as the active Driver Profile.

#### ENMEM-REQ-099694/B-Driver Profile Recall Event

A Driver Profile recall event is denoted by the increment of PersonalityRecallCount\_St. The purpose of the counter is to indicate when a recall event has occurred and the active Driver Profile needs to be updated. The newly recalled Driver Profile may and may not be different than the previous active Driver Profile in terms of name of the Driver Profile and actual settings of Driver Profile.

* EnhancedMemoryProfileServer shall increment the recall counter PersonalityRecallCount\_St each time a recall event occurs. The recall event includes memory seat button momently pressing, door unlock events and infotainment recall via InfotainmentRecall\_Rq. Definitions and requirements for seat button press recall and door unlock recall shall follow the design and requirements of Classic memory.
* When detecting an increment of PersonalityRecallCount\_St, EnhancedMemoryServers shall update the active Driver Profile according to ActivePersonality\_St which may and may not be changed.
* In error case when the ActivePersonality\_St method changes values without a corresponding increment to the PersonalityRecallCount\_St method, EnhancedMemoryServers shall still update the active Driver Profile based on the change of ActivePersonality\_St.

#### ENMEM-REQ-099673/C-Driver Profile Settings Recall

When an EnhancedMemoryServer receives a Driver Profile recall event, it shall recall all settings for the Driver Profile indicated in the ActivePersonality\_St method within T\_PersRecall. Any reserved or non-valid value of *ActivePersonality\_St* shall be treated as Vehicle.

* The EnhancedMemoryInterfaceClient shall update its driver profile sign-in notification HMI:
  + each time the “Start Screen” is shown as defined by H22g\_SYNC3\_Welcome\_Power\_Modes.
  + within T\_PersRecall of receiving the ActivePersonality\_St update
  + Note: No driver profile sign-in notification will be given when the Driver Profiles feature is disabled
* Any status signals that are updated as a result of the driver profile change shall not be sent until T\_PersRecallStatusUpdate has elapsed since the EnhancedMemoryServer received the ActivePersonality\_St but shall not take more than 500 msec from receiving the updated ActivePersonality\_St signal to send all its status signals with the updated values.

#### ENMEM-TMR-REQ-099762/B-T\_PersRecall

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Name** | **Description** | **Units** | **Range** | **Resolution** | **Default** |
| T\_PersRecall | Maximum time the EnhancedMemoryServer should take to recall all settings for a Driver Profile once the ActivePersonality\_St signal update is received to change a profile.  Note: Use the default value | msec | 50-150 | 5 | 75 |

#### ENMEM-TMR-REQ-134105/B-T\_PersRecallStatusUpdate

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Name** | **Description** | **Units** | **Range** | **Resolution** | **Default** |
| T\_PersRecallStatusUpdate | Minimum time the EnhancedMemoryServer should wait after receiving the ActivePersonality\_St signal update before sending any status messages affected by the change in driver profile.  Note: Use the default value | msec | 100-200 | 5 | 150 |

#### ENMEM-HMI-REQ-099692/B-Driver Profile Sign-In Notification Queue

When a Driver Profile change occurs at a time when the EnhancedMemoryInterfaceClient cannot display a notification to the User, it shall queue up this display update until a time when a notification can then be displayed. This shall only apply for the last recall request.

#### ENMEM-TMR-REQ-134102/B-T\_PersUpdate

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Name** | **Description** | **Units** | **Range** | **Resolution** | **Default** |
| T\_PersUpdate | Maximum time the EnhancedMemoryProfileServer should take to update the PersonalityRecallCounter\_St and ActivePersonality\_St on the vehicle system interface, after receiving a recall request.  Note: Use the default value | msec | 50-150 | 5 | 100 |

#### ENMEM-REQ-099671/E-Keyfob/Phone Detection for Driver Profile Sign-In

The EnhancedMemoryProfileServer shall determine when an unlock event has originated from a keyfob (per the existing Classic Memory Keyfob detection strategy) or phone (per PaaK) and check if the EnhancedMemory\_St method is reporting that the Driver Profiles feature is ON or OFF

* If the feature is ON and if the originating keyfob or phone is associated to a Driver Profile, then the EnhancedMemoryProfileServer shall update the ActivePersonality\_St and MemoryPosition\_St methods with the corresponding Driver Profile number associated to that keyfob or phone.
* If the feature is OFF and if the originating keyfob or phone has been associated to a Driver Profile prior to the feature being set to OFF, then the EnhancedMemoryProfileServer shall update the ActivePersonality\_St method to “Vehicle” and MemoryPosition\_St method to the corresponding Driver Profile number associated to the keyfob or phone.
* Regardless if the feature is ON or OFF, if the originating keyfob or phone is not associated to a Driver Profile, then the EnhancedMemoryProfileServer shall maintain the last known ActivePersonality\_St and MemoryPosition\_St methods. The PersonalityRecallCount\_St shall not increment.

For the latest EnhancedMemoryProfileServer requirements see the latest Enhanced Memory Feature Spec. This requirement may be outdated.

#### ENMEM-REQ-099682/C-Determination of Profile After Recall

When the EnhancedMemoryProfileServer receives a Driver Profile recall request via the MemSwitchRecall\_Rq or InfotainmentRecall\_Rq method, it shall check both the EnhancedMemory\_St to determine if the feature is on or off, and PersonalityOptIn\_St method to determine if that particular Driver Profile exists:

* If the EnhancedMemory\_St method indicates that the feature is on and the PersonalityOptIn\_St method reports that the requested Driver Profile is “Opted-In,” then the EnhancedMemoryProfileServer shall report a Driver Profile recall event by incrementing the PersonalityRecallCount\_St method and updating the ActivePersonality\_St and MemoryPosition\_St methods to the requested Driver Profile.
* If the EnhancedMemory\_St method indicates that the feature is on and the PersonalityOptIn\_St method reports that the requested Driver Profile is “Not Opted-In” then the EnhancedMemoryProfileServer shall report a Driver Profile recall event by incrementing the PersonalityRecallCount\_St method and updating the ActivePersonality\_St method to the Guest profile (ActivePersonality\_St = Vehicle) and MemoryPosition\_St to the requested Driver Profile.
* If the EnhancedMemory\_St method indicates that the feature is off, then the EnhancedMemoryProfileServer shall report a Driver Profile recall event by incrementing the PersonalityRecallCount\_St method and updating the ActivePersonality\_St method to the Guest profile (ActivePersonality\_St = Vehicle) regardless of the PersonalityOptIn\_St method value. The MemoryPosition\_St shall update to the requested Driver Profile

For the latest EnhancedMemoryProfileServer requirements see the latest Enhanced Memory Feature Spec. This requirement may be outdated.

#### ENMEM-REQ-154252/A-Positional Settings Status Update

When receiving the InfotainmentRecall\_Rq, the EnhancedMemoryProfileServer shall update the value of MemoryPosition\_St to the PersIndex value indicated by the recall request. This means that if the InfotainmentRecall\_Rq is received with a PersIndex set to the value of Vehicle, then the MemoryPosition\_St shall be updated to Vehicle as well.

#### ENMEM-REQ-199604/A-Recall Priority

The EnhancedMemoryProfileServer shall prioritize the recall requests in the following descending order:

* Infotainment Recall
* Unlock Event
* Remote Start Event
* Memory Seat button Press

For the latest EnhancedMemoryProfileServer requirements see the latest Enhanced Memory Feature Spec. This requirement may be outdated.

#### ENMEM-REQ-099693/E-Display Data Refresh After Driver Profile Change

After a driver profile change has occurred, the EnhancedMemoryInterfaceClient, and any Client displaying settings status (ex. Cluster, RACM, etc.), shall always refresh all applicable settings data (including the active screen) according to existing module setting HMI standards and requirements. This is to reflect the most recent settings values once a Driver Profile has been recalled.

Ex. The Cluster active screen has information displayed that was originally requested with feature based message protocol. While on the screen the ActivePersonality\_St signal changes from Pers1 to Pers3. When changing to Pers3, the Cluster shall re-request the active screen information even though the screen didn’t change. The Cluster has no knowledge if the feature is personalizable or not, so the Cluster shall always re-request the screen information when the Active Personality changes.

Ex. The Cluster infotainment active screen is displaying radio preset stations. While on the screen the ActivePersonality\_St signal changes from Pers1 to Pers3. When changing to Pers3, the Cluster shall re-request the active screen information even though the screen didn’t change. The Cluster has no knowledge if the feature is personalizable or not, so the Cluster shall always re-request the screen information when the Active Personality changes.

#### ENMEM-REQ-099700/C-Positional Settings Recall

The EnhancedMemoryPositionClient shall recall any positional settings when receiving an update of the MemoryPosition\_St method.

* An update of the MemoryPosition\_St to the value of Vehicle shall not trigger the recall of any positional settings
* A recall, triggered by the pressing of an unassociated Memory Seat button, shall not trigger the recall of any positional settings

For the latest EnhancedMemoryPositionClient requirements see the latest Driver Seat Module Spec. This requirement may be outdated.

#### ENMEM-REQ-198388/A-No Recall for Positional Settings When Vehicle in Motion

The EnhancedMemoryPositionClient shall not recall positional settings that are tied with Classic Memory when vehicle is not in park or vehicle speed is greater than 5kph for manual transmission.

For the latest EnhancedMemoryPositionClient requirements see the latest Driver Seat Module Spec. This requirement may be outdated.

#### ENMEM-SR-REQ-136618/F-Recall Event - Infotainment Audio

**When the user is NOT in a Feature Volume Session:**

For a recall event that results in a change to the Audio Settings (ex Occupancy mode, BTMBF…) if the recall event could cause distortion of audio then:

1. The Audio Setting Server (ex AHU, DSP AMP) shall mute the audio first,
2. Then update the Audio Settings (ex BTMBF, Occ Mode, SCV…), and
3. Then unmute when complete so there is no distortion of the audio.

**When the user IS in a Feature Volume Session:**

The above muting strategy shall not be implemented. The Audio Setting Server shall instead:

1. Maintain the initial profile’s Phone / VR / TA volume setting while the Feature Volume session is active
2. Apply the recalled profile’s Phone / VR / TA volume after the active Feature Volume session ends
   1. If the user makes a volume change during the active Feature Volume session, the Audio Setting Server shall apply and save the changed volume to the recalled profile.

The maximum amount of time to update all audio settings during a recall event, from the time the audio is muted until the unmute, shall not exceed 200 msec. The audio shall gracefully resume operation after the unmute.

The Media Volume shall not be stored individually for different Driver Profiles.

When changing between profiles the current active audio source shall not change.

* Ex. The active audio source is AM and channel X for person 1. The user changes to person 3 and the active audio source remains AM on the same channel X for person 3.

#### ENMEM-REQ-099674/C-Requesting Audio Preset Info After Profile Change

When the EnhancedMemoryInterfaceClient, and any Client displaying audio presets, receives a Driver Profile recall event via ActivePersonality\_St, it shall wait at least T\_PersPresetWait and then shall request the audio preset information from the AudioServer and shall update the audio preset HMI information to the new Driver Profile.

#### ENMEM-TMR-REQ-099763/C-T\_PersPresetWait

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Name** | **Description** | **Units** | **Range** | **Resolution** | **Default** |
| T\_PersPresetWait | Minimum time the EnhancedMemoryInterfaceClient, and any Client displaying audio presets, shall wait before requesting preset data from the AudioServer. | msec | 100-300 | 5 | 200 |

#### ENMEM-SR-REQ-214221/A-Recall behavior when Valet Mode Enabled/Disabled

If EnhancedMemory\_St = ProfilesOn when Valet Mode is enabled, the EnhancedMemoryInterfaceClient shall remember the last active personality profile prior to enabling Valet Mode.

When Valet Mode is then disabled, the EnhancedMemoryInterfaceClient shall recall the remembered personality profile after Enhanced Memory is re-enabled as defined in REQ-214801.

If EnhancedMemory\_St = ProfilesOff when Valet Mode is enabled, the active personality profile shall not be remembered and a recall shall not be performed when Valet Mode is disabled.

The EnhancedMemoryInterfaceClient shall remember the last active personality profile (prior to enabling Valet Mode) between different power mode cycles such as remembering (but not limited to):

* Between network bus sleep and wake-up events, and
* Between ignition cycles

All existing Valet Mode requirements/restrictions apply for Enhanced Memory and supersede any requirements in this specification.

For any conflicts bring to the attention of the Ford D&R.

### White Box View

#### Activity Diagrams

##### ENMEM-ACT-REQ-099387/B-Sign Into Driver Profile Via Memory Seat Button

Activity Diagram



##### ENMEM-ACT-REQ-099388/C-Sign Into Driver Profile Via HMI Menu

Activity Diagram



##### ENMEM-ACT-REQ-099384/D-Sign Into Driver Profile Via Keyfob/Phone

Activity Diagram



#### Sequence Diagrams

##### ENMEM-SD-REQ-099433/C-Sign Into Driver Profile Via Memory Seat Button

Constraints

Pre-Condition

The driver profiles feature is enabled

Scenarios

Normal Usage

A memory seat button press is detected by the EnhancedMemoryPositionClient. A request is sent on the vehicle system interface to change the active personality to the profile associated to the pressed memory seat button. The active personality is set to the associated profile.

Post-Condition

All applicable user settings are recalled for the associated profile.

The associated profile is active.

Note: See sequence diagram below for alternate cases when drivers profile is off, or the requested profile is not OptedIn.

Sequence Diagram



##### ENMEM-SD-REQ-099434/C-Sign Into Driver Profile Via HMI Menu

Constraints

Pre-Condition

The infotainment system is active

The driver profiles feature is enabled

Scenarios

Normal Usage

An HMI selection for signing into a profile is detected by the EnhanceMemoryInterfaceClient. A request is sent on the vehicle system interface to change the active personality to the profile associated to the HMI selection. The active personality is set to the associated profile.

Post-Condition

All applicable user settings are recalled for the associated profile.

The associated profile is active.

Note: See sequence diagram below for alternate cases when drivers profile is off, or the requested profile is not OptedIn.

Sequence Diagram



##### ENMEM-SD-REQ-099432/D-Sign Into Driver Profile Via Keyfob/Phone

Constraints

Pre-Condition

A keyfob or phone is associated to a personality profile

The driver profiles feature is enabled

Scenarios

Normal Usage

The associated keyfob or phone is detected by the EnhancedMemoryProfileServer and the active personality is set to the Opted-In profile associated to the keyfob or phone.

Post-Condition

All applicable user settings are recalled for the associated profile.

The associated profile is active.

Note: See sequence diagram below for alternate cases when keyfob/phone is not associated to profile, drivers profile is off, or the requested profile is not OptedIn.

Sequence Diagram



## ENMEM-FUN-REQ-095958/A-Store Occupant Position Settings

### Use Cases

#### ENMEM-UC-REQ-095720/B-Memory Seat Button Storing with Driver Profiles OFF

|  |  |
| --- | --- |
| **Actors** | Vehicle Occupant |
| **Pre-conditions** | The Driver Profiles feature is set to OFF |
| **Scenario Description** | The user initiates a “store position” operation via any Memory Seat button |
| **Post-conditions** | The current positional settings are stored for that particular pressed button and the user stays signed into the Guest Profile while the Driver Profiles feature is OFF |
| **List of Exception Use Cases** |  |
| **Interfaces** | Personalization Interface |

#### ENMEM-UC-REQ-095931/B-Memory Seat Button Storing of an Alternate Associated Profile

|  |  |
| --- | --- |
| **Actors** | Vehicle Occupant |
| **Pre-conditions** | The Driver Profiles feature is set to ON |
| **Scenario Description** | The User initiates a “store position” operation via a Memory Seat button that is associated to an alternate Driver Profile (other than the active profile.) |
| **Post-conditions** | The current positional settings are stored to the alternate Driver Profile, an HMI indication is given that the user has now signed into the alternate Driver Profile, and all applicable user settings are recalled for that new profile. |
| **List of Exception Use Cases** |  |
| **Interfaces** | Personalization Interface |
| **Note:** | The Guest profile would be considered an “alternate Driver Profile” for any buttons that aren’t associated to a created Driver Profile. |

#### ENMEM-UC-REQ-095938/B-Memory Seat Button Storing of the Active Driver Profile

|  |  |
| --- | --- |
| **Actors** | Vehicle Occupant |
| **Pre-conditions** | The Driver Profiles feature is set to ON |
| **Scenario Description** | The user initiates a “store position” operation via a Memory Seat button that is associated to the Active Driver Profile. |
| **Post-conditions** | The current positional settings are stored to the active Driver Profile. |
| **List of Exception Use Cases** |  |
| **Interfaces** | Personalization Interface |
|  |  |

#### ENMEM-UC-REQ-166195/B-Memory Seat Button Storing of an Unassociated Button

|  |  |
| --- | --- |
| **Actors** | Vehicle Occupant |
| **Pre-conditions** | The Driver Profiles feature is set to ON |
| **Scenario Description** | The user initiates a “store position” operation via a Memory Seat button on the driver door panel that has not been associated to any Driver Profile |
| **Post-conditions** | The current positional settings are stored to the unassociated button. The Guest Profile will be recalled |
| **List of Exception Use Cases** |  |
| **Interfaces** | Personalization Interface |
| **Note:** | The Guest profile would be considered an “alternate Driver Profile” for any buttons that aren’t associated to a created Driver Profile. |

### Requirements

#### ENMEM-REQ-099687/B-Classic Memory Subsystem Store Delay

After detecting a memory seat button press and hold store event,

* EnhancedMemoryPositionClient shall store the current Classic Memory positional settings to a Driver Profile designated by a memory seat button that was pressed and held
* EnhancedMemoryPositionClient then shall wait T\_PersStore before send the recall request via MemSwitchRecall\_Rq to the EnhancedMemoryProfileServer

#### ENMEM-TMR-REQ-099764/B-T\_PersStore

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Name** | **Description** | **Units** | **Range** | **Resolution** | **Default** |
| T\_PersStore | Minimum time the EnhancedMemoryPositionClient should wait before sending a recall request to the EnhancedMemoryProfileServer.  Note: Use the default value | msec | 150-350 | 5 | 250 |

### White Box View

#### Activity Diagrams

##### ENMEM-ACT-REQ-099389/B-Store Position Settings To Driver Profile

Activity Diagram



#### Sequence Diagrams

##### ENMEM-SD-REQ-099435/C-Store Position Settings To Driver Profile

Constraints

Pre-Condition

The driver profiles feature is enabled

Scenarios

Normal Usage

A memory seat button store operation is detected by the EnhancedMemoryPositionClient.

Post-Condition

All applicable user settings are stored to the associated profile.

The associated profile is active.

Note: See sequence diagram below for alternate cases when drivers profile is off, or the requested profile is not OptedIn.

Sequence Diagram



## ENMEM-FUN-REQ-095959/A-Create/Edit Driver Profile (Modified for soft button)

### Use Cases

#### ENMEM-UC-REQ-095721/C-Create a Driver Profile

|  |  |
| --- | --- |
| **Actors** | Vehicle Occupant |
| **Pre-conditions** | The ignition status is in Run.  The vehicle is in Park.  The Driver Profiles feature is set to ON  The vehicle speed is less than 8 KPH  The maximum number of profiles has not yet been reached |
| **Scenario Description** | The User accesses the Driver Profiles, chooses to create a new Driver Profile, ~~and then chooses to associate a memory seat button to that profile~~ |
| **Post-conditions** | A new profile is created with:   * all applicable non-positional settings copied from the previous profile to the new profile * all applicable positional settings copied from the currently active settings (from previous profile, or from recently changed but not saved settings) to the new profile   ~~The chosen memory seat button is associated to the new profile~~ |
| **Interfaces** | Personalization Interface |
| **Notes** |  |

#### ENMEM-UC-REQ-134147/C-Create or Edit Driver Profile Name

|  |  |
| --- | --- |
| **Actors** | Vehicle Occupant |
| **Pre-conditions** | The ignition status is in Run.  The vehicle is in Park.  The vehicle speed is less than 8 KPH  The user is in the process of creating or editing a Driver Profile |
| **Scenario Description** | The user chooses to create or edit a new Driver Profile Name, and has entered the new name for that Driver Profile |
| **Post-conditions** | The entered name has now been assigned to the new Driver Profile  or  The Driver Profile name has now been updated to the new name |
| **List of Exception Use Cases** | NMEM-UC-REQ-198925/A-Attempt to give a Driver Profile an Existing Name |
| **Interfaces** | Personalization Interface |
| **Notes** | User must choose a name that is not identical to an existing Driver Profile name. |

#### ENMEM-UC-REQ-198925/A-Attempt to Give a Driver Profile an Existing Name

|  |  |
| --- | --- |
| **Actors** | Vehicle Occupant |
| **Pre-conditions** | The ignition status is in Run.  The vehicle speed is less than 8 KPH  The user is in the process of creating or editing a Driver Profile |
| **Scenario Description** | The user enters an existing Driver Profile name |
| **Post-conditions** | * The user is informed by HMI indication that Driver Profile name already exists * The user is given opportunity to retry |
| **Interfaces** | Personalization Interface |
| **Notes** |  |

#### ~~ENMEM-UC-REQ-197170/A-Attempt to Associate Already Associated Memory Seat Button~~

|  |  |
| --- | --- |
| **~~Actors~~** | ~~Vehicle Occupant~~ |
| **~~Pre-conditions~~** | ~~The ignition status is in Run.~~  ~~The vehicle speed is less than 8 KPH~~  ~~Enhanced Memory HMI prompts the user to press a Memory Seat button at door panel during creating Driver Profile process~~ |
| **~~Scenario Description~~** | ~~The user presses a Memory Seat button that had been associated to other Driver Profile~~ |
| **~~Post-conditions~~** | * ~~The user is informed by HMI indication that the chosen Memory Seat button is already associated to another Driver Profile~~ * ~~The user is given multiple opportunities to retry~~ |
| **~~Interfaces~~** | ~~Personalization Interface~~ |
| **~~Notes~~** | ~~See requirement “ENMEM-REQ-197965-No overwrite for Memory Seat Buttons already associated to Existing Driver Profiles”~~ |

#### ENMEM-UC-REQ-095908/D-Associate Keyfob/Phone to a Driver Profile

|  |  |
| --- | --- |
| **Actors** | Vehicle Occupant |
| **Pre-conditions** | The ignition status is in Run.  The vehicle speed is less than 8 KPH  The user is in the process of creating or editing a Driver Profile  Phone is registered, authenticated, and connected as a PaaK (refer to the Phone-As-A-Key SPSS) |
| **Scenario Description** | The user accesses the Driver Profiles HMI, chooses to create or edit a new Driver Profile, and has chosen to associate a keyfob or phone to that profile. |
| **Post-conditions** | The chosen keyfob or phone is now associated to the active Driver Profile. |
| **List of Exception Use Cases** | ENMEM-UC-REQ-095925-Attempt to Associate Already Associated Keyfob/Phone |
| **Interfaces** | Personalization Interface |
| **Notes** |  |

#### ENMEM-UC-REQ-095925/C-Attempt to Associate Already Associated Keyfob/Phone

|  |  |
| --- | --- |
| **Actors** | Vehicle Occupant |
| **Pre-conditions** | The ignition status is in Run.  The vehicle speed is less than 8 KPH  The user is in the process of associating a keyfob to a Driver Profile  Phone is registered, authenticated, and connected as a PaaK (refer to the Phone-As-A-Key SPSS) |
| **Scenario Description** | The user attempts to associate a keyfob/phone that is already associated to another Driver Profile. |
| **Post-conditions** | * The user is informed by HMI indication that the chosen keyfob/phone is already associated to another Driver Profile * The user is given the option to overwrite the chosen keyfob/phone |
| **Interfaces** | Personalization Interface |
| **Notes** |  |

#### ENMEM-UC-REQ-195889/C-Associate a Keyfob with Incorrect Method

|  |  |
| --- | --- |
| **Actor** | Vehicle Occupant |
| **Pre-conditions** | Ignition is Run  The vehicle speed is less than 8 KPH  At least one set of positional settings is set (one Memory Seat button is defined) |
| **Scenario Description** | The User tries to associate a keyfob to the saved positional setting Memory Seat button without using the Driver Profiles menu (ex. using Press & Hold or Set method) |
| **Post-conditions** | No chime, indicating a successful keyfob association, is given.  The keyfob is not associated to any preset positional settings  The keyfob is not associated to any existing Driver Profile |
| **Interfaces** | Personalization Interface |
| **Notes** | - For vehicles with Enhanced Memory, keyfob association must be done through the Enhanced Memory keyfob association menu. If the user does not create a Driver Profile, the user cannot associate the keyfob to any Memory Seat button. When Driver Profiles are created, the user can only associate a keyfob via menu.  - Phone association to a Driver Profile (via PaaK) must also be done through the Driver Profiles menu. No other phone association method shall be supported. |

#### ENMEM-UC-REQ-095927/C-Disassociate Keyfob/Phone from a Driver Profile

|  |  |
| --- | --- |
| **Actors** | Vehicle Occupant |
| **Pre-conditions** | The ignition status is in Run.  The vehicle speed is less than 8 KPH  User is in the process of editing a Driver Profile |
| **Scenario Description** | The User accesses the Driver Profiles HMI, chooses to edit a new Driver Profile, and has chosen to remove a keyfob or phone association from that profile. |
| **Post-conditions** | The previous keyfob or phone association is now removed from the active Driver Profile. |
| **Interfaces** | Personalization Interface |
| **Note** | Disassociating a keyfob or phone does not delete the profile, it only removes the link between the selected profile and the keyfob or phone. |

#### ENMEM-UC-REQ-194188/A-Disassociate Keyfobs from Driver Profiles after Keyfobs Are Erased from a Vehicle

|  |  |
| --- | --- |
| **Actors** | Ford Dealership Technician and Vehicle Occupant |
| **Pre-conditions** | At least one key fob is associated to a Drive Profile |
| **Scenario Description** | Keyfobs are erased by diagnostic tool and then Keyfobs (new or original ones) are reprogrammed to the vehicle  The user starts up the vehicle and selects Driver Profile menu |
| **Post-conditions** | All Driver Profiles remain the same after Keyfobs were reprogrammed  All Keyfob reprogrammed to the vehicle will not be associated to any Driver Profile.  HMI does not display Keyfob association indicator for any Driver Profile |
| **Interfaces** | Personalization Interface |
| **Notes** | Fob association will be erased at the same time Keyfobs are erased via diagnostic tool. For EnhancedMemoryInteraceClient HMI Keyfob indication associated with this see requirement “*ENMEM-HMI-REQ-202226-Keyfob HMI Indication”.* |

#### ENMEM-UC-REQ-232959/A-Disassociate Phone from Driver Profiles after Phone is Erased/Revoked

|  |  |
| --- | --- |
| **Actors** | Vehicle Occupant |
| **Pre-conditions** | At least one phone is associated to a Driver Profile |
| **Scenario Description** | Phones are Erased or Revoked by the user from outside the vehicle  The user starts up the vehicle and selects the Driver Profile menu |
| **Post-conditions** | All Driver Profiles remain the same after phones have been removed  HMI does not display Phone association indicator for any Driver Profile |
| **Interfaces** | Personalization Interface |
| **Notes** | - Phone association will be erased at the same time Phones are erased or revoked from outside the vehicle (see Phone-As-A-Key SPSS for such methods).  - For EnhancedMemoryInteraceClient HMI Phone indication, see “*ENMEM-HMI-REQ-202226-Keyfob/Phone HMI Indication”.* |

#### ENMEM-UC-REQ-095929/D-Delete a Driver Profile

|  |  |
| --- | --- |
| **Actors** | Vehicle Occupant |
| **Pre-conditions** | The ignition status is in Run  The vehicle speed is less than 8 KPH  At least one Driver Profile has been created |
| **Scenario Description** | The user accesses the Driver Profiles HMI and chooses to delete a Driver Profile (need not to be the active Driver Profile) |
| **Post-conditions** | * The Driver Profile selected by the user now is deleted * If the active profile is deleted, Guest Profile is recalled automatically. Positional settings remain unchanged * Positional settings that were associated to the deleted Driver Profile remain associated to the Memory Seat button. Pressing the disassociated Memory Seat button will recall the stored positional settings * The keyfob and/or phone that was previously associated to the deleted Driver Profile is automatically disassociated * Pressing the disassociated keyfob and/or phone will no longer trigger a recall. * Positional settings will also not respond to keyfob or phone pressing * HMI disables Edit menu and deletes the name, keyfob, and/or phone association status for the deleted Driver Profile |
| **Interfaces** | Personalization Interface |
| **Notes** | Deleting a Driver Profile does not delete/erase/revoke the PaaK, it only deletes the association between the phone and the once existing Driver Profile (refer to Phone-As-A-Key SPSS on removal methods). |

#### ENMEM-UC-REQ-195890/B-Delete All Driver Profiles via Master Reset

|  |  |
| --- | --- |
| **Actor** | Vehicle Occupant |
| **Pre-conditions** | Infotainment system is ON  At least one Driver Profile is created |
| **Scenario Description** | The user presses the Master Reset button |
| **Post-conditions** | * All Driver Profiles are deleted and Enhanced Memory feature is turned off * Upon return to the Driver Profiles HMI Menu Enhanced Memory feature is OFF. All Driver Profile menus, except Enhanced Memory feature ON/OFF, are disabled * All keyfobs and phones are disassociated from Driver Profiles and Memory Seat buttons * Positional settings remain associated to the Memory Seat buttons |
| **Interfaces** | Personalization Interface |
| **Notes** | When performing Master Reset, the Enhanced Memory requirements for Deleting a Driver Profile also apply.  See Vehicle Settings SPSS and applicable Master Reset documents for performing a Master Reset.  See Master Reset requirements to see if there are any driver distraction requirements |

#### ENMEM-UC-REQ-096801/B-User Aborts or System Cancel Event Occurs During Driver Profile Creation Process

|  |  |
| --- | --- |
| **Actors** | Vehicle Occupant |
| **Pre-conditions** | The ignition status is in Run.  The vehicle speed is less than 8 KPH  The user is in the process of creating a Driver Profile |
| **Scenario Description** | * The user cancels out of the pairing process   or   * A system event occurs that terminates the pairing process as shown in some examples below:   + Vehicle gear shifts out of Park, Vehicle in motion (i.e. follow Driver Distraction requirements)   + System Timeout   + Ignition no longer in Run   + System shutdown |
| **Post-conditions** | * The profile creation process has been aborted and a Driver Profile was not successfully created * HMI provides Abort notification and instruction to restart the Driver Profile creation process |
| **Interfaces** | Personalization Interface |
| **Notes** |  |

#### ENMEM-UC-REQ-096802/D-User Aborts or System Cancel Event Occurs During Keyfob/Phone Association Process

|  |  |
| --- | --- |
| **Actors** | Vehicle Occupant |
| **Pre-conditions** | The ignition status is in Run.  The vehicle speed is less than 8 KPH  The user is in the process of associating a keyfob or phone to a Driver Profile  Phone is registered, authenticated, and connected as a PaaK (refer to the Phone-As-A-Key SPSS) |
| **Scenario Description** | * The user cancels out of the pairing process   or   * A system event occurs that terminates the pairing process as shown in some examples below:   + Vehicle gear shifts out of Park, Vehicle in motion (i.e. follow Driver Distraction requirements)   + System Timeout   + Ignition no longer in Run   + System shutdown |
| **Post-conditions** | * The keyfob or phone pairing process has been aborted and a keyfob or phone was not successfully paired to the desired Driver Profile * HMI provides Abort notification and instruction to restart the keyfob or phone association process |
| **Interfaces** | Personalization Interface |
| **Notes** |  |

### Requirements

#### ENMEM-REQ-138622/B-Configurable Parameter for Personal Entry Code Association

The EnhancedMemoryProfileServer shall have a configurable parameter to determine whether the vehicle supports the Enhanced Memory feature:

* If the parameter indicates that the vehicle is to support “Enhanced Memory”, then a user-created personal entry code shall not be associated to auser created profile or Memory Seat location
* If the parameter indicates that the vehicle is to support “Classic Memory”, then association of user-created personal entry codes shall be handled as defined by the Classic Memory systemstrategy.

For the latest EnhancedMemoryProfileServer requirements see the latest Enhanced Memory Feature Spec. This requirement may be outdated.

#### ENMEM-SR-REQ-232984/A-Configurable Parameter to Enable PaaK HMI

The EnhancedMemoryInterfaceClient shall have a configurable parameter to determine whether the vehicle supports the PaaK feature. If the parameter indicates that the vehicle is to support “PaaK”, then the following functionality shall be enabled:

* Phone HMI Indication
* Phone Association via the Edit Menu
* Phone Disassociation via the Edit Menu
* The option during Driver Profile creation to enter Phone Association, either on its own or after Keyfob Association
* And all applicable PaaK screens as depicted in “H84a\_SYNC3\_EMDriverProfile”

#### ENMEM-REQ-138631/B-Missing Message DTC

* The EnhancedMemoryInterfaceClient shall set a “lost communication” DTC for any expected Enhanced Memory periodic messages that are not received for more than 5 seconds.
* The EnhancedMemoryPositionClient shall set a “lost communication” DTC for any expected Enhanced Memory periodic messages that are not received for more than 5 seconds.
* The EnhancedMemoryProfileServer shall set a “lost communication” DTC for any expected Enhanced Memory periodic messages that are not received for more than 5 seconds.

#### ENMEM-REQ-099681/C-Driver Profile Opt-In Status

The EnhancedMemoryInterfaceClient shall notify the EnhancedMemoryProfileServer of all Driver Profiles that have been created via the PersonalityOptIn\_St method.

#### ENMEM-REQ-099684/B-Driver Profile to Personality Mapping

The EnhancedMemoryInterfaceClient shall determine which Driver Profile value, reported in the ActivePersonality\_St method, is mapped to which Driver Profile name. This mapping is done during Profile Creation and shall be stored and maintained by the EnhancedMemoryInterfaceClient until that Driver Profile is deleted.

See sequence diagram “ENMEM-SD-REQ-099425-Create Driver Profile” for a detailed example.

#### ENMEM-REQ-116801/D-Retain Enhanced Memory Settings After Software Reflash

The EnhancedMemoryInterfaceClient shall retain Driver Profile information and internally managed settings values after a software reflash occurs. This is to prevent the customer from recreating Driver Profiles and associating keyfobs and/or phone’s after a software reflash service is done at dealership.

The information to be retained shall include opted in and opted out (created and deleted) status of all Driver Profiles, Driver Profile’s keyed-in name and the association of Driver Profile name to Memory Seat button number.

#### ENMEM-SR-REQ-095961/B-Maximum Number of Driver Profiles

The EnhancedMemoryInterfaceClient shall have configurable parameters to indicate the max number of possible Driver Profiles that the vehicle can support. This parameter shall be set equal to the number of Memory Seat buttons, excluding SET button, on the driver door panel.

#### ENMEM-REQ-198384/A-Alignment between Opt-in Driver Profile and Memory Seat Button

The number in Personal Index of PersonalityOptIn\_St shall align with the number of the pressed Memory Seat button, not the order of Driver Profile creation. In other words, the number of Personal Index in PersonalityOptIn\_St shall not be aligned with the order of Driver Profile creation.

Example: the first created Driver Profile is associated to Memory seat button #2

Precondition: Before any Driver Profile is created, the status of PersonalityOptIn\_St is

|  |  |  |  |
| --- | --- | --- | --- |
| Logic Method Name | Logic Parameter Name | GSDB Encoding Name | GSDB Encoding Value |
| PersonalityOptIn\_St | Pers1Status | NotOptedIn | 0x0 |
| Pers2Status | NotOptedIn | 0x0 |
| Pers3Status | NotOptedIn | 0x0 |
| Pers4Status | NotOptedIn | 0x0 |

Scenario: The user creates the first Driver Profile and presses Memory Seat button #2

during profile creation process

Post Condition: After the first Driver Profile is created, the status of PersonalityOptIn\_St shall be

|  |  |  |  |
| --- | --- | --- | --- |
| Logic Method Name | Logic Parameter Name | GSDB Encoding Name and Value | GSDB Signal Name |
| PersonalityOptIn\_St | Pers1Status | NotOptedIn | 0x0 |
| **Pers2Status** | **OptedIn** | **0x1** |
| Pers3Status | NotOptedIn | 0x0 |
| Pers4Status | NotOptedIn | 0x0 |

#### ENMEM-REQ-099699/E-Disable Driver Profile Creation and Editing When Key is Not in Run or Vehicle Speed is greater than 8KPH

The EnhancedMemoryInterfaceClient shall disable Driver Profile creation and editing if:

1. the Ignition Status is any value other than Run, or
2. the Gear Lever Position Status is any value other than Park (for Automatic Transmissions only, see relevant config. bit), or
3. the Vehicle Speed is greater than 8KPH

* For driver restrictions related to vehicle in motion follow whatever is specified in the Driver Restrictions SPSS (DRIVE-RESv2-FUR-REQ-025157-HMI Driving Restriction – General Applications (TcSE ROIN-279695-1)).
  + If the vehicle in motion driver restrictions called out in the Enhanced Memory Spec (ex. 8KPH) differs from what is in Req-025157-HMI Driver Restriction, than Req-025157-HMI Driver Restriction shall take precedence.

#### ENMEM-REQ-116802/F-Profile Creation Interruption

If the profile creation process is interrupted prior to completion (For Example: Ignition cycle, vehicle transitions out of park, vehicle speed becomes greater than 8 KPH, user initiated HMI domain change\*, Infotainment system reset, etc.), then the process shall be aborted. The EnhancedMemoryInterfaceClient shall:

* Set EnMemProfilePairing\_Rq(ButtonPairing = ExitButtonPairing) if in Button Association Mode
* Set EnMemProfilePairing\_Rq(KeyPairing = ExitKeyPairing) if in Keyfob or Phone Association Mode
* Revert the Pers#Status for PersonalityOptIn\_St back to “NotOptedIn” for the Memory Seat Button selected if it was already set
* Not send Feature\_Rq(Operation = Copy) if it was not yet sent
* Not perform a Driver Profile recall
* Erase mapping of Profile Number to selected Memory Seat Button
* Erase Driver Profile name from internal memory
* Turn Enhanced Memory Feature Off if there is no other existing Driver Profiles
* Update the user as per ENMEM-HMI-REQ-212764

\*A user initiated HMI domain change is one where the customer intentionally changes domain via the HMI. A non-user initiated domain change is one where a system behavior/function causes a domain change (ex. an incoming phone call). In the case of the non-user initiated domain change, the profile creation shall continue to proceed and the abort behavior detailed above shall not occur.

#### ENMEM-HMI-REQ-202226/A-Keyfob HMI Indication

The EnhancedMemoryInterfaceClient shall monitor PersKeyPairing\_St to maintain and display a Keyfob Association Icon for exsiting Driver Profiles:

* When PersKeyPairing\_St = KeyAssociated, the icon shall be displayed
* When PersKeyPairing\_St = KeyUnAssociated or Null, the icon shall not be displayed

#### ENMEM-HMI-REQ-233009/A-Phone HMI Indication

The EnhancedMemoryInterfaceClient shall monitor PersPhonePairing\_St to maintain and display a Phone Association Icon for existing Driver Profiles:

* When PersPhonePairing\_St = NoPhonesAssociated, the icon shall not be displayed
* When PersPhonePairing\_St = OnePhoneAssociated, the icon shall be displayed

#### Memory Seat Button Association

In order to include Positional settings in Enhanced Memory, a Driver Profile is required to associate to a Memory Seat button automatically according to creation order.

##### ENMEM-REQ-099685/E-Request Enter Memory Seat Button Association Mode

When associating a Driver Memory Seat Button during the Profile Creation process, the EnhancedMemoryInterfaceClient will command the EnhancedMemoryPositionClient to enter a button pairing state where certain functions are to be disabled in the EnhancedMemoryPositionClient. This button pairing state is communicated to the EnhancedMemoryPositionClient via the EnMemProfilePairing\_Rq(ButtonPairing) method.

This button pairing state shall also be re-entered between Driver Memory Seat Button Association attempts (limited to ENMEM-REQ-179346-N\_NumberOfRetries) if an unsuccessful attempt should occur (i.e. timer expires or an already associated Driver Memory Seat button is pressed, as detailed in ENMEM-REQ-116803-Request Exit Memory Seat Button Association Mode).

Once the button pairing state is entered (EnMemProfilePairing\_Rq(ButtonPairing = EnterButtonPairing)), the EnhancedMemoryPositionClient shall prevent driver position recalls (seat, mirrors, etc.), and suppress the transmission of MemSwitchRecall\_Rq and Memory\_Cmd (legacy signal) methods when a Driver Memory Seat button is pressed during this state.

The EnhancedMemoryPositionClient shall exit this button pairing state when indicated by EnMemProfilePairing\_Rq(ButtonPairing = ExitButtonPairing) or when Ignition\_Status transitions out of *Run*, whichever comes first.

##### ENMEM-REQ-198930/A-No Request for Memory Seat Button Association Mode When Editing

When editing the Drive Profile name, even if an unique Driver Profile name is successfully entered, EnhancedMemoryInterfaceClient shall not command the EnhancedMemoryPositionClient to enter button association mode.

##### ENMEM-REQ-198931/A-Retry and Error Handling Strategies for Seat Button Association Mode

* After sending the request for entering Memory Seat Button Association Mode (EnMemProfilePairing\_Rq(ButtonPairing = EnterButtonPairing)), if there is no response (EnMemButtonPairing\_St(ButtonPairing = ButtonPairingEntered, ButtonPairingFailed)) within 500 msec or communication data is invalid or corrupted, then the EnhancedMemoryInterfaceClient shall resend the request up to 3 times.
  + When multiple requests do not yield correct response, the EnhancedMemoryInterfaceClient shall abort Driver Profile creation process entirely by doing the following actions:
    - Set EnMemProfilePairing\_Rq(ButtonPairing = ExitButtonPairing)
    - Erase Driver Profile name from internal memory
    - Turn Enhanced Memory Feature Off if the there is no other existing Driver Profiles
  + The EnhancedMemoryInterfaceClient shall provide the user HMI notification about the abort process status
* After sending the request for exiting Memory Seat Button Association Mode (EnMemProfilePairing\_Rq(ButtonPairing = ExitButtonPairing)), if there is no response (EnMemButtonPairing\_St(ButtonPairing = ButtonPairingExited, ButtonPairingFailed)) within 500 msec or communication data is invalid or corrupted, then the EnhancedMemoryInterfaceClient shall resend the request up to 3 times.
  + When multiple requests do not yield correct response, the EnhancedMemoryInterfaceClient shall do the following actions:
    - Revert the Pers#Status for PersonalityOptIn\_St back to NotOptedIn for the Memory Seat Button selected
    - Do not perform a Driver Profile recall
    - Do not store mapping of Profile Number to selected Memory Seat Button
    - Turn Enhanced Memory Feature Off if the there is no other existing Driver Profiles
  + The EnhancedMemoryInterfaceClient shall provide the user HMI notification about the abort process status

##### ~~ENMEM-REQ-198928/B-Button Press in Button Association Mode~~

~~In Memory Seat button association mode, button presses as well as press and hold actions are not meant to recall Driver Profiles or save positional settings. Instead, button press actions shall only serve as the indicator of a button being associated to a new Driver Profile.~~

* ~~In Memory Seat button association mode, EnhancedMemoryPositionClient shall suppress the transmission of MemSwitchRecall\_Rq when a Memory Seat button is pressed during this mode.~~
* ~~When detecting a button press in Memory Seat button association mode, EnhancedMemoryPositionClient shall inform the EnhancedMemoryInterfaceClient which button is pressed via EnMemButtonPairing\_St (ButtonPairing).~~

##### ~~ENMEM-REQ-198934/A-Button Press Error Strategy~~

~~The EnhancedMemoryPositionClient shall report ButtonPairingFailed via EnMemButtonPairing\_St(ButtonPairing) whenever the user presses SET button during Memory Seat button association process.~~

~~Other customer button press errors, defined by Classic Memory feature specification, shall also trigger EnhancedMemoryPositionClient to report ButtonPairingFailed during Memory Seat button association process.~~

##### ENMEM-REQ-199236/A-No Recall in Button Association Mode

During Memory Seat Button Association Mode, all profile recall requests (regardless of recall method) shall be ignored by the EnhancedMemoryProfileServer. This is to prevent any confusion regarding what settings will be copied to a Driver Profile during Profile Creation.

##### ENMEM-REQ-199352/A-Successful Memory Button Association

A successful Memory Seat button association event shall be defined as when in button association mode the EnhancedMemoryInterfaceClient receives a valid button press status and internally determines that the pressed button is not associated to any existing Driver Profiles.

A valid memory button press shall be defined as EnMemButtonPairing\_St(ButtonPairing) with encoding value in the range from 1 to 4 (i.e. Button1Pressed, Button2Pressed, Button3Pressed, Button4Pressed)

The EnhancedMemoryInterfaceClient HMI shall display a retry popup when:

1. EnMemButtonPairing\_St(ButtonPairing) is not in valid range

2. EnMemButtonPairing\_St(ButtonPairing) is in failure state

3. Pressed button is already associated to another Driver Profile

##### ENMEM-REQ-197965/A-No overwrite for Memory Seat Buttons already associated to Existing Driver Profiles

The EnhancedMemoryInterfaceClient shall not permit a user to overwrite a Memory Seat Button already associated to an existing Driver Profile, to a newly created Driver Profile.

##### ENMEM-REQ-116803/C-Request Exit Memory Seat Button Association Mode

EnhancedMemoryInterfaceClient shall command the EnhancedMemoryPositionClient to exit Button Association Mode via EnMemProfilePairing\_Rq(ButtonPairing = ButtonPairingExited) for the following cases:

* The user cancels out of the association process (ex. presses touch screen exit/back button)
* The user is inactive after T\_SeatAssocOneTime expires. This is indicated through no change state of EnMemButtonPairing\_St(ButtonPairing = ButtonPairingEntered)
* The user presses the Driver Memory Seat’s SET button. This is indicated via EnMemButtonPairing\_St(ButtonPairing= ButtonPairingFailed)
* The user presses an already associated Driver Memory Seat button
* The Association Retry Counter, N\_NumberOfRetries, as defined in ENMEM-REQ-179346, is exceeded
* If the profile creation process is not active (not in process of creating a new profile) and the EnhancedMemoryInterfaceClient receives EnMemButtonPairing\_St(ButtonPairing != Null)
* A system event occurs that terminates the association process
  + Vehicle speed is greater than 8kph (see ENMEM-REQ-099699)
  + Vehicle ignition is no longer in Run
  + Infotainment System is powered down (ex. Load Shed event)
  + Communication data is invalid, corrupted or Communication with EnhancedMemoryPositionClient is lost

##### ENMEM-REQ-198935/A-Exit Memory Seat Button Association Mode

EnhancedMemoryPositionClient shall exit Button Association Mode and set EnMemButtonPairing\_St(ButtonPairing = ButtonPairingExited) for the following cases:

* When receiveing EnMemProfilePairing\_Rq(ButtonPairing = ExitButtonPairing)
* The Association timer, T\_SeatAssocOneTime2, as defined in ENMEM-TMR-REQ-197339, has expired
* Communication with EnhancedMemoryInterfaceClient is lost

##### ENMEM-REQ-197340/A-Button Pairing Timer Expired

When T\_SeatAssocOneTime2 expires, the EnhancedMemoryPositionClient shall exit Button Association Mode and update the status of EnMemButtonPairing\_St(ButtonPairing) to ButtonPairingExited for a time of T\_ReturnToNull, followed by Null.

##### ENMEM-TMR-REQ-197339/A-T\_SeatAssocOneTime2

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Name** | **Description** | **Units** | **Range** | **Resolution** | **Default** |
| T\_SeatAssocOneTime2 | Maximum time the EnhancedMemoryPositionClient shall wait before exiting Button Association Mode.  Note: Use the default value | sec | 40-130 | 5 | 70 |

#### Driver Profile Creation via Copy Operation

A new Driver Profile is created by copying the current active settings to the target Driver Profile that’s being created.

This Driver Profile creation task is accomplished through a Copy operation that is designed to allow multiple features to be saved to a different profile at once with one signal command. Unlike other Feature Based Message Protocol operations such as Query and Set, the Copy command is not designed to be issued one at a time for each feature.

##### ENMEM-REQ-198923/A-Copy Request

After a Memory Seat button is successfully associated to a Driver Profile, EnhancedMemoryInterfaceClient shall send the Copy operation request via Feature\_Rq(Operation = Copy, FeatureID = 0,Configuration = 0xFFFF, PersIndex)to all EnhancedMemoryServers.

To prevent FeatureID and Configuration from being used in Copy command, FeatureID shall be set to zero to indicate an invalid feature ID whereas Configuration shall be set to 0xFFFF to indicate a non-existing setting.

##### ENMEM-REQ-198922/A-Driver Profile Index for Copy Command

In the Copy request, via Feature\_Rq(PersIndex), the PersIndex shall be the same number as the unassociated Memory Seat button pressed by the user.

Example:

If the Memory Seat button X is pressed, indicated by EnMemButtonPairing\_St(ButtonPairing=ButtonXPressed), the EnhancedMemoryInterfaceClient will then determine that Memory Seat button’s association status internally.

* If the status is not associated, the EnhancedMemoryInterfaceClient will then set Feature\_Rq(PersIndex) to PERS\_X
* If the status is associated, the EnhancedMemoryInterfaceClient will send EnMemProfilePairing\_Rq(ButtonPairing=ExitButtonPairing) to the EnhancedMemoryPositionClient and the EnhancedMemoryInterfaceClient will display a retry prompt to the user.

##### ENMEM-REQ-198920/B-Execute Copy Operation

When receiving a Copy command via Feature\_Rq(Operation = Copy), an EnhancedMemoryServer shall copy all applicable personalized features’ current active settings (not the active Driver Profile settings as that could be different than current active settings) to the new Driver Profile indicated by Feature\_Rq(PersIndex = PERS\_X).

Personalized features that are to be copied to the new Driver Profile shall be internally managed by the EnhancedMemoryServer itself and shall be determined by a separate program-specific document for each EnhancedMemoryServer.

The Copy command shall only be used as an indicator for the EnhancedMemoryServer to perform an internal copy of all applicable personalized features. It shall not be used as a series of Copy commands for each individual FeatureID and Configuration supported by an EnhancedMemoryServer. For this reason, the Feature\_Rq(FeatureID) and Feature\_Rq(Configuration) values shall be ignored by the EnhancedMemoryServer for all Copy commands sent by the EnhancedMemoryInterfaceClient.

##### ENMEM-REQ-198919/B-Performance Requirement for Copy Operation

All EnhancedMemoryServers shall perform the Copy operation within T\_PersCopy.

##### ENMEM-REQ-099698/B-Wait Response From AudioServer While Copy Operation is Still in Progress

The AudioServer shall complete all Copy operations within T\_PersCopy. In the case that an Enhanced Memory related Copy operation is still in progress at the time a request for preset data (GetTUPresetInfo\_Rq) is received, then the AudioServer shall respond to the GetTUPresetInfo\_Rq method with a CES response code of "Intermediate Result - Wait” until the Copy operation has been successfully completed. Upon completion of the Enhanced Memory related Copy operation, the AudioServer will provide the requested preset data.

##### ENMEM-TMR-REQ-105579/B-T\_PersCopy

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Name** | **Description** | **Units** | **Range** | **Resolution** | **Default** |
| T\_PersCopy | Maximum time the EnhancedMemoryServers shall take to complete all Enhanced Memory related Copy operations for a given Driver Profile upon request.  Note: Use the default value | msec | 1500-4500 | 500 | 3000 |

##### ENMEM-REQ-199347/A-Request Exit Memory Button Association Mode After Copy

After sending the FBMP Copy request, EnhancedMemoryInterfaceClient shall wait a minimum of T\_PersCopy before sending a request (EnMemProfilePairing\_Rq(ButtonPairing = ExitButtonPairing)) to exit Memory Seat button association mode.

##### ENMEM-REQ-198918/A-Recall New Driver Profile After Copy

* After sending the Copy request and then sending an exit Memory Seat Button Association request, the EnhancedMemoryInterfaceClient shall ensure EnMemButtonPairing\_St(ButtonPairing= ButtonPairingExited) is received and shall wait a minimum of T\_RecallDelay from the time the FBMP Copy request was first sent, before sending a request to update to the new Driver Profile via the InfotainmentRecall\_Rq method
* The value of T\_RecallDelay shall be a configurable value

##### ENMEM-TMR-REQ-099765/B-T\_RecallDelay

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Name** | **Description** | **Units** | **Range** | **Resolution** | **Default** |
| T\_RecallDelay | The time from when the EnhancedMemoryInterfaceClient sends the FBMP Copy command until it sends the recall request  Note: Use the default value + or - 10% | msec | 3000-7000 | 500 | 5000 |

##### ENMEM-TMR-REQ-134146/B-T\_OptInRecallSeparation

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Name** | **Description** | **Units** | **Range** | **Resolution** | **Default** |
| T\_OptInRecallSeparation | Minimum separation time the EnhancedMemoryInterfaceClient shall have between sending the PersonalityOptIn\_St and sending the InfotainmentRecall\_Rq.  Note: Use the default value | msec |  | 5 | 100 |

##### ENMEM-REQ-099683/D-Storing Positional Settings for the Copy Operation

When creating a Driver Profile, during the copy operation, the EnhancedMemoryPositionClient’s current positional settings shall be copied to the new Driver Profile that’s being created. In order to guarantee this task is accomplished, an infotainment positional setting store operation shall be issued before the recall request.

* The EnhancedMemoryInterfaceClient shall send a store positional settings request via InfotainmentPersStore\_Rq to the EnhancedMemoryPositionClient before sending the recall request for the new Driver Profile
* The EnhancedMemoryPositionClient shall store all current Classic Memory settings to the indicated memory seat button (which may include performing a Classic Memory subsystem store operation) upon reception of the InfotainmentPersStore\_Rq method and respond with InfotainmentPersStore\_St(Status = Complete) when complete.
  + While the store operation is being performed, the EnhancedMemoryPositionClient shall respond with InfotainmentPersStore\_St(Status = InProgress).

Reference sequence diagram ENMEM-SD-REQ-099425-Create Driver Profile for details.

#### Keyfob/Phone Association

The pairing of a Keyfob or Phone is an optional operation in the Enhanced Memory feature set. This can be done during or after profile creation. This can only be completed through the Enhanced Memory feature and is not available when Enhanced Memory is not OptedIn.

##### ENMEM-REQ-099672/C-Configurable Parameter for Key/Phone Pairing

The EnhancedMemoryProfileServer shall have a configurable parameter to determine whether the vehicle supports the Enhanced Memory feature:

* If the parameter indicates that the vehicle is to support “Classic Memory”, then the EnMemProfilePairing\_Rq(KeyPairing) method shall be ignored since keyfob association will instead be coordinated via the legacy MemSwtch\_D\_RqAssoc method, which is defined in the existing Classic Memory subsystem specifications.
* If the parameter indicates that the vehicle is to support “Enhanced Memory”, then the legacy MemSwtch\_D\_RqAssoc method shall be ignored since keyfob association will instead be coordinated via the EnMemProfilePairing\_Rq(KeyPairing) method.
  + Phone association shall only be supported when the parameter indicates that the vehicle is to support “Enhanced Memory” and shall be coordinated via the EnMemProfilePairing\_Rq(KeyPairing) method

##### ENMEM-REQ-099697/B-Configurable Parameter to Disable Classic Keyfob Pairing

The EnhancedMemoryPositionClient shall have a configurable parameter to determine whether the vehicle supports the Enhanced Memory feature. If the parameter indicates that the vehicle is to support “Enhanced Memory”, then the legacy MemSwtch\_D\_RqAssoc method shall be sent with null values to the EnhancedMemoryProfileServer and any associated chimes/tones for key pairing shall be suppressed.

##### ENMEM-REQ-099686/C-Keyfob Pairing Mode

To associate a Driver Profile to a keyfob, the EnhancedMemoryInterfaceClient shall communicate to the EnhancedMemoryProfileServer that the Key Pairing mode has been entered via the EnMemProfilePairing\_Rq (PersIndex=PersX, KeyPairing=EnterKeyPairing) method.

* Once EnMemProfilePairing\_Rq (PersIndex=PersX, KeyPairing=EnterKeyPairing) is sent, the EnhancedMemoryProfileServer shall respond with EnMemKeyPairing\_St(KeyPairing = KeyPairingEntered) upon successful entering of the Keyfob Pairing Mode.
* The EnhancedMemoryProfileServer shall begin looking for a “Lock” button press from PersX keyfob to associate to the requested Driver Profile. If the Keyfob detected is not already associated to another Driver Profile, the EnhancedMemoryProfileServer shall transmit EnMemKeyPairing\_St(KeyPairing = KeyAssociateSuccess) after associating the detected keyfob to the requested Driver Profile.
* The EnhancedMemoryProfileServer shall update the status of PersKeyPairing\_St(PersXKeyStatus=Key Associated).
* The EnhancedMemoryProfileServer shall exit Key Pairing mode when indicated by:
  + EnMemProfilePairing\_Rq(KeyPairing = ExitKeyPairing)
  + EnMemKeyPairing\_St(KeyPairing = KeyAssociateSuccess)
  + Ignition\_Status transitions out of *Run*,
  + Gear Lever Position transitions out of *Park*,
  + Vehicle speed exceeds 8kph, whichever comes first.

Reference sequence diagram ENMEM-SD-REQ-099422-Associate Key Fob for details

##### ENMEM-REQ-233118/B-Phone Pairing Mode

To associate a Driver Profile to a phone, the EnhancedMemoryInterfaceClient shall communicate to the EnhancedMemoryProfileServer that the Phone Pairing mode has been entered via the EnMemProfilePairing\_Rq (PersIndex=PersX, KeyPairing=EnterPhonePairing) method.

* Once EnMemProfilePairing\_Rq (PersIndex=PersX, KeyPairing=EnterPhonePairing) is sent, the EnhancedMemoryProfileServer shall respond with EnMemKeyPairing\_St(KeyPairing = KeyPairingEntered) upon successful entering of the Phone Pairing Mode.
* The EnhancedMemoryProfileServer shall begin looking for a “Lock” button press from PersX Phone to associate to the requested Driver Profile. If the Phone detected is not already associated to another Driver Profile, the EnhancedMemoryProfileServer shall transmit EnMemKeyPairing\_St(KeyPairing = KeyAssociateSuccess) after associating the detected Phone to the requested Driver Profile.
* The EnhancedMemoryProfileServer shall update the status of PersPhonePairing\_St(PersXPhoneStatus=OnePhoneAssociated).
* The EnhancedMemoryProfileServer shall exit Phone Pairing mode when indicated by:
  + EnMemProfilePairing\_Rq(KeyPairing = ExitKeyPairing)
  + EnMemKeyPairing\_St(KeyPairing = KeyAssociateSuccess)
  + Ignition\_Status transitions out of *Run*,
  + Gear Lever Position transitions out of *Park*,
  + Vehicle speed exceeds 8kph, whichever comes first.

Reference sequence diagram ENMEM-SD-REQ-233258-Associate Phone for details

##### ENMEM-REQ-234278/A-Detection of a Keyfob/Phone in Opposite Pairing Mode

When a keyfob is detected during the Phone Association process, or when a phone is detected during the Keyfob Association process, the EnhancedMemoryProfileServer shall update the status of EnMemKeyPairing\_St(KeyPairing) to WrongDeviceSelected for 1 second, and then return to KeyPairingEntered to resume the ongoing association mode operation.

##### ENMEM-HMI-REQ-234279/A-Wrong Device Detected HMI

In the Keyfob or Phone Association Process, the EnhancedMemoryInterfaceClient shall monitor EnMemKeyPairing\_St to provide the wrong device HMI notification to the user.

When a value of WrongDeviceSelected is detected via EnMemKeyPairing\_St(KeyPairing):

* The EnhancedMemoryInterfaceClient shall provide a temporary notification to the user that the wrong device was selected
* This notification shall be triggered, not sustained, by the above signal value (See H31a\_SYNC3\_EMDriverProfile for notification duration).

##### ENMEM-REQ-198044/B-Detection of Associated Keyfob/Phone

When a keyfob or phone is detected in their respective Keyfob or Phone Association processes, the EnhancedMemoryProfileServer shall check if the detected keyfob or phone is already associated to an existing Driver Profile.

In the case where the detected keyfob or phone is already associated to an existing Driver Profile, the EnhancedMemoryProfileServer shall update the status of EnMemKeyPairing\_St(KeyPairing) to KeyAlreadyInUse.

##### ENMEM-SR-REQ-198055/C-Enhanced Memory HMI Option for Associated Keyfob/Phone

In the Keyfob or Phone Association process,

* The EnhancedMemoryInterfaceClient shall monitor EnMemKeyPairing\_St to determine when a user attempts to associate an already associated keyfob or phone to a new Driver Profile.
* When receiving KeyAlreadyInUse via EnMemKeyPairing\_St(KeyPairing):
* EnhancedMemoryInterfaceClient shall provide notification to the user that the keyfob or phone is already associated to an existing Driver Profile
* EnhancedMemoryInterfaceClient shall provide the user an option to over-write the associated keyfob or phone, or to cancel the keyfob or phone association process
* When the user opts to over-write the associated keyfob or phone, the EnhancedMemoryInterfaceClient shall set EnMemProfilePairing\_Rq(KeyPairing) to OverwriteKey.

##### ENMEM-REQ-198100/B-Overwrite Associated Keyfob

When receiving OverwriteKey via EnMemProfilePairing\_Rq(KeyPairing):

* EnhancedMemoryProfileServer shall erase the existing keyfob association and associate the new keyfob to the Driver Profile denoted by EnMemProfilePairing\_Rq (PersIndex)
* EnhancedMemoryProfileServer shall update PersKeyPairing\_St accordingly:
* The Driver Profile whose keyfob association was erased shall be updated from KeyAssociated to KeyUnAssociated
* The Driver Profile with the newly associated keyfob shall be updated from KeyUnAssociated to KeyAssociated

##### ENMEM-REQ-233161/A-Overwrite Associated Phone

When receiving OverwritePhone via EnMemProfilePairing\_Rq(KeyPairing):

* EnhancedMemoryProfileServer shall erase the existing phone association and associate the new phone to the Driver Profile denoted by EnMemProfilePairing\_Rq (PersIndex)
* EnhancedMemoryProfileServer shall update PersPhonePairing\_St accordingly:
* The Driver Profile whose phone association was erased shall be updated from OnePhoneAssociated to NoPhonesAssociated
* The Driver Profile with the newly associated phone shall be updated from NoPhonesAssociated to OnePhoneAssociated

##### ENMEM-REQ-099690/D-Keyfob/Phone Pairing Failed

Any fault of the EnhancedMemoryProfileServer that prevents Keyfob or Phone Pairing shall result in the EnhancedMemoryProfileServer communicating to the EnhancedMemoryInterfaceClient that the keyfob or phone was not able to be associated by updating the status of EnMemKeyPairing\_St(KeyPairing) to KeyAssociateFailed.

When the EnhancedMemoryInterfaceClient receives EnMemKeyPairing\_St(KeyPairing = KeyAssociateFailed), the EnhancedMemoryInterfaceClient HMI shall notify the user that the Keyfob or Phone Pairing process has failed and shall exit the Keyfob or Phone Pairing process.

##### ENMEM-REQ-194169/B-Keyfob/Phone Pairing Timer Expired

When T\_FobAssocTotal2 expires, the EnhancedMemoryProfileServer shall exit Keyfob or Phone Pairing Mode and update the status of EnMemKeyPairing\_St(KeyPairing) to KeyAssociateFailed for 1 second, followed by Null.

##### ENMEM-TMR-REQ-194101/C-T\_FobAssocTotal2

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Name** | **Description** | **Units** | **Range** | **Resolution** | **Default** |
| T\_FobAssocTotal2 | After entering Keyfob or Phone Pairing Mode, the maximum time the EnhancedMemoryProfileServer shall wait before exiting Keyfob or Phone Pairing Mode. | msec | 300000-420000 | 60000 | 360000 |

##### ENMEM-REQ-116804/F-Keyfob/Phone Pairing Error

If the Keyfob or Phone Pairing process is not active (not in process of pairing a keyfob or phone to a profile) and the EnhancedMemoryInterfaceClient receives EnMemKeyPairing\_St(KeyPairing != Null), then the EnhancedMemoryInterfaceClient shall send EnMemProfilePairing\_Rq(KeyPairing = ExitKeyPairing).

The EnhancedMemoryInterfaceClient shall abort the process by sending EnMemProfilePairing\_Rq(KeyPairing = ExitKeyPairing) to the EnhancedMemoryProfileServer in the event the EnhancedMemoryInterfaceClient detects that:

* the vehicle is in motion (>8kph), or
* the vehicle transitions out of Run or Park, or
* the user exits Keyfob or Phone Pairing Mode via the HMI in the middle of the Keyfob Phone Pairing process
  + including a user initiated HMI domain change\* (see REQ-11680)

\*In the case of a non-user initiated domain change, the Keyfob or Phone Pairing process shall continue to proceed and the abort shall not occur (see REQ-116802).

If the EnhancedMemoryInterfaceClient receives EnMemKeyPairing\_St(KeyPairing = Null) after already entering Keyfob or Phone Pairing Mode, then the EnhancedMemoryInterfaceClient shall treat the Null as KeyAssociateExited.

##### ENMEM-SR-REQ-212303/B-PersIndex used for Keyfob/Phone Association

When requesting to enter Keyfob or Phone Association Mode, the EnhancedMemoryInterfaceClient shall set the PersIndex of the EnMemProfilePairing\_Rq to the value of:

* The Driver Memory Seat Button selected during the Create Driver Profile process, which is indicated by EnMemButtonPairing\_St(ButtonPairing), OR
* The PersIndex of the selected Driver Profile Edit button when attempting associate a keyfob or phone

If a recall should occur any time after the Driver Memory Seat Button Association and the start of the Keyfob or Phone Association process, the recalled PersIndex shall not be used for the Keyfob or Phone Association.

#### Delete Driver Profiles

The Delete Profile operation is used to erase a user’s Profile Name, Keyfob Icon, Phone Icon, Memory Seat Button Association, Keyfob Association, and Phone Association. This is a permanent operation and cannot be undone.

##### ENMEM-REQ-134465/D-Delete Driver Profile

When a created Driver Profile is deleted the EnhancedMemoryInterfaceClient shall:

1. If a keyfob is associated to the profile being deleted, the EnhancedMemoryInterfaceClient shall send a keyfob disassociation request, via  EnMemProfilePairing\_Rq(KeyPairing=DisassociateKey), without requiring a separate disassociation request from the user
2. If a phone is associated to the profile being deleted, the EnhancedMemoryInterfaceClient shall send a phone disassociation request, via  EnMemProfilePairing\_Rq(KeyPairing=DisassociatePhone), without requiring a separate disassociation request from the user
3. If the profile being deleted is the active profile, the EnhancedMemoryInterfaceClient shall send an infotainment recall request to recall Vehicle via InfotainmentRecall\_Rq
4. The EnhancedMemoryInterfaceClient shall update the PersonalityOptIn\_St to indicate that the deleted Driver Profile is "Opted-Out"
5. If the profile being deleted is the last available profile, the EnhancedMemoryInterfaceClient shall set the Enhanced Memory feature status to Off via EnhancedMemory\_St(Status=ProfilesOff).

Reference sequence diagram ENMEM-SD-REQ-099427- Delete Driver Profile for details

##### ENMEM-HMI-REQ-197502/B-Enhanced Memory HMI Indications for Delete a Driver Profile

When a Driver Profile is deleted:

* The EnhancedMemoryInterfaceClient shall remove and disable the Edit Driver Profile functionality
* The EnhancedMemoryInterfaceClient shall remove the name for the deleted Driver Profile
* The EnhancedMemoryInterfaceClient shall update the keyfob association icon status based on PersKeyPairing\_St for the deleted Driver Profile
* The EnhancedMemoryInterfaceClient shall update the phone association icon status based on PersPhonePairing\_St for the deleted Driver Profile

##### ENMEM-REQ-105569/D-Driver Profiles Deleted During Master Reset

The storage and maintenance of the Driver Profiles of Enhanced Memory shall comply with the design and requirements of Master Reset (refer to the latest version of VS-FUN-REQ-025341-Master Reset to Factory Defaults).

When a Master Reset operation is executed:

1. The EnhancedMemoryInterfaceClient shall delete all internal Driver Profile data (i.e. Profile Name, Button Association) for all Driver Profiles
2. If a keyfob is associated to a Driver Profile(s) the following actions shall be performed:
   * The EnhancedMemoryInterfaceClient shall request to disassociate the keyfob via EnMemProfilePairingRq(KeyPairing=DisassociateKey)
   * The EnhancedMemoryProfileServer shall respond with a successful keyfob disassociation via EnMemKeyPairing\_St(KeyPairing=KeyDisassociated)
   * The EnhancedMemoryProfileServer shall update the status of PersKeyPairing\_St to KeyNotAssociated for the Driver Profile deleted
   * If there are more than one profile with keys paired, the EnhancedMemoryInterfaceClient shall repeat steps 2 and 3 above until all the keyfobs are dissociated from all profiles
3. If a phone is associated to a Driver Profile(s) the following actions shall be performed:
   * The EnhancedMemoryInterfaceClient shall request to disassociate the phone via EnMemProfilePairingRq(KeyPairing=DisassociatePhone)
   * The EnhancedMemoryProfileServer shall respond with a successful phone disassociation via EnMemKeyPairing\_St(KeyPairing=KeyDisassociated)
   * The EnhancedMemoryProfileServer shall update the status of PersPhonePairing\_St to NoPhonesAssociated for the Driver Profile deleted
   * If there are more than one profile with phones paired, the EnhancedMemoryInterfaceClient shall repeat steps 2 and 3 above until all the phones are dissociated from all profiles
4. The EnhancedMemoryInterfaceClient shall send a recall request for Vehicle Profile via InfotainmentRecall\_Rq(PersIndex = Vehicle)
5. The EnhancedMemoryInterfaceClient shall OptOut of all profiles and set all active personalities in PersonalityOptIn\_St to NotOptedIn
6. The EnhancedMemoryInterfaceClient shall set the Enhanced Memory feature status to Off via EnhancedMemory\_St(Status = ProfileOff)
7. The EnhancedMemoryProfileServer shall send a recall request for Vehicle to the EnhancedMemoryPositionClient via MemoryPosition\_St. Note: this step does not apply to the EnhancedMemoryInterfaceClient and is don’t care for the EnhancedMemoryInterfaceClient
8. The EnhancedMemoryInterfaceClient shall send a Factory Reset request to the EnhancedMemoryServers via FactoryReset\_Rq(Type = Reset) to perform Master Reset on the EnhancedMemoryServers that support Master Reset (ex. AHU resets SDARS presets - see SDARS SPSS for details). If the EnhancedMemoryServer supports FactoryReset\_Rq, all profiles shall reset (ex. SDARS presets reset for all profiles).
9. The EnhancedMemoryInterfaceClient performs a reboot for Master Reset following VS-FUN-REQ-025341-Master Reset to Factory Defaults).
   * Note: the EnhancedMemoryInterfaceClient/Infotainment System Master shall send the FactoryReset\_Rq before shutting down the Infotainment System (i.e. sends FactoryReset\_Rq(Type = Reset) while HMI\_HMIMode\_St = On).

Reference sequence diagram ENMEM-SD-REQ-197509-Master Reset for details

#### Keyfob/Phone Disassociation

The Keyfob and Phone Disassociation processes can be completed manually via the HMI. It will be automatically performed when the user delete’s a profile or performs a Master Reset.

##### ENMEM-REQ-197506/B-Disassociate the Keyfob per User Request

When a user requests to disassociate a keyfob from a Driver Profile, the EnhancedMemoryInterfaceClient shall send EnMemProfilePairing\_Rq(KeyPairing = DisassociateKey) to the EnhancedMemoryProfileServer for the requested Driver Profile. The EnhancedMemoryProfileServer shall then respond with EnMemKeyPairing\_St (PersIndex = Pers#, KeyPairing = KeyDisassociated) upon successful disassociation of the keyfob.

##### ENMEM-REQ-233209/A-Disassociate the Phone per User Request

When a user requests to disassociate a phone from a Driver Profile, the EnhancedMemoryInterfaceClient shall send EnMemProfilePairing\_Rq(KeyPairing = DisassociatePhone) to the EnhancedMemoryProfileServer for the requested Driver Profile. The EnhancedMemoryProfileServer shall then respond with EnMemKeyPairing\_St (PersIndex = Pers#, KeyPairing = KeyDisassociated) upon successful disassociation of the phone.

##### ENMEM-REQ-197505/A-Keyfob Disassociation Status

The EnhancedMemoryProfileServer shall send PersKeyPairing\_St(PersXKeyStatus = KeyNotAssociated) to the EnhancedMemoryInterfaceClient for the applicable personality when:

* a keyfob is successfully disassociated for a Driver profile
* all keyfobs are erased from a vehicle by Diagnostic tool for all Driver Profiles

##### ENMEM-REQ-233210/A-Phone Disassociation Status

The EnhancedMemoryProfileServer shall send PersPhonePairing\_St(PersXPhoneStatus = NoPhonesAssociated) to the EnhancedMemoryInterfaceClient for the applicable personality when:

* a phone is successfully disassociated from a Driver Profile
* a phone is erased or revoked from outside the vehicle (see Phone-As-A-Key SPSS for such methods).

##### ENMEM-HMI-REQ-202226/A-Keyfob HMI Indication

The EnhancedMemoryInterfaceClient shall monitor PersKeyPairing\_St to maintain and display a Keyfob Association Icon for exsiting Driver Profiles:

* When PersKeyPairing\_St = KeyAssociated, the icon shall be displayed
* When PersKeyPairing\_St = KeyUnAssociated or Null, the icon shall not be displayed

##### ENMEM-HMI-REQ-233009/A-Phone HMI Indication

The EnhancedMemoryInterfaceClient shall monitor PersPhonePairing\_St to maintain and display a Phone Association Icon for existing Driver Profiles:


* When PersPhonePairing\_St = NoPhonesAssociated, the icon shall not be displayed
* When PersPhonePairing\_St = OnePhoneAssociated, the icon shall be displayed

### White Box View

#### Activity Diagrams

##### ENMEM-ACT-REQ-099377/C-Create Driver Profile

Activity Diagram



##### ENMEM-ACT-REQ-099376/B-Associate Key Fob To Driver Profile

Activity Diagram



##### ENMEM-ACT-REQ-233257/A-Associate Phone To Driver Profile

Activity Diagram



##### ENMEM-ACT-REQ-099379/D-Delete Driver Profile

Activity Diagram



##### ENMEM-ACT-REQ-197508/B-Master Reset

Activity Diagram



#### Sequence Diagrams

##### ENMEM-SD-REQ-099425/F-Create Driver Profile

Constraints

Pre-Condition

Ignition Status = Run

Vehicle is in Park

Vehicle speed is less than 8 KPH.

Maximum number of personality profiles has not yet been reached

Scenarios

Normal Usage

The driver chooses to create a new personality profile and memory seat button to associate to that profile.


Post-Condition

Driver profiles feature is enabled

A new profile is created

The chosen memory seat button is associated to the new profile

Sequence Diagram



Note: The Profile creating order, if any profile deleted, EnhancedMemoryInterfaceClient need keep the PersIndex.

For example: Driver creates 3 profile A, B and C. A.PersIndex=1, B.PersIndex=2, C.PersIndex=3. If we delete Profile B, and new created profile D, the result is as below:

A.PersIndex=1, C.PersIndex=3, D.PersIndex=2.

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Name** | **Description** | **Units** | **Range** | **Resolution** | **Default** |
| T\_ShortPress | T\_ShortPress indicate the button short press time duration for button association | msec | 50-1500 | 5 | 100 |

##### ~~ENMEM-SD-REQ-197169/B-User Chooses a Seat Button That is Already Associated to Another Driver Profile~~

~~Constraints~~

~~Pre-Condition~~

~~Ignition Status = Run~~

~~Vehicle speed is less than 8 KPH~~

~~Vehicle HMI prompts the user to press a seat button at door panel during creating Driver profile process~~

~~Scenarios~~

~~Normal Usage~~

~~The user presses a button that is already associated to another Driver profile~~

~~Post-Condition~~

~~Vehicle HMI provides indication that the button is already associated to another profile and provides the user opportunities to retry~~

Sequence Diagram



##### ENMEM-SD-REQ-099422/D-Associate Key Fob

Constraints

Pre-Condition

Ignition Status = Run

Vehicle is in Park

Vehicle speed is less than 8 KPH.

Scenarios

Normal Usage

The driver chooses to associate a key fob to a selected personality profile.

Post-Condition

The selected key fob is associated to the selected personality profile.

Sequence Diagram



##### ENMEM-SD-REQ-233258/B-Associate Phone

Constraints

Pre-Condition

Ignition Status = Run

Vehicle is in Park

Vehicle speed is less than 8 KPH.

Scenarios

Normal Usage

The driver chooses to associate a phone to a selected personality profile.

Post-Condition

The selected phone is associated to the selected personality profile.

Sequence Diagram



##### ENMEM-SD-REQ-099423/B-Disassociate Key Fob

Constraints

Pre-Condition

Ignition Status = Run

Vehicle speed is less than 8 KPH.

Scenarios

Normal Usage

The driver chooses to disassociate a key fob from a selected personality profile.

Post-Condition

The selected key fob is disassociated from the selected personality profile.

Sequence Diagram



##### ENMEM-SD-REQ-233259/A-Disassociate Phone

Constraints

Pre-Condition

Ignition Status = Run

Vehicle speed is less than 8 KPH.

Scenarios

Normal Usage

The driver chooses to disassociate a phone from a selected personality profile.

Post-Condition

The selected phone is disassociated from the selected personality profile.

Sequence Diagram

****

##### ENMEM-SD-REQ-099427/D-Delete Driver Profile

Constraints

Pre-Condition

Ignition Status = Run

Vehicle speed is less than 8 KPH.

Infotainment system is active

Scenarios

Normal Usage

The driver chooses to delete a personality profile.

Post-Condition

The selected profile is deleted.

Any keyfobs associated to the deleted profile are disassociated.

Any phones associated to the deleted profile are disassociated.

Sequence Diagram



##### ENMEM-SD-REQ-197509/B-Master Reset

Constraints

Pre-Condition

Ignition Status = Run

Vehicle speed is less than 8KPH

Infotainment system is on

Driver profiles feature is enabled

Scenarios

Normal Usage

The driver performs a Master Reset

Post-Condition

The Driver Profiles feature is disabled (set to off).

All Driver Profiles are deleted.

All associated keyfobs are disassociated.

All associated phones are disassociated.

The active Driver Profile is set to “Guest”.

Applicable personalized infotainment settings are reset to factory default values for all profiles.

Sequence Diagram



## ENMEM-FUN-REQ-195573/C-EnhancedMemoryInterfaceClient HMI Requirements – APIM

### Requirements

#### ENMEM-HMI-REQ-195574/B-HMI Timeout for Overall Keyfob/Phone Pairing Process

On the HMI screen flows when the user starts the keyfob or phone pairing process to a particular profile, the HMI shall timeout and exit the process after T\_FobAssocTotal.

When the HMI screen flow is exited, the EnhancedMemoryIntefaceClient shall send EnMemProfilePairing\_Rq(KeyPairing = ExitKeyPairing) to the EnhancedMemoryProfileServer.

#### ENMEM-TMR-REQ-194098/C-T\_FobAssocTotal

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Name** | **Description** | **Units** | **Range** | **Resolution** | **Default** |
| T\_FobAssocTotal | Maximum time the EnhancedMemoryInterfaceClient shall allow user to assign a Keyfob or Phone to a Driver Profile for all attempts.  Note: use the default value | sec | 180-600 | 60 | 300 |

#### ENMEM-HMI-REQ-195576/B-HMI Timeout for One Keyfob/Phone Pairing Attempt

On the HMI screen flows when the user starts the keyfob or phone pairing process to a particular profile, the HMI shall timeout and offer a retry after T\_FobAssocOneTime.

When the HMI screen flow is entered for the keyfob pairing process, the EnhancedMemoryIntefaceClient shall send EnMemProfilePairing\_Rq(KeyPairing = EnterKeyPairing) to the EnhancedMemoryProfileServer.

When the HMI screen flow is entered for the phone pairing process, the EnhancedMemoryIntefaceClient shall send EnMemProfilePairing\_Rq(KeyPairing = EnterPhonePairing) to the EnhancedMemoryProfileServer.

When the timer expires and the HMI screen flow is exited the EnhancedMemoryIntefaceClient shall send EnMemProfilePairing\_Rq(KeyPairing = ExitKeyPairing) to the EnhancedMemoryProfileServer.

#### ENMEM-TMR-REQ-194099/C-T\_FobAssocOneTime

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Name** | **Description** | **Units** | **Range** | **Resolution** | **Default** |
| T\_FobAssocOneTime | Maximum time the EnhancedMemoryInterfaceClient shall allow user to assign a Keyfob or Phone to a Driver Profile within one attempt.  Note: use the default value | sec | 10-60 | 5 | 15 |

#### ENMEM-HMI-REQ-195575/B-Number of Retries on HMI for Keyfob/Phone Pairing

On the HMI screen flows, when the user fails to associate a Memory Seat button, keyfob, or phone to a Driver Profile and the screen flow timeout occurs, the HMI shall offer the user a retry. The number of retries offered is defined by N\_NumberOfRetries.

#### ENMEM-REQ-179346/B-N\_NumberOfRetries

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Name** | **Description** | **Units** | **Range** | **Resolution** | **Default** |
| N\_NumberOfRetries | N\_NumberOfRetries is the number of retries offered to the user to associate a Memory Seat button, keyfob, or phone to a Driver Profile before the association process is declared unsuccessful and terminated |  | 2-5 | 1 | 3 |

#### ENMEM-HMI-REQ-197344/A-HMI Timeout for One Button Pairing Attempt

On the HMI screen flows when the user starts the button pairing process upon profile creation, the HMI shall timeout and offer a retry after T\_SeatAssocOneTime.

When the HMI screen flow is entered for the pairing process, the EnhancedMemoryIntefaceClient shall send EnMemProfilePairing\_Rq (ButtonPairing = EnterButtonPairing) to the EnhancedMemoryPositionClient. When the timer expires and the HMI screen flow is exited the EnhancedMemoryIntefaceClient shall send EnMemProfilePairing\_Rq (ButtonPairing = ExitButtonPairing) to the EnhancedMemoryPositionClient.

#### ENMEM-TMR-REQ-197338/B-T\_SeatAssocOneTime

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Name** | **Description** | **Units** | **Range** | **Resolution** | **Default** |
| T\_SeatAssocOneTime | Maximum time the EnhancedMemoryInterfaceClient shall allow for the button pairing process.  Note: use the default value | sec | 30-120 | 5 | 60 |

#### ENMEM-HMI-REQ-099692/B-Driver Profile Sign-In Notification Queue

When a Driver Profile change occurs at a time when the EnhancedMemoryInterfaceClient cannot display a notification to the User, it shall queue up this display update until a time when a notification can then be displayed. This shall only apply for the last recall request.

#### ENMEM-HMI-REQ-202226/A-Keyfob HMI Indication

The EnhancedMemoryInterfaceClient shall monitor PersKeyPairing\_St to maintain and display a Keyfob Association Icon for exsiting Driver Profiles:

* When PersKeyPairing\_St = KeyAssociated, the icon shall be displayed
* When PersKeyPairing\_St = KeyUnAssociated or Null, the icon shall not be displayed

#### ENMEM-HMI-REQ-233009/A-Phone HMI Indication

The EnhancedMemoryInterfaceClient shall monitor PersPhonePairing\_St to maintain and display a Phone Association Icon for existing Driver Profiles:

* When PersPhonePairing\_St = NoPhonesAssociated, the icon shall not be displayed
* When PersPhonePairing\_St = OnePhoneAssociated, the icon shall be displayed

#### ENMEM-HMI-REQ-202357/B-Logical Signal to HMI Mapping

In order to help establish a link between the Enhanced Memory SPSS and the Enhanced Memory HMI Specification, a third document “EnhancedMemory\_SPSS\_HMI\_Mapping” was created. This document identifies where certain logic signals, timers, and other variables (that are defined in this SPSS) can be found in the HMI Specification.

#### ENMEM-HMI-REQ-197850/B-Enhanced Memory HMI Indications for Driver Profile

The Enhanced Memory HMI indication of an existing Driver Profile shall include the number of the associated Memory Seat button, the User’s keyed in Profile Name, and an associated keyfob icon and/or an associated phone icon shown only when one has been associated.

#### ENMEM-REQ-199352/A-Successful Memory Button Association

A successful Memory Seat button association event shall be defined as when in button association mode the EnhancedMemoryInterfaceClient receives a valid button press status and internally determines that the pressed button is not associated to any existing Driver Profiles.

A valid memory button press shall be defined as EnMemButtonPairing\_St(ButtonPairing) with encoding value in the range from 1 to 4 (i.e. Button1Pressed, Button2Pressed, Button3Pressed, Button4Pressed)

The EnhancedMemoryInterfaceClient HMI shall display a retry popup when:

1. EnMemButtonPairing\_St(ButtonPairing) is not in valid range

2. EnMemButtonPairing\_St(ButtonPairing) is in failure state

3. Pressed button is already associated to another Driver Profile

#### ENMEM-SR-REQ-198055/C-Enhanced Memory HMI Option for Associated Keyfob/Phone

In the Keyfob or Phone Association process,

* The EnhancedMemoryInterfaceClient shall monitor EnMemKeyPairing\_St to determine when a user attempts to associate an already associated keyfob or phone to a new Driver Profile.
* When receiving KeyAlreadyInUse via EnMemKeyPairing\_St(KeyPairing):
* EnhancedMemoryInterfaceClient shall provide notification to the user that the keyfob or phone is already associated to an existing Driver Profile
* EnhancedMemoryInterfaceClient shall provide the user an option to over-write the associated keyfob or phone, or to cancel the keyfob or phone association process
* When the user opts to over-write the associated keyfob or phone, the EnhancedMemoryInterfaceClient shall set EnMemProfilePairing\_Rq(KeyPairing) to OverwriteKey.

#### ENMEM-HMI-REQ-197502/B-Enhanced Memory HMI Indications for Delete a Driver Profile

When a Driver Profile is deleted:

* The EnhancedMemoryInterfaceClient shall remove and disable the Edit Driver Profile functionality
* The EnhancedMemoryInterfaceClient shall remove the name for the deleted Driver Profile
* The EnhancedMemoryInterfaceClient shall update the keyfob association icon status based on PersKeyPairing\_St for the deleted Driver Profile
* The EnhancedMemoryInterfaceClient shall update the phone association icon status based on PersPhonePairing\_St for the deleted Driver Profile

#### ENMEM-HMI-REQ-205014/A-Opt-In HMI Display

The Opt-In HMI display shall be displayed when all of the following conditions are met:

* The user presses "Driver Profiles" on the HMI Menu
* EnhancedMemory\_St(Status = ProfilesOff)
* No Driver Profile’s have been created (indicated by PersonalityOptIn\_St)

After displaying the Opt-In HMI, the following actions shall apply:

* Upon receiving a user’s “Opt-In” selection, the EnhancedMemoryInterfaceClient shall set EnhancedMemory\_St(Status = ProfilesOn) and begin the Create a Driver Profile process.
* Upon receiving a user’s “Not Opt-In” selection, the EnhancedMemoryInterfaceClient shall return to the previous Menu leaving EnhancedMemory\_St(Status = ProfilesOff)

#### ENMEM-HMI-REQ-207327/B-Driver Profile Name Restrictions

* The Driver Profile Names created and maintained by the EnhancedMemoryInterfaceClient shall be unique.
* In the event when an existing name is entered by the user, the EnhancedMemoryInterfaceClient shall:
  + provide notification to the user that the name already exists
  + not allow the existing name to be overwritten
  + provide the user retry opportunities until a unique name is entered before proceeding to next step

#### ENMEM-HMI-REQ-212764/A-Enhanced Memory HMI Notification of Profile Creation Abort

When Driver Profile creation is interrupted and aborted, per ENMEM-REQ-116802, the EnhancedMemoryInterfaceClient shall notify the user that the process has been aborted.

#### ENMEM-HMI-REQ-233260/A-Keyfob & Phone Association During Profile Creation

During Profile Creation, the EnhancedMemoryInterfaceClient shall offer the user the ability to pair a keyfob, a phone, both a keyfob and phone, or neither.

* A selection of “keyfob” shall begin the Keyfob Association Process
* A selection of “phone” shall begin the Phone Association Process
* A selection of “both” shall begin the Keyfob Association Process, followed by the Phone Association Process
* The EnhancedMemoryInterfaceClient shall remember a user selection of “both” in order to support the below functionality:
  + If the Keyfob Association Process successfully completes or is cancelled by the user, the Phone Association Process shall follow
  + If the Keyfob Association Process times-out (and after all retry attempts), the Phone Association Process shall follow
  + If the Keyfob Association Process is aborted by the system (see REQ-099690), the Phone Association Process shall not follow

#### ENMEM-HMI-REQ-234279/A-Wrong Device Detected HMI

In the Keyfob or Phone Association Process, the EnhancedMemoryInterfaceClient shall monitor EnMemKeyPairing\_St to provide the wrong device HMI notification to the user.

When a value of WrongDeviceSelected is detected via EnMemKeyPairing\_St(KeyPairing):

* The EnhancedMemoryInterfaceClient shall provide a temporary notification to the user that the wrong device was selected
* This notification shall be triggered, not sustained, by the above signal value (See H31a\_SYNC3\_EMDriverProfile for notification duration).

#### ENMEM-HMI-REQ-233264/B-Phone Association HMI Option

The EnhancedMemoryInterfaceClient shall monitor PaakConnection\_St and make active/inactive the offered “phone” and “both” pairing selections (see REQ-233260) and the ability to pair a phone via an edit menu as such:


* When PaakConnection\_St = Connected, the above shall be made active
* When PaakConnection\_St = NoneConnected, the above shall be made inactive (greyed-out, hidden, etc.)

## New Added Function - Dialog

### Dialog Function Description

With a active driver profile, if the driver adjusts the left/right mirror or seat position, DuerOS shall display three options: ‘Save’, ’Restore’ and ‘Cancel’.

The Duer OS shall not pop up in Drive mode!



### Use Cases

#### ENMEM-UC-REQ-xxx/x-Dialog display after seat position adjustment

|  |  |
| --- | --- |
| **Actors** | Vehicle Occupant |
| **Pre-conditions** | The Ignition Status is in Run  The vehicle transmission is in Park OR vehicle speed is less than the Driving Restriction threshold\* for a manual transmission  Profile A active. |
| **Scenario Description** | The driver adjusts the seat position |
| **Post-conditions** | DuerOS display dialog ‘Save’, ‘Restore’ and ‘Cancel’ |
| **List of Exception Use Cases** | If there no active driver profile present, DuerOS shall not display dialog. |
| **Interfaces** | Personalization Interface |
| **Notes** | \*Driving Restriction threshold is defined in DRIVE-RESv2-FUR-REQ-025157-HMI Driving Restriction |

### Requirements

#### ENMEM-REQ-xxx/x-Dialog Precondition

One profile active is the precondition of Dialog function.


*Note: Except the vehicle profile.*


#### ENMEM-REQ-xxx/x-Save Function

If driver chooses the ‘save’ option, DuerOS shall send the save command to DCU, DCU will transfer the command to DSM. So that, the adjusted position will be saved in the current profile.

Also, the DuerOS need show a save progress bar after save button click and stop it when receive the ‘PersStore\_D\_Actl=Complete’ or 3s timeout.

Note: Because there must be a positional operation before the appearance of save, even if the complete is not received within 3s, the save popup will disappear without any problem, and the next time the save will be prompted again





#### ENMEM-REQ-xxx/x-Restore Function


If driver chooses the ‘Restore’ option, DuerOS shall send the restore command to BCM, BCM will broadcast the current profile recall command to DSM and Enhanced Memory Servers. So that, the adjusted position will be restored in current profile.

#### ENMEM-REQ-xxx/x-Cancel Function

If driver chooses the ‘Cancel’ option, DuerOS shall cancel the dialog, and back to the original screen.

### White Box View

#### Activity Diagrams



#### Sequence Diagrams

##### ENMEM-SD-REQ-xxx/x-DuerOS dialog after positional settings changed

Constraints

Pre-Condition

One driver profile is in activate state.

Scenarios


Normal Usage

The user adjusts the left/right mirrors or seat position.

Post-Condition

DuerOS display three options: ‘Save’, ’Restore’ and ‘Cancel’.

Sequence Diagram



## New Added Function – Save from IVI

### Save function description

Save the newest positional settings to the active profile.

### Use Cases


#### ENMEM-UC-REQ-xxx/x-Save the newest positional settings to the current profile


|  |  |
| --- | --- |
| **Actors** | Vehicle Occupant |
| **Pre-conditions** | The Ignition Status is in Run  The vehicle transmission is in Park OR vehicle speed is less than the Driving Restriction threshold\* for a manual transmission  Profile A is active. |
| **Scenario Description** | 1. The driver adjusts the seat and mirrors position  2. The driver chooses the ‘save’ button after dialog displayed |
| **Post-conditions** | The adjusted seat and mirrors position are stored in profile A |
| **List of Exception Use Cases** | If there no active driver profile present, DuerOS shall not display dialog. |
| **Interfaces** | Personalization Interface |
| **Notes** | \*Driving Restriction threshold is defined in DRIVE-RESv2-FUR-REQ-025157-HMI Driving Restriction |

### Requirement

#### ENMEM-REQ-xxx/x-Save entrance

Driver can access the save soft button from sub-menu or dialog.






#### ENMEM-REQ-xxx/x-DuerOS show save progress bar

DuerOS shall show save progress bar after save operation and stop it when receive PersStore\_D\_Actl=complete or 3s timeout. Refer the 5.14.2.2 ENMEM-REQ-xxx/x-Save Function

### White Box View

#### Activity Diagrams



#### Sequence Diagram

##### Click save soft button after positional settings changed

**Constraints**

**Pre-Condition**

One profile is in activate state. And the user adjusts the left/right or seat position.

**Scenarios**

**Normal Usage**

Driver click the save soft button from DuerOS dialog.

**Post-Condition**

The newest positional settings are saved in the current profile.



##### ENMEM-TMR-REQ-xxx/x-T\_LongPress

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Name** | **Description** | **Units** | **Range** | **Resolution** | **Default** |
| T\_LongPress | T\_LongPress indicate the button long press time duration for saving operation | msec | 1500-3000 | 5 | 2000 |

##### ENMEM-TMR-REQ-xxx/x-CheckTheButtonPressedStatusIsNull

DCU shall confirm the signal ‘EmButtn\_D\_Stat’ equal to Null in the save sequence diagram

## New Added Function - Restore

### Restore function description

If driver choose the Restore option from the dialog, the DuerOS need send the current profile recall command to BCM. And all the changed positional settings will be restored to the settings previously stored in current profile.

### Use Cases


#### ENMEM-UC-REQ-xxx/x-Restore the mirrors and seat position

|  |  |
| --- | --- |
| **Actors** | Vehicle Occupant |
| **Pre-conditions** | The Ignition Status is in Run  The vehicle transmission is in Park OR vehicle speed is less than the Driving Restriction threshold\* for a manual transmission  Profile A is active. |
| **Scenario Description** | 1.The driver adjusts the seat or mirror position  2.The driver chooses the ‘Restore’ button after dialog displayed |
| **Post-conditions** | The mirrors and seat position are restored to the settings stored in profile A previously |
| **List of Exception Use Cases** | If there no active driver profile present, DuerOS shall not display dialog. |
| **Interfaces** | Personalization Interface |
| **Notes** | \*Driving Restriction threshold is defined in DRIVE-RESv2-FUR-REQ-025157-HMI Driving Restriction |

### Requirement

#### ENMEM-REQ-xxx/x-Restore entrance

Driver can access the Restore option from the dialog:



#### ENMEM-REQ-xxx/x-Restore times

Pressing the ‘Restore’ button will send the recall command each time.

*Note: Restore function is same as ‘Sign into Driver Profile via HMI menu’ function, there are no times limit for recall event of the same profile.*

### White Box View

#### Activity Diagrams



#### Sequence Diagram

##### Click restore soft button after positional settings changed

**Constraints**

**Pre-Condition**

One profile is in activate state. And the user adjusts the left/right or seat position.

*Note: for this example, the current profile index is Pers\_3*

**Scenarios**

**Normal Usage**

Driver click the restore soft button from DuerOS dialog.

**Post-Condition**

The positional settings will be restored to the settings previously stored in the driver profile.



# Appendix: Reference Documents

|  |  |
| --- | --- |
| Reference # | Document Title |
| 1 | Enhanced Memory APIM Implementation Guide |
| 2 | Vehicle Settings APIM SPSS - feature/functions tied to Enhanced Memory (ex. Ambient Lighting Variant 2, Language update….) |
| 3 | APIM Enhanced Memory HMI specification |
| 4 | FBMP SPSS (Feature Based Message Protocol SPSS spec) |
| 5 | APIM Infotainment Diagnostic Specification with enhanced memory updates |
| 6 | EnhancedMemory\_SPSS\_HMI\_Mapping |