

**Research & Vehicle Technology**

**“Infotainment Systems Product Development”**

**Feature – Behavior Coaching Display Client v2**

**APIM Infotainment Subsystem Part Specific Specification (SPSS)**

Version 1.0

**UNCONTROLLED COPY IF PRINTED**

**Version Date: November 19, 2018**

**FORD CONFIDENTIALF**

**Revision History**

|  |  |  |  |
| --- | --- | --- | --- |
| **Date** | **Version** | **Notes** | |
| **November 19, 2018** | **1.0** | **Initial Release** |  |
|  |  |  |  |
|  |  |  |  |
|  |  | |  |
|  |  | |  |
|  |  | |  |
|  |  | |  |

**Table of Contents**

[Revision History 2](#_Toc530391903)

[1 Architectural Design 4](#_Toc530391904)

[1.1 EVBI-SV-REQ-333146/A-Behavior Coaching Display System 4](#_Toc530391905)

[1.2 EVBI-CLD-REQ-333147/A-Behavior Coaching Display Client 4](#_Toc530391906)

[1.3 BehaviorCoachingDisplayClient Interface 4](#_Toc530391907)

[1.3.1 EVBI-IIR-REQ-333148/A-BehaviorCoachingDisplayClient\_Tx 4](#_Toc530391908)

[1.3.2 EVBI-IIR-REQ-333149/A-BehaviorCoachingDisplayClient\_Rx 4](#_Toc530391909)

[1.4 EVBI-IIR-REQ-323259/A-Logical to Physical CAN signal mapping - Behavior Coaching Display 5](#_Toc530391910)

[2 Functional Definition 6](#_Toc530391911)

[2.1 EVBI-FUN-REQ-333151/A-Behavior Coaching Display Active 6](#_Toc530391912)

[2.1.1 Requirements 6](#_Toc530391913)

[2.1.2 Use Cases 6](#_Toc530391914)

[2.1.3 White Box View 7](#_Toc530391915)

[3 Appendix: Reference Documents 9](#_Toc530391916)

# Architectural Design

## EVBI-SV-REQ-333146/A-Behavior Coaching Display System

Internal Block Diagram



## EVBI-CLD-REQ-333147/A-Behavior Coaching Display Client

The behavior coaching display client outputs behavior coaching information to the user based on data received from the behavior coaching display server. Please refer to the relevant HMI specification for information on display format/rules.

## BehaviorCoachingDisplayClient Interface

### EVBI-IIR-REQ-333148/A-BehaviorCoachingDisplayClient\_Tx

This class does not transmit any signals. However, it provides output to the user.

### EVBI-IIR-REQ-333149/A-BehaviorCoachingDisplayClient\_Rx

#### MD-REQ-333150/A-BehaviorCoaching\_St

Message Type: Status

This signal communicates behavior coaching information.

|  |  |  |  |
| --- | --- | --- | --- |
| **Name** | **Literals** | **Value** | **Description** |
| AccelTip | - | - | Acceleration tip value (percent / 0.1 resolution) |
|  | 0.0 | 0x0 |  |
|  | 0.1 | 0x1 |  |
|  | … |  |  |
|  | 102.1 | 0x3FD |  |
|  | No\_Data\_Exists | 0x3FE |  |
|  | Faulty | 0x3FF |  |
| DecelTip | - | - | Deceleration tip value (percent / 0.1 resolution) |
|  | 0.0 | 0x0 |  |
|  | 0.1 | 0x1 |  |
|  | … |  |  |
|  | 102.1 | 0x3FD |  |
|  | No\_Data\_Exists | 0x3FE |  |
|  | Faulty | 0x3FF |  |
| VelTip | - | - | Velocity tip value (percent / 0.1 resolution) |
|  | 0.0 | 0x0 |  |
|  | 0.1 | 0x1 |  |
|  | … |  |  |
|  | 102.1 | 0x3FD |  |
|  | No\_Data\_Exists | 0x3FE |  |
|  | Faulty | 0x3FF |  |

## EVBI-IIR-REQ-323259/A-Logical to Physical CAN signal mapping - Behavior Coaching Display

This Behavior Coaching Display deployment table maps the Behavior Coaching Display logical signals to the physical CAN signals.

Note: This is for reference only. If there is a conflict between the name in the CAN signal name column and what is found in the actual CAN dB then the CAN dB takes precedent. Please bring to Ford’s attention if there is a conflict.

|  |  |  |
| --- | --- | --- |
| **Logical Signal Name** | | **CAN signal name** |
| BehaviorCoaching\_st | AccelTip | EcoCochA\_Pc\_Dsply |
| DecelTip | EcoCochDecel\_Pc\_Dsply |
| VelTip | EcoCochCrus\_Pc\_Dsply |

# Functional Definition

## EVBI-FUN-REQ-333151/A-Behavior Coaching Display Active

This function includes use-cases that describe the behavior coaching display feature in an active state.

### Requirements

#### EVBI-REQ-016430/A-Signals with Percent Values - Erroneous Values (TcSE ROIN-267327-1)

Signals with percent definitions should always receive values within a standard percent range: *0-100%.*

Individual signal definitions may include additional values outside of this range (i.e., 100.4%, 102.1%, etc); however, these erroneous values will be treated as a faulty signal and not be processed by the display client.

### Use Cases

#### EVBI-UC-REQ-016431/A-Behavior Coaching Display Selected (TcSE ROIN-291734)

**Linked Elements**

EVBI-REQ-016430/A-Signals with Percent Values - Erroneous Values (TcSE ROIN-267327-1)

|  |  |
| --- | --- |
| **Actors** | User |
| **Pre-conditions** | Ignition Status is equal to Run. |
| **Scenario Description** | The user selects the behavior coaching display. |
| **Post-conditions** | The behavior coaching display is active.  Current behavior coaching information is displayed to the user. |
| **List of Exception Use Cases** | E1 – Absence of new Behavior Coaching data |
| **Interfaces** | G-HMI, Vehicle System Interface |

#### EVBI-UC-REQ-016432/A-Absence of new Behavior Coaching data (TcSE ROIN-291735)

**Linked Elements**

EVBI-REQ-016430/A-Signals with Percent Values - Erroneous Values (TcSE ROIN-267327-1)

|  |  |
| --- | --- |
| **Actors** | User |
| **Pre-conditions** | Same as normal use case. |
| **Scenario Description** | The user selects the behavior coaching display and there is no new/updated data being sent to this display. |
| **Post-conditions** | The display functions as defined in the relevant HMI specification. |
| **List of Exception Use Cases** | N/A |
| **Interfaces** | G-HMI, Vehicle System Interface |

#### EVBI-UC-REQ-016433/A-Vehicle power mode change for Behavior Coaching (TcSE ROIN-291736)

**Linked Elements**

EVBI-REQ-016430/A-Signals with Percent Values - Erroneous Values (TcSE ROIN-267327-1)

|  |  |
| --- | --- |
| **Actors** | User |
| **Pre-conditions** | Ignition status is equal to Run.  Behavior coaching display is active. |
| **Scenario Description** | Ignition status changes to a value less than run. |
| **Post-conditions** | The display functions as defined in the relevant HMI specification. |
| **List of Exception Use Cases** | N/A |
| **Interfaces** | G-HMI, Vehicle System Interface |

### White Box View

#### Activity Diagrams

##### EVBI-ACT-REQ-333152/A-Behavior Coaching Display Selected

**Linked Elements**

EVBI-SD-REQ-333153/A-Behavior Coaching Display Selected



#### White Box Scenarios

##### EVBI-SD-REQ-333153/A-Behavior Coaching Display Selected



# Appendix: Reference Documents

|  |  |
| --- | --- |
| Reference # | Document Title |
| 1 |  |
| 2 |  |
| 3 |  |
| 4 |  |
| 5 |  |