|  |  |  |
| --- | --- | --- |
| **TEST REPORT**  **Ford Motor (Nanjing) Research and Engineering Co., Ltd.**  Asia Pacific Region  Product Development | | DISPOSE of Copies  (Black Stamped) by  RETAIN Master.Copy  (Red Stamped) thru  GIS Item No |
| **PROGRAM:** MY23 CDX707  **Milestone:** PEC | **TO:** PMT5  **DVP Team:**  **REQ ENG:** | |
| **RQMT ID:** N/A  **RQMT TITLE:** SYNC FUNCTIONAL TESTING\_Camera  **PRIORITY LEVEL:** | **DVM ID:** N/A  **DVM TITLE:** N/A  **DVM TYPE:** | |
| **PART NUMBER:**  **NOTE:** | **Vehicle:** LV645  (VIN: LVSHNCAC2NH999988)  **Location:** REC, Nanjing, China | |
| **RESULT:**  Failed    Notes:   * 手动进入360界面或360延时显示时，要按两次Camera键才能退出360界面 APIMCIM-8055 * 需求变更超速时按Camera键进入360的提醒没有实现； * 需求变更360延时显示切换到前视没有实现； * 乌龟图没有白天黑夜区分 APIMCIM-7931 * 雷达PrkSns\_D\_Stat为Off时，乌龟图色块显示错误，应为透明 APIMCIM-7630 | | |
| **Tool CALIBRATION:**  Tool used, calibration Number | | |
| **TESTED BY:**  Liu Shiwang (sliu141)  06/29/2022 | **APPROVED BY:** | |